<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Transformers For DC/DC Converter - WE-FLYLT&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; 
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-11-17&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-FLYLT_EP10_6052">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP10,SMT,8pins
&lt;br&gt;Bobbin: 070-6052</description>
</package>
<package name="WE-FLYLT_EP13_5465">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP13,SMT,10pins
&lt;br&gt;Bobbin: 070-5465</description>
</package>
<package name="WE-FLYLT_EP7_5801">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP7,SMT,6pins
&lt;br&gt;Bobbin: 070-5801</description>
</package>
<package name="WE-FLYLT_EP7_4436">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EP7,SMT,8pins
&lt;br&gt;Bobbin: 070-4436</description>
</package>
<package name="WE-FLYLT_EP7_0353">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP7,SMT,6pins
&lt;br&gt;Bobbin: 071-0353</description>
</package>
<package name="WE-FLYLT_EP13_2381">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP13,SMT,10pins
&lt;br&gt;Bobbin: 070-2381</description>
</package>
</packages>
<symbols>
<symbol name="750315826">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="750313970">
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="750315825">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="750313975">
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="750313974">
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="750313972">
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="750315126">
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="750313973">
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="750313976">
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="750315125">
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="750313460">
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="750313457">
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="750313445">
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="750313442">
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="750313441">
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="750313443">
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="750313439">
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="750312558">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="750312366">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="750312504">
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="750311838">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="750312557">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="750312365">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="750312559">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="750312367">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="750311659">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="750311558">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="750311660">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="750315827">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="750315833">
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="750311559">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="750315830">
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="750315829">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="750315831">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="750311019">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="750315834">
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="750315832">
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="750315837">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="750315828">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="750315835">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="750315839">
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="750315836">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="750313976" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750313976"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP10_6052">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313976?ae"/>
<attribute name="IC-REFERENCE" value="LT8301"/>
<attribute name="IOUT1" value="35mA"/>
<attribute name="IOUT2" value="35mA"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="40uH"/>
<attribute name="LS" value="1uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:4:4"/>
<attribute name="PART-NUMBER" value=" 750313976 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750313976 "/>
<attribute name="VIN" value="8 - 32 V (DC)"/>
<attribute name="VOUT1" value="48V"/>
<attribute name="VOUT2" value="48V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313972" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750313972"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP10_6052">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313972?ae"/>
<attribute name="IC-REFERENCE" value="LT8301"/>
<attribute name="IOUT1" value="275mA"/>
<attribute name="IOUT2" value="275mA"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="40uH"/>
<attribute name="LS" value="1uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1:1"/>
<attribute name="PART-NUMBER" value=" 750313972 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750313972 "/>
<attribute name="VIN" value="18 - 42 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313970" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750313970"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP10_6052">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313970?ae"/>
<attribute name="IC-REFERENCE" value="LT8301"/>
<attribute name="IOUT1" value="500mA"/>
<attribute name="IOUT2" value="500mA"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="40uH"/>
<attribute name="LS" value="1uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:1:1"/>
<attribute name="PART-NUMBER" value=" 750313970 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750313970 "/>
<attribute name="VIN" value="18 - 42 V (DC)"/>
<attribute name="VOUT1" value="3.3V"/>
<attribute name="VOUT2" value="3.3V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313973" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750313973"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP10_6052">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313973?ae"/>
<attribute name="IC-REFERENCE" value="LT8301"/>
<attribute name="IOUT1" value="500mA"/>
<attribute name="IOUT2" value="500mA"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="40uH"/>
<attribute name="LS" value="1uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="4:1:1"/>
<attribute name="PART-NUMBER" value=" 750313973 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750313973 "/>
<attribute name="VIN" value="8 - 32 V (DC)"/>
<attribute name="VOUT1" value="3.3V"/>
<attribute name="VOUT2" value="3.3V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313974" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750313974"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP10_6052">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313974?ae"/>
<attribute name="IC-REFERENCE" value="LT8301"/>
<attribute name="IOUT1" value="360mA"/>
<attribute name="IOUT2" value="360mA"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="40uH"/>
<attribute name="LS" value="1uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="3:1:1"/>
<attribute name="PART-NUMBER" value=" 750313974 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750313974 "/>
<attribute name="VIN" value="8 - 32 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313443" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750313443"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP10_6052">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313443?ae"/>
<attribute name="IC-REFERENCE" value="LT8302"/>
<attribute name="IOUT1" value="375mA"/>
<attribute name="IOUT2" value="375mA"/>
<attribute name="ISAT" value="7.3A"/>
<attribute name="L" value="9uH"/>
<attribute name="LS" value="1uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1:1"/>
<attribute name="PART-NUMBER" value=" 750313443 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750313443 "/>
<attribute name="VIN" value="8 - 32 V (DC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313445" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750313445"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP10_6052">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5" route="any"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313445?ae"/>
<attribute name="IC-REFERENCE" value="LT8302"/>
<attribute name="IOUT1" value="320mA"/>
<attribute name="IOUT2" value="500mA"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="L" value="9uH"/>
<attribute name="LS" value="1uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2"/>
<attribute name="PART-NUMBER" value=" 750313445 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750313445 "/>
<attribute name="VIN" value="8 - 32 V (DC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VOUT2" value="3.3V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313460" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750313460"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP10_6052">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313460?ae"/>
<attribute name="IC-REFERENCE" value="LT8302"/>
<attribute name="IOUT1" value="1200mA"/>
<attribute name="IOUT2" value="500mA"/>
<attribute name="ISAT" value="7.75A"/>
<attribute name="L" value="12uH"/>
<attribute name="LS" value="1.5uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="4:1"/>
<attribute name="PART-NUMBER" value=" 750313460 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750313460 "/>
<attribute name="VIN" value="4 - 8 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="3.3V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313441" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750313441"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP10_6052">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313441?ae"/>
<attribute name="IC-REFERENCE" value="LT8302"/>
<attribute name="IOUT1" value="1750mA"/>
<attribute name="IOUT2" value="130mA"/>
<attribute name="ISAT" value="8A"/>
<attribute name="L" value="9uH"/>
<attribute name="LS" value="1.5uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:1"/>
<attribute name="PART-NUMBER" value=" 750313441 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750313441 "/>
<attribute name="VIN" value="8 - 32 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313457" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750313457"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP10_6052">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313457?ae"/>
<attribute name="IC-REFERENCE" value="LT8302"/>
<attribute name="IOUT1" value="180mA"/>
<attribute name="IOUT2" value="275mA"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="L" value="9uH"/>
<attribute name="LS" value="1uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2:2"/>
<attribute name="PART-NUMBER" value=" 750313457 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750313457 "/>
<attribute name="VIN" value="8 - 32 V (DC)"/>
<attribute name="VOUT1" value="48V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313975" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750313975"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP10_6052">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313975?ae"/>
<attribute name="IC-REFERENCE" value="LT8301"/>
<attribute name="IOUT1" value="70mA"/>
<attribute name="IOUT2" value="70mA"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="40uH"/>
<attribute name="LS" value="1uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2:2"/>
<attribute name="PART-NUMBER" value=" 750313975 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750313975 "/>
<attribute name="VIN" value="8 - 32 V (DC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VOUT2" value="24V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315836" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315836"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP13_5465">
<connects>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315836?ae"/>
<attribute name="IC-REFERENCE" value="LT8304"/>
<attribute name="IOUT1" value="600mA"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="L" value="40uH"/>
<attribute name="LS" value="0.9uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 750315836 "/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value=" 750315836 "/>
<attribute name="VIN" value="36 - 75 V (DC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315839" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315839"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP13_5465">
<connects>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315839?ae"/>
<attribute name="IC-REFERENCE" value="LT8304"/>
<attribute name="IOUT1" value="12mA"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="L" value="40uH"/>
<attribute name="LS" value="0.5uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:10"/>
<attribute name="PART-NUMBER" value=" 750315839 "/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value=" 750315839 "/>
<attribute name="VIN" value="4 - 36 V (DC)"/>
<attribute name="VOUT1" value="200V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315829" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315829"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_5801">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315829?ae"/>
<attribute name="IC-REFERENCE" value="LT8303"/>
<attribute name="IOUT1" value="130mA"/>
<attribute name="IOUT2" value="375mA"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="150uH"/>
<attribute name="LS" value="3uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 750315829 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750315829 "/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315830" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315830"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_5801">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315830?ae"/>
<attribute name="IC-REFERENCE" value="LT8303"/>
<attribute name="IOUT1" value="60mA"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="150uH"/>
<attribute name="LS" value="3.8uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2"/>
<attribute name="PART-NUMBER" value=" 750315830 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750315830 "/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VOUT1" value="48V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315827" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315827"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_5801">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315827?ae"/>
<attribute name="IC-REFERENCE" value="LT8303"/>
<attribute name="IOUT1" value="580mA"/>
<attribute name="IOUT2" value="35mA"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="150uH"/>
<attribute name="LS" value="3.6uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="4:1"/>
<attribute name="PART-NUMBER" value=" 750315827 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750315827 "/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="48V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315126" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315126"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP13_5465">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315126?ae"/>
<attribute name="IC-REFERENCE" value="LT8304"/>
<attribute name="IOUT1" value="1250mA"/>
<attribute name="ISAT" value="3.8A"/>
<attribute name="L" value="40uH"/>
<attribute name="LS" value="1uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:1"/>
<attribute name="PART-NUMBER" value=" 750315126 "/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value=" 750315126 "/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313442" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750313442"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP10_6052">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6" route="any"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313442?ae"/>
<attribute name="IC-REFERENCE" value="LT8302"/>
<attribute name="IOUT1" value="1500mA"/>
<attribute name="IOUT2" value="350mA"/>
<attribute name="ISAT" value="7.3A"/>
<attribute name="L" value="12uH"/>
<attribute name="LS" value="1.5uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.5:1"/>
<attribute name="PART-NUMBER" value=" 750313442 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750313442 "/>
<attribute name="VIN" value="8 - 40 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315125" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315125"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP13_5465">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315125?ae"/>
<attribute name="IC-REFERENCE" value="LT8304"/>
<attribute name="IOUT1" value="4500mA"/>
<attribute name="ISAT" value="3.8A"/>
<attribute name="L" value="40uH"/>
<attribute name="LS" value="2uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="6:1"/>
<attribute name="PART-NUMBER" value=" 750315125 "/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value=" 750315125 "/>
<attribute name="VIN" value="18 - 72 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315837" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315837"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP13_5465">
<connects>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315837?ae"/>
<attribute name="IC-REFERENCE" value="LT8304"/>
<attribute name="IOUT1" value="300mA"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="L" value="40uH"/>
<attribute name="LS" value="1uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2"/>
<attribute name="PART-NUMBER" value=" 750315837 "/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value=" 750315837 "/>
<attribute name="VIN" value="36 - 75 V (DC)"/>
<attribute name="VOUT1" value="48V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313439" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750313439"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP10_6052">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313439?ae"/>
<attribute name="IC-REFERENCE" value="LT8302"/>
<attribute name="IOUT1" value="2000mA"/>
<attribute name="ISAT" value="8A"/>
<attribute name="L" value="12uH"/>
<attribute name="LS" value="1.5uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:1"/>
<attribute name="PART-NUMBER" value=" 750313439 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750313439 "/>
<attribute name="VIN" value="8 - 40 V (DC)"/>
<attribute name="VOUT1" value="3.3V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315825" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315825"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_5801">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315825?ae"/>
<attribute name="IC-REFERENCE" value="LT8303"/>
<attribute name="IOUT1" value="1000mA"/>
<attribute name="IOUT2" value="360mA"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="L" value="150uH"/>
<attribute name="LS" value="6uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="8:1"/>
<attribute name="PART-NUMBER" value=" 750315825 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750315825 "/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VOUT1" value="3.3V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315831" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315831"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_5801">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315831?ae"/>
<attribute name="IC-REFERENCE" value="LT8303"/>
<attribute name="IOUT1" value="350mA"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="150uH"/>
<attribute name="LS" value="8uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="10:1"/>
<attribute name="PART-NUMBER" value=" 750315831 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750315831 "/>
<attribute name="VIN" value="9 - 36 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315835" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315835"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP13_5465">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315835?ae"/>
<attribute name="IC-REFERENCE" value="LT8304"/>
<attribute name="IOUT1" value="4800mA"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="L" value="40uH"/>
<attribute name="LS" value="2uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="8:1"/>
<attribute name="PART-NUMBER" value=" 750315835 "/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value=" 750315835 "/>
<attribute name="VIN" value="36 - 75 V (DC)"/>
<attribute name="VOUT1" value="3.3V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315833" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315833"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_5801">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315833?ae"/>
<attribute name="IC-REFERENCE" value="LT8303"/>
<attribute name="IOUT1" value="130mA"/>
<attribute name="IOUT2" value="130mA"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="150uH"/>
<attribute name="LS" value="3uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:1:1"/>
<attribute name="PART-NUMBER" value=" 750315833 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750315833 "/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315826" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315826"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_5801">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315826?ae"/>
<attribute name="IC-REFERENCE" value="LT8303"/>
<attribute name="IOUT1" value="720mA"/>
<attribute name="IOUT2" value="70mA"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="L" value="150uH"/>
<attribute name="LS" value="4uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="6:1"/>
<attribute name="PART-NUMBER" value=" 750315826 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750315826 "/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="24V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315834" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315834"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_5801">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315834?ae"/>
<attribute name="IC-REFERENCE" value="LT8303"/>
<attribute name="IOUT1" value="350mA"/>
<attribute name="IOUT2" value="350mA"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="150uH"/>
<attribute name="LS" value="5.2uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="6:1:1"/>
<attribute name="PART-NUMBER" value=" 750315834 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750315834 "/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315832" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315832"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_5801">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315832?ae"/>
<attribute name="IC-REFERENCE" value="LT8303"/>
<attribute name="IOUT1" value="15mA"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="150uH"/>
<attribute name="LS" value="3.4uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:4"/>
<attribute name="PART-NUMBER" value=" 750315832 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750315832 "/>
<attribute name="VIN" value="9 - 36 V (DC)"/>
<attribute name="VOUT1" value="100V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315828" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315828"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_5801">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315828?ae"/>
<attribute name="IC-REFERENCE" value="LT8303"/>
<attribute name="IOUT1" value="260mA"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="150uH"/>
<attribute name="LS" value="3.2uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:1"/>
<attribute name="PART-NUMBER" value=" 750315828 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750315828 "/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750312558" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750312558"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_4436">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750312558?ae"/>
<attribute name="IC-REFERENCE" value="LT8300"/>
<attribute name="IOUT1" value="70mA"/>
<attribute name="IOUT2" value="70mA"/>
<attribute name="ISAT" value="0.54A"/>
<attribute name="L" value="300uH"/>
<attribute name="LS" value="4uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:1:1"/>
<attribute name="PART-NUMBER" value=" 750312558 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750312558 "/>
<attribute name="VAUX" value="5V"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750311838" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750311838"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_4436">
<connects>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750311838?ae"/>
<attribute name="IC-REFERENCE" value="LT8300"/>
<attribute name="IOUT1" value="70mA"/>
<attribute name="IOUT2" value="70mA"/>
<attribute name="ISAT" value="0.52A"/>
<attribute name="L" value="350uH"/>
<attribute name="LS" value="4.5uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:1:1"/>
<attribute name="PART-NUMBER" value=" 750311838 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750311838 "/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VOUT1" value="15V"/>
<attribute name="VOUT2" value="15V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750311659" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750311659"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_4436">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750311659?ae"/>
<attribute name="IC-REFERENCE" value="LT8300"/>
<attribute name="IOUT1" value="80mA"/>
<attribute name="ISAT" value="0.56A"/>
<attribute name="L" value="300uH"/>
<attribute name="LS" value="3uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="5:5:1"/>
<attribute name="PART-NUMBER" value=" 750311659 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750311659 "/>
<attribute name="VAUX" value="5V"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750311558" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750311558"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_4436">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750311558?ae"/>
<attribute name="IC-REFERENCE" value="LT8300"/>
<attribute name="IOUT1" value="400mA"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="L" value="300uH"/>
<attribute name="LS" value="3uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="4:1:1"/>
<attribute name="PART-NUMBER" value=" 750311558 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750311558 "/>
<attribute name="VAUX" value="5V"/>
<attribute name="VIN" value="35 - 75 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750311660" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750311660"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_4436">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750311660?ae"/>
<attribute name="IC-REFERENCE" value="LT8300"/>
<attribute name="IOUT1" value="140mA"/>
<attribute name="IOUT2" value="70mA"/>
<attribute name="ISAT" value="0.52A"/>
<attribute name="L" value="350uH"/>
<attribute name="LS" value="4.5uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="6:3:1"/>
<attribute name="PART-NUMBER" value=" 750311660 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750311660 "/>
<attribute name="VAUX" value="5V"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VOUT1" value="15V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750311559" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750311559"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_4436">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750311559?ae"/>
<attribute name="IC-REFERENCE" value="LT8300"/>
<attribute name="IOUT1" value="400mA"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="175uH"/>
<attribute name="LS" value="3uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="4:1:1"/>
<attribute name="PART-NUMBER" value=" 750311559 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750311559 "/>
<attribute name="VAUX" value="5V"/>
<attribute name="VIN" value="35 - 75 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750311019" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750311019"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_4436">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750311019?ae"/>
<attribute name="IC-REFERENCE" value="LT8300"/>
<attribute name="IOUT1" value="600mA"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="L" value="400uH"/>
<attribute name="LS" value="8uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="6:1:2"/>
<attribute name="PART-NUMBER" value=" 750311019 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750311019 "/>
<attribute name="VAUX" value="6.6V"/>
<attribute name="VIN" value="35 - 75 V (DC)"/>
<attribute name="VOUT1" value="3.3V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750312559" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750312559"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_0353">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750312559?ae"/>
<attribute name="IC-REFERENCE" value="LT8300"/>
<attribute name="IOUT1" value="70mA"/>
<attribute name="IOUT2" value="70mA"/>
<attribute name="ISAT" value="0.45A"/>
<attribute name="L" value="300uH"/>
<attribute name="LS" value="4uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 750312559 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750312559 "/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VOUT2" value="15V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750312367" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750312367"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_0353">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750312367?ae"/>
<attribute name="IC-REFERENCE" value="LT8300"/>
<attribute name="IOUT1" value="500mA"/>
<attribute name="ISAT" value="0.45A"/>
<attribute name="L" value="300uH"/>
<attribute name="LS" value="4uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="8.4:1"/>
<attribute name="PART-NUMBER" value=" 750312367 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750312367 "/>
<attribute name="VAUX" value="5V"/>
<attribute name="VIN" value="22 - 72 V (DC)"/>
<attribute name="VOUT1" value="3.3V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750312557" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750312557"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_0353">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750312557?ae"/>
<attribute name="IC-REFERENCE" value="LT8300"/>
<attribute name="IOUT1" value="380mA"/>
<attribute name="ISAT" value="0.45A"/>
<attribute name="L" value="300uH"/>
<attribute name="LS" value="5uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="6:1"/>
<attribute name="PART-NUMBER" value=" 750312557 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750312557 "/>
<attribute name="VAUX" value="5V"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750312365" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750312365"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_0353">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750312365?ae"/>
<attribute name="IC-REFERENCE" value="LT8300"/>
<attribute name="IOUT1" value="300mA"/>
<attribute name="ISAT" value="0.6A"/>
<attribute name="L" value="300uH"/>
<attribute name="LS" value="4uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="4:1"/>
<attribute name="PART-NUMBER" value=" 750312365 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750312365 "/>
<attribute name="VAUX" value="6.6V"/>
<attribute name="VIN" value="30 - 72 V (DC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750312366" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750312366"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP7_0353">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750312366?ae"/>
<attribute name="IC-REFERENCE" value="LT8300"/>
<attribute name="IOUT1" value="300mA"/>
<attribute name="ISAT" value="0.58A"/>
<attribute name="L" value="400uH"/>
<attribute name="LS" value="8uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="7.11:1"/>
<attribute name="PART-NUMBER" value=" 750312366 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750312366 "/>
<attribute name="VAUX" value="5V"/>
<attribute name="VIN" value="18 - 75 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="1500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750312504" prefix="T">
<description>&lt;b&gt;WE-FLYLT Flyback Transformers for Linear Technology
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Characteristics
&lt;br&gt; Low leakage inductance
&lt;br&gt; High saturation current for low-power, DC/DC transformers
&lt;br&gt; Self-shielding and space efficient
&lt;br&gt; Functional insulation
&lt;br&gt; Isolation voltage: Up to 1875VAC at 1 second
&lt;br&gt; Lead free and RoHS compliant
&lt;br&gt; Operating temp: -40°C to 125°C
&lt;br&gt; Package sizes: EP7, EP10, EP13 and ETD34
&lt;br&gt; Designed to meet IEC/UL/EN60950-1
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial &amp; medical power supplies
&lt;br&gt; Isolated auxiliary/housekeeping power supplies
&lt;br&gt; Isolated DC/DC supplies
&lt;br&gt; Home automation

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o718711v209%20family-WE-UtFLYLT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-FLYLT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-FLYLT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-11-17&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750312504"/>
</gates>
<devices>
<device name="" package="WE-FLYLT_EP13_2381">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750312504?ae"/>
<attribute name="IC-REFERENCE" value="LTC3300"/>
<attribute name="IOUT1" value="250mA"/>
<attribute name="ISAT" value="10.2A"/>
<attribute name="L" value="3.46uH"/>
<attribute name="LS" value="0.12uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 750312504 "/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value=" 750312504 "/>
<attribute name="VIN" value="2 - 5.5 V (DC)"/>
<attribute name="VOUT1" value="20V"/>
<attribute name="VT" value="500V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
