<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Signal &amp; Communications - Signal Transformers - WE-LAN&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-05-13&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="7490100110A">
<description>&lt;B&gt;WE-LAN LAN Transformer 
&lt;/B&gt;&lt;Br&gt;&lt;Br&gt;10/100BASE-TX</description>
</package>
<package name="7490220123">
<description>&lt;B&gt;WE-LAN LAN Transformer 
&lt;/B&gt;&lt;Br&gt;&lt;Br&gt;1000 Base-T</description>
</package>
<package name="7490100111A">
<description>&lt;B&gt;WE-LAN LAN Transformer 
&lt;/B&gt;&lt;Br&gt;&lt;Br&gt;10/100BASE-TX</description>
</package>
<package name="7490220115">
<description>&lt;B&gt;WE-LAN LAN Transformer 1000 Base-T</description>
</package>
<package name="749020100A">
<description>&lt;B&gt;WE-LAN LAN Transformer 1000 Base-T</description>
</package>
<package name="749020111A">
<description>&lt;B&gt;WE-LAN LAN Transformer 
&lt;/B&gt;&lt;Br&gt;&lt;Br&gt;1000 Base-T</description>
</package>
<package name="7490140122B">
<description>&lt;B&gt;WE-LAN LAN Transformer 10/100 Base-T</description>
</package>
<package name="7490140125">
<description>&lt;b&gt;WE-LAN&lt;/b&gt;&lt;br&gt;100BT 1 Port SMT OH Transformer,1 Port,24Pins</description>
</package>
<package name="749020022A">
<description>&lt;B&gt;WE-LAN LAN Transformer 1000 Base-T</description>
</package>
<package name="7490240120">
<description>&lt;b&gt;WE-LAN&lt;/b&gt;&lt;br&gt;1000BT 1 Port Medical ETR SMT Transformer,40Pins</description>
</package>
<package name="7490240142">
<description>&lt;b&gt;WE-LAN&lt;/b&gt;&lt;br&gt; 1000BT OH 1 Port SMT Transformer,24Pins</description>
</package>
<package name="7490140123">
<description>&lt;b&gt;WE-LAN&lt;/b&gt;&lt;br&gt;100BT 1 Port SMT OH Transformer,16Pins</description>
</package>
<package name="7490120110">
<description>&lt;B&gt;WE-LAN LAN Transformer 10/100 Base-T</description>
</package>
<package name="7490140141">
<description>&lt;b&gt;WE-LAN&lt;/b&gt;&lt;br&gt;100BT 1 Port PoE+ SMD Transformer,12Pins</description>
</package>
<package name="7490140112">
<description>&lt;B&gt;WE-LAN LAN Transformer 10/100 Base-T</description>
</package>
<package name="749023010A">
<description>&lt;B&gt;WE-LAN LAN Transformer 
&lt;/B&gt;&lt;Br&gt;&lt;Br&gt;1000 Base-T</description>
</package>
<package name="7490140142">
<description>&lt;b&gt;WE-LAN&lt;/b&gt;&lt;br&gt;100BT 1 Port SMT OH SMD Transformer,24Pins</description>
</package>
<package name="7490220122">
<description>&lt;B&gt;WE-LAN LAN Transformer 1000 Base-T</description>
</package>
<package name="749014012">
<description>&lt;B&gt;WE-LAN LAN Transformer 10/100 Base-T</description>
</package>
<package name="7490100161A">
<description>&lt;B&gt;WE-LAN LAN Transformer 
&lt;/B&gt;&lt;Br&gt;&lt;Br&gt;10/100 Base-T</description>
</package>
<package name="749020010A">
<description>&lt;B&gt;WE-LAN LAN Transformer 
&lt;/B&gt;&lt;Br&gt;&lt;Br&gt;1000 Base-T</description>
</package>
<package name="7490220120">
<description>&lt;B&gt;WE-LAN LAN Transformer 1000 Base-T</description>
</package>
<package name="7490240121">
<description>&lt;b&gt;WE-LAN&lt;/b&gt;&lt;br&gt;1000BT 1 Port SMT OH SMT Transformer,48Pins</description>
</package>
<package name="7490140117C">
<description>&lt;B&gt;WE-LAN LAN Transformer 10/100 Base-T</description>
</package>
<package name="749020023A">
<description>&lt;B&gt;WE-LAN LAN Transformer 
&lt;/B&gt;&lt;Br&gt;&lt;Br&gt;1000 Base-T</description>
</package>
<package name="749023113C">
<description>&lt;b&gt;WE-LAN LAN Transformer
&lt;br&gt;&lt;/b&gt;24pins, pitch 1.27mm</description>
</package>
<package name="749082010">
<description>&lt;b&gt;WE-LAN LAN Transformer
&lt;br&gt;&lt;/b&gt;24pins, pitch 1.27mm</description>
</package>
<package name="7490220121">
<description>&lt;B&gt;WE-LAN LAN Transformer 1000 Base-T</description>
</package>
<package name="749013011A">
<description>&lt;B&gt;WE-LAN LAN Transformer 
&lt;/B&gt;&lt;Br&gt;&lt;Br&gt;10/100 Base-T</description>
</package>
<package name="7490140123B">
<description>&lt;B&gt;WE-LAN LAN Transformer 10/100 Base-T</description>
</package>
<package name="7490240141">
<description>&lt;b&gt;WE-LAN&lt;/b&gt;&lt;br&gt;10/100 Base-T SMT Transformer,1 Port,48Pins</description>
</package>
<package name="749024015C">
<description>&lt;B&gt;WE-LAN LAN Transformer 10/100 Base-T</description>
</package>
<package name="7490140140">
<description>&lt;b&gt;WE-LAN&lt;/b&gt;&lt;br&gt;100BT 1 Port SMT OH SMD Transformer,16Pins</description>
</package>
<package name="749010012A">
<description>&lt;B&gt;WE-LAN LAN Transformer 
&lt;/B&gt;&lt;Br&gt;&lt;Br&gt;10/100 Base-T</description>
</package>
<package name="749020011A">
<description>&lt;B&gt;WE-LAN LAN Transformer 
&lt;/B&gt;&lt;Br&gt;&lt;Br&gt;1000 Base-T</description>
</package>
<package name="7490240140">
<description>&lt;b&gt;WE-LAN&lt;/b&gt;&lt;br&gt;1000BT 1 Port Medical ETR SMT Transformer,40Pins</description>
</package>
<package name="7490140124">
<description>&lt;b&gt;WE-LAN&lt;/b&gt;&lt;br&gt;100BT 1 Port PoE+ SMD Transformer,12Pins</description>
</package>
<package name="749080010">
<description>&lt;b&gt;WE-LAN LAN Transformer
&lt;br&gt;&lt;/b&gt;24pins, pitch 0.99mm</description>
</package>
<package name="749020112B">
<description>&lt;b&gt;WE-LAN LAN Transformer
&lt;br&gt;&lt;/b&gt;24pins, pitch 1.27mm</description>
</package>
</packages>
<symbols>
<symbol name="2CHANNELS">
<pin name="RX+" direction="pas"/>
<pin name="CRX" direction="pas"/>
<pin name="RX-" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="RD+" direction="pas"/>
<pin name="TX+" direction="pas"/>
<pin name="CTX" direction="pas"/>
<pin name="TX-" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="TD+" direction="pas"/>
</symbol>
<symbol name="4CHANNELS">
<pin name="D1+" direction="pas"/>
<pin name="CD1" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="X1-" direction="pas"/>
<pin name="CX1" direction="pas"/>
<pin name="X1+" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="CD2" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="X2-" direction="pas"/>
<pin name="CX2" direction="pas"/>
<pin name="X2+" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="CD3" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="X3-" direction="pas"/>
<pin name="CX3" direction="pas"/>
<pin name="X3+" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="CD4" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="X4-" direction="pas"/>
<pin name="CX4" direction="pas"/>
<pin name="X4+" direction="pas"/>
</symbol>
<symbol name="2CHANNELS-1">
<pin name="RX+" direction="pas"/>
<pin name="CRX" direction="pas"/>
<pin name="RX-" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="RD+" direction="pas"/>
<pin name="TX+" direction="pas"/>
<pin name="CTX" direction="pas"/>
<pin name="TX-" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="TD+" direction="pas"/>
</symbol>
<symbol name="8CHANNELS">
<pin name="CD1" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="X1-" direction="pas"/>
<pin name="X1+" direction="pas"/>
<pin name="CX1" direction="pas"/>
<pin name="CD2" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="X2-" direction="pas"/>
<pin name="X2+" direction="pas"/>
<pin name="CX2" direction="pas"/>
<pin name="CD3" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="X3-" direction="pas"/>
<pin name="X3+" direction="pas"/>
<pin name="CX3" direction="pas"/>
<pin name="CD4" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="X4-" direction="pas"/>
<pin name="X4+" direction="pas"/>
<pin name="CX4" direction="pas"/>
<pin name="CD5" direction="pas"/>
<pin name="D5+" direction="pas"/>
<pin name="D5-" direction="pas"/>
<pin name="X5-" direction="pas"/>
<pin name="X5+" direction="pas"/>
<pin name="CX5" direction="pas"/>
<pin name="CD6" direction="pas"/>
<pin name="D6+" direction="pas"/>
<pin name="D6-" direction="pas"/>
<pin name="X6-" direction="pas"/>
<pin name="X6+" direction="pas"/>
<pin name="CX6" direction="pas"/>
<pin name="CD7" direction="pas"/>
<pin name="D7+" direction="pas"/>
<pin name="D7-" direction="pas"/>
<pin name="X7-" direction="pas"/>
<pin name="X7+" direction="pas"/>
<pin name="CX7" direction="pas"/>
<pin name="CD8" direction="pas"/>
<pin name="D8+" direction="pas"/>
<pin name="D8-" direction="pas"/>
<pin name="X8-" direction="pas"/>
<pin name="X8+" direction="pas"/>
<pin name="CX8" direction="pas"/>
</symbol>
<symbol name="4CHANNELS-1">
<pin name="D1+" direction="pas"/>
<pin name="CD1" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="X1-" direction="pas"/>
<pin name="CX1" direction="pas"/>
<pin name="X1+" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="CD2" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="X2-" direction="pas"/>
<pin name="CX2" direction="pas"/>
<pin name="X2+" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="CD3" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="X3-" direction="pas"/>
<pin name="CX3" direction="pas"/>
<pin name="X3+" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="CD4" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="X4-" direction="pas"/>
<pin name="CX4" direction="pas"/>
<pin name="X4+" direction="pas"/>
</symbol>
<symbol name="2CHANNELS_2">
<pin name="RX+" direction="pas"/>
<pin name="CRX" direction="pas"/>
<pin name="RX-" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="RD+" direction="pas"/>
<pin name="TX+" direction="pas"/>
<pin name="CTX" direction="pas"/>
<pin name="TX-" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="TD+" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="7490100110A" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-03-21&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS"/>
</gates>
<devices>
<device name="" package="7490100110A">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CRX" pad="10"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="CTX" pad="15"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="11"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="16"/>
<connect gate="G$1" pin="TX-" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-TX"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490100110A?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="7490100110A"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490100110A"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490220115" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="7490220115">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100/1000BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490220115?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7490220115"/>
<attribute name="POE" value="4PPoE (up to 800 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490220115"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490220123" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-03-21&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="7490220123">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490220123?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="180uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="7490220123"/>
<attribute name="POE" value="4PPoE (up to 1500 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490220123"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490100111A" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-03-21&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS"/>
</gates>
<devices>
<device name="" package="7490100111A">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CRX" pad="10"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="CTX" pad="15"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="11"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="16"/>
<connect gate="G$1" pin="TX-" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-TX"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490100111A?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="7490100111A"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490100111A"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749020100A" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS"/>
</gates>
<devices>
<device name="" package="749020100A">
<connects>
<connect gate="G$1" pin="CRD" pad="6"/>
<connect gate="G$1" pin="CRX" pad="11"/>
<connect gate="G$1" pin="CTD" pad="3"/>
<connect gate="G$1" pin="CTX" pad="14"/>
<connect gate="G$1" pin="RD+" pad="7"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="10"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="G$1" pin="TX+" pad="16"/>
<connect gate="G$1" pin="TX-" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100/1000BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749020100A?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="749020100A"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 0.5 "/>
<attribute name="VALUE" value="749020100A"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490140122B" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS"/>
</gates>
<devices>
<device name="" package="7490140122B">
<connects>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CRX" pad="8"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="CTX" pad="11"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="RX+" pad="9"/>
<connect gate="G$1" pin="RX-" pad="7"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="12"/>
<connect gate="G$1" pin="TX-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490140122B?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7490140122B"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490140122B"/>
<attribute name="VT" value="4500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490140125" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Created by Ella Wu, 2020-07-08&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS-1"/>
</gates>
<devices>
<device name="" package="7490140125">
<connects>
<connect gate="G$1" pin="CRD" pad="10"/>
<connect gate="G$1" pin="CRX" pad="15"/>
<connect gate="G$1" pin="CTD" pad="1"/>
<connect gate="G$1" pin="CTX" pad="24"/>
<connect gate="G$1" pin="RD+" pad="11"/>
<connect gate="G$1" pin="RD-" pad="12"/>
<connect gate="G$1" pin="RX+" pad="14"/>
<connect gate="G$1" pin="RX-" pad="13"/>
<connect gate="G$1" pin="TD+" pad="2"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="23"/>
<connect gate="G$1" pin="TX-" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490140125?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7490140125"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490140125"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749020111A" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-03-21&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="749020111A">
<connects>
<connect gate="G$1" pin="CD1" pad="3"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="9"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="22"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="16"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="2"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="7"/>
<connect gate="G$1" pin="D3-" pad="8"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="24"/>
<connect gate="G$1" pin="X1-" pad="23"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="18"/>
<connect gate="G$1" pin="X3-" pad="17"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749020111A?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="749020111A"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="749020111A"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749020022A" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8CHANNELS"/>
</gates>
<devices>
<device name="" package="749020022A">
<connects>
<connect gate="G$1" pin="CD1" pad="2"/>
<connect gate="G$1" pin="CD2" pad="5"/>
<connect gate="G$1" pin="CD3" pad="8"/>
<connect gate="G$1" pin="CD4" pad="11"/>
<connect gate="G$1" pin="CD5" pad="15"/>
<connect gate="G$1" pin="CD6" pad="18"/>
<connect gate="G$1" pin="CD7" pad="21"/>
<connect gate="G$1" pin="CD8" pad="24"/>
<connect gate="G$1" pin="CX1" pad="49"/>
<connect gate="G$1" pin="CX2" pad="46"/>
<connect gate="G$1" pin="CX3" pad="43"/>
<connect gate="G$1" pin="CX4" pad="40"/>
<connect gate="G$1" pin="CX5" pad="36"/>
<connect gate="G$1" pin="CX6" pad="33"/>
<connect gate="G$1" pin="CX7" pad="30"/>
<connect gate="G$1" pin="CX8" pad="27"/>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="7"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="10"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="D5+" pad="14"/>
<connect gate="G$1" pin="D5-" pad="16"/>
<connect gate="G$1" pin="D6+" pad="17"/>
<connect gate="G$1" pin="D6-" pad="19"/>
<connect gate="G$1" pin="D7+" pad="20"/>
<connect gate="G$1" pin="D7-" pad="22"/>
<connect gate="G$1" pin="D8+" pad="23"/>
<connect gate="G$1" pin="D8-" pad="25"/>
<connect gate="G$1" pin="X1+" pad="48"/>
<connect gate="G$1" pin="X1-" pad="50"/>
<connect gate="G$1" pin="X2+" pad="47"/>
<connect gate="G$1" pin="X2-" pad="45"/>
<connect gate="G$1" pin="X3+" pad="42"/>
<connect gate="G$1" pin="X3-" pad="44"/>
<connect gate="G$1" pin="X4+" pad="41"/>
<connect gate="G$1" pin="X4-" pad="39"/>
<connect gate="G$1" pin="X5+" pad="35"/>
<connect gate="G$1" pin="X5-" pad="37"/>
<connect gate="G$1" pin="X6+" pad="34"/>
<connect gate="G$1" pin="X6-" pad="32"/>
<connect gate="G$1" pin="X7+" pad="29"/>
<connect gate="G$1" pin="X7-" pad="31"/>
<connect gate="G$1" pin="X8+" pad="28"/>
<connect gate="G$1" pin="X8-" pad="26"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749020022A?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="749020022A"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 2 "/>
<attribute name="VALUE" value="749020022A"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490240120" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS-1"/>
</gates>
<devices>
<device name="" package="7490240120">
<connects>
<connect gate="G$1" pin="CD1" pad="2"/>
<connect gate="G$1" pin="CD2" pad="7"/>
<connect gate="G$1" pin="CD3" pad="12"/>
<connect gate="G$1" pin="CD4" pad="17"/>
<connect gate="G$1" pin="CX1" pad="39"/>
<connect gate="G$1" pin="CX2" pad="34"/>
<connect gate="G$1" pin="CX3" pad="29"/>
<connect gate="G$1" pin="CX4" pad="24"/>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="6"/>
<connect gate="G$1" pin="D2-" pad="8"/>
<connect gate="G$1" pin="D3+" pad="11"/>
<connect gate="G$1" pin="D3-" pad="13"/>
<connect gate="G$1" pin="D4+" pad="16"/>
<connect gate="G$1" pin="D4-" pad="18"/>
<connect gate="G$1" pin="X1+" pad="40"/>
<connect gate="G$1" pin="X1-" pad="38"/>
<connect gate="G$1" pin="X2+" pad="35"/>
<connect gate="G$1" pin="X2-" pad="33"/>
<connect gate="G$1" pin="X3+" pad="30"/>
<connect gate="G$1" pin="X3-" pad="28"/>
<connect gate="G$1" pin="X4+" pad="25"/>
<connect gate="G$1" pin="X4-" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490240120?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="7490240120"/>
<attribute name="POE" value="4PPoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490240120"/>
<attribute name="VT" value="4000VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490240142" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Created by Ella Wu, 2020-07-08
&lt;br&gt;2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS-1"/>
</gates>
<devices>
<device name="" package="7490240142">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490240142?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7490240142"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490240142"/>
<attribute name="VT" value="4000VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490140123" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS-1"/>
</gates>
<devices>
<device name="" package="7490140123">
<connects>
<connect gate="G$1" pin="CRD" pad="6"/>
<connect gate="G$1" pin="CRX" pad="11"/>
<connect gate="G$1" pin="CTD" pad="1"/>
<connect gate="G$1" pin="CTX" pad="16"/>
<connect gate="G$1" pin="RD+" pad="7"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="10"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="2"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="15"/>
<connect gate="G$1" pin="TX-" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490140123?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7490140123"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490140123"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490120110" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS"/>
</gates>
<devices>
<device name="" package="7490120110">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CRX" pad="10"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="CTX" pad="15"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="11"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="16"/>
<connect gate="G$1" pin="TX-" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-TX"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490120110?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="120uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7490120110"/>
<attribute name="POE" value="PoE+ (up to 720 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490120110"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490140141" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Created by Ella Wu, 2020-07-08&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS-1"/>
</gates>
<devices>
<device name="" package="7490140141">
<connects>
<connect gate="G$1" pin="CRD" pad="4"/>
<connect gate="G$1" pin="CRX" pad="9"/>
<connect gate="G$1" pin="CTD" pad="1"/>
<connect gate="G$1" pin="CTX" pad="12"/>
<connect gate="G$1" pin="RD+" pad="5"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="RX+" pad="8"/>
<connect gate="G$1" pin="RX-" pad="7"/>
<connect gate="G$1" pin="TD+" pad="2"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="11"/>
<connect gate="G$1" pin="TX-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490140141?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7490140141"/>
<attribute name="POE" value="PoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490140141"/>
<attribute name="VT" value="4000VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749023010A" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-03-21&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="749023010A">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749023010A?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="749023010A"/>
<attribute name="POE" value="PoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="749023010A"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490140142" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Created by Ella Wu, 2020-07-08&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS-1"/>
</gates>
<devices>
<device name="" package="7490140142">
<connects>
<connect gate="G$1" pin="CRD" pad="10"/>
<connect gate="G$1" pin="CRX" pad="15"/>
<connect gate="G$1" pin="CTD" pad="1"/>
<connect gate="G$1" pin="CTX" pad="24"/>
<connect gate="G$1" pin="RD+" pad="11"/>
<connect gate="G$1" pin="RD-" pad="12"/>
<connect gate="G$1" pin="RX+" pad="14"/>
<connect gate="G$1" pin="RX-" pad="13"/>
<connect gate="G$1" pin="TD+" pad="2"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="23"/>
<connect gate="G$1" pin="TX-" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490140142?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7490140142"/>
<attribute name="POE" value="PoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490140142"/>
<attribute name="VT" value="4000VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490140112" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-07-17&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS"/>
</gates>
<devices>
<device name="" package="7490140112">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CRX" pad="10"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="CTX" pad="15"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="11"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="16"/>
<connect gate="G$1" pin="TX-" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490140112?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7490140112"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490140112"/>
<attribute name="VT" value="6000VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490220122" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="7490220122">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100/1000BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490220122?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="7490220122"/>
<attribute name="POE" value="4PPoE (up to 1000 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490220122"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749014012" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-07-17&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS_2"/>
</gates>
<devices>
<device name="" package="749014012">
<connects>
<connect gate="G$1" pin="CRD" pad="2"/>
<connect gate="G$1" pin="CRX" pad="15"/>
<connect gate="G$1" pin="CTD" pad="7"/>
<connect gate="G$1" pin="CTX" pad="10"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="3"/>
<connect gate="G$1" pin="RX+" pad="16"/>
<connect gate="G$1" pin="RX-" pad="14"/>
<connect gate="G$1" pin="TD+" pad="6"/>
<connect gate="G$1" pin="TD-" pad="8"/>
<connect gate="G$1" pin="TX+" pad="11"/>
<connect gate="G$1" pin="TX-" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749014012?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="749014012"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="749014012"/>
<attribute name="VT" value="4000VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749020010A" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-03-21&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="749020010A">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749020010A?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="749020010A"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="749020010A"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490220120" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="7490220120">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100/1000BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490220120?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="7490220120"/>
<attribute name="POE" value="4PPoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490220120"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490100161A" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-03-21&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS"/>
</gates>
<devices>
<device name="" package="7490100161A">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CRX" pad="10"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="CTX" pad="15"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="11"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="16"/>
<connect gate="G$1" pin="TX-" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-TX"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490100161A?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value="7490100161A"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490100161A"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490240121" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Created by Ella Wu, 2020-07-08&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS-1"/>
</gates>
<devices>
<device name="" package="7490240121">
<connects>
<connect gate="G$1" pin="CD1" pad="2"/>
<connect gate="G$1" pin="CD2" pad="8"/>
<connect gate="G$1" pin="CD3" pad="14"/>
<connect gate="G$1" pin="CD4" pad="20"/>
<connect gate="G$1" pin="CX1" pad="47"/>
<connect gate="G$1" pin="CX2" pad="41"/>
<connect gate="G$1" pin="CX3" pad="35"/>
<connect gate="G$1" pin="CX4" pad="29"/>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="7"/>
<connect gate="G$1" pin="D2-" pad="9"/>
<connect gate="G$1" pin="D3+" pad="13"/>
<connect gate="G$1" pin="D3-" pad="15"/>
<connect gate="G$1" pin="D4+" pad="19"/>
<connect gate="G$1" pin="D4-" pad="21"/>
<connect gate="G$1" pin="X1+" pad="48"/>
<connect gate="G$1" pin="X1-" pad="46"/>
<connect gate="G$1" pin="X2+" pad="42"/>
<connect gate="G$1" pin="X2-" pad="40"/>
<connect gate="G$1" pin="X3+" pad="36"/>
<connect gate="G$1" pin="X3-" pad="34"/>
<connect gate="G$1" pin="X4+" pad="30"/>
<connect gate="G$1" pin="X4-" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490240121?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7490240121"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490240121"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490140117C" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 ��C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS"/>
</gates>
<devices>
<device name="" package="7490140117C">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CRX" pad="10"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="CTX" pad="15"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="11"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="16"/>
<connect gate="G$1" pin="TX-" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-TX"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490140117C?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="7490140117C"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490140117C"/>
<attribute name="VT" value="2500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749023113C" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="749023113C">
<connects>
<connect gate="G$1" pin="CD1" pad="3"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="9"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="22"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="16"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="2"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="7"/>
<connect gate="G$1" pin="D3-" pad="8"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="24"/>
<connect gate="G$1" pin="X1-" pad="23"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="18"/>
<connect gate="G$1" pin="X3-" pad="17"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100/1000BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749023113C?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="749023113C"/>
<attribute name="POE" value="PoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="749023113C"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749020023A" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-03-21&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="749020023A">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749020023A?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="749020023A"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="749020023A"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749082010" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="749082010">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="2.5/5G Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749082010?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="120uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="749082010"/>
<attribute name="POE" value="4PPoE (up to 1500 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="749082010"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490220121" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="7490220121">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100/1000BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490220121?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="7490220121"/>
<attribute name="POE" value="4PPoE (up to 600 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490220121"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749013011A" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-03-21&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS"/>
</gates>
<devices>
<device name="" package="749013011A">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CRX" pad="10"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="CTX" pad="15"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="11"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="16"/>
<connect gate="G$1" pin="TX-" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-TX"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749013011A?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="749013011A"/>
<attribute name="POE" value="PoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="749013011A"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490140123B" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2019-11-05&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS"/>
</gates>
<devices>
<device name="" package="7490140123B">
<connects>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CRX" pad="8"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="CTX" pad="11"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="RX+" pad="9"/>
<connect gate="G$1" pin="RX-" pad="7"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="12"/>
<connect gate="G$1" pin="TX-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490140123B?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7490140123B"/>
<attribute name="POE" value="PoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490140123B"/>
<attribute name="VT" value="4500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490240141" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Created by Ella Wu, 2020-07-08
&lt;br&gt;2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS-1"/>
</gates>
<devices>
<device name="" package="7490240141">
<connects>
<connect gate="G$1" pin="CD1" pad="2"/>
<connect gate="G$1" pin="CD2" pad="8"/>
<connect gate="G$1" pin="CD3" pad="14"/>
<connect gate="G$1" pin="CD4" pad="20"/>
<connect gate="G$1" pin="CX1" pad="47"/>
<connect gate="G$1" pin="CX2" pad="41"/>
<connect gate="G$1" pin="CX3" pad="35"/>
<connect gate="G$1" pin="CX4" pad="29"/>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="7"/>
<connect gate="G$1" pin="D2-" pad="9"/>
<connect gate="G$1" pin="D3+" pad="13"/>
<connect gate="G$1" pin="D3-" pad="15"/>
<connect gate="G$1" pin="D4+" pad="19"/>
<connect gate="G$1" pin="D4-" pad="21"/>
<connect gate="G$1" pin="X1+" pad="48"/>
<connect gate="G$1" pin="X1-" pad="46"/>
<connect gate="G$1" pin="X2+" pad="42"/>
<connect gate="G$1" pin="X2-" pad="40"/>
<connect gate="G$1" pin="X3+" pad="36"/>
<connect gate="G$1" pin="X3-" pad="34"/>
<connect gate="G$1" pin="X4+" pad="30"/>
<connect gate="G$1" pin="X4-" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490240141?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7490240141"/>
<attribute name="POE" value="4PPoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490240141"/>
<attribute name="VT" value="4000VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490140140" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Created by Ella Wu, 2020-07-08&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS-1"/>
</gates>
<devices>
<device name="" package="7490140140">
<connects>
<connect gate="G$1" pin="CRD" pad="6"/>
<connect gate="G$1" pin="CRX" pad="11"/>
<connect gate="G$1" pin="CTD" pad="1"/>
<connect gate="G$1" pin="CTX" pad="16"/>
<connect gate="G$1" pin="RD+" pad="7"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="10"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="2"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="15"/>
<connect gate="G$1" pin="TX-" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490140140?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7490140140"/>
<attribute name="POE" value="PoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490140140"/>
<attribute name="VT" value="4000VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749024015C" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="749024015C">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100/1000BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749024015C?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="749024015C"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="749024015C"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749010012A" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-03-21&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS"/>
</gates>
<devices>
<device name="" package="749010012A">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CRX" pad="10"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="CTX" pad="15"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="11"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="16"/>
<connect gate="G$1" pin="TX-" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-TX"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749010012A?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="749010012A"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="749010012A"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749020011A" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-03-21&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="749020011A">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749020011A?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="Yes"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="749020011A"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="749020011A"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490240140" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Created by Ella Wu, 2020-07-08
&lt;br&gt;2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS-1"/>
</gates>
<devices>
<device name="" package="7490240140">
<connects>
<connect gate="G$1" pin="CD1" pad="2"/>
<connect gate="G$1" pin="CD2" pad="7"/>
<connect gate="G$1" pin="CD3" pad="12"/>
<connect gate="G$1" pin="CD4" pad="17"/>
<connect gate="G$1" pin="CX1" pad="39"/>
<connect gate="G$1" pin="CX2" pad="34"/>
<connect gate="G$1" pin="CX3" pad="29"/>
<connect gate="G$1" pin="CX4" pad="24"/>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="6"/>
<connect gate="G$1" pin="D2-" pad="8"/>
<connect gate="G$1" pin="D3+" pad="11"/>
<connect gate="G$1" pin="D3-" pad="13"/>
<connect gate="G$1" pin="D4+" pad="16"/>
<connect gate="G$1" pin="D4-" pad="18"/>
<connect gate="G$1" pin="X1+" pad="40"/>
<connect gate="G$1" pin="X1-" pad="38"/>
<connect gate="G$1" pin="X2+" pad="35"/>
<connect gate="G$1" pin="X2-" pad="33"/>
<connect gate="G$1" pin="X3+" pad="30"/>
<connect gate="G$1" pin="X3-" pad="28"/>
<connect gate="G$1" pin="X4+" pad="25"/>
<connect gate="G$1" pin="X4-" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490240140?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7490240140"/>
<attribute name="POE" value="4PPoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490240140"/>
<attribute name="VT" value="4000VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7490140124" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Created by Ella Wu, 2020-07-08&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS-1"/>
</gates>
<devices>
<device name="" package="7490140124">
<connects>
<connect gate="G$1" pin="CRD" pad="4"/>
<connect gate="G$1" pin="CRX" pad="9"/>
<connect gate="G$1" pin="CTD" pad="1"/>
<connect gate="G$1" pin="CTX" pad="12"/>
<connect gate="G$1" pin="RD+" pad="5"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="RX+" pad="8"/>
<connect gate="G$1" pin="RX-" pad="7"/>
<connect gate="G$1" pin="TD+" pad="2"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="11"/>
<connect gate="G$1" pin="TX-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7490140124?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7490140124"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="7490140124"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749080010" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="749080010">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="2.5/5G Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749080010?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="200uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="749080010"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="749080010"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749020112B" prefix="T">
<description>&lt;b&gt;WE-LAN LAN Transformer

&lt;BR&gt;&lt;BR&gt;Characteristics 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Suitable for industrial temperatures from –40 °C up to +125 °C
&lt;BR&gt;Different version available from 1.5 kV isolation to 6 kV.
&lt;BR&gt;HPLE version
&lt;BR&gt;Additional CMC for higher attenuation
&lt;BR&gt;Non PoE, PoE and PoE++ up to 2 A
&lt;BR&gt;PoE up to 150 W and speeds up to 1 Gbit/s
&lt;BR&gt;Available in SMT
&lt;BR&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and IEEE 802.3bt
&lt;BR&gt;UL Recognized
&lt;BR&gt;

&lt;b&gt;&lt;BR&gt;Applications 
&lt;BR&gt;&lt;BR&gt;&lt;/b&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;BR&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;BR&gt;Router, switches, sensors, robotics, automation, IP cameras, IoT applications
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14800v209%20WE-LAN%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-05-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="749020112B">
<connects>
<connect gate="G$1" pin="CD1" pad="3"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="9"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="22"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="16"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="2"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="7"/>
<connect gate="G$1" pin="D3-" pad="8"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="24"/>
<connect gate="G$1" pin="X1-" pad="23"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="18"/>
<connect gate="G$1" pin="X3-" pad="17"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100/1000BASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749020112B?ae"/>
<attribute name="HPLE" value="No"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="749020112B"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="749020112B"/>
<attribute name="VT" value="1500VRMS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
