<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Signal &amp; Communications - Signal Transformers - WE-LAN 10G&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-04-01&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-LAN_10G_749052011">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T</description>
</package>
<package name="WE-LAN_10G_749052012">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T</description>
</package>
<package name="WE-LAN_10G_749052050">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T</description>
</package>
<package name="WE-LAN_10G_749050017">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T</description>
</package>
<package name="WE-LAN_10G_749053011">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T</description>
</package>
<package name="WE-LAN_10G_749053012">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T</description>
</package>
<package name="WE-LAN_10G_749052051">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T</description>
</package>
<package name="WE-LAN_10G_749054010">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T</description>
</package>
<package name="WE-LAN_10G_749050010U">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T</description>
</package>
<package name="WE-LAN_10G_749052014">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T</description>
</package>
<package name="WE-LAN_10G_749053013">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T</description>
</package>
<package name="WE-LAN_10G_749053010">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T</description>
</package>
<package name="WE-LAN_10G_749050018">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T</description>
</package>
<package name="WE-LAN_10G_749050010A">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T</description>
</package>
</packages>
<symbols>
<symbol name="4CHANNELS">
<pin name="D1+" direction="pas"/>
<pin name="CD1" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="X1-" direction="pas"/>
<pin name="CX1" direction="pas"/>
<pin name="X1+" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="CD2" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="X2-" direction="pas"/>
<pin name="CX2" direction="pas"/>
<pin name="X2+" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="CD3" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="X3-" direction="pas"/>
<pin name="CX3" direction="pas"/>
<pin name="X3+" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="CD4" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="X4-" direction="pas"/>
<pin name="CX4" direction="pas"/>
<pin name="X4+" direction="pas"/>
</symbol>
<symbol name="5CHANNELS">
<pin name="D1+" direction="pas"/>
<pin name="CD1" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="X1-" direction="pas"/>
<pin name="CX1" direction="pas"/>
<pin name="X1+" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="CD2" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="X2-" direction="pas"/>
<pin name="CX2" direction="pas"/>
<pin name="X2+" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="CD3" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="X3-" direction="pas"/>
<pin name="CX3" direction="pas"/>
<pin name="X3+" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="CD4" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="X4-" direction="pas"/>
<pin name="CX4" direction="pas"/>
<pin name="X4+" direction="pas"/>
<pin name="D5+" direction="pas"/>
<pin name="CD5" direction="pas"/>
<pin name="D5-" direction="pas"/>
<pin name="X5-" direction="pas"/>
<pin name="CX5" direction="pas"/>
<pin name="X5+" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-LAN_10G_749052050" prefix="T">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs up to 150 W
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +105°C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-10G&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu  2019-07-22&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="WE-LAN_10G_749052050">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10G Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749052050?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="180uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="749052050"/>
<attribute name="POE" value="PoE+ (up to 1 A)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="180uH"/>
<attribute name="VT" value="1500V(RMS)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_10G_749052012" prefix="T">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs up to 150 W
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +105°C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-10G&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu  2019-07-22&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="WE-LAN_10G_749052012">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10G Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749052012?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="120uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 up to +70 °C"/>
<attribute name="PART-NUMBER" value="749052012"/>
<attribute name="POE" value="PoE+ (up to 600 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="120uH"/>
<attribute name="VT" value="1500V(RMS)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_10G_749050017" prefix="T">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs up to 150 W
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +105°C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-10G&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu  2019-07-22&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="WE-LAN_10G_749050017">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10G Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749050017?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="120uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="749050017"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="120uH"/>
<attribute name="VT" value="1500V(RMS)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_10G_749052011" prefix="T">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs up to 150 W
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +105°C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-10G&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu  2019-07-22&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="WE-LAN_10G_749052011">
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10G Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749052011?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="120uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="749052011"/>
<attribute name="POE" value="PoE+ (up to 600 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="120uH"/>
<attribute name="VT" value="1500V(RMS)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_10G_749053011" prefix="T">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs up to 150 W
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +105°C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-10G&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2019-04-18&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="WE-LAN_10G_749053011">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10G Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749053011?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="200uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="749053011"/>
<attribute name="POE" value="PoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="200uH"/>
<attribute name="VT" value="1500V(RMS)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_10G_749052051" prefix="T">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs up to 150 W
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +105°C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-10G&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu  2019-07-22&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="WE-LAN_10G_749052051">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10G Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749052051?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="120uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="749052051"/>
<attribute name="POE" value="PoE+ (up to 1 A)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="120uH"/>
<attribute name="VT" value="1500V(RMS)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_10G_749054010" prefix="T">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs up to 150 W
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +105°C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-10G&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-04-01&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="WE-LAN_10G_749054010">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10G Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749054010?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="120uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="749054010"/>
<attribute name="POE" value="PoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="120uH"/>
<attribute name="VT" value="4000V(RMS)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_10G_749053012" prefix="T">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs up to 150 W
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +105°C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-10G&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu  2019-07-22&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="WE-LAN_10G_749053012">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10G Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749053012?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="200uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="749053012"/>
<attribute name="POE" value="PoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="200uH"/>
<attribute name="VT" value="1500V(RMS)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_10G_749052014" prefix="T">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs up to 150 W
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +105°C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-10G&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu  2019-07-22&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5CHANNELS"/>
</gates>
<devices>
<device name="" package="WE-LAN_10G_749052014">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CD5" pad="13"/>
<connect gate="G$1" pin="CX1" pad="30"/>
<connect gate="G$1" pin="CX2" pad="27"/>
<connect gate="G$1" pin="CX3" pad="24"/>
<connect gate="G$1" pin="CX4" pad="21"/>
<connect gate="G$1" pin="CX5" pad="18"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="D5+" pad="14"/>
<connect gate="G$1" pin="D5-" pad="15"/>
<connect gate="G$1" pin="X1+" pad="29"/>
<connect gate="G$1" pin="X1-" pad="28"/>
<connect gate="G$1" pin="X2+" pad="26"/>
<connect gate="G$1" pin="X2-" pad="25"/>
<connect gate="G$1" pin="X3+" pad="23"/>
<connect gate="G$1" pin="X3-" pad="22"/>
<connect gate="G$1" pin="X4+" pad="20"/>
<connect gate="G$1" pin="X4-" pad="19"/>
<connect gate="G$1" pin="X5+" pad="17"/>
<connect gate="G$1" pin="X5-" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10G Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749052014?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="180uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="749052014"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="180uH"/>
<attribute name="VT" value="1500V(RMS)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_10G_749053010" prefix="T">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs up to 150 W
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +105°C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-10G&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu  2019-07-22&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="WE-LAN_10G_749053010">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10G Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749053010?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="120uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="749053010"/>
<attribute name="POE" value="PoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="120uH"/>
<attribute name="VT" value="1500V(RMS)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_10G_749050010A" prefix="T">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs up to 150 W
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +105°C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-10G&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-02-17&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="WE-LAN_10G_749050010A">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10G Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749050010A?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="200uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="749050010A"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="200uH"/>
<attribute name="VT" value="1500V(RMS)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_10G_749053013" prefix="T">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs up to 150 W
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +105°C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-10G&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu  2019-07-22&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="WE-LAN_10G_749053013">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10G Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749053013?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="120uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="749053013"/>
<attribute name="POE" value="PoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="120uH"/>
<attribute name="VT" value="1500V(RMS)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_10G_749050018" prefix="T">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs up to 150 W
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +105°C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-10G&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu  2019-07-22&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="WE-LAN_10G_749050018">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10G Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749050018?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="120uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="749050018"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="120uH"/>
<attribute name="VT" value="1500V(RMS)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_10G_749050010U" prefix="T">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs up to 150 W
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +105°C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84657v209%20WE-LAN_749050010-749052012_4C%20-%20Kopie.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-10G&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu  2019-07-22&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="WE-LAN_10G_749050010U">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10G Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749050010U?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="L" value="200uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="749050010U"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value="200uH"/>
<attribute name="VT" value="1500V(RMS)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
