<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Signal &amp; Communications - Signal Transformers - WE-LAN AQ&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-10-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-LANAQ_749010310">
<description>&lt;b&gt;WE-LAN AQ Transformer 10/100 Base-T</description>
</package>
<package name="WE-LANAQ_749020310">
<description>&lt;b&gt;WE-LAN AQ Transformer 10/100/1000 Base-T</description>
</package>
<package name="WE-LANAQ_749013310">
<description>&lt;b&gt;WE-LAN AQ Transformer 10/100 Base-T</description>
</package>
<package name="WE-LANAQ_749022310">
<description>&lt;b&gt;WE-LAN AQ Transformer 10/100/1000 Base-T</description>
</package>
<package name="WE-LANAQ_749012310">
<description>&lt;b&gt;WE-LAN AQ Transformer 10/100 Base-T</description>
</package>
<package name="WE-LANAQ_749023310">
<description>&lt;b&gt;WE-LAN AQ Transformer 10/100/1000 Base-T</description>
</package>
</packages>
<symbols>
<symbol name="4CHANNELS">
<pin name="D1+"/>
<pin name="CD1"/>
<pin name="D1-"/>
<pin name="X1-"/>
<pin name="CX1"/>
<pin name="X1+"/>
<pin name="D2+"/>
<pin name="CD2"/>
<pin name="D2-"/>
<pin name="X2-"/>
<pin name="CX2"/>
<pin name="X2+"/>
<pin name="D3+"/>
<pin name="CD3"/>
<pin name="D3-"/>
<pin name="X3-"/>
<pin name="CX3"/>
<pin name="X3+"/>
<pin name="D4+"/>
<pin name="CD4"/>
<pin name="D4-"/>
<pin name="X4-"/>
<pin name="CX4"/>
<pin name="X4+"/>
</symbol>
<symbol name="2CHANNELS">
<pin name="RX+"/>
<pin name="CRX"/>
<pin name="RX-"/>
<pin name="RD-"/>
<pin name="CRD"/>
<pin name="RD+"/>
<pin name="TX+"/>
<pin name="CTX"/>
<pin name="TX-"/>
<pin name="TD-"/>
<pin name="CTD"/>
<pin name="TD+"/>
</symbol>
<symbol name="2CHANNELS-1">
<pin name="RX+"/>
<pin name="CRX"/>
<pin name="RX-"/>
<pin name="RD-"/>
<pin name="CRD"/>
<pin name="RD+"/>
<pin name="TX+"/>
<pin name="CTX"/>
<pin name="TX-"/>
<pin name="TD-"/>
<pin name="CTD"/>
<pin name="TD+"/>
</symbol>
<symbol name="4CHANNELS-1">
<pin name="D1+"/>
<pin name="CD1"/>
<pin name="D1-"/>
<pin name="X1-"/>
<pin name="CX1"/>
<pin name="X1+"/>
<pin name="D2+"/>
<pin name="CD2"/>
<pin name="D2-"/>
<pin name="X2-"/>
<pin name="CX2"/>
<pin name="X2+"/>
<pin name="D3+"/>
<pin name="CD3"/>
<pin name="D3-"/>
<pin name="X3-"/>
<pin name="CX3"/>
<pin name="X3+"/>
<pin name="D4+"/>
<pin name="CD4"/>
<pin name="D4-"/>
<pin name="X4-"/>
<pin name="CX4"/>
<pin name="X4+"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-LAN_AQ_749010310" prefix="T">
<description>&lt;b&gt;WE-LAN AQ Transformer 10/100 Base-T&lt;/b&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;100 % automatic production
&lt;br&gt;Ethernet with speeds up to 1 Gbit/s
&lt;br&gt;Low profile height of 4 mm
&lt;br&gt;Improved Return Loss and Crosstalk properties
&lt;br&gt;Improved solderability and AOI inspection due to half-vias with gold plating
&lt;br&gt;Compatible with existing LAN products
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;&lt;br&gt;Suitable for industrial temperatures from –40 °C up to +85 °C
&lt;br&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;br&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;br&gt;Hubs, Routers, Switches, IP cameras, IoT applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o97650v209%20Family_WE-LAN%20AQ_10_100_1000BaseT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o97650v209%20Family_WE-LAN%20AQ_10_100_1000BaseT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-LANAQ"&gt;https://www.we-online.com/catalog/en/WE-LANAQ&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Updated by Ella Wu  2019-07-22&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS"/>
</gates>
<devices>
<device name="" package="WE-LANAQ_749010310">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CRX" pad="10"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="CTX" pad="15"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="11"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="16"/>
<connect gate="G$1" pin="TX-" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/749010310.pdf"/>
<attribute name="L" value="300uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 749010310 "/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value=" 749010310 "/>
<attribute name="VT" value="1500  V (RMS) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_AQ_749020310" prefix="T">
<description>&lt;b&gt;WE-LAN AQ Transformer 10/100/1000 Base-T &lt;/b&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;100 % automatic production
&lt;br&gt;Ethernet with speeds up to 1 Gbit/s
&lt;br&gt;Low profile height of 4 mm
&lt;br&gt;Improved Return Loss and Crosstalk properties
&lt;br&gt;Improved solderability and AOI inspection due to half-vias with gold plating
&lt;br&gt;Compatible with existing LAN products
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;&lt;br&gt;Suitable for industrial temperatures from –40 °C up to +85 °C
&lt;br&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;br&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;br&gt;Hubs, Routers, Switches, IP cameras, IoT applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o97650v209%20Family_WE-LAN%20AQ_10_100_1000BaseT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o97650v209%20Family_WE-LAN%20AQ_10_100_1000BaseT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-LANAQ"&gt;https://www.we-online.com/catalog/en/WE-LANAQ&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Updated by Ella Wu  2019-07-22&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS"/>
</gates>
<devices>
<device name="" package="WE-LANAQ_749020310">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100/1000 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/749020310.pdf"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 749020310 "/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value=" 749020310 "/>
<attribute name="VT" value="1500  V (RMS) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_AQ_749013310" prefix="T">
<description>&lt;b&gt;WE-LAN AQ Transformer 10/100 Base-T&lt;/b&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;100 % automatic production
&lt;br&gt;Ethernet with speeds up to 1 Gbit/s
&lt;br&gt;Low profile height of 4 mm
&lt;br&gt;Improved Return Loss and Crosstalk properties
&lt;br&gt;Improved solderability and AOI inspection due to half-vias with gold plating
&lt;br&gt;Compatible with existing LAN products
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;&lt;br&gt;Suitable for industrial temperatures from –40 °C up to +85 °C
&lt;br&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;br&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;br&gt;Hubs, Routers, Switches, IP cameras, IoT applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o97650v209%20Family_WE-LAN%20AQ_10_100_1000BaseT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o97650v209%20Family_WE-LAN%20AQ_10_100_1000BaseT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-LANAQ"&gt;https://www.we-online.com/catalog/en/WE-LANAQ&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Created by Ella Wu  2020-10-26&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS-1"/>
</gates>
<devices>
<device name="" package="WE-LANAQ_749013310">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CRX" pad="10"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="CTX" pad="15"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="11"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="16"/>
<connect gate="G$1" pin="TX-" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/749013310.pdf"/>
<attribute name="L" value="180uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 749013310 "/>
<attribute name="POE" value="PoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value=" 749013310 "/>
<attribute name="VT" value="1500  V (RMS) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_AQ_749012310" prefix="T">
<description>&lt;b&gt;WE-LAN AQ Transformer 10/100 Base-T&lt;/b&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;100 % automatic production
&lt;br&gt;Ethernet with speeds up to 1 Gbit/s
&lt;br&gt;Low profile height of 4 mm
&lt;br&gt;Improved Return Loss and Crosstalk properties
&lt;br&gt;Improved solderability and AOI inspection due to half-vias with gold plating
&lt;br&gt;Compatible with existing LAN products
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;&lt;br&gt;Suitable for industrial temperatures from –40 °C up to +85 °C
&lt;br&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;br&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;br&gt;Hubs, Routers, Switches, IP cameras, IoT applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o97650v209%20Family_WE-LAN%20AQ_10_100_1000BaseT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o97650v209%20Family_WE-LAN%20AQ_10_100_1000BaseT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-LANAQ"&gt;https://www.we-online.com/catalog/en/WE-LANAQ&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Created by Ella Wu  2020-10-26&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2CHANNELS-1"/>
</gates>
<devices>
<device name="" package="WE-LANAQ_749012310">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CRX" pad="10"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="CTX" pad="15"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="11"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="16"/>
<connect gate="G$1" pin="TX-" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/749012310.pdf"/>
<attribute name="L" value="150uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 749012310 "/>
<attribute name="POE" value="PoE+ (up to 720 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value=" 749012310 "/>
<attribute name="VT" value="1500  V (RMS) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_AQ_749022310" prefix="T">
<description>&lt;b&gt;WE-LAN AQ Transformer 10/100 Base-T&lt;/b&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;100 % automatic production
&lt;br&gt;Ethernet with speeds up to 1 Gbit/s
&lt;br&gt;Low profile height of 4 mm
&lt;br&gt;Improved Return Loss and Crosstalk properties
&lt;br&gt;Improved solderability and AOI inspection due to half-vias with gold plating
&lt;br&gt;Compatible with existing LAN products
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;&lt;br&gt;Suitable for industrial temperatures from –40 °C up to +85 °C
&lt;br&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;br&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;br&gt;Hubs, Routers, Switches, IP cameras, IoT applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o97650v209%20Family_WE-LAN%20AQ_10_100_1000BaseT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o97650v209%20Family_WE-LAN%20AQ_10_100_1000BaseT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-LANAQ"&gt;https://www.we-online.com/catalog/en/WE-LANAQ&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Created by Ella Wu  2020-10-26&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS-1"/>
</gates>
<devices>
<device name="" package="WE-LANAQ_749022310">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1001 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/749022310.pdf"/>
<attribute name="L" value="150uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 749022310 "/>
<attribute name="POE" value="PoE+ (up to 720 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value=" 749022310 "/>
<attribute name="VT" value="1500  V (RMS) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_AQ_749023310" prefix="T">
<description>&lt;b&gt;WE-LAN AQ Transformer 10/100 Base-T&lt;/b&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;100 % automatic production
&lt;br&gt;Ethernet with speeds up to 1 Gbit/s
&lt;br&gt;Low profile height of 4 mm
&lt;br&gt;Improved Return Loss and Crosstalk properties
&lt;br&gt;Improved solderability and AOI inspection due to half-vias with gold plating
&lt;br&gt;Compatible with existing LAN products
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;&lt;br&gt;Suitable for industrial temperatures from –40 °C up to +85 °C
&lt;br&gt;Compatible to Industrial Ethernet systems like EtherCAT or Profinet
&lt;br&gt;Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
&lt;br&gt;Hubs, Routers, Switches, IP cameras, IoT applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o97650v209%20Family_WE-LAN%20AQ_10_100_1000BaseT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o97650v209%20Family_WE-LAN%20AQ_10_100_1000BaseT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-LANAQ"&gt;https://www.we-online.com/catalog/en/WE-LANAQ&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Created by Ella Wu  2020-10-26&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4CHANNELS-1"/>
</gates>
<devices>
<device name="" package="WE-LANAQ_749023310">
<connects>
<connect gate="G$1" pin="CD1" pad="1"/>
<connect gate="G$1" pin="CD2" pad="4"/>
<connect gate="G$1" pin="CD3" pad="7"/>
<connect gate="G$1" pin="CD4" pad="10"/>
<connect gate="G$1" pin="CX1" pad="24"/>
<connect gate="G$1" pin="CX2" pad="21"/>
<connect gate="G$1" pin="CX3" pad="18"/>
<connect gate="G$1" pin="CX4" pad="15"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/749023310.pdf"/>
<attribute name="L" value="180uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 749023310 "/>
<attribute name="POE" value="PoE (up to 350 mA)"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="VALUE" value=" 749023310 "/>
<attribute name="VT" value="1500  V (RMS) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
