<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Single Coil Power Inductors - WE-LQSH&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-03-18&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-LQSH_4020">
<description>&lt;b&gt;WE-LQSH  SMD High Saturation Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: &lt;/b&gt;4020, SMT, 2pins
&lt;br&gt;LXWXH=4X4X2mm</description>
</package>
<package name="WE-LQSH_2010">
<description>&lt;b&gt;WE-LQSH  SMD High Saturation Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: &lt;/b&gt;2010, SMT, 2pins
&lt;br&gt;LXWXH=2X1.6X1mm</description>
</package>
<package name="WE-LQSH_3012">
<description>&lt;b&gt;WE-LQSH  SMD High Saturation Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: &lt;/b&gt;3012, SMT, 2pins
&lt;br&gt;LXWXH=3X3X1.2mm</description>
</package>
<package name="WE-LQSH_2512">
<description>&lt;b&gt;WE-LQSH  SMD High Saturation Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: &lt;/b&gt;2512, SMT, 2pins
&lt;br&gt;LXWXH=2.5X2X1.2mm</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-LQSH_4020" prefix="L">
<description>&lt;b&gt;WE-LQSH SMT High Saturation Power Inductor&lt;br&gt;
Semi Shielded
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;High Current semi-shielded power Inductor
&lt;br&gt;70% higher saturation current than WE-LQS series
&lt;br&gt;Soft Saturation Current
&lt;br&gt;Magnetically shielded through magnetic glue
&lt;br&gt;25 V maximum Peak Voltage
&lt;br&gt;Operating Temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications

&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Integrated DC/DC Converters with high ripple currents
&lt;br&gt;Switching controllers requiring high efficiency
&lt;br&gt;Portable devices (Smartphone, Digital cameras, Tablet, etc.)
&lt;br&gt;Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o85073v209%20Family_WE-LQSH_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o85073v209%20Family_WE-LQSH_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LQSH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LQSH&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-18&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-LQSH_4020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744050420047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744050420047?ae"/>
<attribute name="FRES" value="89MHz"/>
<attribute name="IR" value="4.5A"/>
<attribute name="ISAT" value="15.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744050420047 "/>
<attribute name="RDC-MAX" value="22mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_74405042010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405042010?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405042010 "/>
<attribute name="RDC-MAX" value="26mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74405042015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405042015?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="3.2A"/>
<attribute name="ISAT" value="8.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405042015 "/>
<attribute name="RDC-MAX" value="36mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74405042022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405042022?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IR" value="2.6A"/>
<attribute name="ISAT" value="7.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405042022 "/>
<attribute name="RDC-MAX" value="48mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74405042033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405042033?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="5.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405042033 "/>
<attribute name="RDC-MAX" value="72mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74405042047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405042047?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="4.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405042047 "/>
<attribute name="RDC-MAX" value="108mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74405042068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405042068?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="1.9A"/>
<attribute name="ISAT" value="4.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405042068 "/>
<attribute name="RDC-MAX" value="156mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74405042100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405042100?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="1.7A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405042100 "/>
<attribute name="RDC-MAX" value="216mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQSH_2010" prefix="L">
<description>&lt;b&gt;WE-LQSH SMT High Saturation Power Inductor&lt;br&gt;
Semi Shielded
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;High Current semi-shielded power Inductor
&lt;br&gt;70% higher saturation current than WE-LQS series
&lt;br&gt;Soft Saturation Current
&lt;br&gt;Magnetically shielded through magnetic glue
&lt;br&gt;25 V maximum Peak Voltage
&lt;br&gt;Operating Temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications

&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Integrated DC/DC Converters with high ripple currents
&lt;br&gt;Switching controllers requiring high efficiency
&lt;br&gt;Portable devices (Smartphone, Digital cameras, Tablet, etc.)
&lt;br&gt;Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o85073v209%20Family_WE-LQSH_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o85073v209%20Family_WE-LQSH_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LQSH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LQSH&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-18&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-LQSH_2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744050200047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744050200047?ae"/>
<attribute name="FRES" value="159MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="4.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744050200047 "/>
<attribute name="RDC-MAX" value="49mOhm"/>
<attribute name="SIZE" value=" 2010 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_74405020010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405020010?ae"/>
<attribute name="FRES" value="84MHz"/>
<attribute name="IR" value="1.65A"/>
<attribute name="ISAT" value="3.85A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405020010 "/>
<attribute name="RDC-MAX" value="90mOhm"/>
<attribute name="SIZE" value=" 2010 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74405020015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405020015?ae"/>
<attribute name="FRES" value="74MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="2.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405020015 "/>
<attribute name="RDC-MAX" value="132mOhm"/>
<attribute name="SIZE" value=" 2010 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74405020022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405020022?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IR" value="1.25A"/>
<attribute name="ISAT" value="2.15A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405020022 "/>
<attribute name="RDC-MAX" value="170mOhm"/>
<attribute name="SIZE" value=" 2010 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74405020047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405020047?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405020047 "/>
<attribute name="RDC-MAX" value="444mOhm"/>
<attribute name="SIZE" value=" 2010 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74405020100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405020100?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="0.58A"/>
<attribute name="ISAT" value="0.95A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405020100 "/>
<attribute name="RDC-MAX" value="816mOhm"/>
<attribute name="SIZE" value=" 2010 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQSH_3012" prefix="L">
<description>&lt;b&gt;WE-LQSH SMT High Saturation Power Inductor&lt;br&gt;
Semi Shielded
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;High Current semi-shielded power Inductor
&lt;br&gt;70% higher saturation current than WE-LQS series
&lt;br&gt;Soft Saturation Current
&lt;br&gt;Magnetically shielded through magnetic glue
&lt;br&gt;25 V maximum Peak Voltage
&lt;br&gt;Operating Temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications

&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Integrated DC/DC Converters with high ripple currents
&lt;br&gt;Switching controllers requiring high efficiency
&lt;br&gt;Portable devices (Smartphone, Digital cameras, Tablet, etc.)
&lt;br&gt;Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o85073v209%20Family_WE-LQSH_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o85073v209%20Family_WE-LQSH_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LQSH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LQSH&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-18&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-LQSH_3012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744050310047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744050310047?ae"/>
<attribute name="FRES" value="121MHz"/>
<attribute name="IR" value="3.15A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744050310047 "/>
<attribute name="RDC-MAX" value="34mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_74405031010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405031010?ae"/>
<attribute name="FRES" value="66MHz"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT" value="5.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405031010 "/>
<attribute name="RDC-MAX" value="54mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74405031015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405031015?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="4.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405031015 "/>
<attribute name="RDC-MAX" value="77mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74405031022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405031022?ae"/>
<attribute name="FRES" value="46MHz"/>
<attribute name="IR" value="1.75A"/>
<attribute name="ISAT" value="3.35A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405031022 "/>
<attribute name="RDC-MAX" value="108mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74405031033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405031033?ae"/>
<attribute name="FRES" value="39MHz"/>
<attribute name="IR" value="1.55A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405031033 "/>
<attribute name="RDC-MAX" value="155mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74405031047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405031047?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405031047 "/>
<attribute name="RDC-MAX" value="235mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74405031100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405031100?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="0.85A"/>
<attribute name="ISAT" value="1.45A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405031100 "/>
<attribute name="RDC-MAX" value="474mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQSH_2512" prefix="L">
<description>&lt;b&gt;WE-LQSH SMT High Saturation Power Inductor&lt;br&gt;
Semi Shielded
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;High Current semi-shielded power Inductor
&lt;br&gt;70% higher saturation current than WE-LQS series
&lt;br&gt;Soft Saturation Current
&lt;br&gt;Magnetically shielded through magnetic glue
&lt;br&gt;25 V maximum Peak Voltage
&lt;br&gt;Operating Temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications

&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Integrated DC/DC Converters with high ripple currents
&lt;br&gt;Switching controllers requiring high efficiency
&lt;br&gt;Portable devices (Smartphone, Digital cameras, Tablet, etc.)
&lt;br&gt;Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o85073v209%20Family_WE-LQSH_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o85073v209%20Family_WE-LQSH_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LQSH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LQSH&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-18&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-LQSH_2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744050240047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744050240047?ae"/>
<attribute name="FRES" value="129MHz"/>
<attribute name="IR" value="2.9A"/>
<attribute name="ISAT" value="5.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744050240047 "/>
<attribute name="RDC-MAX" value="35mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_74405024010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405024010?ae"/>
<attribute name="FRES" value="87MHz"/>
<attribute name="IR" value="2.35A"/>
<attribute name="ISAT" value="4.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405024010 "/>
<attribute name="RDC-MAX" value="58mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74405024015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405024015?ae"/>
<attribute name="FRES" value="68MHz"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405024015 "/>
<attribute name="RDC-MAX" value="72mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74405024022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405024022?ae"/>
<attribute name="FRES" value="46MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405024022 "/>
<attribute name="RDC-MAX" value="120mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74405024033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405024033?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405024033 "/>
<attribute name="RDC-MAX" value="163mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74405024047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405024047?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405024047 "/>
<attribute name="RDC-MAX" value="270mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74405024100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74405024100?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74405024100 "/>
<attribute name="RDC-MAX" value="522mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
