<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - Ferrites For PCB Assembly - WE-MLS&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2020-05-07&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-MLS_74273031">
<description>&lt;b&gt;WE-MLS Multiline EMI Suppression Ferrite
&lt;/b&gt;&lt;br&gt;&lt;br&gt;3 Lines</description>
</package>
<package name="WE-MLS_74273001">
<description>&lt;b&gt;WE-MLS Multiline EMI Suppression Ferrite
&lt;/b&gt;&lt;br&gt;&lt;br&gt;3 Lines</description>
</package>
<package name="WE-MLS_74273002">
<description>&lt;b&gt;WE-MLS Multiline EMI Suppression Ferrite
&lt;/b&gt;&lt;br&gt;&lt;br&gt;4 Lines</description>
</package>
<package name="WE-MLS_742730021">
<description>&lt;b&gt;WE-MLS Multiline EMI Suppression Ferrite
&lt;/b&gt;&lt;br&gt;&lt;br&gt;4 Lines</description>
</package>
<package name="WE-MLS_742730022">
<description>&lt;b&gt;WE-MLS Multiline EMI Suppression Ferrite
&lt;/b&gt;&lt;br&gt;&lt;br&gt;4 Lines</description>
</package>
<package name="WE-MLS_742730023">
<description>&lt;b&gt;WE-MLS Multiline EMI Suppression Ferrite
&lt;/b&gt;&lt;br&gt;&lt;br&gt;4 Lines</description>
</package>
<package name="WE-MLS_742730123">
<description>&lt;b&gt;WE-MLS Multiline EMI Suppression Ferrite
&lt;/b&gt;&lt;br&gt;&lt;br&gt;4 Lines</description>
</package>
<package name="WE-MLS_742730321">
<description>&lt;b&gt;WE-MLS Multiline EMI Suppression Ferrite
&lt;/b&gt;&lt;br&gt;&lt;br&gt;4 Lines</description>
</package>
<package name="WE-MLS_742730223">
<description>&lt;b&gt;WE-MLS Multiline EMI Suppression Ferrite
&lt;/b&gt;&lt;br&gt;&lt;br&gt;4 Lines</description>
</package>
<package name="WE-MLS_74273012">
<description>&lt;b&gt;WE-MLS Multiline EMI Suppression Ferrite
&lt;/b&gt;&lt;br&gt;&lt;br&gt;4 Lines</description>
</package>
</packages>
<symbols>
<symbol name="L_3LINES">
<description>&lt;B&gt;WE-MLS mULTILINE emi Suppression Ferrite&lt;/b&gt;&lt;br&gt;
3 WAYS</description>
<pin name="6" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="L_4LINES">
<description>&lt;B&gt;WE-MLS mULTILINE emi Suppression Ferrite&lt;/b&gt;&lt;br&gt;
4 WAYS</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-MLS_3LINES" prefix="L">
<description>&lt;b&gt;WE-MLS Multiline EMI Suppression Ferrite
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High impedance common mode inductor with 2x2 windings made by PCB line connection
&lt;br&gt;High rated current with typ. 4 A
&lt;br&gt;Broadband filtering because of the NiZn-ferrite core
&lt;br&gt;RF common mode inductor for 2, 3 or 4 lines in one component
&lt;br&gt;Compact size
&lt;br&gt;Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;With the appropriate layout the impedance (i.e. 4 windings) respectively the current (parallel circuit) could be increased
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfect suitable for absorption of common or differential mode interferences in the field of EMC
&lt;br&gt;With one turn the component performes like a 3 or 4 times common mode choke for the signal
&lt;br&gt;Multi-conductor systems and power electronics
&lt;br&gt;Filtering components of low voltage power supplies
&lt;br&gt;4-line sensor application
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/o14821v209%20Family_WE-MLS.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/o14821v209%20Family_WE-MLS.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-MLS?"&gt;https://www.we-online.com/catalog/en/WE-MLS?&lt;/a&gt;&lt;p&gt;


Updated  by  Ella Wu  2020-04-23&lt;br&gt;
2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3LINES"/>
</gates>
<devices>
<device name="_74273001" package="WE-MLS_74273001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74273001.pdf"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74273001 "/>
<attribute name="RDC-MAX" value="2mohm"/>
<attribute name="TYPE" value="3 Lines"/>
<attribute name="VALUE" value="264Ohm@100MHz"/>
<attribute name="Z" value="212Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_74273031" package="WE-MLS_74273031">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74273031.pdf"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74273031 "/>
<attribute name="RDC-MAX" value="2mohm"/>
<attribute name="TYPE" value="3 Lines"/>
<attribute name="VALUE" value="264Ohm@100MHz"/>
<attribute name="Z" value="212Ohm@25MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MLS_4LINES" prefix="L">
<description>&lt;b&gt;WE-MLS Multiline EMI Suppression Ferrite
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High impedance common mode inductor with 2x2 windings made by PCB line connection
&lt;br&gt;High rated current with typ. 4 A
&lt;br&gt;Broadband filtering because of the NiZn-ferrite core
&lt;br&gt;RF common mode inductor for 2, 3 or 4 lines in one component
&lt;br&gt;Compact size
&lt;br&gt;Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;With the appropriate layout the impedance (i.e. 4 windings) respectively the current (parallel circuit) could be increased
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfect suitable for absorption of common or differential mode interferences in the field of EMC
&lt;br&gt;With one turn the component performes like a 3 or 4 times common mode choke for the signal
&lt;br&gt;Multi-conductor systems and power electronics
&lt;br&gt;Filtering components of low voltage power supplies
&lt;br&gt;4-line sensor application
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/katalog/media/o14821v209%20Family_WE-MLS.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/katalog/media/o14821v209%20Family_WE-MLS.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-MLS?"&gt;https://www.we-online.com/catalog/en/WE-MLS?&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-05-07&lt;br&gt;
2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_4LINES"/>
</gates>
<devices>
<device name="_74273002" package="WE-MLS_74273002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74273002.pdf"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74273002 "/>
<attribute name="RDC-MAX" value="2mohm"/>
<attribute name="TYPE" value="4 Lines"/>
<attribute name="VALUE" value="249Ohm@100MHz"/>
<attribute name="Z" value="209Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_742730021" package="WE-MLS_742730021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/742730021.pdf"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 742730021 "/>
<attribute name="RDC-MAX" value="2mohm"/>
<attribute name="TYPE" value="4 Lines"/>
<attribute name="VALUE" value="170Ohm@100MHz"/>
<attribute name="Z" value="136Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_742730022" package="WE-MLS_742730022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/742730022.pdf"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 742730022 "/>
<attribute name="RDC-MAX" value="2mohm"/>
<attribute name="TYPE" value="4 Lines"/>
<attribute name="VALUE" value="248Ohm@100MHz"/>
<attribute name="Z" value="208Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_742730023" package="WE-MLS_742730023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/742730023.pdf"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 742730023 "/>
<attribute name="RDC-MAX" value="2mohm"/>
<attribute name="TYPE" value="4 Lines"/>
<attribute name="VALUE" value="334Ohm@100MHz"/>
<attribute name="Z" value="292Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_742730321" package="WE-MLS_742730321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/742730321.pdf"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 742730321 "/>
<attribute name="RDC-MAX" value="2mohm"/>
<attribute name="TYPE" value="4 Lines"/>
<attribute name="VALUE" value="150Ohm@100MHz"/>
<attribute name="Z" value="115Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_74273012" package="WE-MLS_74273012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74273012.pdf"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74273012 "/>
<attribute name="RDC-MAX" value="2mohm"/>
<attribute name="TYPE" value="4 Lines"/>
<attribute name="VALUE" value="249Ohm@100MHz"/>
<attribute name="Z" value="209Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_742730123" package="WE-MLS_742730123">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/742730123.pdf"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 742730123 "/>
<attribute name="RDC-MAX" value="2mohm"/>
<attribute name="TYPE" value="4 Lines"/>
<attribute name="VALUE" value="334Ohm@100MHz"/>
<attribute name="Z" value="292Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_742730223" package="WE-MLS_742730223">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/742730223.pdf"/>
<attribute name="IR" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 742730223 "/>
<attribute name="RDC-MAX" value="2mohm"/>
<attribute name="TYPE" value="4 Lines"/>
<attribute name="VALUE" value="334Ohm@100MHz"/>
<attribute name="Z" value="292Ohm@25MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
