<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - Ferrites For PCB Assembly - WE-MPSB&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-MPSB_2220(H=1.5)">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;2220
&lt;/pre&gt;</description>
</package>
<package name="WE-MPSB_2220(H=1.8)">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;2220</description>
</package>
<package name="WE-MPSB_2220(H=3.2)">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;2220</description>
</package>
<package name="WE-MPSB_2220(H=2.0)">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;2220</description>
</package>
<package name="WE-MPSB_3312">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;3312</description>
</package>
<package name="WE-MPSB_0603(W=2.6)">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;0603</description>
</package>
<package name="WE-MPSB_1812">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1812</description>
</package>
<package name="WE-MPSB_0805(W=4.0)">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;0805
&lt;/pre&gt;</description>
</package>
<package name="WE-MPSB_1612">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1612</description>
</package>
<package name="WE-MPSB_1206(W=5.2)">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1206</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-MPSB_3312" prefix="L">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Specified peak current capability
&lt;br&gt;Ultra low RDC
&lt;br&gt;High Rated Current up to 10.5 A
&lt;br&gt;Operating Temperature: -55°C to +125°C
&lt;br&gt;Produkt-Spotlight: Huge peak, strong bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter with high inrush current peaks
&lt;br&gt;For motor interference suppression
&lt;br&gt;EMI suppression of DC/DC converters and DC power supply
&lt;br&gt;Broadband suppression
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation:&lt;br&gt;
&lt;/b&gt;&lt;br&gt;WB = Wide Band 
&lt;br&gt;HS=High Speed
&lt;br&gt;HC=High Current &lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14822v209%20Family_WE-MPSB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14822v209%20Family_WE-MPSB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MPSB?"&gt;http://katalog.we-online.de/en/pbs/WE-MPSB?&lt;/a&gt;&lt;p&gt;


Updated  by  Ella Wu 2019-01-02&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_HC" package="WE-MPSB_3312">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74279225101">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279225101.pdf"/>
<attribute name="IR" value="10000mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279225101 "/>
<attribute name="RDC-MAX" value="4mOhm"/>
<attribute name="RDC-TYP" value="3mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="100Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="160Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MPSB_2220" prefix="L">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Specified peak current capability
&lt;br&gt;Ultra low RDC
&lt;br&gt;High Rated Current up to 10.5 A
&lt;br&gt;Operating Temperature: -55°C to +125°C
&lt;br&gt;Produkt-Spotlight: Huge peak, strong bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter with high inrush current peaks
&lt;br&gt;For motor interference suppression
&lt;br&gt;EMI suppression of DC/DC converters and DC power supply
&lt;br&gt;Broadband suppression
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation:&lt;br&gt;
&lt;/b&gt;&lt;br&gt;WB = Wide Band 
&lt;br&gt;HS=High Speed
&lt;br&gt;HC=High Current &lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14822v209%20Family_WE-MPSB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14822v209%20Family_WE-MPSB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MPSB?"&gt;http://katalog.we-online.de/en/pbs/WE-MPSB?&lt;/a&gt;&lt;p&gt;


Updated  by  Ella Wu 2019-01-02&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="(H=1.5)" package="WE-MPSB_2220(H=1.5)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74279224171">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279224171.pdf"/>
<attribute name="IR" value="4000mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279224171 "/>
<attribute name="RDC-MAX" value="15mOhm"/>
<attribute name="RDC-TYP" value="11mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="170Ohm@ 100 MHz"/>
<attribute name="VLAUE" value="170Ω@100MHz/4A"/>
<attribute name="ZMAX" value="280Ohm"/>
</technology>
</technologies>
</device>
<device name="(H=1.8)" package="WE-MPSB_2220(H=1.8)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74279224101">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279224101.pdf"/>
<attribute name="IR" value="7000mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279224101 "/>
<attribute name="RDC-MAX" value="5mOhm"/>
<attribute name="RDC-TYP" value="3.5mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="100Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="160Ohm"/>
</technology>
<technology name="_74279224151">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279224151.pdf"/>
<attribute name="IR" value="5000mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279224151 "/>
<attribute name="RDC-MAX" value="10mOhm"/>
<attribute name="RDC-TYP" value="7mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="150Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="230Ohm"/>
</technology>
<technology name="_74279224181">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279224181.pdf"/>
<attribute name="IR" value="5000mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279224181 "/>
<attribute name="RDC-MAX" value="10mOhm"/>
<attribute name="RDC-TYP" value="7.5mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="180Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="240Ohm"/>
</technology>
<technology name="_74279224251">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279224251.pdf"/>
<attribute name="IR" value="4000mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279224251 "/>
<attribute name="RDC-MAX" value="12mOhm"/>
<attribute name="RDC-TYP" value="8.5mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="250Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="300Ohm"/>
</technology>
</technologies>
</device>
<device name="(H=2.0)" package="WE-MPSB_2220(H=2.0)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74279224551">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279224551.pdf"/>
<attribute name="IR" value="4000mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279224551 "/>
<attribute name="RDC-MAX" value="35mOhm"/>
<attribute name="RDC-TYP" value="28mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="550Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="660Ohm"/>
</technology>
</technologies>
</device>
<device name="(H=3.2)" package="WE-MPSB_2220(H=3.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74279224271">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279224271.pdf"/>
<attribute name="IR" value="4000mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279224271 "/>
<attribute name="RDC-MAX" value="20mOhm"/>
<attribute name="RDC-TYP" value="10mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="270Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="350Ohm"/>
</technology>
<technology name="_74279224401">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279224401.pdf"/>
<attribute name="IR" value="4500mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279224401 "/>
<attribute name="RDC-MAX" value="20mOhm"/>
<attribute name="RDC-TYP" value="15mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="400Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="460Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MPSB_0603" prefix="L">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Specified peak current capability
&lt;br&gt;Ultra low RDC
&lt;br&gt;High Rated Current up to 10.5 A
&lt;br&gt;Operating Temperature: -55°C to +125°C
&lt;br&gt;Produkt-Spotlight: Huge peak, strong bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter with high inrush current peaks
&lt;br&gt;For motor interference suppression
&lt;br&gt;EMI suppression of DC/DC converters and DC power supply
&lt;br&gt;Broadband suppression
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:&lt;br&gt;&lt;br&gt;
Package: 
&lt;/b&gt;&lt;br&gt;Wide Band /High Speed: W=Width= 2.2
&lt;br&gt;High Current: W=Width= 2.6
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation:
&lt;/b&gt;&lt;br&gt;WB = Wide Band 
&lt;br&gt;HS=High Speed
&lt;br&gt;HC=High Current 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14822v209%20Family_WE-MPSB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14822v209%20Family_WE-MPSB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MPSB?"&gt;http://katalog.we-online.de/en/pbs/WE-MPSB?&lt;/a&gt;&lt;p&gt;


Updated  by  Ella Wu 2019-01-02&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_HC" package="WE-MPSB_0603(W=2.6)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7427922808">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/7427922808.pdf"/>
<attribute name="IR" value="9500mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7427922808 "/>
<attribute name="RDC-MAX" value="5mOhm"/>
<attribute name="RDC-TYP" value="2.5mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="8Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="25Ohm"/>
</technology>
<technology name="_74279228111">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279228111.pdf"/>
<attribute name="IR" value="4100mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279228111 "/>
<attribute name="RDC-MAX" value="20mOhm"/>
<attribute name="RDC-TYP" value="14.5mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="110Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="135Ohm"/>
</technology>
<technology name="_74279228260">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279228260.pdf"/>
<attribute name="IR" value="6500mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279228260 "/>
<attribute name="RDC-MAX" value="8mOhm"/>
<attribute name="RDC-TYP" value="5mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="26Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="39Ohm"/>
</technology>
<technology name="_74279228600">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279228600.pdf"/>
<attribute name="IR" value="5100mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279228600 "/>
<attribute name="RDC-MAX" value="15mOhm"/>
<attribute name="RDC-TYP" value="8.5mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="60Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="99Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MPSB_1812" prefix="L">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Specified peak current capability
&lt;br&gt;Ultra low RDC
&lt;br&gt;High Rated Current up to 10.5 A
&lt;br&gt;Operating Temperature: -55°C to +125°C
&lt;br&gt;Produkt-Spotlight: Huge peak, strong bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter with high inrush current peaks
&lt;br&gt;For motor interference suppression
&lt;br&gt;EMI suppression of DC/DC converters and DC power supply
&lt;br&gt;Broadband suppression
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation:&lt;br&gt;
&lt;/b&gt;&lt;br&gt;WB = Wide Band 
&lt;br&gt;HS=High Speed
&lt;br&gt;HC=High Current &lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14822v209%20Family_WE-MPSB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14822v209%20Family_WE-MPSB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MPSB?"&gt;http://katalog.we-online.de/en/pbs/WE-MPSB?&lt;/a&gt;&lt;p&gt;


Updated  by  Ella Wu 2019-01-02&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_HC" package="WE-MPSB_1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74279226101">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279226101.pdf"/>
<attribute name="IR" value="8000mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279226101 "/>
<attribute name="RDC-MAX" value="6mOhm"/>
<attribute name="RDC-TYP" value="4.5mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="100Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="160Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MPSB_0805" prefix="L">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Specified peak current capability
&lt;br&gt;Ultra low RDC
&lt;br&gt;High Rated Current up to 10.5 A
&lt;br&gt;Operating Temperature: -55°C to +125°C
&lt;br&gt;Produkt-Spotlight: Huge peak, strong bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter with high inrush current peaks
&lt;br&gt;For motor interference suppression
&lt;br&gt;EMI suppression of DC/DC converters and DC power supply
&lt;br&gt;Broadband suppression
&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Package name and Variant abbreviation:&lt;br&gt;&lt;br&gt;
Package: 
&lt;/b&gt;&lt;br&gt;Wide Band /High Speed: W=Width= 3.0
&lt;br&gt;High Current: W=Width= 4.0
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation:
&lt;/b&gt;&lt;br&gt;WB = Wide Band 
&lt;br&gt;HS=High Speed
&lt;br&gt;HC=High Current 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14822v209%20Family_WE-MPSB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14822v209%20Family_WE-MPSB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MPSB?"&gt;http://katalog.we-online.de/en/pbs/WE-MPSB?&lt;/a&gt;&lt;p&gt;


Updated  by  Ella Wu 2019-01-02&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_HC" package="WE-MPSB_0805(W=4.0)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74279220181">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279220181.pdf"/>
<attribute name="IR" value="3100mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279220181 "/>
<attribute name="RDC-MAX" value="37mOhm"/>
<attribute name="RDC-TYP" value="26.5mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="180Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="202Ohm"/>
</technology>
<technology name="_74279220321">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279220321.pdf"/>
<attribute name="IR" value="2500mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279220321 "/>
<attribute name="RDC-MAX" value="50mOhm"/>
<attribute name="RDC-TYP" value="30.5mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="320Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="347Ohm"/>
</technology>
<technology name="_74279220601">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279220601.pdf"/>
<attribute name="IR" value="2100mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279220601 "/>
<attribute name="RDC-MAX" value="80mOhm"/>
<attribute name="RDC-TYP" value="43mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="600Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="551Ohm"/>
</technology>
<technology name="_74279220800">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279220800.pdf"/>
<attribute name="IR" value="4000mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279220800 "/>
<attribute name="RDC-MAX" value="18mOhm"/>
<attribute name="RDC-TYP" value="13mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="80Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="120Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MPSB_1612" prefix="L">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Specified peak current capability
&lt;br&gt;Ultra low RDC
&lt;br&gt;High Rated Current up to 10.5 A
&lt;br&gt;Operating Temperature: -55°C to +125°C
&lt;br&gt;Produkt-Spotlight: Huge peak, strong bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter with high inrush current peaks
&lt;br&gt;For motor interference suppression
&lt;br&gt;EMI suppression of DC/DC converters and DC power supply
&lt;br&gt;Broadband suppression
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation:&lt;br&gt;
&lt;/b&gt;&lt;br&gt;WB = Wide Band 
&lt;br&gt;HS=High Speed
&lt;br&gt;HC=High Current &lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14822v209%20Family_WE-MPSB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14822v209%20Family_WE-MPSB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MPSB?"&gt;http://katalog.we-online.de/en/pbs/WE-MPSB?&lt;/a&gt;&lt;p&gt;


Updated  by  Ella Wu 2019-01-02&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_HC" package="WE-MPSB_1612">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74279223560">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279223560.pdf"/>
<attribute name="IR" value="10000mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279223560 "/>
<attribute name="RDC-MAX" value="4mOhm"/>
<attribute name="RDC-TYP" value="2.5mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="56Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="90Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MPSB_1206" prefix="L">
<description>&lt;b&gt;WE-MPSB EMI Multilayer Power Suppression Bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Specified peak current capability
&lt;br&gt;Ultra low RDC
&lt;br&gt;High Rated Current up to 10.5 A
&lt;br&gt;Operating Temperature: -55°C to +125°C
&lt;br&gt;Produkt-Spotlight: Huge peak, strong bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter with high inrush current peaks
&lt;br&gt;For motor interference suppression
&lt;br&gt;EMI suppression of DC/DC converters and DC power supply
&lt;br&gt;Broadband suppression
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt; Package name and Variant abbreviation:&lt;br&gt;&lt;br&gt;
Package: 
&lt;/b&gt;&lt;br&gt;Wide Band /High Speed: W=Width= 4.2
&lt;br&gt;High Current: W=Width= 5.2
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation:
&lt;/b&gt;&lt;br&gt;WB = Wide Band 
&lt;br&gt;HS=High Speed
&lt;br&gt;HC=High Current 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14822v209%20Family_WE-MPSB.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14822v209%20Family_WE-MPSB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MPSB?"&gt;http://katalog.we-online.de/en/pbs/WE-MPSB?&lt;/a&gt;&lt;p&gt;


Updated  by  Ella Wu 2019-01-02&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_HC" package="WE-MPSB_1206(W=5.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74279221100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279221100.pdf"/>
<attribute name="IR" value="10500mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279221100 "/>
<attribute name="RDC-MAX" value="3mOhm"/>
<attribute name="RDC-TYP" value="1mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="10Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="41Ohm"/>
</technology>
<technology name="_74279221111">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279221111.pdf"/>
<attribute name="IR" value="5400mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279221111 "/>
<attribute name="RDC-MAX" value="15mOhm"/>
<attribute name="RDC-TYP" value="9.5mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="110Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="118Ohm"/>
</technology>
<technology name="_74279221281">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279221281.pdf"/>
<attribute name="IR" value="3500mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279221281 "/>
<attribute name="RDC-MAX" value="35mOhm"/>
<attribute name="RDC-TYP" value="22mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="280Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="288Ohm"/>
</technology>
<technology name="_74279221601">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74279221601.pdf"/>
<attribute name="IR" value="2500mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279221601 "/>
<attribute name="RDC-MAX" value="50mOhm"/>
<attribute name="RDC-TYP" value="38mOhm"/>
<attribute name="TYPE" value="High Current"/>
<attribute name="VALUE" value="600Ohm@ 100 MHz"/>
<attribute name="ZMAX" value="610Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
