<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Transformers For AC/DC Converter - WE-OLTI&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-02-07&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-OLTI_EE16/8/5_L17.78W26.9H13.8">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EE16/8/5,SMT,12pins
&lt;br&gt;LXWXH=17.78X26.9X13.8mm
&lt;br&gt;Bobbin: 070-5642</description>
</package>
<package name="WE-OLTI_EP13_L14.22W14.22H12.7">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP13,THT,10pins
&lt;br&gt;LXWXH=14.22X14.22X12.7mm
&lt;br&gt;Bobbin: 070-4821</description>
</package>
<package name="WE-OLTI_ER28/14_L31W31H25">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: ER28/14,THT,12pins
&lt;br&gt;LXWXH=31X31X25mm
&lt;br&gt;Bobbin: 070-4869</description>
</package>
<package name="WE-OLTI_ER28/17_L32W39H36">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: ER28/17,THT,12pins
&lt;br&gt;LXWXH=32X39X36mm
&lt;br&gt;Bobbin: 070-5652</description>
</package>
<package name="WE-OLTI_ETD29_L35.56W24.38H44.2">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: ETD29,THT,14pins
&lt;br&gt;LXWXH=35.56X24.38X44.2mm
&lt;br&gt;Bobbin: 070-4772</description>
</package>
<package name="WE-OLTI_EE20/10/6_L22.2W26H16.5">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers 
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EE20/10/6,THT,14pins
&lt;br&gt;LXWXH=22.2X26X16mm
&lt;br&gt;Bobbin: 070-5643</description>
</package>
<package name="WE-OLTI_EE20/10/6_L22.2W25H16.5_12PINS">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers 
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EE20/10/6,THT,12pins
&lt;br&gt;LXWXH=22.2X25X16mm
&lt;br&gt;Bobbin: 070-5643</description>
</package>
<package name="WE-OLTI_PQ2625_L29.2W30.35H29.3">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: PQ2625,THT,10pins
&lt;br&gt;LXWXH=29.2X30.35X29.3
&lt;br&gt;Bobbin: 070-5649</description>
</package>
<package name="WE-OLTI_EE16/7/5_L18.8W17.5H14.2">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EE16/7/5,THT,10pins
&lt;br&gt;LXWXH=18.8X17.5X14.2mm
&lt;br&gt;Bobbin: 070-5472</description>
</package>
<package name="WE-OLTI_EE13/7/4_L13.72W20.45H10.54">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: EE13/7/4,THT,9pins
&lt;br&gt;LXWXH=13.72X20.45X10.54mm
&lt;br&gt;Bobbin: 070-5662</description>
</package>
<package name="WE-OLTI_EFD25_L26.3W33H14.76">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EFD25,THT,12pins
&lt;br&gt;LXWXH=26.3X33X14.76mm
&lt;br&gt;Bobbin: 070-6008</description>
</package>
<package name="WE-OLTI_EFD20_L21.5W29H12.45">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EFD20,THT,10pins
&lt;br&gt;LXWXH=21.5X29X12.45mm
&lt;br&gt;Bobbin: 070-5982</description>
</package>
<package name="WE-OLTI_ER28/14_L30.5W24H33">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: ER28/14,THT,10pins
&lt;br&gt;LXWXH=30.5X24X33mm
&lt;br&gt;Bobbin: 070-5576</description>
</package>
<package name="WE-OLTI_EE25/13/7_L27.05W32.25H22.86">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EE25/13/7,THT,14pins
&lt;br&gt;LXWXH=27.05X32.25X22.86mm
&lt;br&gt;Bobbin: 070-5644</description>
</package>
<package name="WE-OLTI_EE16/7/5_L20W17.5H14">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EE16/7/5,THT,10pins
&lt;br&gt;LXWXH=20X17.5X14mm
&lt;br&gt;Bobbin: 070-7101</description>
</package>
<package name="WE-OLTI_EE25/13/7_L27.05W32.25H22.86_13PINS">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EE25/13/7,THT,13pins
&lt;br&gt;LXWXH=27.05X32.25X22.86mm
&lt;br&gt;Bobbin: 070-5644</description>
</package>
<package name="WE-OLTI_ERL35_L36.5W44H28.5">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: ERL35,THT,14pins
&lt;br&gt;LXWXH=36.5X44X28.5mm
&lt;br&gt;Bobbin: 070-5783</description>
</package>
<package name="WE-OLTI_EE16/8/5_L20.32W24.38H16">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EE16/8/5,THT,9pins
&lt;br&gt;LXWXH=20.32X24.38X16mm
&lt;br&gt;Bobbin: 070-5280</description>
</package>
<package name="WE-OLTI_ETD39_L49W41.9H31.75">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: ETD39,THT,16pins
&lt;br&gt;LXWXH=49X41.9X31.75mm
&lt;br&gt;Bobbin: 070-5724</description>
</package>
</packages>
<symbols>
<symbol name="WE-OLTI_EE16/8/5_2W:2W">
<pin name="1" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EP13_2W:1W">
<pin name="P2" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="P1" direction="pas"/>
<pin name="A1" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_ER28/14_2W:2W">
<pin name="P2" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="P1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="S4" direction="pas"/>
<pin name="S3" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_ER28/17_3W:1W">
<pin name="2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EE20/10/6_2W:3W_PARALLEL">
<pin name="1" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EE20/10/6_2W:2W">
<pin name="P2" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="P1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="S4" direction="pas"/>
<pin name="S3" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_PQ2625_2W:1W">
<pin name="P2" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="P1" direction="pas"/>
<pin name="A1" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EFD20_2W:3W_CENTERTAP">
<pin name="1" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EE20/10/6_2W:3W">
<pin name="1" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_ETD29_2W:4W_CENTERTAP">
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_ER28/14_2W:2W_PARALLEL">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EE16/7/5_2W:1W">
<pin name="P2" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="P1" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EE13/7/4_2W:1W">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EFD25_2W:3W_PARALLEL">
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EE20/10/6_2W:2W_CENTERTAP">
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="10+11" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="13+14" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EE25/13/7_2W:4W">
<pin name="1" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EE20/10/6_2W:1W">
<pin name="P2" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="P1" direction="pas"/>
<pin name="A1" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EE16/7/5_2W:2W_PARALLEL">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EE25/13/7_2W:3W_PARALLEL">
<pin name="2" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EE16/7/5_2W:2W">
<pin name="1" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_ERL35_3W:3W_PARALLEL">
<pin name="2" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EE16/8/5_2W:1W">
<pin name="1" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EE25/13/7_3W:4W_PARALLEL">
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_EE16/8/5_2W:2W_PARALLEL">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="WE-OLTI_ETD39_3W:3W_PARALLEL">
<pin name="2" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="7508111323" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE16/8/5_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE16/8/5_L17.78W26.9H13.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508111323?ae"/>
<attribute name="FSWITCH" value="50 - 102kHz"/>
<attribute name="HEIGHT" value="13.8mm"/>
<attribute name="IOUT1" value="1000mA"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="L" value="2000uH"/>
<attribute name="LENGTH" value="17.78mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="8:1:1:1"/>
<attribute name="PART-NUMBER" value="7508111323"/>
<attribute name="SIZE" value="EE16/8/5"/>
<attribute name="VALUE" value="2000uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="625V(AC)"/>
<attribute name="WIDTH" value="26.9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508110151" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EP13_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EP13_L14.22W14.22H12.7">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="P1" pad="3"/>
<connect gate="G$1" pin="P2" pad="5"/>
<connect gate="G$1" pin="S1" pad="9"/>
<connect gate="G$1" pin="S2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508110151?ae"/>
<attribute name="FSWITCH" value="70kHz"/>
<attribute name="HEIGHT" value="12.7mm"/>
<attribute name="IOUT1" value="1000mA"/>
<attribute name="ISAT" value="0.425A"/>
<attribute name="L" value="1500uH"/>
<attribute name="LENGTH" value="14.22mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="15.42:1:3.14"/>
<attribute name="PART-NUMBER" value="7508110151"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="1500uH"/>
<attribute name="VAUX" value="15V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="4000V(AC)"/>
<attribute name="WIDTH" value="14.22mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508110127" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EP13_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EP13_L14.22W14.22H12.7">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="P1" pad="3"/>
<connect gate="G$1" pin="P2" pad="5"/>
<connect gate="G$1" pin="S1" pad="9"/>
<connect gate="G$1" pin="S2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508110127?ae"/>
<attribute name="FSWITCH" value="120kHz"/>
<attribute name="HEIGHT" value="12.7mm"/>
<attribute name="IOUT1" value="1000mA"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="L" value="1050uH"/>
<attribute name="LENGTH" value="14.22mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="14.16:1:3.17"/>
<attribute name="PART-NUMBER" value="7508110127"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="1050uH"/>
<attribute name="VAUX" value="15V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="4000V(AC)"/>
<attribute name="WIDTH" value="14.22mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750813743" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_ER28/14_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_ER28/14_L31W31H25">
<connects>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="P1" pad="3"/>
<connect gate="G$1" pin="P2" pad="1"/>
<connect gate="G$1" pin="S1" pad="7"/>
<connect gate="G$1" pin="S2" pad="9"/>
<connect gate="G$1" pin="S3" pad="10"/>
<connect gate="G$1" pin="S4" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750813743?ae"/>
<attribute name="FSWITCH" value="60kHz"/>
<attribute name="HEIGHT" value="25mm"/>
<attribute name="IOUT1" value="4050mA"/>
<attribute name="IOUT2" value="4050mA"/>
<attribute name="ISAT" value="7.3A"/>
<attribute name="L" value="180uH"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="10:1:1:1"/>
<attribute name="PART-NUMBER" value="750813743"/>
<attribute name="SIZE" value="ER28/14"/>
<attribute name="VALUE" value="180uH"/>
<attribute name="VAUX" value="15V"/>
<attribute name="VIN" value="90 - 144 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VT" value="3750V(AC)"/>
<attribute name="WIDTH" value="31mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508113417" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_ER28/17_3W:1W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_ER28/17_L32W39H36">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508113417?ae"/>
<attribute name="FSWITCH" value="30 - 130kHz"/>
<attribute name="HEIGHT" value="36mm"/>
<attribute name="IOUT1" value="3850mA"/>
<attribute name="ISAT" value="9.1A"/>
<attribute name="L" value="140uH"/>
<attribute name="LENGTH" value="32mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="3.25:1:0.58"/>
<attribute name="PART-NUMBER" value="7508113417"/>
<attribute name="SIZE" value="ER28/17"/>
<attribute name="VALUE" value="140uH"/>
<attribute name="VAUX" value="11V"/>
<attribute name="VIN" value="64 - 265 V (AC)"/>
<attribute name="VOUT1" value="19V"/>
<attribute name="VT" value="3000V(AC)"/>
<attribute name="WIDTH" value="39mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750317406" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE20/10/6_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE20/10/6_L22.2W26H16.5">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="P1" pad="3"/>
<connect gate="G$1" pin="P2" pad="1"/>
<connect gate="G$1" pin="S1" pad="11"/>
<connect gate="G$1" pin="S2" pad="13"/>
<connect gate="G$1" pin="S3" pad="8"/>
<connect gate="G$1" pin="S4" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750317406?ae"/>
<attribute name="FSWITCH" value="100kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="1100mA"/>
<attribute name="IOUT2" value="10mA"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L" value="600uH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="21:3:1:6"/>
<attribute name="PART-NUMBER" value="750317406"/>
<attribute name="SIZE" value="EE20/10/6"/>
<attribute name="VALUE" value="600uH"/>
<attribute name="VAUX" value="25V"/>
<attribute name="VIN" value="85 - 400 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VOUT2" value="4V"/>
<attribute name="VT" value="4800V(AC)"/>
<attribute name="WIDTH" value="25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508112339" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE20/10/6_2W:3W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE20/10/6_L22.2W26H16.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508112339?ae"/>
<attribute name="FSWITCH" value="100kHz"/>
<attribute name="HEIGHT" value="16.5mm"/>
<attribute name="IOUT1" value="3000mA"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="L" value="220uH"/>
<attribute name="LENGTH" value="22.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="7:1:1.5:0.5"/>
<attribute name="PART-NUMBER" value="7508112339"/>
<attribute name="SIZE" value="EE20/10/6"/>
<attribute name="VALUE" value="220uH"/>
<attribute name="VAUX" value="18V"/>
<attribute name="VAUX2" value="6V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="4500V(AC)"/>
<attribute name="WIDTH" value="25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750342585" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_ETD29_2W:4W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-OLTI_ETD29_L35.56W24.38H44.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750342585?ae"/>
<attribute name="FSWITCH" value="68kHz"/>
<attribute name="HEIGHT" value="44.2mm"/>
<attribute name="IOUT1" value="2000mA"/>
<attribute name="IOUT2" value="140mA"/>
<attribute name="IOUT3" value="140mA"/>
<attribute name="ISAT" value="0.0062A"/>
<attribute name="L" value="2500uH"/>
<attribute name="LENGTH" value="35.56mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="35.5:1:2:2:0.75:2"/>
<attribute name="PART-NUMBER" value="750342585"/>
<attribute name="SIZE" value="ETD29"/>
<attribute name="VALUE" value="2500uH"/>
<attribute name="VAUX" value="16V"/>
<attribute name="VIN" value="400 - 690 V (AC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VOUT2" value="16V"/>
<attribute name="VOUT3" value="16V"/>
<attribute name="VT" value="3800V(AC)"/>
<attribute name="WIDTH" value="24.38mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750316585" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE20/10/6_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE20/10/6_L22.2W26H16.5">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="P1" pad="3"/>
<connect gate="G$1" pin="P2" pad="1"/>
<connect gate="G$1" pin="S1" pad="12"/>
<connect gate="G$1" pin="S2" pad="14"/>
<connect gate="G$1" pin="S3" pad="8"/>
<connect gate="G$1" pin="S4" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316585?ae"/>
<attribute name="FSWITCH" value="30kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="1500mA"/>
<attribute name="IOUT2" value="2000mA"/>
<attribute name="ISAT" value="2.75A"/>
<attribute name="L" value="600uH"/>
<attribute name="LENGTH" value="22.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="5.81:3:2.18:1:5.81"/>
<attribute name="PART-NUMBER" value="750316585"/>
<attribute name="SIZE" value="EE20/10/6"/>
<attribute name="VALUE" value="600uH"/>
<attribute name="VAUX" value="17V"/>
<attribute name="VIN" value="177 - 473 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VT" value="4000V(AC)"/>
<attribute name="WIDTH" value="25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750811647" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE20/10/6_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE20/10/6_L22.2W26H16.5">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="P1" pad="3"/>
<connect gate="G$1" pin="P2" pad="1"/>
<connect gate="G$1" pin="S1" pad="8"/>
<connect gate="G$1" pin="S2" pad="11"/>
<connect gate="G$1" pin="S3" pad="10"/>
<connect gate="G$1" pin="S4" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811647?ae"/>
<attribute name="FSWITCH" value="100kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="1000mA"/>
<attribute name="IOUT2" value="1000mA"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="L" value="250uH"/>
<attribute name="LENGTH" value="22.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="10:1:2.5:2.75"/>
<attribute name="PART-NUMBER" value="750811647"/>
<attribute name="SIZE" value="EE16/8/5"/>
<attribute name="VALUE" value="250uH"/>
<attribute name="VAUX" value="18V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="17.4V"/>
<attribute name="VOUT2" value="6.6V"/>
<attribute name="VT" value="3500V(AC)"/>
<attribute name="WIDTH" value="26mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750817930" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE20/10/6_2W:3W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE20/10/6_L22.2W25H16.5_12PINS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750817930?ae"/>
<attribute name="FSWITCH" value="100kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="700mA"/>
<attribute name="IOUT2" value="700mA"/>
<attribute name="IOUT3" value="700mA"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="L" value="350uH"/>
<attribute name="LENGTH" value="22.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="7:1:1:1:1.5"/>
<attribute name="PART-NUMBER" value="750817930"/>
<attribute name="SIZE" value="EE20/10/6"/>
<attribute name="VALUE" value="350uH"/>
<attribute name="VAUX" value="18V"/>
<attribute name="VIN" value="71 - 481 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VOUT3" value="12V"/>
<attribute name="VT" value="3000V(AC)"/>
<attribute name="WIDTH" value="25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750343068" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_PQ2625_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_PQ2625_L29.2W30.35H29.3">
<connects>
<connect gate="G$1" pin="A1" pad="7"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="P1" pad="3"/>
<connect gate="G$1" pin="P2" pad="1"/>
<connect gate="G$1" pin="S1" pad="12"/>
<connect gate="G$1" pin="S2" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750343068?ae"/>
<attribute name="FSWITCH" value="65kHz"/>
<attribute name="HEIGHT" value="29.3mm"/>
<attribute name="IOUT1" value="2500mA"/>
<attribute name="ISAT" value="4.4A"/>
<attribute name="L" value="230uH"/>
<attribute name="LENGTH" value="29.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="3.88:1:0.83"/>
<attribute name="PART-NUMBER" value="750343068"/>
<attribute name="SIZE" value="PQ2625"/>
<attribute name="VALUE" value="230uH"/>
<attribute name="VAUX" value="18V"/>
<attribute name="VIN" value="60 - 283 V (AC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VT" value="3000V(AC)"/>
<attribute name="WIDTH" value="30.35mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750343661" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE20/10/6_2W:2W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE20/10/6_L22.2W26H16.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10+11" pad="10 11"/>
<connect gate="G$1" pin="13+14" pad="13 14"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750343661?ae"/>
<attribute name="FSWITCH" value="85kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="250mA"/>
<attribute name="IOUT2" value="3000mA"/>
<attribute name="ISAT" value="6A"/>
<attribute name="L" value="500uH"/>
<attribute name="LENGTH" value="22.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="8:1.75:1:2.75"/>
<attribute name="PART-NUMBER" value="750343661"/>
<attribute name="SIZE" value="EE20/10/6"/>
<attribute name="VALUE" value="500uH"/>
<attribute name="VAUX" value="15V"/>
<attribute name="VIN" value="71 - 301 V (AC)"/>
<attribute name="VOUT1" value="15V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VT" value="3000V(AC)"/>
<attribute name="WIDTH" value="25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315526" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE16/7/5_2W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE16/7/5_L18.8W17.5H14.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315526?ae"/>
<attribute name="FSWITCH" value="100kHz"/>
<attribute name="HEIGHT" value="13.8mm"/>
<attribute name="IOUT1" value="2000mA"/>
<attribute name="ISAT" value="1.25A"/>
<attribute name="L" value="435uH"/>
<attribute name="LENGTH" value="17.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="13.2:1:3.8"/>
<attribute name="PART-NUMBER" value="750315526"/>
<attribute name="SIZE" value="EE16/7/5"/>
<attribute name="VALUE" value="435uH"/>
<attribute name="VAUX" value="20V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="3900V(AC)"/>
<attribute name="WIDTH" value="18.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750815039" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE16/7/5_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE16/7/5_L18.8W17.5H14.2">
<connects>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="P1" pad="3"/>
<connect gate="G$1" pin="P2" pad="1"/>
<connect gate="G$1" pin="S1" pad="7"/>
<connect gate="G$1" pin="S2" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750815039?ae"/>
<attribute name="FSWITCH" value="40 - 130kHz"/>
<attribute name="HEIGHT" value="14.2mm"/>
<attribute name="IOUT1" value="300mA"/>
<attribute name="ISAT" value="0.225A"/>
<attribute name="L" value="6600uH"/>
<attribute name="LENGTH" value="17.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="18:1:1"/>
<attribute name="PART-NUMBER" value="750815039"/>
<attribute name="SIZE" value="EE16/7/5"/>
<attribute name="VALUE" value="6600uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VIN" value="184 - 265 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="4000V(AC)"/>
<attribute name="WIDTH" value="18.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508110329" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE16/7/5_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE16/7/5_L18.8W17.5H14.2">
<connects>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="P1" pad="3"/>
<connect gate="G$1" pin="P2" pad="1"/>
<connect gate="G$1" pin="S1" pad="7"/>
<connect gate="G$1" pin="S2" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508110329?ae"/>
<attribute name="FSWITCH" value="130kHz"/>
<attribute name="HEIGHT" value="17.5mm"/>
<attribute name="IOUT1" value="340mA"/>
<attribute name="ISAT" value="0.575A"/>
<attribute name="L" value="700uH"/>
<attribute name="LENGTH" value="17.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="6.6:1:1"/>
<attribute name="PART-NUMBER" value="7508110329"/>
<attribute name="SIZE" value="EE16/7/5"/>
<attribute name="VALUE" value="700uH"/>
<attribute name="VAUX" value="15V"/>
<attribute name="VIN" value="70 - 265 V (AC)"/>
<attribute name="VOUT1" value="15V"/>
<attribute name="VT" value="4000V(AC)"/>
<attribute name="WIDTH" value="18.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315241" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE20/10/6_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE20/10/6_L22.2W26H16.5">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="P1" pad="3"/>
<connect gate="G$1" pin="P2" pad="1"/>
<connect gate="G$1" pin="S1" pad="9"/>
<connect gate="G$1" pin="S2" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315241?ae"/>
<attribute name="FSWITCH" value="45kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="1000mA"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="L" value="1100uH"/>
<attribute name="LENGTH" value="22.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="4:1:0.5"/>
<attribute name="PART-NUMBER" value="750315241"/>
<attribute name="SIZE" value="EE20/10/6"/>
<attribute name="VALUE" value="1100uH"/>
<attribute name="VAUX" value="18V"/>
<attribute name="VIN" value="142 - 284 V (AC)"/>
<attribute name="VOUT1" value="36V"/>
<attribute name="VT" value="3000V(AC)"/>
<attribute name="WIDTH" value="25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508112341" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EFD25_2W:3W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EFD25_L26.3W33H14.76">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508112341?ae"/>
<attribute name="FSWITCH" value="60 - 120kHz"/>
<attribute name="HEIGHT" value="14.76mm"/>
<attribute name="IOUT1" value="3000mA"/>
<attribute name="ISAT" value="3.3A"/>
<attribute name="L" value="380uH"/>
<attribute name="LENGTH" value="26.3mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="7:1:1"/>
<attribute name="PART-NUMBER" value="7508112341"/>
<attribute name="SIZE" value="EFD25"/>
<attribute name="VALUE" value="380uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="4500V(AC)"/>
<attribute name="WIDTH" value="33mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750318383" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EFD20_2W:3W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EFD20_L21.5W29H12.45">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750318383?ae"/>
<attribute name="FSWITCH" value="66kHz"/>
<attribute name="HEIGHT" value="12.45mm"/>
<attribute name="IOUT1" value="300mA"/>
<attribute name="IOUT2" value="2000mA"/>
<attribute name="IOUT3" value="300mA"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="L" value="680uH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="29.33:1:1.67:3:3"/>
<attribute name="PART-NUMBER" value="750318383"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="VALUE" value="680uH"/>
<attribute name="VAUX" value="15V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VOUT2" value="7V"/>
<attribute name="VOUT3" value="-15V"/>
<attribute name="VT" value="3750V(AC)"/>
<attribute name="WIDTH" value="29mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750343466" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE20/10/6_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE20/10/6_L22.2W26H16.5">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="P1" pad="3"/>
<connect gate="G$1" pin="P2" pad="1"/>
<connect gate="G$1" pin="S1" pad="8 9"/>
<connect gate="G$1" pin="S2" pad="12 13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750343466?ae"/>
<attribute name="FSWITCH" value="100kHz"/>
<attribute name="HEIGHT" value="16.5mm"/>
<attribute name="IOUT1" value="1500mA"/>
<attribute name="ISAT" value="1.88A"/>
<attribute name="L" value="280uH"/>
<attribute name="LENGTH" value="22.2mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="4.29 : 1 : 0.72"/>
<attribute name="PART-NUMBER" value="750343466"/>
<attribute name="SIZE" value="EE20/10/6"/>
<attribute name="VALUE" value="280uH"/>
<attribute name="VAUX" value="16.5V"/>
<attribute name="VIN" value="60 - 282 V (AC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VT" value="3000V(AC)"/>
<attribute name="WIDTH" value="25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508110331" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE13/7/4_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE13/7/4_L13.72W20.45H10.54">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508110331?ae"/>
<attribute name="FSWITCH" value="130kHz"/>
<attribute name="HEIGHT" value="10.54mm"/>
<attribute name="IOUT1" value="250mA"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="L" value="500uH"/>
<attribute name="LENGTH" value="13.72mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="3.25:1:1"/>
<attribute name="PART-NUMBER" value="7508110331"/>
<attribute name="SIZE" value="EE13/7/4"/>
<attribute name="VALUE" value="500uH"/>
<attribute name="VAUX" value="15V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="15V"/>
<attribute name="VT" value="3000V(AC)"/>
<attribute name="WIDTH" value="20.45mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315046" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE25/13/7_2W:3W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE25/13/7_L27.05W32.25H22.86">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315046?ae"/>
<attribute name="FSWITCH" value="60kHz"/>
<attribute name="HEIGHT" value="22.86mm"/>
<attribute name="IOUT1" value="2100mA"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="1000uH"/>
<attribute name="LENGTH" value="27.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="8.67:1:1"/>
<attribute name="PART-NUMBER" value="750315046"/>
<attribute name="SIZE" value="EE25/13/7"/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="VAUX" value="24V"/>
<attribute name="VIN" value="141 - 403 V (AC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VT" value="3000V(AC)"/>
<attribute name="WIDTH" value="32.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750344367" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE16/7/5_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE16/7/5_L20W17.5H14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750344367?ae"/>
<attribute name="FSWITCH" value="110kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="IOUT1" value="100mA"/>
<attribute name="IOUT2" value="900mA"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="L" value="1600uH"/>
<attribute name="LENGTH" value="17.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="16:2:1:2"/>
<attribute name="PART-NUMBER" value="750344367"/>
<attribute name="SIZE" value="EE16/7/5"/>
<attribute name="VALUE" value="1600uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VIN" value="269 - 282 V (AC)"/>
<attribute name="VOUT1" value="18V"/>
<attribute name="VOUT2" value="6V"/>
<attribute name="VT" value="3000V(AC)"/>
<attribute name="WIDTH" value="20mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750343004" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_ER28/14_2W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-OLTI_ER28/14_L30.5W24H33">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750343004?ae"/>
<attribute name="FSWITCH" value="65kHz"/>
<attribute name="HEIGHT" value="33mm"/>
<attribute name="IOUT1" value="3850mA"/>
<attribute name="ISAT" value="4.7A"/>
<attribute name="L" value="160uH"/>
<attribute name="LENGTH" value="30.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="4:1:0.78"/>
<attribute name="PART-NUMBER" value="750343004"/>
<attribute name="SIZE" value="ER28/14"/>
<attribute name="VALUE" value="160uH"/>
<attribute name="VAUX" value="18V"/>
<attribute name="VIN" value="106 - 286 V (AC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VT" value="3750V(AC)"/>
<attribute name="WIDTH" value="24mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750342851" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE25/13/7_2W:4W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE25/13/7_L27.05W32.25H22.86_13PINS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750342851?ae"/>
<attribute name="FSWITCH" value="75kHz"/>
<attribute name="HEIGHT" value="22.86mm"/>
<attribute name="IOUT1" value="1000mA"/>
<attribute name="IOUT2" value="65mA"/>
<attribute name="IOUT3" value="65mA"/>
<attribute name="ISAT" value="2.78A"/>
<attribute name="L" value="150uH"/>
<attribute name="LENGTH" value="27.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="3.75:1.5:1:1:1:1"/>
<attribute name="PART-NUMBER" value="750342851"/>
<attribute name="SIZE" value="EE25/13/7"/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VAUX" value="15V"/>
<attribute name="VIN" value="43 - 318 V (AC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VOUT2" value="15V"/>
<attribute name="VOUT3" value="15V"/>
<attribute name="VT" value="1250V(AC)"/>
<attribute name="WIDTH" value="32.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315242" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE25/13/7_3W:4W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE25/13/7_L27.05W32.25H22.86">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315242?ae"/>
<attribute name="FSWITCH" value="45kHz"/>
<attribute name="HEIGHT" value="22.86mm"/>
<attribute name="IOUT1" value="1800mA"/>
<attribute name="IOUT2" value="1800mA"/>
<attribute name="ISAT" value="2.3A"/>
<attribute name="L" value="600uH"/>
<attribute name="LENGTH" value="27.05mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="12:1:1:1.67:1.33"/>
<attribute name="PART-NUMBER" value="750315242"/>
<attribute name="SIZE" value="EE25/13/7"/>
<attribute name="VALUE" value="600uH"/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX2" value="16V"/>
<attribute name="VIN" value="141 - 283 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VT" value="3000V(AC)"/>
<attribute name="WIDTH" value="32.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750316686" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE16/8/5_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE16/8/5_L20.32W24.38H16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316686?ae"/>
<attribute name="FSWITCH" value="70kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="1000mA"/>
<attribute name="ISAT" value="0.925A"/>
<attribute name="L" value="500uH"/>
<attribute name="LENGTH" value="20.32mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="6:1:1"/>
<attribute name="PART-NUMBER" value="750316686"/>
<attribute name="SIZE" value="EE16/8/5"/>
<attribute name="VALUE" value="500uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="3000V(AC)"/>
<attribute name="WIDTH" value="24.38mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313739" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_EE16/8/5_2W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-OLTI_EE16/8/5_L20.32W24.38H16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313739?ae"/>
<attribute name="FSWITCH" value="115kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="1200mA"/>
<attribute name="ISAT" value="0.65A"/>
<attribute name="L" value="1100uH"/>
<attribute name="LENGTH" value="20.32mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="16.5:1:3.5"/>
<attribute name="PART-NUMBER" value="750313739"/>
<attribute name="SIZE" value="EE16/8/5"/>
<attribute name="VALUE" value="1100uH"/>
<attribute name="VAUX" value="17V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="4500V(AC)"/>
<attribute name="WIDTH" value="24.38mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315340" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_ETD39_3W:3W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-OLTI_ETD39_L49W41.9H31.75">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315340?ae"/>
<attribute name="FSWITCH" value="60kHz"/>
<attribute name="HEIGHT" value="31.75mm"/>
<attribute name="IOUT1" value="10000mA"/>
<attribute name="ISAT" value="15A"/>
<attribute name="L" value="200uH"/>
<attribute name="LENGTH" value="49mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="4.5:1:0.5"/>
<attribute name="PART-NUMBER" value="750315340"/>
<attribute name="SIZE" value="ETD39"/>
<attribute name="VALUE" value="200uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VIN" value="200 - 265 V (AC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VT" value="3000V(AC)"/>
<attribute name="WIDTH" value="41.9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750316326" prefix="T">
<description>&lt;b&gt;WE-OLTI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Nominal input voltage: 85–265 VAC (120–375 VDC)
&lt;br&gt;Small size
&lt;br&gt;Low leakage inductance
&lt;br&gt;Multiple-output options
&lt;br&gt;Operating temperature: −40 °C to +125 °C
&lt;br&gt;Isolation Voltage: 2 kVAC to 5 kVAC
&lt;br&gt;Options for fixed frequency or quasi-resonant mode operation
&lt;br&gt;Most products meet reinforced insulation
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial controls
&lt;br&gt;USB chargers
&lt;br&gt;Utility metering devices
&lt;br&gt;Process controls
&lt;br&gt;Factory automation
&lt;br&gt;Security systems
&lt;br&gt;Garage door opener auxiliary supplies
&lt;br&gt;Home appliances
&lt;br&gt;Especially designed for several ICs from Texas Instruments
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o814034v209%20UtOLTI%20Group%20CGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-06&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLTI_ERL35_3W:3W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-OLTI_ERL35_L36.5W44H28.5">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316326?ae"/>
<attribute name="FSWITCH" value="120kHz"/>
<attribute name="HEIGHT" value="28.5mm"/>
<attribute name="IOUT1" value="6000mA"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="L" value="250uH"/>
<attribute name="LENGTH" value="36.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="4:1:0.5"/>
<attribute name="PART-NUMBER" value="750316326"/>
<attribute name="SIZE" value="ERL35"/>
<attribute name="VALUE" value="250uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="27V"/>
<attribute name="VT" value="3600V(AC)"/>
<attribute name="WIDTH" value="44mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
