<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - Ferrites For PCB Assembly - WE-PBF&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-08-17&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PBF_4030_5X3X3.1(LXWXH)">
<description>&lt;b&gt;WE-PBF Flat Wire High Current SMT Ferrite Bead&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;/b&gt; Size: 4030, SMT, 2pins
&lt;br&gt;L X W X H X FI=5mmX3mmX3.1mmX1.5mm</description>
</package>
<package name="WE-PBF_4030_4X3X2.5(LXWXH)">
<description>&lt;b&gt;WE-PBF Flat Wire High Current SMT Ferrite Bead&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;/b&gt; Size: 4030, SMT, 2pins
&lt;br&gt;L X W X H X FI=4mmX3mmX2.5mmX1.3mm</description>
</package>
<package name="WE-PBF_8530">
<description>&lt;b&gt;WE-PBF Flat Wire High Current SMT Ferrite Bead&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;/b&gt; Size: 8530, SMT, 2pins
&lt;br&gt;L X W X H X FI=8.5mmX3mmX2.55mmX1.45mm</description>
</package>
<package name="WE-PBF_3029">
<description>&lt;b&gt;WE-PBF Flat Wire High Current SMT Ferrite Bead&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;/b&gt; Size: 3029, SMT, 2pins
&lt;br&gt;L X W X H X FI=3.1mmX2.9mmX2.41mmX0.8mm</description>
</package>
<package name="WE-PBF_7847">
<description>&lt;b&gt;WE-PBF Flat Wire High Current SMT Ferrite Bead&lt;/b&gt;
&lt;br&gt;&lt;br&gt;&lt;/b&gt; Size: 7847, SMT, 2pins
&lt;br&gt;L X W X H X FI=7.8mmX4.75mmX3mmX1.45mm</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PBF_4030" prefix="L">
<description>&lt;b&gt;WE-PBF Flat Wire High Current SMT Ferrite Bead
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Flat wire
&lt;br&gt; Suitable for applications with high currents up to 6 A
&lt;br&gt; Glued version: High mechanical stability
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Voltage supply for high load current
&lt;br&gt; Glued version: Especially for applications with permanent vibrations
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14824v209%20Family_WE-PBF.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14824v209%20Family_WE-PBF.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-PBF"&gt;https://www.we-online.com/catalog/en/WE-PBF&lt;/a&gt;&lt;p&gt;


Updated  by Ella Wu 2021-08-17&lt;br&gt;
20121 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_5X3X3.1(LXWXH)" package="WE-PBF_4030_5X3X3.1(LXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7427930">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7427930.pdf"/>
<attribute name="HEIGHT" value="2.55mm"/>
<attribute name="IR" value="16A"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7427930 "/>
<attribute name="RDC-MAX" value="0.6mOhm"/>
<attribute name="VALUE" value="42Ohm @100 MHz"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="Z" value="28Ohm @25 MHz"/>
</technology>
<technology name="_74279390">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74279390.pdf"/>
<attribute name="HEIGHT" value="2.55mm"/>
<attribute name="IR" value="16A"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279390 "/>
<attribute name="RDC-MAX" value="0.6mOhm"/>
<attribute name="VALUE" value="42Ohm @100 MHz"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="Z" value="28Ohm @25 MHz"/>
</technology>
</technologies>
</device>
<device name="_4X3X2.5(LXWXH)" package="WE-PBF_4030_4X3X2.5(LXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7427934">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7427934.pdf"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="IR" value="15A"/>
<attribute name="LENGTH" value="4.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7427934 "/>
<attribute name="RDC-MAX" value="0.6mOhm"/>
<attribute name="VALUE" value="42Ohm @100 MHz"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="Z" value="28Ohm @25 MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PBF_3029" prefix="L">
<description>&lt;b&gt;WE-PBF Flat Wire High Current SMT Ferrite Bead
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Flat wire
&lt;br&gt; Suitable for applications with high currents up to 6 A
&lt;br&gt; Glued version: High mechanical stability
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Voltage supply for high load current
&lt;br&gt; Glued version: Especially for applications with permanent vibrations
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14824v209%20Family_WE-PBF.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14824v209%20Family_WE-PBF.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-PBF"&gt;https://www.we-online.com/catalog/en/WE-PBF&lt;/a&gt;&lt;p&gt;


Updated  by Ella Wu 2021-08-17&lt;br&gt;
20121 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PBF_3029">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7427933">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7427933.pdf"/>
<attribute name="HEIGHT" value="2.41mm"/>
<attribute name="IR" value="14A"/>
<attribute name="LENGTH" value="3.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7427933 "/>
<attribute name="RDC-MAX" value="0.6mOhm"/>
<attribute name="VALUE" value="39Ohm @100 MHz"/>
<attribute name="WIDTH" value="2.9mm"/>
<attribute name="Z" value="23Ohm @25 MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PBF_8530" prefix="L">
<description>&lt;b&gt;WE-PBF Flat Wire High Current SMT Ferrite Bead
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Flat wire
&lt;br&gt; Suitable for applications with high currents up to 6 A
&lt;br&gt; Glued version: High mechanical stability
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Voltage supply for high load current
&lt;br&gt; Glued version: Especially for applications with permanent vibrations
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14824v209%20Family_WE-PBF.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14824v209%20Family_WE-PBF.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-PBF"&gt;https://www.we-online.com/catalog/en/WE-PBF&lt;/a&gt;&lt;p&gt;


Updated  by Ella Wu 2021-08-17&lt;br&gt;
20121 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PBF_8530">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7427931">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7427931.pdf"/>
<attribute name="HEIGHT" value="2.55mm"/>
<attribute name="IR" value="17A"/>
<attribute name="LENGTH" value="8.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7427931 "/>
<attribute name="RDC-MAX" value="0.9mOhm"/>
<attribute name="VALUE" value="91Ohm @100 MHz"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="Z" value="58Ohm @25 MHz"/>
</technology>
<technology name="_74279391">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74279391.pdf"/>
<attribute name="HEIGHT" value="2.55mm"/>
<attribute name="IR" value="17A"/>
<attribute name="LENGTH" value="8.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279391 "/>
<attribute name="RDC-MAX" value="0.9mOhm"/>
<attribute name="VALUE" value="91Ohm @100 MHz"/>
<attribute name="WIDTH" value="3mm"/>
<attribute name="Z" value="58Ohm @25 MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PBF_7847">
<description>&lt;b&gt;WE-PBF Flat Wire High Current SMT Ferrite Bead
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Flat wire
&lt;br&gt; Suitable for applications with high currents up to 6 A
&lt;br&gt; Glued version: High mechanical stability
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Voltage supply for high load current
&lt;br&gt; Glued version: Especially for applications with permanent vibrations
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14824v209%20Family_WE-PBF.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14824v209%20Family_WE-PBF.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-PBF"&gt;https://www.we-online.com/catalog/en/WE-PBF&lt;/a&gt;&lt;p&gt;


Updated  by Ella Wu 2021-08-17&lt;br&gt;
20121 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PBF_7847">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7427932">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7427932.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="18A"/>
<attribute name="LENGTH" value="7.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7427932 "/>
<attribute name="RDC-MAX" value="0.9mOhm"/>
<attribute name="VALUE" value="98Ohm @100 MHz"/>
<attribute name="WIDTH" value="4.75mm"/>
<attribute name="Z" value="65Ohm @25 MHz"/>
</technology>
<technology name="_74279392">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74279392.pdf"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="18A"/>
<attribute name="LENGTH" value="7.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74279392 "/>
<attribute name="RDC-MAX" value="0.9mOhm"/>
<attribute name="VALUE" value="98Ohm @100 MHz"/>
<attribute name="WIDTH" value="4.75mm"/>
<attribute name="Z" value="65Ohm @25 MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
