<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - High Voltage Power Inductors - WE-PD HV&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-06-10&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PDHV_7332">
<description>&lt;b&gt;WE-PD HV SMT Power Inductor (High Voltage)&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 7332, SMT, 2pins
&lt;br&gt;LXWXH=7.3x7.3x3.2mm</description>
</package>
<package name="WE-PDHV_1060">
<description>&lt;b&gt;WE-PD HV SMT Power Inductor (High Voltage)&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 1060, SMT, 2pins
&lt;br&gt;LXWXH=10x10x6mm</description>
</package>
<package name="WE-PDHV_7345">
<description>&lt;b&gt;WE-PD HV SMT Power Inductor (High Voltage)&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 7345, SMT, 2pins
&lt;br&gt;LXWXH=7.3x7.3x4.5mm</description>
</package>
<package name="WE-PDHV_1040">
<description>&lt;b&gt;WE-PD HV SMT Power Inductor (High Voltage)&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 1040, SMT, 2pins
&lt;br&gt;LXWXH=10x10x4mm</description>
</package>
<package name="WE-PDHV_1210">
<description>&lt;b&gt;WE-PD HV SMT Power Inductor (High Voltage)&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 1210, SMT, 2pins
&lt;br&gt;LXWXH=12x12x10.5mm</description>
</package>
<package name="WE-PDHV_1280">
<description>&lt;b&gt;WE-PD HV SMT Power Inductor (High Voltage)&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 1280, SMT, 2pins
&lt;br&gt;LXWXH=12x12x8.5mm</description>
</package>
</packages>
<symbols>
<symbol name="L_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PDHV_7332" prefix="L">
<description>&lt;b&gt;WE-PD HV SMT Power Inductor (High Voltage)
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Shielded part for ideal wire protection
&lt;br&gt;Operating Temperature: -40°C - 125°C
&lt;br&gt;Magnetically shielded
&lt;br&gt;Designed for 400VDC Applications
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Non-isolated buck or Buck-Boost Converter like PI LinkSwitch-TN
&lt;br&gt;constant current LED Driver
&lt;br&gt;Utility metering
&lt;br&gt;Filter for power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14828v209%20WE-PD_HV.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14828v209%20WE-PD_HV.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PD-HV/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PD-HV&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-10&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT"/>
</gates>
<devices>
<device name="" package="WE-PDHV_7332">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7687789102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687789102?ae"/>
<attribute name="FRES" value="2.5MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="0.17A"/>
<attribute name="ISAT" value="0.2A"/>
<attribute name="L" value="1000uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687789102"/>
<attribute name="RDC-MAX" value="9000mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_7687789471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687789471?ae"/>
<attribute name="FRES" value="4.9MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="0.25A"/>
<attribute name="ISAT" value="0.35A"/>
<attribute name="L" value="470uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687789471"/>
<attribute name="RDC-MAX" value="3500mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="470uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_7687789681">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687789681?ae"/>
<attribute name="FRES" value="3.5MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="0.22A"/>
<attribute name="ISAT" value="0.26A"/>
<attribute name="L" value="680uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687789681"/>
<attribute name="RDC-MAX" value="5200mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="680uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_7687789821">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687789821?ae"/>
<attribute name="FRES" value="3.3MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="0.18A"/>
<attribute name="ISAT" value="0.23A"/>
<attribute name="L" value="820uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687789821"/>
<attribute name="RDC-MAX" value="8200mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="820uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PDHV_1060" prefix="L">
<description>&lt;b&gt;WE-PD HV SMT Power Inductor (High Voltage)
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Shielded part for ideal wire protection
&lt;br&gt;Operating Temperature: -40°C - 125°C
&lt;br&gt;Magnetically shielded
&lt;br&gt;Designed for 400VDC Applications
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Non-isolated buck or Buck-Boost Converter like PI LinkSwitch-TN
&lt;br&gt;constant current LED Driver
&lt;br&gt;Utility metering
&lt;br&gt;Filter for power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14828v209%20WE-PD_HV.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14828v209%20WE-PD_HV.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PD-HV/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PD-HV&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-10&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT"/>
</gates>
<devices>
<device name="" package="WE-PDHV_1060">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7687714102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687714102?ae"/>
<attribute name="FRES" value="1.7MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="0.55A"/>
<attribute name="L" value="1000uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687714102"/>
<attribute name="RDC-MAX" value="3200mOhm"/>
<attribute name="SIZE" value="1060"/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7687714152">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687714152?ae"/>
<attribute name="FRES" value="1.4MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="0.32A"/>
<attribute name="ISAT" value="0.46A"/>
<attribute name="L" value="1500uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687714152"/>
<attribute name="RDC-MAX" value="4600mOhm"/>
<attribute name="SIZE" value="1060"/>
<attribute name="VALUE" value="1500uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7687714221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687714221?ae"/>
<attribute name="FRES" value="3.9MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="0.95A"/>
<attribute name="ISAT" value="1.15A"/>
<attribute name="L" value="220uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687714221"/>
<attribute name="RDC-MAX" value="680mOhm"/>
<attribute name="SIZE" value="1060"/>
<attribute name="VALUE" value="220uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7687714222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687714222?ae"/>
<attribute name="FRES" value="1.2MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="0.26A"/>
<attribute name="ISAT" value="0.37A"/>
<attribute name="L" value="2200uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687714222"/>
<attribute name="RDC-MAX" value="6500mOhm"/>
<attribute name="SIZE" value="1060"/>
<attribute name="VALUE" value="2200uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7687714470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687714470?ae"/>
<attribute name="FRES" value="10.2MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="1.7A"/>
<attribute name="ISAT" value="2.3A"/>
<attribute name="L" value="47uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687714470"/>
<attribute name="RDC-MAX" value="156mOhm"/>
<attribute name="SIZE" value="1060"/>
<attribute name="VALUE" value="47uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7687714471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687714471?ae"/>
<attribute name="FRES" value="2.7MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="470uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687714471"/>
<attribute name="RDC-MAX" value="1450mOhm"/>
<attribute name="SIZE" value="1060"/>
<attribute name="VALUE" value="470uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7687714681">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687714681?ae"/>
<attribute name="FRES" value="2MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="0.55A"/>
<attribute name="ISAT" value="0.61A"/>
<attribute name="L" value="680uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687714681"/>
<attribute name="RDC-MAX" value="2250mOhm"/>
<attribute name="SIZE" value="1060"/>
<attribute name="VALUE" value="680uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PDHV_7345" prefix="L">
<description>&lt;b&gt;WE-PD HV SMT Power Inductor (High Voltage)
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Shielded part for ideal wire protection
&lt;br&gt;Operating Temperature: -40°C - 125°C
&lt;br&gt;Magnetically shielded
&lt;br&gt;Designed for 400VDC Applications
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Non-isolated buck or Buck-Boost Converter like PI LinkSwitch-TN
&lt;br&gt;constant current LED Driver
&lt;br&gt;Utility metering
&lt;br&gt;Filter for power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14828v209%20WE-PD_HV.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14828v209%20WE-PD_HV.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PD-HV/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PD-HV&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-10&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT"/>
</gates>
<devices>
<device name="" package="WE-PDHV_7345">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7687779102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687779102?ae"/>
<attribute name="FRES" value="2.3MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="IR" value="0.24A"/>
<attribute name="ISAT" value="0.25A"/>
<attribute name="L" value="1000uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687779102"/>
<attribute name="RDC-MAX" value="6000mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_7687779221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687779221?ae"/>
<attribute name="FRES" value="4.9MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="IR" value="0.56A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="L" value="220uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687779221"/>
<attribute name="RDC-MAX" value="1300mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="220uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_7687779470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687779470?ae"/>
<attribute name="FRES" value="11.3MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="L" value="47uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687779470"/>
<attribute name="RDC-MAX" value="280mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="47uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_7687779471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687779471?ae"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="IR" value="0.35A"/>
<attribute name="ISAT" value="0.37A"/>
<attribute name="L" value="470uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687779471"/>
<attribute name="RDC-MAX" value="3200mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="470uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_7687779561">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687779561?ae"/>
<attribute name="FRES" value="2.9MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="IR" value="0.33A"/>
<attribute name="ISAT" value="0.35A"/>
<attribute name="L" value="560uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687779561"/>
<attribute name="RDC-MAX" value="3600mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="560uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_7687779681">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687779681?ae"/>
<attribute name="FRES" value="2.8MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="L" value="680uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687779681"/>
<attribute name="RDC-MAX" value="4000mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="680uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PDHV_1210" prefix="L">
<description>&lt;b&gt;WE-PD HV SMT Power Inductor (High Voltage)
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Shielded part for ideal wire protection
&lt;br&gt;Operating Temperature: -40°C - 125°C
&lt;br&gt;Magnetically shielded
&lt;br&gt;Designed for 400VDC Applications
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Non-isolated buck or Buck-Boost Converter like PI LinkSwitch-TN
&lt;br&gt;constant current LED Driver
&lt;br&gt;Utility metering
&lt;br&gt;Filter for power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14828v209%20WE-PD_HV.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14828v209%20WE-PD_HV.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PD-HV/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PD-HV&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-10&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT"/>
</gates>
<devices>
<device name="" package="WE-PDHV_1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7687709102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687709102?ae"/>
<attribute name="FRES" value="1.2MHz"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="IR" value="0.72A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="L" value="1000uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687709102"/>
<attribute name="RDC-MAX" value="1400mOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_7687709152">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687709152?ae"/>
<attribute name="FRES" value="0.9MHz"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="IR" value="0.52A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="1500uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687709152"/>
<attribute name="RDC-MAX" value="2200mOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1500uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_7687709221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687709221?ae"/>
<attribute name="FRES" value="2.2MHz"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="220uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687709221"/>
<attribute name="RDC-MAX" value="350mOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="220uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_7687709222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687709222?ae"/>
<attribute name="FRES" value="0.8MHz"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="IR" value="0.43A"/>
<attribute name="ISAT" value="0.65A"/>
<attribute name="L" value="2200uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687709222"/>
<attribute name="RDC-MAX" value="3700mOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="2200uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_7687709332">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687709332?ae"/>
<attribute name="FRES" value="0.6MHz"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="IR" value="0.37A"/>
<attribute name="ISAT" value="0.52A"/>
<attribute name="L" value="3300uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687709332"/>
<attribute name="RDC-MAX" value="5200mOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="3300uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_7687709471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687709471?ae"/>
<attribute name="FRES" value="1.9MHz"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="IR" value="0.97A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="L" value="470uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687709471"/>
<attribute name="RDC-MAX" value="800mOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="470uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_7687709472">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687709472?ae"/>
<attribute name="FRES" value="0.5MHz"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.48A"/>
<attribute name="L" value="4700uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687709472"/>
<attribute name="RDC-MAX" value="7800mOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="4700uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_7687709681">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687709681?ae"/>
<attribute name="FRES" value="1.5MHz"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="L" value="680uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687709681"/>
<attribute name="RDC-MAX" value="1150mOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="680uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_7687709682">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687709682?ae"/>
<attribute name="FRES" value="0.45MHz"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="IR" value="0.28A"/>
<attribute name="ISAT" value="0.38A"/>
<attribute name="L" value="6800uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687709682"/>
<attribute name="RDC-MAX" value="9600mOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="6800uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_7687709821">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687709821?ae"/>
<attribute name="FRES" value="1.4MHz"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="IR" value="0.76A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="L" value="820uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687709821"/>
<attribute name="RDC-MAX" value="1250mOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="820uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PDHV_1040" prefix="L">
<description>&lt;b&gt;WE-PD HV SMT Power Inductor (High Voltage)
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Shielded part for ideal wire protection
&lt;br&gt;Operating Temperature: -40°C - 125°C
&lt;br&gt;Magnetically shielded
&lt;br&gt;Designed for 400VDC Applications
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Non-isolated buck or Buck-Boost Converter like PI LinkSwitch-TN
&lt;br&gt;constant current LED Driver
&lt;br&gt;Utility metering
&lt;br&gt;Filter for power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14828v209%20WE-PD_HV.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14828v209%20WE-PD_HV.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PD-HV/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PD-HV&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-06-10&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT"/>
</gates>
<devices>
<device name="" package="WE-PDHV_1040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7687719102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687719102?ae"/>
<attribute name="FRES" value="2.3MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="0.54A"/>
<attribute name="ISAT" value="0.37A"/>
<attribute name="L" value="1000uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687719102"/>
<attribute name="RDC-MAX" value="2900mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7687719821">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7687719821?ae"/>
<attribute name="FRES" value="2.5MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IRP" value="0.61A"/>
<attribute name="ISAT" value="0.4A"/>
<attribute name="L" value="820uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7687719821"/>
<attribute name="RDC-MAX" value="2600mOhm"/>
<attribute name="SIZE" value=" 1040 "/>
<attribute name="VALUE" value="820uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PDHV_1280" prefix="L">
<description>&lt;b&gt;WE-PD HV SMT Power Inductor (High Voltage)
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Shielded part for ideal wire protection
&lt;br&gt;Operating Temperature: -40°C - 125°C
&lt;br&gt;Magnetically shielded
&lt;br&gt;Designed for 400VDC Applications
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Non-isolated buck or Buck-Boost Converter like PI LinkSwitch-TN
&lt;br&gt;constant current LED Driver
&lt;br&gt;Utility metering
&lt;br&gt;Filter for power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14828v209%20WE-PD_HV.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14828v209%20WE-PD_HV.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PD-HV/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PD-HV&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-10&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT"/>
</gates>
<devices>
<device name="" package="WE-PDHV_1280">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_768770331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/768770331?ae"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="HEIGHT" value="8.5mm"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="L" value="330uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="768770331"/>
<attribute name="RDC-MAX" value="650mOhm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="330uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
