<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Single Coil Power Inductors - WE-PD2 HV&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PD2HV_1054">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PD2 HV SMD Power Inductor (High Voltage)&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1054</description>
</package>
<package name="WE-PD2HV_7850">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PD2 HV SMD Power Inductor (High Voltage)&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;7850</description>
</package>
<package name="WE-PD2HV_5848">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PD2 HV SMD Power Inductor (High Voltage)&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;5848</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PD2HV_7850" prefix="L">
<description>&lt;b&gt;WE-PD2 HV SMD Power Inductor (High Voltage)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;unshielded construction
&lt;br&gt;Designed for 400 VDC
&lt;br&gt;Operating temperature: –40°C to +125°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Non-isolated buck or Buck-Boost Converter like PI LinkSwitch-TN
&lt;br&gt;constant current LED Driver
&lt;br&gt;Utility metering
&lt;br&gt;Filter for power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14829v209%20Family_WE-PD2A.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14829v209%20Family_WE-PD2A.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-PD2-HV"&gt;https://katalog.we-online.com/en/pbs/WE-PD2-HV&lt;/a&gt;&lt;p&gt;


Updated  by  Yingchun,Shan 2019-08-13&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD2HV_7850">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_768775256">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/768775256.pdf"/>
<attribute name="FRES" value="2.8MHz"/>
<attribute name="IR" value="0.41A"/>
<attribute name="ISAT" value="0.41A"/>
<attribute name="PART-NUMBER" value=" 768775256 "/>
<attribute name="RDC-MAX" value="2.08Ohm"/>
<attribute name="RDC-TYP" value="1.77Ohm"/>
<attribute name="VALUE" value="560uH"/>
</technology>
<technology name="_768775268">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/768775268.pdf"/>
<attribute name="FRES" value="2.7MHz"/>
<attribute name="IR" value="0.38A"/>
<attribute name="ISAT" value="0.38A"/>
<attribute name="PART-NUMBER" value=" 768775268 "/>
<attribute name="RDC-MAX" value="2.4Ohm"/>
<attribute name="RDC-TYP" value="2.04Ohm"/>
<attribute name="VALUE" value="680uH"/>
</technology>
<technology name="_768775282">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/768775282.pdf"/>
<attribute name="FRES" value="2.6MHz"/>
<attribute name="IR" value="0.35A"/>
<attribute name="ISAT" value="0.35A"/>
<attribute name="PART-NUMBER" value=" 768775282 "/>
<attribute name="RDC-MAX" value="2.77Ohm"/>
<attribute name="RDC-TYP" value="2.35Ohm"/>
<attribute name="VALUE" value="820uH"/>
</technology>
<technology name="_76877530">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/76877530.pdf"/>
<attribute name="FRES" value="2.4MHz"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="PART-NUMBER" value=" 76877530 "/>
<attribute name="RDC-MAX" value="3.3Ohm"/>
<attribute name="RDC-TYP" value="2.78Ohm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
<technology name="_768775312">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/768775312.pdf"/>
<attribute name="FRES" value="2.1MHz"/>
<attribute name="IR" value="0.28A"/>
<attribute name="ISAT" value="0.28A"/>
<attribute name="PART-NUMBER" value=" 768775312 "/>
<attribute name="RDC-MAX" value="4.5Ohm"/>
<attribute name="RDC-TYP" value="3.77Ohm"/>
<attribute name="VALUE" value="1200uH"/>
</technology>
<technology name="_768775322">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/768775322.pdf"/>
<attribute name="FRES" value="1.6MHz"/>
<attribute name="IR" value="0.15A"/>
<attribute name="ISAT" value="0.2A"/>
<attribute name="PART-NUMBER" value=" 768775322 "/>
<attribute name="RDC-MAX" value="7.2Ohm"/>
<attribute name="RDC-TYP" value="6.0Ohm"/>
<attribute name="VALUE" value="2200uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2HV_1054" prefix="L">
<description>&lt;b&gt;WE-PD2 HV SMD Power Inductor (High Voltage)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;unshielded construction
&lt;br&gt;Designed for 400 VDC
&lt;br&gt;Operating temperature: –40°C to +125°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Non-isolated buck or Buck-Boost Converter like PI LinkSwitch-TN
&lt;br&gt;constant current LED Driver
&lt;br&gt;Utility metering
&lt;br&gt;Filter for power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14829v209%20Family_WE-PD2A.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14829v209%20Family_WE-PD2A.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-PD2-HV"&gt;https://katalog.we-online.com/en/pbs/WE-PD2-HV&lt;/a&gt;&lt;p&gt;


Updated  by  Yingchun,Shan 2019-08-13&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD2HV_1054">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_76877630">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/76877630.pdf"/>
<attribute name="FRES" value="1.9MHz"/>
<attribute name="IR" value="0.38A"/>
<attribute name="ISAT" value="0.38A"/>
<attribute name="PART-NUMBER" value=" 76877630 "/>
<attribute name="RDC-MAX" value="2.6Ohm"/>
<attribute name="RDC-TYP" value="2.2Ohm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
<technology name="_768776312">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/768776312.pdf"/>
<attribute name="FRES" value="1.8MHz"/>
<attribute name="IR" value="0.35A"/>
<attribute name="ISAT" value="0.35A"/>
<attribute name="PART-NUMBER" value=" 768776312 "/>
<attribute name="RDC-MAX" value="3Ohm"/>
<attribute name="RDC-TYP" value="2.48Ohm"/>
<attribute name="VALUE" value="1200uH"/>
</technology>
<technology name="_768776322">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/768776322.pdf"/>
<attribute name="FRES" value="1.3MHz"/>
<attribute name="IR" value="0.18A"/>
<attribute name="ISAT" value="0.26A"/>
<attribute name="PART-NUMBER" value=" 768776322 "/>
<attribute name="RDC-MAX" value="5.3Ohm"/>
<attribute name="RDC-TYP" value="4.4Ohm"/>
<attribute name="VALUE" value="2200uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2HV_5848" prefix="L">
<description>&lt;b&gt;WE-PD2 HV SMD Power Inductor (High Voltage)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;unshielded construction
&lt;br&gt;Designed for 400 VDC
&lt;br&gt;Operating temperature: –40°C to +125°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Non-isolated buck or Buck-Boost Converter like PI LinkSwitch-TN
&lt;br&gt;constant current LED Driver
&lt;br&gt;Utility metering
&lt;br&gt;Filter for power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14829v209%20Family_WE-PD2A.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14829v209%20Family_WE-PD2A.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-PD2-HV"&gt;https://katalog.we-online.com/en/pbs/WE-PD2-HV&lt;/a&gt;&lt;p&gt;


Updated  by  Yingchun,Shan 2019-08-13&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD2HV_5848">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_768774268">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/768774268.pdf"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="IR" value="0.2A"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="PART-NUMBER" value=" 768774268 "/>
<attribute name="RDC-MAX" value="4.8Ohm"/>
<attribute name="RDC-TYP" value="4Ohm"/>
<attribute name="VALUE" value="380uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
