<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - PFC Chokes - WE-PFC&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PFC_RM10">
<description>&lt;B&gt;WE-PFC  PFC Chokes&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Size RM10, THT 12Pin &lt;BR&gt;</description>
</package>
<package name="WE-PFC_EFD30">
<description>&lt;B&gt;WE-PFC  PFC Chokes&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Size EFD30, THT 11Pin &lt;BR&gt;</description>
</package>
<package name="WE-PFC_EE20/10/6">
<description>&lt;B&gt;WE-PFC  PFC Chokes&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Size EE20/10/6, THT 10Pin &lt;BR&gt;</description>
</package>
<package name="WE-PFC_RM14">
<description>&lt;B&gt;WE-PFC  PFC Chokes&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Size RM14, THT 12Pin &lt;BR&gt;</description>
</package>
<package name="WE-PFC_EFD25">
<description>&lt;B&gt;WE-PFC  PFC Chokes&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Size EFD25, THT 10Pin &lt;BR&gt;</description>
</package>
<package name="WE-PFC_RM12">
<description>&lt;B&gt;WE-PFC  PFC Chokes&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Size RM12, THT 12Pin &lt;BR&gt;</description>
</package>
<package name="WE-PFC_EER28">
<description>&lt;B&gt;WE-PFC  PFC Chokes&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Size EER28, THT 9Pin &lt;BR&gt;</description>
</package>
<package name="WE-PFC_PQ38/11">
<description>&lt;B&gt;WE-PFC  PFC Chokes&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Size PQ38/11, THT 6Pin &lt;BR&gt;</description>
</package>
</packages>
<symbols>
<symbol name="CM2W-V">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PFC_RM10" prefix="T">
<description>&lt;b&gt;WE-PFC PFC Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; PFC choke for power up to 250 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; PQ 38/11 construction height &lt;10 mm above PCB
&lt;br&gt; Auxiliary winding
&lt;br&gt; RF strand for low losses due to skin and proximity effects
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Active Power Factor correction
&lt;br&gt; For all ICs CPU PFC ON Semiconductor
&lt;br&gt; Lighting applications
&lt;br&gt; Switchmode power supplies
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14837v209%20Family_WE-PFC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14837v209%20Family_WE-PFC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/PFC_CHOKES#vs_ct:1"&gt;https://katalog.we-online.com/en/pbs/PFC_CHOKES#vs_ct:1&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated  by  Yingchun,Shan 2019-08-21
&lt;br&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="" package="WE-PFC_RM10">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="6"/>
</connects>
<technologies>
<technology name="_760801020">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760801020.pdf"/>
<attribute name="IR" value="06.A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="N" value="12:1"/>
<attribute name="PART-NUMBER" value=" 760801020 "/>
<attribute name="RDC1" value="360mOhm"/>
<attribute name="RDC2" value="180mOhm"/>
<attribute name="VALUE" value="500uH"/>
<attribute name="VI" value="195-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_760801030">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760801030.pdf"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="3.9A"/>
<attribute name="N" value="10.71:1"/>
<attribute name="PART-NUMBER" value=" 760801030 "/>
<attribute name="RDC1" value="480mOhm"/>
<attribute name="RDC2" value="260mOhm"/>
<attribute name="VALUE" value="650uH"/>
<attribute name="VI" value="195-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_760801130">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760801130.pdf"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="3.9A"/>
<attribute name="N" value="90:8"/>
<attribute name="PART-NUMBER" value=" 760801130 "/>
<attribute name="RDC1" value="720mOhm"/>
<attribute name="RDC2" value="320mOhm"/>
<attribute name="VALUE" value="750uH"/>
<attribute name="VI" value="195-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_760802112">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760802112.pdf"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="5.4A"/>
<attribute name="N" value="12:1"/>
<attribute name="PART-NUMBER" value=" 760802112 "/>
<attribute name="RDC1" value="360mOhm"/>
<attribute name="RDC2" value="180mOhm"/>
<attribute name="VALUE" value="375uH"/>
<attribute name="VI" value="195-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_760804110">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760804110.pdf"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="5.6A"/>
<attribute name="N" value="44:5"/>
<attribute name="PART-NUMBER" value=" 760804110 "/>
<attribute name="RDC1" value="150mOhm"/>
<attribute name="RDC2" value="200mOhm"/>
<attribute name="VALUE" value="250uH"/>
<attribute name="VI" value="195-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PFC_RM14" prefix="T">
<description>&lt;b&gt;WE-PFC PFC Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; PFC choke for power up to 250 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; PQ 38/11 construction height &lt;10 mm above PCB
&lt;br&gt; Auxiliary winding
&lt;br&gt; RF strand for low losses due to skin and proximity effects
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Active Power Factor correction
&lt;br&gt; For all ICs CPU PFC ON Semiconductor
&lt;br&gt; Lighting applications
&lt;br&gt; Switchmode power supplies
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14837v209%20Family_WE-PFC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14837v209%20Family_WE-PFC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/PFC_CHOKES#vs_ct:1"&gt;https://katalog.we-online.com/en/pbs/PFC_CHOKES#vs_ct:1&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated  by  Yingchun,Shan 2019-08-21
&lt;br&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="" package="WE-PFC_RM14">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="6"/>
</connects>
<technologies>
<technology name="_760805410">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760805410.pdf"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT" value="12.4A"/>
<attribute name="N" value="39:4"/>
<attribute name="PART-NUMBER" value=" 760805410 "/>
<attribute name="RDC1" value="87mOhm"/>
<attribute name="RDC2" value="200mOhm"/>
<attribute name="VALUE" value="225uH"/>
<attribute name="VI" value="85-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_760806400">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760806400.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="13.2A"/>
<attribute name="N" value="9:1"/>
<attribute name="PART-NUMBER" value=" 760806400 "/>
<attribute name="RDC1" value="78mOhm"/>
<attribute name="RDC2" value="200mOhm"/>
<attribute name="VALUE" value="180uH"/>
<attribute name="VI" value="85-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PFC_EE20/10/6" prefix="T">
<description>&lt;b&gt;WE-PFC PFC Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; PFC choke for power up to 250 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; PQ 38/11 construction height &lt;10 mm above PCB
&lt;br&gt; Auxiliary winding
&lt;br&gt; RF strand for low losses due to skin and proximity effects
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Active Power Factor correction
&lt;br&gt; For all ICs CPU PFC ON Semiconductor
&lt;br&gt; Lighting applications
&lt;br&gt; Switchmode power supplies
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14837v209%20Family_WE-PFC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14837v209%20Family_WE-PFC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/PFC_CHOKES#vs_ct:1"&gt;https://katalog.we-online.com/en/pbs/PFC_CHOKES#vs_ct:1&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated  by  Yingchun,Shan 2019-08-21
&lt;br&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="" package="WE-PFC_EE20/10/6">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="9"/>
<connect gate="G$1" pin="4" pad="10"/>
</connects>
<technologies>
<technology name="_760800080">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760800080.pdf"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="N" value="12.9:1"/>
<attribute name="PART-NUMBER" value=" 760800080 "/>
<attribute name="RDC1" value="1550mOhm"/>
<attribute name="RDC2" value="1200mOhm"/>
<attribute name="VALUE" value="1800uH"/>
<attribute name="VI" value="85-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PFC_EFD30" prefix="T">
<description>&lt;b&gt;WE-PFC PFC Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; PFC choke for power up to 250 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; PQ 38/11 construction height &lt;10 mm above PCB
&lt;br&gt; Auxiliary winding
&lt;br&gt; RF strand for low losses due to skin and proximity effects
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Active Power Factor correction
&lt;br&gt; For all ICs CPU PFC ON Semiconductor
&lt;br&gt; Lighting applications
&lt;br&gt; Switchmode power supplies
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14837v209%20Family_WE-PFC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14837v209%20Family_WE-PFC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/PFC_CHOKES#vs_ct:1"&gt;https://katalog.we-online.com/en/pbs/PFC_CHOKES#vs_ct:1&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated  by  Yingchun,Shan 2019-08-21
&lt;br&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="" package="WE-PFC_EFD30">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="11"/>
</connects>
<technologies>
<technology name="_760801021">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760801021.pdf"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="4.2A"/>
<attribute name="N" value="21:2"/>
<attribute name="PART-NUMBER" value="760801021"/>
<attribute name="RDC1" value="620mOhm"/>
<attribute name="RDC2" value="540mOhm"/>
<attribute name="VALUE" value="500uH"/>
<attribute name="VI" value="195-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_760801131">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760801131.pdf"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="3.3A"/>
<attribute name="N" value="34:3"/>
<attribute name="PART-NUMBER" value=" 760801131 "/>
<attribute name="RDC1" value="950mOhm"/>
<attribute name="RDC2" value="580mOhm"/>
<attribute name="VALUE" value="750uH"/>
<attribute name="VI" value="85-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_760802113">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760802113.pdf"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="N" value="65:6"/>
<attribute name="PART-NUMBER" value="760802113"/>
<attribute name="RDC1" value="470mOhm"/>
<attribute name="RDC2" value="390mOhm"/>
<attribute name="VALUE" value="375uH"/>
<attribute name="VI" value="195-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_760804111">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760804111.pdf"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="4.8A"/>
<attribute name="N" value="50:5"/>
<attribute name="PART-NUMBER" value=" 760804111 "/>
<attribute name="RDC1" value="300mOhm"/>
<attribute name="RDC2" value="350mOhm"/>
<attribute name="VALUE" value="250uH"/>
<attribute name="VI" value="195-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_760805211">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760805211.pdf"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="N" value="50:5"/>
<attribute name="PART-NUMBER" value=" 760805211 "/>
<attribute name="RDC1" value="300mOhm"/>
<attribute name="RDC2" value="350mOhm"/>
<attribute name="VALUE" value="200uH"/>
<attribute name="VI" value="195-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_760806201">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760806201.pdf"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="6.8A"/>
<attribute name="N" value="42:5"/>
<attribute name="PART-NUMBER" value=" 760806201 "/>
<attribute name="RDC1" value="190mOhm"/>
<attribute name="RDC2" value="350mOhm"/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VI" value="195-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PFC_EFD25" prefix="T">
<description>&lt;b&gt;WE-PFC PFC Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; PFC choke for power up to 250 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; PQ 38/11 construction height &lt;10 mm above PCB
&lt;br&gt; Auxiliary winding
&lt;br&gt; RF strand for low losses due to skin and proximity effects
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Active Power Factor correction
&lt;br&gt; For all ICs CPU PFC ON Semiconductor
&lt;br&gt; Lighting applications
&lt;br&gt; Switchmode power supplies
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14837v209%20Family_WE-PFC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14837v209%20Family_WE-PFC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/PFC_CHOKES#vs_ct:1"&gt;https://katalog.we-online.com/en/pbs/PFC_CHOKES#vs_ct:1&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated  by  Yingchun,Shan 2019-08-21
&lt;br&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="" package="WE-PFC_EFD25">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="9"/>
</connects>
<technologies>
<technology name="_760801031">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760801031.pdf"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="N" value="90:8"/>
<attribute name="PART-NUMBER" value=" 760801031 "/>
<attribute name="RDC1" value="1020mOhm"/>
<attribute name="RDC2" value="460mOhm"/>
<attribute name="VALUE" value="650uH"/>
<attribute name="VI" value="195-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PFC_RM12" prefix="T">
<description>&lt;b&gt;WE-PFC PFC Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; PFC choke for power up to 250 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; PQ 38/11 construction height &lt;10 mm above PCB
&lt;br&gt; Auxiliary winding
&lt;br&gt; RF strand for low losses due to skin and proximity effects
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Active Power Factor correction
&lt;br&gt; For all ICs CPU PFC ON Semiconductor
&lt;br&gt; Lighting applications
&lt;br&gt; Switchmode power supplies
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14837v209%20Family_WE-PFC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14837v209%20Family_WE-PFC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/PFC_CHOKES#vs_ct:1"&gt;https://katalog.we-online.com/en/pbs/PFC_CHOKES#vs_ct:1&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated  by  Yingchun,Shan 2019-08-21
&lt;br&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="" package="WE-PFC_RM12">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="6"/>
</connects>
<technologies>
<technology name="_760802122">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760802122.pdf"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="5.6A"/>
<attribute name="N" value="10:1"/>
<attribute name="PART-NUMBER" value=" 760802122 "/>
<attribute name="RDC1" value="330mOhm"/>
<attribute name="RDC2" value="200mOhm"/>
<attribute name="VALUE" value="450uH"/>
<attribute name="VI" value="85-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_760804310">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760804310.pdf"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT" value="7.4A"/>
<attribute name="N" value="52:5"/>
<attribute name="PART-NUMBER" value=" 760804310 "/>
<attribute name="RDC1" value="170mOhm"/>
<attribute name="RDC2" value="250mOhm"/>
<attribute name="VALUE" value="300uH"/>
<attribute name="VI" value="85-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_760805210">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760805210.pdf"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="8.4A"/>
<attribute name="N" value="39:5"/>
<attribute name="PART-NUMBER" value=" 760805210 "/>
<attribute name="RDC1" value="120mOhm"/>
<attribute name="RDC2" value="250mOhm"/>
<attribute name="VALUE" value="200uH"/>
<attribute name="VI" value="195-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_760806200">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760806200.pdf"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="11A"/>
<attribute name="N" value="33:4"/>
<attribute name="PART-NUMBER" value=" 760806200 "/>
<attribute name="RDC1" value="80mOhm"/>
<attribute name="RDC2" value="180mOhm"/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VI" value="195-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PFC_EER28" prefix="T">
<description>&lt;b&gt;WE-PFC PFC Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; PFC choke for power up to 250 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; PQ 38/11 construction height &lt;10 mm above PCB
&lt;br&gt; Auxiliary winding
&lt;br&gt; RF strand for low losses due to skin and proximity effects
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Active Power Factor correction
&lt;br&gt; For all ICs CPU PFC ON Semiconductor
&lt;br&gt; Lighting applications
&lt;br&gt; Switchmode power supplies
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14837v209%20Family_WE-PFC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14837v209%20Family_WE-PFC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/PFC_CHOKES#vs_ct:1"&gt;https://katalog.we-online.com/en/pbs/PFC_CHOKES#vs_ct:1&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated  by  Yingchun,Shan 2019-08-21
&lt;br&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="" package="WE-PFC_EER28">
<connects>
<connect gate="G$1" pin="1" pad="9"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="6"/>
</connects>
<technologies>
<technology name="_760803200">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760803200.pdf"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="12A"/>
<attribute name="N" value="9.17:1"/>
<attribute name="PART-NUMBER" value=" 760803200 "/>
<attribute name="RDC1" value="190mOhm"/>
<attribute name="RDC2" value="140mOhm"/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VI" value="85-265V(AC)"/>
<attribute name="VT" value="800V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PFC_PQ38/11" prefix="T">
<description>&lt;b&gt;WE-PFC PFC Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; PFC choke for power up to 250 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; PQ 38/11 construction height &lt;10 mm above PCB
&lt;br&gt; Auxiliary winding
&lt;br&gt; RF strand for low losses due to skin and proximity effects
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Active Power Factor correction
&lt;br&gt; For all ICs CPU PFC ON Semiconductor
&lt;br&gt; Lighting applications
&lt;br&gt; Switchmode power supplies
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14837v209%20Family_WE-PFC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14837v209%20Family_WE-PFC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/PFC_CHOKES#vs_ct:1"&gt;https://katalog.we-online.com/en/pbs/PFC_CHOKES#vs_ct:1&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated  by  Yingchun,Shan 2019-08-21
&lt;br&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="" package="WE-PFC_PQ38/11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_760806302">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760806302.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="5.1A"/>
<attribute name="N" value="8.75:1"/>
<attribute name="PART-NUMBER" value=" 760806302 "/>
<attribute name="RDC1" value="197.3mOhm"/>
<attribute name="RDC2" value="310mOhm"/>
<attribute name="VALUE" value="300uH"/>
<attribute name="VI" value="85-265V(AC)"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
