<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Single Coil Power Inductors - WE-PMCI&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-03-12&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PMCI_201210">
<description>&lt;b&gt; WE-PMCI Power Molded Chip Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 201210, SMT, 2pins
&lt;br&gt;LxWxHxFI=2x1.2x1x0.5mm</description>
</package>
<package name="WE-PMCI_322515">
<description>&lt;b&gt; WE-PMCI Power Molded Chip Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 322515, SMT, 2pins
&lt;br&gt;LxWxHxFI=3.2x2.5x1.5x0.6mm</description>
</package>
<package name="WE-PMCI_322512">
<description>&lt;b&gt; WE-PMCI Power Molded Chip Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 322512, SMT, 2pins
&lt;br&gt;LxWxHxFI=3.2x2.5x1.2x0.6mm</description>
</package>
<package name="WE-PMCI_160808">
<description>&lt;b&gt; WE-PMCI Power Molded Chip Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 160808, SMT, 2pins
&lt;br&gt;LxWxHxFI=1.6x0.8x0.8x0.3mm</description>
</package>
<package name="WE-PMCI_252012">
<description>&lt;b&gt; WE-PMCI Power Molded Chip Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 252012, SMT, 2pins
&lt;br&gt;LxWxHxFI=2.5x2x1.2x0.6mm</description>
</package>
<package name="WE-PMCI_252010">
<description>&lt;b&gt; WE-PMCI Power Molded Chip Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 252010, SMT, 2pins
&lt;br&gt;LxWxHxFI=2.5x2x1x0.6mm</description>
</package>
<package name="WE-PMCI_201610">
<description>&lt;b&gt; WE-PMCI Power Molded Chip Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 201610, SMT, 2pins
&lt;br&gt;LxWxHxFI=2x1.6x1x0.5mm</description>
</package>
<package name="WE-PMCI_322510">
<description>&lt;b&gt; WE-PMCI Power Molded Chip Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 322510, SMT, 2pins
&lt;br&gt;LxWxHxFI=3.2x2.5x1x0.6mm</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PMCI_201210" prefix="L">
<description>&lt;b&gt;WE-PMCI Power Molded Chip Inductor&lt;br&gt;
Shielded

&lt;/b&gt;&lt;P&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;br&gt;
&lt;br&gt;Very compact design
&lt;br&gt;High efficiency due to low total losses
&lt;br&gt;High rated current values, up to 9.05 And high saturation currents
&lt;br&gt;Low RDC-values, starting at 21 mΩ
&lt;br&gt;Magnetically shielded construction
&lt;br&gt;Side termination for best soldering result
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended soldering profile: Reflow

&lt;P&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;High current power supply, Battery powered devices
&lt;br&gt;Powerable electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o55384v209%20Family-PMCI-744792XXXXX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o55384v209%20Family-PMCI-744792XXXXX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMCI&lt;/a&gt;&lt;p&gt;

 Updated by Ella 2025-03-12
&lt;br&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMCI_201210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479275147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479275147?ae"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="4.3A"/>
<attribute name="ISAT1" value="2.55A@10%"/>
<attribute name="ISAT2" value="5.15A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479275147"/>
<attribute name="RDC-MAX" value="44mOhm"/>
<attribute name="SIZE" value="201210"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_74479275210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479275210?ae"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="3.3A"/>
<attribute name="ISAT1" value="1.55A@10%"/>
<attribute name="ISAT2" value="3.45A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479275210"/>
<attribute name="RDC-MAX" value="75mOhm"/>
<attribute name="SIZE" value="201210"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_74479275222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479275222?ae"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT1" value="1.2A@10%"/>
<attribute name="ISAT2" value="2.4A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479275222"/>
<attribute name="RDC-MAX" value="190mOhm"/>
<attribute name="SIZE" value="201210"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMCI_322515" prefix="L">
<description>&lt;b&gt;WE-PMCI Power Molded Chip Inductor&lt;br&gt;
Shielded

&lt;/b&gt;&lt;P&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;br&gt;
&lt;br&gt;Very compact design
&lt;br&gt;High efficiency due to low total losses
&lt;br&gt;High rated current values, up to 9.05 And high saturation currents
&lt;br&gt;Low RDC-values, starting at 21 mΩ
&lt;br&gt;Magnetically shielded construction
&lt;br&gt;Side termination for best soldering result
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended soldering profile: Reflow

&lt;P&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;High current power supply, Battery powered devices
&lt;br&gt;Powerable electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o55384v209%20Family-PMCI-744792XXXXX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o55384v209%20Family-PMCI-744792XXXXX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMCI&lt;/a&gt;&lt;p&gt;

 Updated by Ella 2025-03-12
&lt;br&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMCI_322515">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479290125">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479290125?ae"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="FRES" value="150MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IR" value="9.05A"/>
<attribute name="ISAT1" value="8.5A@10%"/>
<attribute name="ISAT2" value="15.65A@30%"/>
<attribute name="L" value="0.25uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479290125"/>
<attribute name="RDC-MAX" value="31mOhm"/>
<attribute name="SIZE" value="322515"/>
<attribute name="VALUE" value="0.25uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMCI_160808" prefix="L">
<description>&lt;b&gt;WE-PMCI Power Molded Chip Inductor&lt;br&gt;
Shielded

&lt;/b&gt;&lt;P&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;br&gt;
&lt;br&gt;Very compact design
&lt;br&gt;High efficiency due to low total losses
&lt;br&gt;High rated current values, up to 9.05 And high saturation currents
&lt;br&gt;Low RDC-values, starting at 21 mΩ
&lt;br&gt;Magnetically shielded construction
&lt;br&gt;Side termination for best soldering result
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended soldering profile: Reflow

&lt;P&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;High current power supply, Battery powered devices
&lt;br&gt;Powerable electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o55384v209%20Family-PMCI-744792XXXXX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o55384v209%20Family-PMCI-744792XXXXX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMCI&lt;/a&gt;&lt;p&gt;

 Updated by Ella 2025-03-12
&lt;br&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMCI_160808">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479262147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479262147?ae"/>
<attribute name="FI" value="0.3mm"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="IR" value="3.95A"/>
<attribute name="ISAT1" value="1.5A@10%"/>
<attribute name="ISAT2" value="3.35A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479262147"/>
<attribute name="RDC-MAX" value="75mOhm"/>
<attribute name="SIZE" value="160808"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_74479262210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479262210?ae"/>
<attribute name="FI" value="0.3mm"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="IR" value="2.6A"/>
<attribute name="ISAT1" value="1.2A@10%"/>
<attribute name="ISAT2" value="2.6A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479262210"/>
<attribute name="RDC-MAX" value="115mOhm"/>
<attribute name="SIZE" value="160808"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMCI_322512" prefix="L">
<description>&lt;b&gt;WE-PMCI Power Molded Chip Inductor&lt;br&gt;
Shielded

&lt;/b&gt;&lt;P&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;br&gt;
&lt;br&gt;Very compact design
&lt;br&gt;High efficiency due to low total losses
&lt;br&gt;High rated current values, up to 9.05 And high saturation currents
&lt;br&gt;Low RDC-values, starting at 21 mΩ
&lt;br&gt;Magnetically shielded construction
&lt;br&gt;Side termination for best soldering result
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended soldering profile: Reflow

&lt;P&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;High current power supply, Battery powered devices
&lt;br&gt;Powerable electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o55384v209%20Family-PMCI-744792XXXXX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o55384v209%20Family-PMCI-744792XXXXX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMCI&lt;/a&gt;&lt;p&gt;

 Updated by Ella 2025-03-12
&lt;br&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMCI_322512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479299147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479299147?ae"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="7.1A"/>
<attribute name="ISAT1" value="5.15A@10%"/>
<attribute name="ISAT2" value="9.95A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479299147"/>
<attribute name="RDC-MAX" value="22mOhm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_74479299210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479299210?ae"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT1" value="3.25A@10%"/>
<attribute name="ISAT2" value="6.95A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479299210"/>
<attribute name="RDC-MAX" value="35mOhm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_74479299222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479299222?ae"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="3.65A"/>
<attribute name="ISAT1" value="2.25A@10%"/>
<attribute name="ISAT2" value="4.8A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479299222"/>
<attribute name="RDC-MAX" value="75mOhm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMCI_252012" prefix="L">
<description>&lt;b&gt;WE-PMCI Power Molded Chip Inductor&lt;br&gt;
Shielded

&lt;/b&gt;&lt;P&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;br&gt;
&lt;br&gt;Very compact design
&lt;br&gt;High efficiency due to low total losses
&lt;br&gt;High rated current values, up to 9.05 And high saturation currents
&lt;br&gt;Low RDC-values, starting at 21 mΩ
&lt;br&gt;Magnetically shielded construction
&lt;br&gt;Side termination for best soldering result
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended soldering profile: Reflow

&lt;P&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;High current power supply, Battery powered devices
&lt;br&gt;Powerable electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o55384v209%20Family-PMCI-744792XXXXX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o55384v209%20Family-PMCI-744792XXXXX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMCI&lt;/a&gt;&lt;p&gt;

 Updated by Ella 2025-03-12
&lt;br&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMCI_252012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479288147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479288147?ae"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="FRES" value="140MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="6.8A"/>
<attribute name="ISAT1" value="3.75A@10%"/>
<attribute name="ISAT2" value="7.9A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479288147"/>
<attribute name="RDC-MAX" value="22mOhm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479288210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479288210?ae"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="4.6A"/>
<attribute name="ISAT1" value="1.75A@10%"/>
<attribute name="ISAT2" value="4.1A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479288210"/>
<attribute name="RDC-MAX" value="44mOhm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479288215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479288215?ae"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="3.2A"/>
<attribute name="ISAT1" value="1.35A@10%"/>
<attribute name="ISAT2" value="3.05A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479288215"/>
<attribute name="RDC-MAX" value="77mOhm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479288222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479288222?ae"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT1" value="1.4A@10%"/>
<attribute name="ISAT2" value="3.25A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479288222"/>
<attribute name="RDC-MAX" value="89mOhm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMCI_252010" prefix="L">
<description>&lt;b&gt;WE-PMCI Power Molded Chip Inductor&lt;br&gt;
Shielded

&lt;/b&gt;&lt;P&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;br&gt;
&lt;br&gt;Very compact design
&lt;br&gt;High efficiency due to low total losses
&lt;br&gt;High rated current values, up to 9.05 And high saturation currents
&lt;br&gt;Low RDC-values, starting at 21 mΩ
&lt;br&gt;Magnetically shielded construction
&lt;br&gt;Side termination for best soldering result
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended soldering profile: Reflow

&lt;P&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;High current power supply, Battery powered devices
&lt;br&gt;Powerable electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o55384v209%20Family-PMCI-744792XXXXX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o55384v209%20Family-PMCI-744792XXXXX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMCI&lt;/a&gt;&lt;p&gt;

 Updated by Ella 2025-03-12
&lt;br&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMCI_252010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479287147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479287147?ae"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="FRES" value="150MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="7.35A"/>
<attribute name="ISAT1" value="3.6A@10%"/>
<attribute name="ISAT2" value="7.4A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479287147"/>
<attribute name="RDC-MAX" value="29mOhm"/>
<attribute name="SIZE" value="252010"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479287210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479287210?ae"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="4.9A"/>
<attribute name="ISAT1" value="2.4A@10%"/>
<attribute name="ISAT2" value="5.1A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479287210"/>
<attribute name="RDC-MAX" value="52mOhm"/>
<attribute name="SIZE" value="252010"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479287222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479287222?ae"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="3.15A"/>
<attribute name="ISAT1" value="1.5A@10%"/>
<attribute name="ISAT2" value="3.1A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479287222"/>
<attribute name="RDC-MAX" value="110mOhm"/>
<attribute name="SIZE" value="252010"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMCI_201610" prefix="L">
<description>&lt;b&gt;WE-PMCI Power Molded Chip Inductor&lt;br&gt;
Shielded

&lt;/b&gt;&lt;P&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;br&gt;
&lt;br&gt;Very compact design
&lt;br&gt;High efficiency due to low total losses
&lt;br&gt;High rated current values, up to 9.05 And high saturation currents
&lt;br&gt;Low RDC-values, starting at 21 mΩ
&lt;br&gt;Magnetically shielded construction
&lt;br&gt;Side termination for best soldering result
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended soldering profile: Reflow

&lt;P&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;High current power supply, Battery powered devices
&lt;br&gt;Powerable electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o55384v209%20Family-PMCI-744792XXXXX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o55384v209%20Family-PMCI-744792XXXXX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMCI&lt;/a&gt;&lt;p&gt;

 Updated by Ella 2025-03-12
&lt;br&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMCI_201610">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479276124">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479276124?ae"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="FRES" value="280MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="6.9A"/>
<attribute name="ISAT1" value="2.8A@10%"/>
<attribute name="ISAT2" value="6.7A@30%"/>
<attribute name="L" value="0.24uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479276124"/>
<attribute name="RDC-MAX" value="21mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="0.24uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479276147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479276147?ae"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="FRES" value="165MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="5.4A"/>
<attribute name="ISAT1" value="2.95A@10%"/>
<attribute name="ISAT2" value="6.3A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479276147"/>
<attribute name="RDC-MAX" value="30mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479276147C">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479276147C?ae"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="FRES" value="165MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="5.4A"/>
<attribute name="ISAT1" value="2.95A@10%"/>
<attribute name="ISAT2" value="6.3A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479276147C"/>
<attribute name="RDC-MAX" value="30mOhm"/>
<attribute name="SIZE" value=" 201610 "/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479276168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479276168?ae"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="FRES" value="130MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="3.8A"/>
<attribute name="ISAT1" value="1.8A@10%"/>
<attribute name="ISAT2" value="4A@30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479276168"/>
<attribute name="RDC-MAX" value="49mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479276210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479276210?ae"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="FRES" value="95MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="3.15A"/>
<attribute name="ISAT1" value="1.95A@10%"/>
<attribute name="ISAT2" value="4.25A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479276210"/>
<attribute name="RDC-MAX" value="60mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479276210C">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479276210C?ae"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="FRES" value="95MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="3.15A"/>
<attribute name="ISAT1" value="1.95A@10%"/>
<attribute name="ISAT2" value="4.25A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479276210C"/>
<attribute name="RDC-MAX" value="60mOhm"/>
<attribute name="SIZE" value=" 201610 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479276222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479276222?ae"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT1" value="1.25A@10%"/>
<attribute name="ISAT2" value="2.8A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479276222"/>
<attribute name="RDC-MAX" value="140mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479276222C">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479276222C?ae"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT1" value="1.25A@10%"/>
<attribute name="ISAT2" value="2.8A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479276222C"/>
<attribute name="RDC-MAX" value="140mOhm"/>
<attribute name="SIZE" value=" 201610 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMCI_322510" prefix="L">
<description>&lt;b&gt;WE-PMCI Power Molded Chip Inductor&lt;br&gt;
Shielded

&lt;/b&gt;&lt;P&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;br&gt;
&lt;br&gt;Very compact design
&lt;br&gt;High efficiency due to low total losses
&lt;br&gt;High rated current values, up to 9.05 And high saturation currents
&lt;br&gt;Low RDC-values, starting at 21 mΩ
&lt;br&gt;Magnetically shielded construction
&lt;br&gt;Side termination for best soldering result
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended soldering profile: Reflow

&lt;P&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;High current power supply, Battery powered devices
&lt;br&gt;Powerable electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o55384v209%20Family-PMCI-744792XXXXX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o55384v209%20Family-PMCI-744792XXXXX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMCI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMCI&lt;/a&gt;&lt;p&gt;

 Updated by Ella 2025-03-12
&lt;br&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMCI_322510">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479298147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479298147?ae"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="7.3A"/>
<attribute name="ISAT1" value="2.8A@10%"/>
<attribute name="ISAT2" value="5.9A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479298147"/>
<attribute name="RDC-MAX" value="22mOhm"/>
<attribute name="SIZE" value="322510"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_74479298210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479298210?ae"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="4.95A"/>
<attribute name="ISAT1" value="2.7A@10%"/>
<attribute name="ISAT2" value="5.5A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479298210"/>
<attribute name="RDC-MAX" value="49mOhm"/>
<attribute name="SIZE" value="322510"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_74479298222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479298222?ae"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="3.35A"/>
<attribute name="ISAT1" value="1.65A@10%"/>
<attribute name="ISAT2" value="3.95A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479298222"/>
<attribute name="RDC-MAX" value="93mOhm"/>
<attribute name="SIZE" value="322510"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
