<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Shielded Power Inductors - WE-PMI&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-06-09&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PMI_1008_H0.8">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0805, SMT 2pins
&lt;br&gt;L X W X H=2.5mmX2mmX0.8mm</description>
</package>
<package name="WE-PMI_0603_H0.5">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0603, SMT 2pins
&lt;br&gt;L X W X H=1.6mmX0.8mmX0.5mm</description>
</package>
<package name="WE-PMI_0603_H0.8">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0603, SMT 2pins
&lt;br&gt;L X W X H=1.6mmX0.8mmX1mm</description>
</package>
<package name="WE-PMI_0805_H0.5">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0805, SMT 2pins
&lt;br&gt;L X W X H=2mmX1.25mmX0.5mm</description>
</package>
<package name="WE-PMI_0805_H1.25">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0805, SMT 2pins
&lt;br&gt;L X W X H=2mmX1.25mmX1.2mm</description>
</package>
<package name="WE-PMI_1008_H1">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0805, SMT 2pins
&lt;br&gt;L X W X H=2.5mmX2mmX1mm</description>
</package>
<package name="WE-PMI_0805_H1">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0805, SMT 2pins
&lt;br&gt;L X W X H=2mmX1.2mmX1mm</description>
</package>
<package name="WE-PMI_1008_H1.2">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0805, SMT 2pins
&lt;br&gt;L X W X H=2.5mmX2mmX1.2mm</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PMI_0603" prefix="L">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact multilayer type
&lt;br&gt;Suitable for applications with high currents up to 2.7 A
&lt;br&gt;Smallest RDC-Values starting at 7 mΩ
&lt;br&gt;Magnetically shielded construction: No crosstalk
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended soldering profile: Reflow
&lt;br&gt;4 sizes and 3 different types available (Low Profile, Low RDC &amp; High Saturation Current)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters especially at high switching frequencies &gt; 1MHz
&lt;br&gt;Electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14838v209%20Family_WE-PMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14838v209%20Family_WE-PMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-16&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_H0.5" package="WE-PMI_0603_H0.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479762122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479762122?ae"/>
<attribute name="FRES" value="250MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IR1" value="900mA"/>
<attribute name="IR2" value="1200mA"/>
<attribute name="ISAT" value="1300mA"/>
<attribute name="L" value="0.22uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="PART-NUMBER" value="74479762122"/>
<attribute name="RDC" value="120mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TYPE" value="Low Profile"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_74479762133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479762133?ae"/>
<attribute name="FRES" value="200MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IR1" value="800mA"/>
<attribute name="IR2" value="1100mA"/>
<attribute name="ISAT" value="1200mA"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="PART-NUMBER" value="74479762133"/>
<attribute name="RDC" value="160mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TYPE" value="Low Profile"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_H0.8" package="WE-PMI_0603_H0.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479763147A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479763147A?ae"/>
<attribute name="FRES" value="190MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="IR1" value="1100mA"/>
<attribute name="IR2" value="1500mA"/>
<attribute name="ISAT" value="1500mA"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="PART-NUMBER" value="74479763147A"/>
<attribute name="RDC" value="90mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_74479763168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479763168?ae"/>
<attribute name="FRES" value="190MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="IR1" value="750mA"/>
<attribute name="IR2" value="1000mA"/>
<attribute name="ISAT" value="950mA"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="PART-NUMBER" value="74479763168"/>
<attribute name="RDC" value="180mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_74479763210A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479763210A?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="IR1" value="700mA"/>
<attribute name="IR2" value="900mA"/>
<attribute name="ISAT" value="650mA"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="PART-NUMBER" value="74479763210A"/>
<attribute name="RDC" value="200mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_74479763215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479763215?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="IR1" value="600mA"/>
<attribute name="IR2" value="850mA"/>
<attribute name="ISAT" value="500mA"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="PART-NUMBER" value="74479763215"/>
<attribute name="RDC" value="230mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_74479763222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479763222?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="IR1" value="550mA"/>
<attribute name="IR2" value="800mA"/>
<attribute name="ISAT" value="280mA"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="PART-NUMBER" value="74479763222"/>
<attribute name="RDC" value="300mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMI_0805" prefix="L">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact multilayer type
&lt;br&gt;Suitable for applications with high currents up to 2.7 A
&lt;br&gt;Smallest RDC-Values starting at 7 mΩ
&lt;br&gt;Magnetically shielded construction: No crosstalk
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended soldering profile: Reflow
&lt;br&gt;4 sizes and 3 different types available (Low Profile, Low RDC &amp; High Saturation Current)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters especially at high switching frequencies &gt; 1MHz
&lt;br&gt;Electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14838v209%20Family_WE-PMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14838v209%20Family_WE-PMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-16&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_H0.5" package="WE-PMI_0805_H0.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479773210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479773210?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IR1" value="800mA"/>
<attribute name="IR2" value="1200mA"/>
<attribute name="ISAT" value="800mA"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479773210"/>
<attribute name="RDC" value="180mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low Profile"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_74479774210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479774210?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IR1" value="800mA"/>
<attribute name="IR2" value="1100mA"/>
<attribute name="ISAT" value="500mA"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479774210"/>
<attribute name="RDC" value="190mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low Profile"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_74479774222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479774222?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IR1" value="500mA"/>
<attribute name="IR2" value="700mA"/>
<attribute name="ISAT" value="250mA"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479774222"/>
<attribute name="RDC" value="340mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low Profile"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_H1" package="WE-PMI_0805_H1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479775147A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479775147A?ae"/>
<attribute name="FRES" value="130MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1100mA"/>
<attribute name="IR2" value="1400mA"/>
<attribute name="ISAT" value="1000mA"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479775147A"/>
<attribute name="RDC" value="100mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479775215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479775215?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="800mA"/>
<attribute name="IR2" value="1100mA"/>
<attribute name="ISAT" value="800mA"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479775215"/>
<attribute name="RDC" value="160mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479775222A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479775222A?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="700mA"/>
<attribute name="IR2" value="1000mA"/>
<attribute name="ISAT" value="700mA"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479775222A"/>
<attribute name="RDC" value="200mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479775233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479775233?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="700mA"/>
<attribute name="IR2" value="1000mA"/>
<attribute name="ISAT" value="280mA"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479775233"/>
<attribute name="RDC" value="200mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479775247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479775247?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="600mA"/>
<attribute name="IR2" value="850mA"/>
<attribute name="ISAT" value="250mA"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479775247"/>
<attribute name="RDC" value="250mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
</technologies>
</device>
<device name="_H1.25" package="WE-PMI_0805_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479777268">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479777268?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="IR1" value="600mA"/>
<attribute name="IR2" value="900mA"/>
<attribute name="ISAT" value="200mA"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479777268"/>
<attribute name="RDC" value="300mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479777310">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479777310?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="IR1" value="450mA"/>
<attribute name="IR2" value="650mA"/>
<attribute name="ISAT" value="125mA"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479777310"/>
<attribute name="RDC" value="500mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479777310A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479777310A?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="IR1" value="600mA"/>
<attribute name="IR2" value="900mA"/>
<attribute name="ISAT" value="120mA"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479777310A"/>
<attribute name="RDC" value="300mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMI_1008" prefix="L">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact multilayer type
&lt;br&gt;Suitable for applications with high currents up to 2.7 A
&lt;br&gt;Smallest RDC-Values starting at 7 mΩ
&lt;br&gt;Magnetically shielded construction: No crosstalk
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended soldering profile: Reflow
&lt;br&gt;4 sizes and 3 different types available (Low Profile, Low RDC &amp; High Saturation Current)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters especially at high switching frequencies &gt; 1MHz
&lt;br&gt;Electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14838v209%20Family_WE-PMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14838v209%20Family_WE-PMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-16&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_H1" package="WE-PMI_1008_H1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479787147B">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479787147B?ae"/>
<attribute name="FRES" value="105MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="2000mA"/>
<attribute name="IR2" value="2700mA"/>
<attribute name="ISAT" value="950mA"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479787147B"/>
<attribute name="RDC" value="40mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479787210A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479787210A?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1300mA"/>
<attribute name="IR2" value="1700mA"/>
<attribute name="ISAT" value="1000mA"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479787210A"/>
<attribute name="RDC" value="71.5mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479787215A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479787215A?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1400mA"/>
<attribute name="IR2" value="1900mA"/>
<attribute name="ISAT" value="1100mA"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479787215A"/>
<attribute name="RDC" value="70mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479887210A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479887210A?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1300mA"/>
<attribute name="IR2" value="1600mA"/>
<attribute name="ISAT" value="1000mA"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479887210A"/>
<attribute name="RDC" value="75mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479887222A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479887222A?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1050mA"/>
<attribute name="IR2" value="1350mA"/>
<attribute name="ISAT" value="825mA"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479887222A"/>
<attribute name="RDC" value="140mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479887247A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479887247A?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="700mA"/>
<attribute name="IR2" value="1000mA"/>
<attribute name="ISAT" value="400mA"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479887247A"/>
<attribute name="RDC" value="230mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479887268A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479887268A?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="650mA"/>
<attribute name="IR2" value="950mA"/>
<attribute name="ISAT" value="300mA"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479887268A"/>
<attribute name="RDC" value="250mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479887310A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479887310A?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="600mA"/>
<attribute name="IR2" value="850mA"/>
<attribute name="ISAT" value="125mA"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479887310A"/>
<attribute name="RDC" value="300mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
<device name="_H1.2" package="WE-PMI_1008_H1.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479889233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479889233?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR1" value="900mA"/>
<attribute name="IR2" value="1300mA"/>
<attribute name="ISAT" value="1300mA"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479889233"/>
<attribute name="RDC" value="250mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479889247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479889247?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR1" value="650mA"/>
<attribute name="IR2" value="900mA"/>
<attribute name="ISAT" value="900mA"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479889247"/>
<attribute name="RDC" value="400mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479889268">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479889268?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR1" value="600mA"/>
<attribute name="IR2" value="800mA"/>
<attribute name="ISAT" value="700mA"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479889268"/>
<attribute name="RDC" value="500mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479889310">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479889310?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR1" value="600mA"/>
<attribute name="IR2" value="800mA"/>
<attribute name="ISAT" value="500mA"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479889310"/>
<attribute name="RDC" value="500mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
