<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Transformers For DC/DC Converter - WE-POE&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-06-12&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-POE_EP13_L17.75W13.46H12.7">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer&lt;/b&gt;

&lt;br&gt;&lt;br&gt;EP13, SMT, 10Pins
&lt;br&gt;LXWXH=17.75X13.46X12.7mm</description>
</package>
<package name="WE-POE_EP7_L9.5W9.78H10.54">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer&lt;/b&gt;

&lt;br&gt;&lt;br&gt;EP7, SMT, 8Pins</description>
</package>
<package name="WE-POE_EP10">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer&lt;/b&gt;

&lt;br&gt;&lt;br&gt;EP10, SMT, 8Pins</description>
</package>
<package name="WE-POE_ER14.5/6">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer&lt;/b&gt;

&lt;br&gt;&lt;br&gt;ER14.5/6, SMT, 12Pins</description>
</package>
<package name="WE-POE_EP7_L13.35W10.8H9.14">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer&lt;/b&gt;

&lt;br&gt;&lt;br&gt;EP7, SMT, 8Pins</description>
</package>
<package name="WE-POE_EFD15">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer&lt;/b&gt;

&lt;br&gt;&lt;br&gt;EFD15, SMT, 12Pins</description>
</package>
<package name="WE-POE_EP13_L13.46W13H12.7">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer&lt;/b&gt;

&lt;br&gt;&lt;br&gt;EP13, SMT, 10Pins
&lt;br&gt;LXWXH=13.46X13X12.7mm</description>
</package>
<package name="WE-POE_EP13_L13.5W13H12.5">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer&lt;/b&gt;

&lt;br&gt;&lt;br&gt;EP13, SMT, 10Pins
&lt;br&gt;LXWXH=13.5X13X12.5mm</description>
</package>
<package name="WE-POE_ER11/5">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer&lt;/b&gt;

&lt;br&gt;&lt;br&gt;ER11/5, SMT, 12Pins</description>
</package>
<package name="WE-POE_EFD20_750344488">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer&lt;/b&gt;

&lt;br&gt;&lt;br&gt;EFD20, SMT, 10Pins</description>
</package>
<package name="WE-POE_EFD20">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer&lt;/b&gt;

&lt;br&gt;&lt;br&gt;EFD20, SMT, 12Pins</description>
</package>
<package name="WE-POE_RM6">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer&lt;/b&gt;

&lt;br&gt;&lt;br&gt;RM6, SMT, 8Pins</description>
</package>
</packages>
<symbols>
<symbol name="WE-POE_EP13_3W:2W_CENTERTAP">
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="750313109">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="WE-POE_EP13_2W:2W_CENTERTAP">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8+9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="WE-POE_EP13_2W:2W_750310377">
<pin name="10" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="WE-POE_EP10_1W:1W">
<pin name="3" direction="pas"/>
<pin name="5+6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7+8" direction="pas"/>
</symbol>
<symbol name="WE-POE_EP13_2W:2W_PARALLEL">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="WE-POE_EP13_3W:2W_PARALLEL">
<pin name="1" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="WE-POE_EP10_2W:1W_PARALLEL">
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="WE-POE_EFR14.5/6_2W:2W">
<pin name="6" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="8+9" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="10+11" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="WE-POE_EFR14.5/6_2W:3W">
<pin name="1" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="WE-POE_EFD15_2W:3W">
<pin name="1" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="750310019">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="WE-POE_EP13_2W:2W_750310007">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="WE-POE_EP13_1W:1W">
<pin name="3" direction="pas"/>
<pin name="7+8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="9+10" direction="pas"/>
</symbol>
<symbol name="750344488">
<pin name="3" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-POE_ER11/5_2W:3W">
<pin name="1" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="WE-POE_EP7_2W:2W_PARALLEL">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="WE-POE_EP13_2W:2W">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="WE-POE_RM6_2W:1W">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="750310002">
<pin name="4" direction="pas"/>
<pin name="2+3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="WE-POE_EFR14.5/6_2W:3W_CENTERTAP">
<pin name="1" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="10+11" direction="pas"/>
<pin name="8+9" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="WE-POE_EP13_2W:3W_CENTERTAP">
<pin name="1" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="750315422">
<pin name="1" direction="pas"/>
<pin name="11+12" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7+8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-POE_EFD15_2W:3W_CENTERTAP">
<pin name="1" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="10+11" direction="pas"/>
<pin name="8+9" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="750314433" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_3W:2W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L17.75W13.46H12.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750314433?ae"/>
<attribute name="IO1" value="2A"/>
<attribute name="L" value="180uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="6:1:1:2.17"/>
<attribute name="PART-NUMBER" value="750314433"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="750314433"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VO2" value="5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313082" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_3W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L17.75W13.46H12.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="9"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313082?ae"/>
<attribute name="IO1" value="4.6A"/>
<attribute name="L" value="37uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="4.5:1:2.5"/>
<attribute name="PART-NUMBER" value="750313082"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="750313082"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="40 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="2400VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310310" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_2W:2W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L17.75W13.46H12.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="8+9" pad="8 9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310310?ae"/>
<attribute name="IO1" value="0.2A"/>
<attribute name="IO2" value="2.5A"/>
<attribute name="L" value="37uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="5.25:1:1:2.75"/>
<attribute name="PART-NUMBER" value="750310310"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="750310310"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="13 - 59 V (DC)"/>
<attribute name="VO1" value="6.6V"/>
<attribute name="VO2" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750314782" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_3W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L17.75W13.46H12.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750314782?ae"/>
<attribute name="IO1" value="1A"/>
<attribute name="L" value="37uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1:0.56"/>
<attribute name="PART-NUMBER" value="750314782"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="750314782"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="40 - 57 V (DC)"/>
<attribute name="VO1" value="24V"/>
<attribute name="VT" value="2400VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310035" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_2W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L17.75W13.46H12.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310035?ae"/>
<attribute name="IO1" value="2.7A"/>
<attribute name="L" value="77.4uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="3.67:1:2.5"/>
<attribute name="PART-NUMBER" value="750310035"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="750310035"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750032173" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_2W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L17.75W13.46H12.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750032173?ae"/>
<attribute name="IO1" value="1.125A"/>
<attribute name="L" value="127uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="3.42:1:0.71"/>
<attribute name="PART-NUMBER" value="750032173"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="750032173"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310377" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_2W:2W_750310377"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L17.75W13.46H12.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310377?ae"/>
<attribute name="IO1" value="1.08A"/>
<attribute name="L" value="127uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:1:1:1"/>
<attribute name="PART-NUMBER" value="750310377"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="750310377"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310007" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_2W:2W_750310007"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L17.75W13.46H12.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310007?ae"/>
<attribute name="IO1" value="2.5A"/>
<attribute name="IO2" value="0.33A"/>
<attribute name="L" value="127uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="6:1:3.4:3.4"/>
<attribute name="PART-NUMBER" value="750310007"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="750310007"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="35 - 57 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VO2" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313109" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750313109"/>
</gates>
<devices>
<device name="" package="WE-POE_EP7_L9.5W9.78H10.54">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313109?ae"/>
<attribute name="IO1" value="2.3A"/>
<attribute name="L" value="44uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="4:1:1:2.5"/>
<attribute name="PART-NUMBER" value="750313109"/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value="750313109"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="2400VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310062" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP10_1W:1W"/>
</gates>
<devices>
<device name="" package="WE-POE_EP10">
<connects>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5+6" pad="5 6"/>
<connect gate="G$1" pin="7+8" pad="7 8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310062?ae"/>
<attribute name="IO1" value="2A"/>
<attribute name="L" value="127uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="4:1"/>
<attribute name="PART-NUMBER" value="750310062"/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value="750310062"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750319936" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP10_2W:1W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE_EP10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750319936?ae"/>
<attribute name="IO1" value="0.6A"/>
<attribute name="L" value="235uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2.75:1:1"/>
<attribute name="PART-NUMBER" value="750319936"/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value="750319936"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="40 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750032395" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_2W:2W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L17.75W13.46H12.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="8+9" pad="8 9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750032395?ae"/>
<attribute name="IO1" value="0.5A"/>
<attribute name="IO2" value="3.2A"/>
<attribute name="L" value="37uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="10.5:1:2:5.5"/>
<attribute name="PART-NUMBER" value="750032395"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="750032395"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="13 - 59 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VO2" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7491192912" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EFR14.5/6_2W:3W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-POE_ER14.5/6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10+11" pad="10 11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8+9" pad="8 9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7491192912?ae"/>
<attribute name="IO1" value="0.58A"/>
<attribute name="IO2" value="1.4A"/>
<attribute name="IO3" value="2.1A"/>
<attribute name="L" value="210uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="12:1.5:1:3.5:5"/>
<attribute name="PART-NUMBER" value="7491192912"/>
<attribute name="SIZE" value="ER14.5/6"/>
<attribute name="VALUE" value="7491192912"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VO2" value="5V"/>
<attribute name="VO3" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749119250" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EFR14.5/6_2W:3W"/>
</gates>
<devices>
<device name="" package="WE-POE_ER14.5/6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749119250?ae"/>
<attribute name="IO1" value="0.47A"/>
<attribute name="IO2" value="0.47A"/>
<attribute name="IO3" value="0.47A"/>
<attribute name="L" value="210uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="6:1:1:1:1.75"/>
<attribute name="PART-NUMBER" value="749119250"/>
<attribute name="SIZE" value="ER14.5/6"/>
<attribute name="VALUE" value="749119250"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VO2" value="5V"/>
<attribute name="VO3" value="5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749119218" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EFR14.5/6_2W:3W"/>
</gates>
<devices>
<device name="" package="WE-POE_ER14.5/6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749119218?ae"/>
<attribute name="IO1" value="1.3A"/>
<attribute name="IO2" value="1.3A"/>
<attribute name="IO3" value="1.3A"/>
<attribute name="L" value="210uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="16.5:1:1:1:5.5"/>
<attribute name="PART-NUMBER" value="749119218"/>
<attribute name="SIZE" value="ER14.5/6"/>
<attribute name="VALUE" value="749119218"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="1.8V"/>
<attribute name="VO2" value="1.8V"/>
<attribute name="VO3" value="1.8V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310019" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750310019"/>
</gates>
<devices>
<device name="" package="WE-POE_EP7_L13.35W10.8H9.14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310019?ae"/>
<attribute name="IO1" value="0.91A"/>
<attribute name="L" value="310uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="5.5:1:1:3.75"/>
<attribute name="PART-NUMBER" value="750310019"/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value="750310019"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310020" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP7_2W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE_EP7_L13.35W10.8H9.14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310020?ae"/>
<attribute name="IO1" value="0.6A"/>
<attribute name="IO2" value="0.02A"/>
<attribute name="L" value="500uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="8:1:1.66"/>
<attribute name="PART-NUMBER" value="750310020"/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value="750310020"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310018" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP7_2W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE_EP7_L13.35W10.8H9.14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310018?ae"/>
<attribute name="IO1" value="0.91A"/>
<attribute name="L" value="500uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="12:1:2.5"/>
<attribute name="PART-NUMBER" value="750310018"/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value="750310018"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310022" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP7_2W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE_EP7_L13.35W10.8H9.14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310022?ae"/>
<attribute name="IO1" value="0.25A"/>
<attribute name="L" value="521uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="3.5:1:0.71"/>
<attribute name="PART-NUMBER" value="750310022"/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value="750310022"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749119350" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EFD15_2W:3W"/>
</gates>
<devices>
<device name="" package="WE-POE_EFD15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749119350?ae"/>
<attribute name="IO1" value="0.9A"/>
<attribute name="IO2" value="0.9A"/>
<attribute name="IO3" value="0.9A"/>
<attribute name="L" value="120uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="7.2:1:1:1:1.8"/>
<attribute name="PART-NUMBER" value="749119350"/>
<attribute name="SIZE" value="EFD15"/>
<attribute name="VALUE" value="749119350"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VO2" value="5V"/>
<attribute name="VO3" value="5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749119233" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EFR14.5/6_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-POE_ER14.5/6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10+11" pad="10 11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8+9" pad="8 9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749119233?ae"/>
<attribute name="IO1" value="0.7A"/>
<attribute name="IO2" value="1.4A"/>
<attribute name="L" value="210uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="12:1:1:3"/>
<attribute name="PART-NUMBER" value="749119233"/>
<attribute name="SIZE" value="ER14.5/6"/>
<attribute name="VALUE" value="749119233"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VO2" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750319935" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP10_2W:1W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE_EP10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750319935?ae"/>
<attribute name="IO1" value="1.4A"/>
<attribute name="L" value="235uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="6.5:1:2.38"/>
<attribute name="PART-NUMBER" value="750319935"/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value="750319935"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="40 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7491199312" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_1W:1W"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L13.46W13H12.7">
<connects>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="7+8" pad="7 8"/>
<connect gate="G$1" pin="9+10" pad="9 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7491199312?ae"/>
<attribute name="IO1" value="1.25A"/>
<attribute name="L" value="40uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value="7491199312"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="7491199312"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7491199332" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_2W:3W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L13.46W13H12.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7491199332?ae"/>
<attribute name="IO1" value="2A"/>
<attribute name="IO2" value="1A"/>
<attribute name="IO3" value="0.05A"/>
<attribute name="L" value="35uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="9:1:1.5:2.5:4.5"/>
<attribute name="PART-NUMBER" value="7491199332"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="7491199332"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VO2" value="5V"/>
<attribute name="VO3" value="5.5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310013" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_1W:1W"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L13.46W13H12.7">
<connects>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7+8" pad="7 8"/>
<connect gate="G$1" pin="9+10" pad="9 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310013?ae"/>
<attribute name="IO1" value="2.6A"/>
<attribute name="L" value="127uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="4:1"/>
<attribute name="PART-NUMBER" value="750310013"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="750310013"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7491199501" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L13.5W13H12.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7491199501?ae"/>
<attribute name="IO1" value="1.3A"/>
<attribute name="IO2" value="1.3A"/>
<attribute name="L" value="127uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="8:1:1:1.67"/>
<attribute name="PART-NUMBER" value="7491199501"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="7491199501"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VO2" value="5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749119933" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L13.5W13H12.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749119933?ae"/>
<attribute name="IO1" value="2A"/>
<attribute name="IO2" value="2A"/>
<attribute name="L" value="127uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="6:1:1:3"/>
<attribute name="PART-NUMBER" value="749119933"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="749119933"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VO2" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310032" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP10_2W:1W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE_EP10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310032?ae"/>
<attribute name="IO1" value="0.58A"/>
<attribute name="L" value="155uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.47:1:1"/>
<attribute name="PART-NUMBER" value="750310032"/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value="750310032"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749119950" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L13.5W13H12.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749119950?ae"/>
<attribute name="IO1" value="1.3A"/>
<attribute name="IO2" value="1.3A"/>
<attribute name="L" value="127uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="4:1:1:2"/>
<attribute name="PART-NUMBER" value="749119950"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="749119950"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VO2" value="5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310031" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP10_2W:1W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE_EP10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310031?ae"/>
<attribute name="IO1" value="0.58A"/>
<attribute name="L" value="264uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="3.5:1:0.71"/>
<attribute name="PART-NUMBER" value="750310031"/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value="750310031"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7491199331" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L13.5W13H12.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7491199331?ae"/>
<attribute name="IO1" value="2A"/>
<attribute name="IO2" value="2A"/>
<attribute name="L" value="127uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="12:1:1:2.5"/>
<attribute name="PART-NUMBER" value="7491199331"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="7491199331"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VO2" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749119133" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-13&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_ER11/5_2W:3W"/>
</gates>
<devices>
<device name="" package="WE-POE_ER11/5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749119133?ae"/>
<attribute name="IO1" value="0.4A"/>
<attribute name="IO2" value="0.4A"/>
<attribute name="IO3" value="0.4A"/>
<attribute name="L" value="400uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="12:1:1:1:3"/>
<attribute name="PART-NUMBER" value="749119133"/>
<attribute name="SIZE" value="ER11/5"/>
<attribute name="VALUE" value="749119133"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VO2" value="3.3V"/>
<attribute name="VO3" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7491199212" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L13.5W13H12.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7491199212?ae"/>
<attribute name="IO1" value="0.55A"/>
<attribute name="IO2" value="0.55A"/>
<attribute name="L" value="127uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="4.8:1.4:1.4:1"/>
<attribute name="PART-NUMBER" value="7491199212"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="7491199212"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VO2" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7491199112" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-12&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP13_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13_L13.5W13H12.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7491199112?ae"/>
<attribute name="IO1" value="0.55A"/>
<attribute name="IO2" value="0.55A"/>
<attribute name="L" value="127uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:1:1:1"/>
<attribute name="PART-NUMBER" value="7491199112"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value="7491199112"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VO2" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749119150" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-13&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_ER11/5_2W:3W"/>
</gates>
<devices>
<device name="" package="WE-POE_ER11/5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749119150?ae"/>
<attribute name="IO1" value="0.27A"/>
<attribute name="IO2" value="0.27A"/>
<attribute name="IO3" value="0.27A"/>
<attribute name="L" value="400uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="7.2:1:1:1:1.8"/>
<attribute name="PART-NUMBER" value="749119150"/>
<attribute name="SIZE" value="ER11/5"/>
<attribute name="VALUE" value="749119150"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VO2" value="5V"/>
<attribute name="VO3" value="5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749119318" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EFD15_2W:3W"/>
</gates>
<devices>
<device name="" package="WE-POE_EFD15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749119318?ae"/>
<attribute name="IO1" value="2.4A"/>
<attribute name="IO2" value="2.4A"/>
<attribute name="IO3" value="2.4A"/>
<attribute name="L" value="120uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="14:1:1:1:5.5"/>
<attribute name="PART-NUMBER" value="749119318"/>
<attribute name="SIZE" value="EFD15"/>
<attribute name="VALUE" value="749119318"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="1.8V"/>
<attribute name="VO2" value="1.8V"/>
<attribute name="VO3" value="1.8V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750344488" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750344488"/>
</gates>
<devices>
<device name="" package="WE-POE_EFD20_750344488">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750344488?ae"/>
<attribute name="IO1" value="2A"/>
<attribute name="L" value="14uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.33:1:1"/>
<attribute name="PART-NUMBER" value="750344488"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="VALUE" value="750344488"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="9 - 60 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7491193912" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EFD15_2W:3W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-POE_EFD15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10+11" pad="10 11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8+9" pad="8 9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7491193912?ae"/>
<attribute name="IO1" value="1.2A"/>
<attribute name="IO2" value="2.8A"/>
<attribute name="IO3" value="4.3A"/>
<attribute name="L" value="120uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="15:1.5:1:3:5"/>
<attribute name="PART-NUMBER" value="7491193912"/>
<attribute name="SIZE" value="EFD15"/>
<attribute name="VALUE" value="7491193912"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VO2" value="5V"/>
<attribute name="VO3" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315422" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750315422"/>
</gates>
<devices>
<device name="" package="WE-POE_EFD20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11+12" pad="11 12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7+8" pad="7 8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315422?ae"/>
<attribute name="IO1" value="2A"/>
<attribute name="L" value="9uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1.12:1"/>
<attribute name="PART-NUMBER" value="750315422"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="VALUE" value="750315422"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="9 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750317123" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_RM6_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-POE_RM6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750317123?ae"/>
<attribute name="IO1" value="1A"/>
<attribute name="L" value="82uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2.5:1:0.75"/>
<attribute name="PART-NUMBER" value="750317123"/>
<attribute name="SIZE" value="RM6"/>
<attribute name="VALUE" value="750317123"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="32 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310027" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP10_2W:1W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE_EP10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310027?ae"/>
<attribute name="IO1" value="3A"/>
<attribute name="L" value="20.4uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="4.5:1:2.5"/>
<attribute name="PART-NUMBER" value="750310027"/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value="750310027"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="9 - 50 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750319924" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EP10_2W:1W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE_EP10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750319924?ae"/>
<attribute name="IO1" value="2.1A"/>
<attribute name="L" value="235uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="9.5:1:3.5"/>
<attribute name="PART-NUMBER" value="750319924"/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value="750319924"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="40 - 57 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749119333" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE_EFD15_2W:3W"/>
</gates>
<devices>
<device name="" package="WE-POE_EFD15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749119333?ae"/>
<attribute name="IO1" value="1.35A"/>
<attribute name="IO2" value="1.35A"/>
<attribute name="IO3" value="1.35A"/>
<attribute name="L" value="120uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="12:1:1:1:3"/>
<attribute name="PART-NUMBER" value="749119333"/>
<attribute name="SIZE" value="EFD15"/>
<attribute name="VALUE" value="749119333"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VO2" value="3.3V"/>
<attribute name="VO3" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310002" prefix="T">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flyback transformer designed for PoE PDs
&lt;br&gt;Input voltage: 36 V to 57 V
&lt;br&gt;Switching frequencies: 200–500 kHz
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Isolation voltage: 1.5 kVAC/1 min
&lt;br&gt;Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Access control terminals
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o766301v209%20Family-POE.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-09&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750310002"/>
</gates>
<devices>
<device name="" package="WE-POE_EFD20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2+3" pad="2 3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310002?ae"/>
<attribute name="IO1" value="4A"/>
<attribute name="L" value="28uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="3.5:1:2.75"/>
<attribute name="PART-NUMBER" value="750310002"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="VALUE" value="750310002"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="20 - 72 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
