<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Transformers For DC/DC Converter - WE-POE+&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 202-11-24&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-POE+_EFD20_L29.65W21.8H11.43">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: EFD20, SMT, 12Pins
&lt;br&gt;LXWXH=29.65X21.8X11.43mm</description>
</package>
<package name="WE-POE+_EFD20_L22W23.11H11.43">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: EFD20, SMT, 12Pins
&lt;br&gt;LXWXH=22X23.11X11.43mm</description>
</package>
<package name="WE-POE+_EP13_PADL1.88W1.17">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer&lt;/b&gt;

&lt;br&gt;&lt;br&gt;EP13, SMT, 10Pins</description>
</package>
<package name="WE-POE+_EPW15">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer&lt;/b&gt;

&lt;br&gt;&lt;br&gt;EPPW15, SMT, 9Pins</description>
</package>
<package name="WE-POE+_EFD20_L29.65W23.11H11.43">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: EFD20, SMT, 12Pins
&lt;br&gt;LXWXH=29.65X23.11X11.43mm</description>
</package>
<package name="WE-POE+_EP13_PADL1.55W1.27">
<description>&lt;b&gt;WE-PoE Power over Ethernet Transformer&lt;/b&gt;

&lt;br&gt;&lt;br&gt;EP13, SMT, 10Pins</description>
</package>
<package name="WE-POE+_EFD20_L25.91W23.11H10.92">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: EFD20, SMT, 12Pins
&lt;br&gt;LXWXH=25.9X23.11X10.92mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-POE+_EFD20_2W:1W">
<pin name="1" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-POE+_EPW15_2W:2W_PARALLEL">
<pin name="5" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-POE+_EP13_3W:2W_CENTERTAP_PARALLEL">
<pin name="5" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WE-POE+_EFD20_3W:3W_PARALLEL">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="WE-POE+_EFD20_3W:2W_PARALLEL">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="WE-POE+_EP13_2W:2W_PARALLEL">
<pin name="5" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-POE+_EP13_2W:1W">
<pin name="1" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="WE-POE+_EFD20_2W:2W">
<pin name="1" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-POE+_EFD20_2W:3W_PARALLEL">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="WE-POE+_EFD20_2W:3W_CENTERTAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="750316116" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EFD20_3W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE+_EFD20_L29.65W21.8H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316116?ae"/>
<attribute name="IO1" value="4A"/>
<attribute name="L" value="18uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750316116"/>
<attribute name="RDC1" value="0.02ohm"/>
<attribute name="RDC2" value="0.011ohm"/>
<attribute name="RDC3" value="0.066ohm"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="2:1:1"/>
<attribute name="VALUE" value="18uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="41 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750318587" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-11-24&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EFD20_3W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE+_EFD20_L29.65W21.8H11.43">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="9"/>
<connect gate="G$1" pin="8" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750318587?ae"/>
<attribute name="IO1" value="1A"/>
<attribute name="L" value="80uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750318587"/>
<attribute name="RDC1" value="0.125ohm"/>
<attribute name="RDC2" value="0.1ohm"/>
<attribute name="RDC3" value="0.165ohm"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="1:1:0.46"/>
<attribute name="VALUE" value="80uH"/>
<attribute name="VAUX" value="10.6V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="17 - 57 V (DC)"/>
<attribute name="VO1" value="24V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310346" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EFD20_3W:3W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE+_EFD20_L29.65W21.8H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310346?ae"/>
<attribute name="IO1" value="2.5A"/>
<attribute name="L" value="100uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750310346"/>
<attribute name="RDC1" value="0.085ohm"/>
<attribute name="RDC2" value="0.025ohm"/>
<attribute name="RDC3" value="0.245ohm"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="3:1:1"/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7491194501" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EFD20_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-POE+_EFD20_L22W23.11H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="10" pad="10 11 12"/>
<connect gate="G$1" pin="3" pad="3 4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7 8 9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7491194501?ae"/>
<attribute name="IO1" value="6A"/>
<attribute name="L" value="42uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7491194501"/>
<attribute name="RDC1" value="0.084ohm"/>
<attribute name="RDC2" value="0.005ohm"/>
<attribute name="RDC3" value="0.17ohm"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="7:1:2.25"/>
<attribute name="VALUE" value="42uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7491194912" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EFD20_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-POE+_EFD20_L22W23.11H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="10" pad="10 11 12"/>
<connect gate="G$1" pin="3" pad="3 4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7 8 9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7491194912?ae"/>
<attribute name="IO1" value="2.5A"/>
<attribute name="L" value="42uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7491194912"/>
<attribute name="RDC1" value="0.061ohm"/>
<attribute name="RDC2" value="0.018ohm"/>
<attribute name="RDC3" value="0.18ohm"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="3:1:1"/>
<attribute name="VALUE" value="42uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310927" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EFD20_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-POE+_EFD20_L22W23.11H11.43">
<connects>
<connect gate="G$1" pin="1" pad="3 4"/>
<connect gate="G$1" pin="10" pad="7 9"/>
<connect gate="G$1" pin="3" pad="1 2"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="8 10" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310927?ae"/>
<attribute name="IO1" value="2.5A"/>
<attribute name="L" value="112uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750310927"/>
<attribute name="RDC1" value="0.15ohm"/>
<attribute name="RDC2" value="0.05ohm"/>
<attribute name="RDC3" value="0.07ohm"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="3:1:0.5"/>
<attribute name="VALUE" value="112uH"/>
<attribute name="VAUX" value="6V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750314783" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EP13_3W:2W_CENTERTAP_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE+_EP13_PADL1.88W1.17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750314783?ae"/>
<attribute name="HEIGHT" value="12.7mm"/>
<attribute name="IO1" value="7A"/>
<attribute name="L" value="26uH"/>
<attribute name="LENGTH" value="13.46mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750314783"/>
<attribute name="RDC1" value="0.094ohm"/>
<attribute name="RDC2" value="0.007ohm"/>
<attribute name="RDC3" value="0.233ohm"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="TURNS-RATIO" value="4.5:1:2.5"/>
<attribute name="VALUE" value="26uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="48 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="2400VAC"/>
<attribute name="WIDTH" value="17.75mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749119450" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EFD20_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-POE+_EFD20_L22W23.11H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="10" pad="10 11 12"/>
<connect gate="G$1" pin="3" pad="3 4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7 8 9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749119450?ae"/>
<attribute name="IO1" value="6A"/>
<attribute name="L" value="65uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="749119450"/>
<attribute name="RDC1" value="0.116ohm"/>
<attribute name="RDC2" value="0.004ohm"/>
<attribute name="RDC3" value="0.23ohm"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="7:1:3"/>
<attribute name="VALUE" value="65uH"/>
<attribute name="VAUX" value="15V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750311320" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EP13_2W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE+_EP13_PADL1.88W1.17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750311320?ae"/>
<attribute name="HEIGHT" value="12.7mm"/>
<attribute name="IO1" value="2.5A"/>
<attribute name="L" value="100uH"/>
<attribute name="LENGTH" value="13.46mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750311320"/>
<attribute name="RDC1" value="0.21ohm"/>
<attribute name="RDC2" value="0.035ohm"/>
<attribute name="RDC3" value="0.58ohm"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="TURNS-RATIO" value="1.8:1:1"/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Active Clamp Forward"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="WIDTH" value="17.75mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310926" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EFD20_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-POE+_EFD20_L22W23.11H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3 4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7 9"/>
<connect gate="G$1" pin="8" pad="8 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310926?ae"/>
<attribute name="IO1" value="6A"/>
<attribute name="IO2" value="0.05A"/>
<attribute name="L" value="40uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750310926"/>
<attribute name="RDC1" value="0.05ohm"/>
<attribute name="RDC2" value="0.01ohm"/>
<attribute name="RDC3" value="0.3ohm"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="5:1:1.25:1.25"/>
<attribute name="VALUE" value="40uH"/>
<attribute name="VAUX" value="6.5V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VO2" value="6.5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7491194924" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-11-24&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EFD20_3W:3W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE+_EFD20_L29.65W23.11H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7491194924?ae"/>
<attribute name="IO1" value="1.25A"/>
<attribute name="L" value="42uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7491194924"/>
<attribute name="RDC1" value="0.06ohm"/>
<attribute name="RDC2" value="0.055ohm"/>
<attribute name="RDC3" value="0.195ohm"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="1.5:1:0.5"/>
<attribute name="VALUE" value="42uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VO1" value="24V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750317723" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-11-24&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EFD20_3W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE+_EFD20_L29.65W23.11H11.43">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="9"/>
<connect gate="G$1" pin="8" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750317723?ae"/>
<attribute name="IO1" value="1.3A"/>
<attribute name="L" value="8uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750317723"/>
<attribute name="RDC1" value="0.03ohm"/>
<attribute name="RDC2" value="0.035ohm"/>
<attribute name="RDC3" value="0.055ohm"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="1:1:0.42"/>
<attribute name="VALUE" value="8uH"/>
<attribute name="VAUX" value="10V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="20 - 48 V (DC)"/>
<attribute name="VO1" value="24V"/>
<attribute name="VT" value="2500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750316332" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EPW15_2W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE+_EPW15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316332?ae"/>
<attribute name="HEIGHT" value="13.5mm"/>
<attribute name="IO1" value="6A"/>
<attribute name="L" value="48uH"/>
<attribute name="LENGTH" value="15.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750316332"/>
<attribute name="RDC1" value="0.065ohm"/>
<attribute name="RDC2" value="0.01ohm"/>
<attribute name="RDC3" value="0.14ohm"/>
<attribute name="SIZE" value="EPW15"/>
<attribute name="TURNS-RATIO" value="5:1:2.2"/>
<attribute name="VALUE" value="48uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="WIDTH" value="21.69mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750316331" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EPW15_2W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE+_EPW15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316331?ae"/>
<attribute name="HEIGHT" value="13.5mm"/>
<attribute name="IO1" value="8A"/>
<attribute name="L" value="54uH"/>
<attribute name="LENGTH" value="15.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750316331"/>
<attribute name="RDC1" value="0.12ohm"/>
<attribute name="RDC2" value="0.01ohm"/>
<attribute name="RDC3" value="0.125ohm"/>
<attribute name="SIZE" value="EPW15"/>
<attribute name="TURNS-RATIO" value="8:1:3.67"/>
<attribute name="VALUE" value="54uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="WIDTH" value="21.69mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310925" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EFD20_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-POE+_EFD20_L22W23.11H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="10" pad="10 11 12"/>
<connect gate="G$1" pin="3" pad="3 4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7 8 9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310925?ae"/>
<attribute name="IO1" value="9A"/>
<attribute name="IO2" value="0.05A"/>
<attribute name="L" value="57uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750310925"/>
<attribute name="RDC1" value="0.06ohm"/>
<attribute name="RDC2" value="0.008ohm"/>
<attribute name="RDC3" value="0.35ohm"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="8:1:2:2"/>
<attribute name="VALUE" value="57uH"/>
<attribute name="VAUX" value="6.5V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VO2" value="6.5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="749119433" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EFD20_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-POE+_EFD20_L22W23.11H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3 4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7 9"/>
<connect gate="G$1" pin="8" pad="8 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/749119433?ae"/>
<attribute name="IO1" value="9A"/>
<attribute name="L" value="42uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="749119433"/>
<attribute name="RDC1" value="0.099ohm"/>
<attribute name="RDC2" value="0.0032ohm"/>
<attribute name="RDC3" value="0.22ohm"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="11:1:3.3"/>
<attribute name="VALUE" value="42uH"/>
<attribute name="VAUX" value="11V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310744" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EP13_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-POE+_EP13_PADL1.55W1.27">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="9 10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6 7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310744?ae"/>
<attribute name="HEIGHT" value="12.7mm"/>
<attribute name="IO1" value="5A"/>
<attribute name="L" value="38uH"/>
<attribute name="LENGTH" value="13.46mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750310744"/>
<attribute name="RDC1" value="0.1ohm"/>
<attribute name="RDC2" value="0.0045ohm"/>
<attribute name="RDC3" value="0.255ohm"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="TURNS-RATIO" value="5:1:2.5"/>
<attribute name="VALUE" value="38uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="37 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="WIDTH" value="17.75mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310743" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EP13_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-POE+_EP13_PADL1.55W1.27">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="9 10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6 7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310743?ae"/>
<attribute name="HEIGHT" value="12.7mm"/>
<attribute name="IO1" value="7.5A"/>
<attribute name="L" value="38uH"/>
<attribute name="LENGTH" value="13.46mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750310743"/>
<attribute name="RDC1" value="0.1ohm"/>
<attribute name="RDC2" value="0.003ohm"/>
<attribute name="RDC3" value="0.182ohm"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="TURNS-RATIO" value="6.67:1:4"/>
<attribute name="VALUE" value="38uH"/>
<attribute name="VAUX" value="12.7V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="37 - 57 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="WIDTH" value="17.75mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310059" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EFD20_2W:3W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE+_EFD20_L25.91W23.11H10.92">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310059?ae"/>
<attribute name="IO1" value="6A"/>
<attribute name="L" value="29.2uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750310059"/>
<attribute name="RDC1" value="0.75ohm"/>
<attribute name="RDC2" value="0.0045ohm"/>
<attribute name="RDC3" value="0.75ohm"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="8:1:3.5"/>
<attribute name="VALUE" value="29.2uH"/>
<attribute name="VAUX" value="17V"/>
<attribute name="VERSION" value="Active Clamp Forward"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310742" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EP13_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-POE+_EP13_PADL1.55W1.27">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310742?ae"/>
<attribute name="HEIGHT" value="12.7mm"/>
<attribute name="IO1" value="2.1A"/>
<attribute name="L" value="38uH"/>
<attribute name="LENGTH" value="13.46mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750310742"/>
<attribute name="RDC1" value="0.085ohm"/>
<attribute name="RDC2" value="0.025ohm"/>
<attribute name="RDC3" value="0.155ohm"/>
<attribute name="SIZE" value="EP13"/>
<attribute name="TURNS-RATIO" value="2:1:1.1"/>
<attribute name="VALUE" value="38uH"/>
<attribute name="VAUX" value="12.5V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="37 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="WIDTH" value="17.75mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310167" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EFD20_2W:3W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-POE+_EFD20_L22W23.11H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="3 4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310167?ae"/>
<attribute name="IO1" value="3A"/>
<attribute name="IO2" value="1.6A"/>
<attribute name="IO3" value="0.4A"/>
<attribute name="L" value="25uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750310167"/>
<attribute name="RDC1" value="0.07ohm"/>
<attribute name="RDC2" value="0.009ohm"/>
<attribute name="RDC3" value="0.023ohm"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="6.67:1:2.67:1.33:2.67"/>
<attribute name="VALUE" value="25uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VO2" value="12V"/>
<attribute name="VO3" value="5V"/>
<attribute name="VT" value="1500VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750316333" prefix="T">
<description>&lt;b&gt;WE-PoE+ Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 30 W PoE+ objectives of IEEE802.3at
&lt;br&gt;Frequency range: 250–400 kHz
&lt;br&gt;Input voltage range: 36–72 V
&lt;br&gt;1.5 kV Hipot test between primary and secondary
&lt;br&gt;Operating temperature: –40 °C to +125 °C (incl. self-heating)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;PoE+ powered devices
&lt;br&gt;IP Phones
&lt;br&gt;WLAN Access Points
&lt;br&gt;Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14840v209%20Family_WE-POE%2B.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-POE-PLUS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-POE-PLUS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-29&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE+_EPW15_2W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE+_EPW15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316333?ae"/>
<attribute name="HEIGHT" value="13.5mm"/>
<attribute name="IO1" value="3A"/>
<attribute name="L" value="41uH"/>
<attribute name="LENGTH" value="15.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750316333"/>
<attribute name="RDC1" value="0.05ohm"/>
<attribute name="RDC2" value="0.02ohm"/>
<attribute name="RDC3" value="0.089ohm"/>
<attribute name="SIZE" value="EPW15"/>
<attribute name="TURNS-RATIO" value="2.67:1:1"/>
<attribute name="VALUE" value="41uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="WIDTH" value="21.69mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
