<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<library>
<description>Würth Elektronik - Passive Components - Power Magnetics - Transformers For DC/DC Converter - WE-POE++

Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, 
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. 
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. 
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. 

Please contact us for more information: libraries@we-online.com 

Würth Elektronik eiSos GmbH &amp; Co. KG
EMC &amp; Inductive Solutions
www.we-online.com

Fusion360, Library Revision 2026a, 2026-07-22
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-POE++_ER19_L23.37W21.08H10.5">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Size: ER19/4.8/15, SMT, 10Pins

LXWXH=23.37X21.08X10.5mm</description>
</package>
<package name="WE-POE++_EFD25_L32.45W27.03H13.97">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Size: EFD20, SMT, 12Pins

LXWXH=29.65X21.8X11.43mm</description>
</package>
<package name="WE-POE++_EFD20_L29.65W21.8H11.43">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Size: EFD20, SMT, 12Pins

LXWXH=29.65X21.8X11.43mm</description>
</package>
<package name="WE-POE++_EPW15_L21.89H15.5H13.5">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

EPPW15, SMT, 9Pins

LXWXH=21.69X15.5X13.5mm</description>
</package>
<package name="WE-POE++_EFD20_L21.08W21.08H10.8">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Size: EFD20, THT, 10Pins

LXWXH=29.65X21.8X11.43mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-POE++_ER19_3W:2W">
<pin name="1" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="WE-POE++_EFD25_3W:2W_PARALLELX2">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="WE-POE++_EFD20_750320237">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="WE-POE++_EFD20_3W:3W_PARALLELX2">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="WE-POE++_EFD25_3W:3W_PARALLELX2">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="WE-POE++_EFD20_3W:2W_PARALLELX2">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="WE-POE++_EFD20_3W:2W_SEC_PARALLEL">
<pin name="1" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-POE++_EFD20_3W:2W_PRI_PARALLEL">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="WE-POE++_EFD20_2W:3W_PARALLEL">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="WE-POE++_EFD20_2W:2W_750319034">
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WE-POE++_EPW15_2W:2W_PARALLEL">
<pin name="5" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-POE++_EFD20_2W:2W">
<pin name="2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="750343576" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_ER19_3W:2W"/>
</gates>
<devices>
<device name="" package="WE-POE++_ER19_L23.37W21.08H10.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="3A"/>
<attribute name="L" value="100uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750343576"/>
<attribute name="SIZE" value="ER19/4.8/15"/>
<attribute name="TURNS-RATIO" value="4:4:4:4:4"/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Forward"/>
<attribute name="VIN" value="40 - 57 V (DC)"/>
<attribute name="VO1" value="24V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="23.37mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750343576?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750343164" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_ER19_3W:2W"/>
</gates>
<devices>
<device name="" package="WE-POE++_ER19_L23.37W21.08H10.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="14A"/>
<attribute name="L" value="153uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750343164"/>
<attribute name="SIZE" value="ER19/4.8/15"/>
<attribute name="TURNS-RATIO" value="4:4:1:1:5"/>
<attribute name="VALUE" value="153uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Forward"/>
<attribute name="VIN" value="40 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="23.37mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750343164?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750341794" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_ER19_3W:2W"/>
</gates>
<devices>
<device name="" package="WE-POE++_ER19_L23.37W21.08H10.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="6A"/>
<attribute name="L" value="153uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750341794"/>
<attribute name="SIZE" value="ER19/4.8/15"/>
<attribute name="TURNS-RATIO" value="4:4:2:2:4"/>
<attribute name="VALUE" value="153uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Forward"/>
<attribute name="VIN" value="37 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="10.5mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="23.37mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750341794?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750319032" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD25_3W:2W_PARALLELX2"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD25_L32.45W27.03H13.97">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="4A"/>
<attribute name="L" value="22uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750319032"/>
<attribute name="SIZE" value="EFD25"/>
<attribute name="TURNS-RATIO" value="2.4:2:1"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="24V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="13.97mm"/>
<attribute name="LENGTH" value="27.03mm"/>
<attribute name="WIDTH" value="32.45mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750319032?ae"/>
<attribute name="ISAT" value="10.8A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750321159" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD20_750320237"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD20_L29.65W21.8H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="9"/>
<connect gate="G$1" pin="11" pad="8"/>
<connect gate="G$1" pin="12" pad="7"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="10"/>
<connect gate="G$1" pin="8" pad="11"/>
<connect gate="G$1" pin="9" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="1.45A"/>
<attribute name="L" value="15.5uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750321159"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="0.5:1:0.25"/>
<attribute name="VALUE" value="15.5uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="48V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="29.65mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750321159?ae"/>
<attribute name="ISAT" value="6.8A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750318938" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD20_3W:3W_PARALLELX2"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD20_L29.65W21.8H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="7"/>
<connect gate="G$1" pin="11" pad="8"/>
<connect gate="G$1" pin="12" pad="9"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="10"/>
<connect gate="G$1" pin="8" pad="11"/>
<connect gate="G$1" pin="9" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="12A"/>
<attribute name="L" value="150uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750318938"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="4:1:2.6"/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VAUX" value="13V"/>
<attribute name="VERSION" value="Forward"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="29.65mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750318938?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750319020" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD25_3W:2W_PARALLELX2"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD25_L32.45W27.03H13.97">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="19A"/>
<attribute name="L" value="17uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750319020"/>
<attribute name="SIZE" value="EFD25"/>
<attribute name="TURNS-RATIO" value="5:1:2.5"/>
<attribute name="VALUE" value="17uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="13.97mm"/>
<attribute name="LENGTH" value="27.03mm"/>
<attribute name="WIDTH" value="32.45mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750319020?ae"/>
<attribute name="ISAT" value="11.4A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750319021" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD25_3W:3W_PARALLELX2"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD25_L32.45W27.03H13.97">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="8A"/>
<attribute name="L" value="22uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750319021"/>
<attribute name="SIZE" value="EFD25"/>
<attribute name="TURNS-RATIO" value="2.4:1:1"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="13.97mm"/>
<attribute name="LENGTH" value="27.03mm"/>
<attribute name="WIDTH" value="32.45mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750319021?ae"/>
<attribute name="ISAT" value="10.8A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750321158" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD20_750320237"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD20_L29.65W21.8H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="9"/>
<connect gate="G$1" pin="11" pad="8"/>
<connect gate="G$1" pin="12" pad="7"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="10"/>
<connect gate="G$1" pin="8" pad="11"/>
<connect gate="G$1" pin="9" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="1.3A"/>
<attribute name="L" value="17.8uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750321158"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="0.5:1:0.25"/>
<attribute name="VALUE" value="17.8uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="48V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="29.65mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750321158?ae"/>
<attribute name="ISAT" value="5.7A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750320237" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Updated by Ella 2026-07-22
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD20_750320237"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD20_L29.65W21.8H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="2.5A"/>
<attribute name="L" value="100uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750320237"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="2:2:1"/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Forward"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="24V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="29.65mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750320237?ae"/>
<attribute name="ISAT" value="1.8A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750319035" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD20_3W:2W_PARALLELX2"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD20_L29.65W21.8H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="6" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="14.6A"/>
<attribute name="L" value="16uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750319035"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="4.67:1:2.33"/>
<attribute name="VALUE" value="16uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="29.65mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750319035?ae"/>
<attribute name="ISAT" value="10.4A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313095" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD20_3W:2W_SEC_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD20_L29.65W21.8H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="17A"/>
<attribute name="L" value="175uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750313095"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="3.5:1:2.25"/>
<attribute name="VALUE" value="175uH"/>
<attribute name="VAUX" value="10.75V"/>
<attribute name="VERSION" value="Forward"/>
<attribute name="VIN" value="40 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="2500VAC"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="29.65mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750313095?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750318962" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD20_3W:2W_PRI_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD20_L29.65W21.8H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="8A"/>
<attribute name="L" value="66uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750318962"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="1.6:1:1:1"/>
<attribute name="VALUE" value="66uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Active Clamp Forward"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="29.65mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750318962?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750319033" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD20_2W:3W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD20_L29.65W21.8H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="14.6A"/>
<attribute name="L" value="66uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750319033"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="4:1:2.5"/>
<attribute name="VALUE" value="66uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Active Clamp Forward"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="29.65mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750319033?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750319069" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD20_3W:2W_PARALLELX2"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD20_L29.65W21.8H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="6" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="3A"/>
<attribute name="L" value="16uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750319069"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="2:1.86:1"/>
<attribute name="VALUE" value="16uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="24V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="29.65mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750319069?ae"/>
<attribute name="ISAT" value="10.4A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750318961" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD20_3W:2W_PARALLELX2"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD20_L29.65W21.8H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="19A"/>
<attribute name="L" value="66uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750318961"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="4:1:2.5"/>
<attribute name="VALUE" value="66uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Active Clamp Forward"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="29.65mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750318961?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313355" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD20_3W:3W_PARALLELX2"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD20_L29.65W21.8H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="7"/>
<connect gate="G$1" pin="11" pad="8"/>
<connect gate="G$1" pin="12" pad="9"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="10"/>
<connect gate="G$1" pin="8" pad="11"/>
<connect gate="G$1" pin="9" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="5A"/>
<attribute name="L" value="100uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750313355"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="2:1:1"/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Forward"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="29.65mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750313355?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750319034" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD20_2W:2W_750319034"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD20_L29.65W21.8H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="6A"/>
<attribute name="L" value="66uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750319034"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="1.6:1:1:1"/>
<attribute name="VALUE" value="66uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Active Clamp Forward"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="29.65mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750319034?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750316336" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EPW15_2W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE++_EPW15_L21.89H15.5H13.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="6A"/>
<attribute name="L" value="50uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750316336"/>
<attribute name="SIZE" value="EPW15"/>
<attribute name="TURNS-RATIO" value="2:1:1"/>
<attribute name="VALUE" value="50uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Forward"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="2400VAC"/>
<attribute name="HEIGHT" value="13.5mm"/>
<attribute name="LENGTH" value="15.5mm"/>
<attribute name="WIDTH" value="21.69mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750316336?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750316335" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EPW15_2W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE++_EPW15_L21.89H15.5H13.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="14A"/>
<attribute name="L" value="50uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750316335"/>
<attribute name="SIZE" value="EPW15"/>
<attribute name="TURNS-RATIO" value="4:1:2.33"/>
<attribute name="VALUE" value="50uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Forward"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="5V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="13.5mm"/>
<attribute name="LENGTH" value="15.5mm"/>
<attribute name="WIDTH" value="21.69mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750316335?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750316334" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EPW15_2W:2W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-POE++_EPW15_L21.89H15.5H13.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="18A"/>
<attribute name="L" value="50uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750316334"/>
<attribute name="SIZE" value="EPW15"/>
<attribute name="TURNS-RATIO" value="7:1:3.5"/>
<attribute name="VALUE" value="50uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Forward"/>
<attribute name="VIN" value="36 - 57 V (DC)"/>
<attribute name="VO1" value="3.3V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="13.5mm"/>
<attribute name="LENGTH" value="15.5mm"/>
<attribute name="WIDTH" value="21.69mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750316334?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310042" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD20_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD20_L21.08W21.08H10.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="5A"/>
<attribute name="L" value="154uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750310042"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="2:1:1:1"/>
<attribute name="VALUE" value="154uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="Forward"/>
<attribute name="VIN" value="30 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="10.8mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="21.08mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750310042?ae"/>
<attribute name="IO2" value="1.6A"/>
<attribute name="VO2" value="-12V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750319036" prefix="T">
<description>WE-PoE++ Power over Ethernet Plus Plus Transformer

Characteristics
Suitable for CCM Flyback or Active Clamp Forward
Different power levels up to 95W
Frequency range: 250-400 kHz
Different output voltages available
Custom designs available

Applications
Telecom
IndustrialApplications
WLAN Access Point
Safety cameras
Intelligent LED Lighting Networks

Details see: www.we-online.com/en/components/products/WE-POE-PLUS-PLUS

Created by Ella 2024-01-30
2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE++_EFD20_3W:3W_PARALLELX2"/>
</gates>
<devices>
<device name="" package="WE-POE++_EFD20_L29.65W21.8H11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="IO1" value="6A"/>
<attribute name="L" value="16uH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="750319036"/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="TURNS-RATIO" value="2.33:1:1"/>
<attribute name="VALUE" value="16uH"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VERSION" value="CCM Flyback"/>
<attribute name="VIN" value="33 - 57 V (DC)"/>
<attribute name="VO1" value="12V"/>
<attribute name="VT" value="1500VAC"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="LENGTH" value="21.08mm"/>
<attribute name="WIDTH" value="29.65mm"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/750319036?ae"/>
<attribute name="ISAT" value="10.4A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
