<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Signal &amp; Communications - Filtered Connectors - WE-RJ45 10G&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2026a, 2026-01-29&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="7499611423">
<description>&lt;b&gt;WE-RJ45 10G Transformer
&lt;/B&gt;&lt;BR&gt;10G Base-T
&lt;br&gt;MAX HEIGHT=11.92mm</description>
</package>
<package name="7499811120">
<description>&lt;b&gt;WE-RJ45 10G Transformer
&lt;/B&gt;&lt;BR&gt;10G Base-T
&lt;br&gt;MAX HEIGHT=11.92mm</description>
</package>
<package name="7499711421">
<description>&lt;b&gt;WE-RJ45 10G Transformer
&lt;/B&gt;&lt;BR&gt;10G Base-T
&lt;br&gt;MAX HEIGHT=13.87mm</description>
</package>
<package name="7499611420">
<description>&lt;b&gt;WE-RJ45 10G Transformer
&lt;/B&gt;&lt;BR&gt;10G Base-T
&lt;br&gt;MAX HEIGHT=11.3mm</description>
</package>
<package name="7499611421">
<description>&lt;b&gt;WE-RJ45 10G Transformer
&lt;/B&gt;&lt;BR&gt;10G Base-T
&lt;br&gt;MAX HEIGHT=13.87mm</description>
</package>
<package name="7499811420">
<description>&lt;b&gt;WE-RJ45 10G Transformer
&lt;/B&gt;&lt;BR&gt;10G Base-T
&lt;br&gt;MAX HEIGHT=13.87mm</description>
</package>
<package name="7499611422">
<description>&lt;b&gt;WE-RJ45 10G Transformer
&lt;/B&gt;&lt;BR&gt;10G Base-T
&lt;br&gt;MAX HEIGHT=11.3mm</description>
</package>
<package name="7499611424">
<description>&lt;b&gt;WE-RJ45 10G Transformer
&lt;/B&gt;&lt;BR&gt;10G Base-T
&lt;br&gt;MAX HEIGHT=11.3mm</description>
</package>
</packages>
<symbols>
<symbol name="7499611423">
<pin name="TRD1+"/>
<pin name="TRCT1"/>
<pin name="TRD1-"/>
<pin name="TRD2+"/>
<pin name="TRCT2"/>
<pin name="TRD2-"/>
<pin name="TRD3+"/>
<pin name="TRCT3"/>
<pin name="TRD3-"/>
<pin name="TRD4+"/>
<pin name="TRCT4"/>
<pin name="TRD4-"/>
<pin name="LED1_G-/Y+"/>
<pin name="LED1_G+/Y-"/>
<pin name="LED2_G+"/>
<pin name="LED2_G-"/>
<pin name="SHIELD1" direction="pwr"/>
<pin name="SHIELD2" direction="pwr"/>
<pin name="CMS+"/>
<pin name="CMCT"/>
<pin name="CMS-"/>
</symbol>
<symbol name="7499611420">
<pin name="D1+"/>
<pin name="CD1"/>
<pin name="D1-"/>
<pin name="D2+"/>
<pin name="CD2"/>
<pin name="D2-"/>
<pin name="D3+"/>
<pin name="CD3"/>
<pin name="D3-"/>
<pin name="D4+"/>
<pin name="CD4"/>
<pin name="D4-"/>
<pin name="LED1_G-"/>
<pin name="LED1_G+"/>
<pin name="LED2_Y-"/>
<pin name="LED2_Y+_G+"/>
<pin name="LED2_G-"/>
<pin name="SHIELD1" direction="pwr"/>
<pin name="SHIELD2" direction="pwr"/>
</symbol>
<symbol name="7499611421">
<pin name="D1+"/>
<pin name="CD1"/>
<pin name="D1-"/>
<pin name="D2+"/>
<pin name="CD2"/>
<pin name="D2-"/>
<pin name="D3+"/>
<pin name="CD3"/>
<pin name="D3-"/>
<pin name="D4+"/>
<pin name="CD4"/>
<pin name="D4-"/>
<pin name="LED1_G-"/>
<pin name="LED1_G+"/>
<pin name="LED2_Y+/G-"/>
<pin name="LED2_Y-/G+"/>
<pin name="SHIELD1" direction="pwr"/>
<pin name="SHIELD2" direction="pwr"/>
</symbol>
<symbol name="7499811120">
<pin name="TRD1+"/>
<pin name="TRCT1"/>
<pin name="TRD1-"/>
<pin name="TRD2+"/>
<pin name="TRCT2"/>
<pin name="TRD2-"/>
<pin name="TRD3+"/>
<pin name="TRCT3"/>
<pin name="TRD3-"/>
<pin name="TRD4+"/>
<pin name="TRCT4"/>
<pin name="TRD4-"/>
<pin name="LED1_Y-"/>
<pin name="LED1_Y+"/>
<pin name="LED2_G-"/>
<pin name="LED2_G+"/>
<pin name="SHIELD1" direction="pwr"/>
<pin name="SHIELD2" direction="pwr"/>
<pin name="VC12"/>
<pin name="VC36"/>
<pin name="VC45"/>
<pin name="VC78"/>
</symbol>
<symbol name="7499711421">
<pin name="D1+"/>
<pin name="CD1"/>
<pin name="D1-"/>
<pin name="D2+"/>
<pin name="CD2"/>
<pin name="D2-"/>
<pin name="D3+"/>
<pin name="CD3"/>
<pin name="D3-"/>
<pin name="D4+"/>
<pin name="CD4"/>
<pin name="D4-"/>
<pin name="LED1_G-"/>
<pin name="LED1_G+"/>
<pin name="LED2_Y+_G-"/>
<pin name="LED2_Y-_G+"/>
<pin name="SHIELD1" direction="pwr"/>
<pin name="SHIELD2" direction="pwr"/>
<pin name="V1" direction="pwr"/>
<pin name="V2" direction="pwr"/>
<pin name="V3" direction="pwr"/>
<pin name="V4" direction="pwr"/>
</symbol>
<symbol name="7499811420">
<pin name="D1+"/>
<pin name="CD1"/>
<pin name="D1-"/>
<pin name="D2+"/>
<pin name="CD2"/>
<pin name="D2-"/>
<pin name="D3+"/>
<pin name="CD3"/>
<pin name="D3-"/>
<pin name="D4+"/>
<pin name="CD4"/>
<pin name="D4-"/>
<pin name="LED1_G-"/>
<pin name="LED1_G+"/>
<pin name="LED2_Y+_G-"/>
<pin name="LED2_Y-_G+"/>
<pin name="SHIELD1" direction="pwr"/>
<pin name="SHIELD2" direction="pwr"/>
<pin name="V1" direction="pwr"/>
<pin name="V2" direction="pwr"/>
<pin name="V3" direction="pwr"/>
<pin name="V4" direction="pwr"/>
</symbol>
<symbol name="7499611424">
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="SHIELD1" direction="pwr"/>
<pin name="SHIELD2" direction="pwr"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="LED1_G+"/>
<pin name="LED1_G-"/>
<pin name="LED1_G+/Y-"/>
<pin name="LED1_G-/Y+"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-RJ45_10G_7499611423" prefix="T">
<description>&lt;b&gt;WE-RJ45 10G Transformer
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RJ45 connector with integrated transformer &amp; common mode choke
&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +85°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122818v209%20Family_WE-RJ45LAN_10G_7499611420_a.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122818v209%20Family_WE-RJ45LAN_10G_7499611420_a.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-RJ45-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-RJ45-10G&lt;/a&gt;&lt;p&gt;

Create By Ella Wu  2020-10-26&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499611423"/>
</gates>
<devices>
<device name="" package="7499611423">
<connects>
<connect gate="G$1" pin="CMCT" pad="13"/>
<connect gate="G$1" pin="CMS+" pad="14"/>
<connect gate="G$1" pin="CMS-" pad="15"/>
<connect gate="G$1" pin="LED1_G+/Y-" pad="18"/>
<connect gate="G$1" pin="LED1_G-/Y+" pad="19"/>
<connect gate="G$1" pin="LED2_G+" pad="17"/>
<connect gate="G$1" pin="LED2_G-" pad="16"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TRCT1" pad="7"/>
<connect gate="G$1" pin="TRCT2" pad="1"/>
<connect gate="G$1" pin="TRCT3" pad="6"/>
<connect gate="G$1" pin="TRCT4" pad="12"/>
<connect gate="G$1" pin="TRD1+" pad="8"/>
<connect gate="G$1" pin="TRD1-" pad="9"/>
<connect gate="G$1" pin="TRD2+" pad="2"/>
<connect gate="G$1" pin="TRD2-" pad="3"/>
<connect gate="G$1" pin="TRD3+" pad="4"/>
<connect gate="G$1" pin="TRD3-" pad="5"/>
<connect gate="G$1" pin="TRD4+" pad="10"/>
<connect gate="G$1" pin="TRD4-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10GBASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7499611423?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="LED" value="yellow/green-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7499611423"/>
<attribute name="PHY-CHIP-MODE" value="current &amp; voltage"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="SHIELD-TABS" value="Yes"/>
<attribute name="TAB" value="Down"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="7499611423"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_10G_7499811120" prefix="T">
<description>&lt;b&gt;WE-RJ45 10G Transformer
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RJ45 connector with integrated transformer &amp; common mode choke
&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +85°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122818v209%20Family_WE-RJ45LAN_10G_7499611420_a.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122818v209%20Family_WE-RJ45LAN_10G_7499611420_a.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-RJ45-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-RJ45-10G&lt;/a&gt;&lt;p&gt;

Create By Ella Wu  2020-10-26&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499811120"/>
</gates>
<devices>
<device name="" package="7499811120">
<connects>
<connect gate="G$1" pin="LED1_Y+" pad="22"/>
<connect gate="G$1" pin="LED1_Y-" pad="21"/>
<connect gate="G$1" pin="LED2_G+" pad="19"/>
<connect gate="G$1" pin="LED2_G-" pad="18"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TRCT1" pad="1"/>
<connect gate="G$1" pin="TRCT2" pad="9"/>
<connect gate="G$1" pin="TRCT3" pad="10"/>
<connect gate="G$1" pin="TRCT4" pad="6"/>
<connect gate="G$1" pin="TRD1+" pad="7"/>
<connect gate="G$1" pin="TRD1-" pad="8"/>
<connect gate="G$1" pin="TRD2+" pad="2"/>
<connect gate="G$1" pin="TRD2-" pad="3"/>
<connect gate="G$1" pin="TRD3+" pad="4"/>
<connect gate="G$1" pin="TRD3-" pad="5"/>
<connect gate="G$1" pin="TRD4+" pad="11"/>
<connect gate="G$1" pin="TRD4-" pad="12"/>
<connect gate="G$1" pin="VC12" pad="13"/>
<connect gate="G$1" pin="VC36" pad="14"/>
<connect gate="G$1" pin="VC45" pad="15"/>
<connect gate="G$1" pin="VC78" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10GBASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7499811120?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7499811120"/>
<attribute name="PHY-CHIP-MODE" value="current &amp; voltage"/>
<attribute name="POE" value="4PPoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="SHIELD-TABS" value="Yes"/>
<attribute name="TAB" value="Down"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="7499811120"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_10G_7499711421" prefix="T">
<description>&lt;b&gt;WE-RJ45 10G Transformer
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RJ45 connector with integrated transformer &amp; common mode choke
&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +85°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122818v209%20Family_WE-RJ45LAN_10G_7499611420_a.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122818v209%20Family_WE-RJ45LAN_10G_7499611420_a.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-RJ45-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-RJ45-10G&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-08-15&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499711421"/>
</gates>
<devices>
<device name="" package="7499711421">
<connects>
<connect gate="G$1" pin="CD1" pad="7"/>
<connect gate="G$1" pin="CD2" pad="1"/>
<connect gate="G$1" pin="CD3" pad="6"/>
<connect gate="G$1" pin="CD4" pad="12"/>
<connect gate="G$1" pin="D1+" pad="8"/>
<connect gate="G$1" pin="D1-" pad="9"/>
<connect gate="G$1" pin="D2+" pad="3"/>
<connect gate="G$1" pin="D2-" pad="2"/>
<connect gate="G$1" pin="D3+" pad="4"/>
<connect gate="G$1" pin="D3-" pad="5"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="10"/>
<connect gate="G$1" pin="LED1_G+" pad="17"/>
<connect gate="G$1" pin="LED1_G-" pad="18"/>
<connect gate="G$1" pin="LED2_Y+_G-" pad="19"/>
<connect gate="G$1" pin="LED2_Y-_G+" pad="20"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="V1" pad="13"/>
<connect gate="G$1" pin="V2" pad="14"/>
<connect gate="G$1" pin="V3" pad="15"/>
<connect gate="G$1" pin="V4" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10GBASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7499711421?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="LED" value="yellow/green-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7499711421"/>
<attribute name="PHY-CHIP-MODE" value="current &amp; voltage"/>
<attribute name="POE" value="PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="SHIELD-TABS" value="Yes"/>
<attribute name="TAB" value="Up"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="7499711421"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_10G_7499611421" prefix="T">
<description>&lt;b&gt;WE-RJ45 10G Transformer
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RJ45 connector with integrated transformer &amp; common mode choke
&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +85°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122818v209%20Family_WE-RJ45LAN_10G_7499611420_a.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122818v209%20Family_WE-RJ45LAN_10G_7499611420_a.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-RJ45-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-RJ45-10G&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-08-15&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499611421"/>
</gates>
<devices>
<device name="" package="7499611421">
<connects>
<connect gate="G$1" pin="CD1" pad="7"/>
<connect gate="G$1" pin="CD2" pad="1"/>
<connect gate="G$1" pin="CD3" pad="6"/>
<connect gate="G$1" pin="CD4" pad="12"/>
<connect gate="G$1" pin="D1+" pad="8"/>
<connect gate="G$1" pin="D1-" pad="9"/>
<connect gate="G$1" pin="D2+" pad="3"/>
<connect gate="G$1" pin="D2-" pad="2"/>
<connect gate="G$1" pin="D3+" pad="4"/>
<connect gate="G$1" pin="D3-" pad="5"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="10"/>
<connect gate="G$1" pin="LED1_G+" pad="14"/>
<connect gate="G$1" pin="LED1_G-" pad="13"/>
<connect gate="G$1" pin="LED2_Y+/G-" pad="15"/>
<connect gate="G$1" pin="LED2_Y-/G+" pad="16"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10GBASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7499611421?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="LED" value="yellow/green-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PART-NUMBER" value="7499611421"/>
<attribute name="PHY-CHIP-MODE" value="current &amp; voltage"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="SHIELD-TABS" value="Yes"/>
<attribute name="TAB" value="Up"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="7499611421"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_10G_7499811420" prefix="T">
<description>&lt;b&gt;WE-RJ45 10G Transformer
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RJ45 connector with integrated transformer &amp; common mode choke
&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +85°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122818v209%20Family_WE-RJ45LAN_10G_7499611420_a.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122818v209%20Family_WE-RJ45LAN_10G_7499611420_a.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-RJ45-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-RJ45-10G&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu  2019-08-15&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499811420"/>
</gates>
<devices>
<device name="" package="7499811420">
<connects>
<connect gate="G$1" pin="CD1" pad="7"/>
<connect gate="G$1" pin="CD2" pad="1"/>
<connect gate="G$1" pin="CD3" pad="6"/>
<connect gate="G$1" pin="CD4" pad="12"/>
<connect gate="G$1" pin="D1+" pad="8"/>
<connect gate="G$1" pin="D1-" pad="9"/>
<connect gate="G$1" pin="D2+" pad="3"/>
<connect gate="G$1" pin="D2-" pad="2"/>
<connect gate="G$1" pin="D3+" pad="4"/>
<connect gate="G$1" pin="D3-" pad="5"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="10"/>
<connect gate="G$1" pin="LED1_G+" pad="17"/>
<connect gate="G$1" pin="LED1_G-" pad="18"/>
<connect gate="G$1" pin="LED2_Y+_G-" pad="19"/>
<connect gate="G$1" pin="LED2_Y-_G+" pad="20"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="V1" pad="13"/>
<connect gate="G$1" pin="V2" pad="14"/>
<connect gate="G$1" pin="V3" pad="15"/>
<connect gate="G$1" pin="V4" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10GBASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7499811420?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="LED" value="yellow/green-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7499811420"/>
<attribute name="PHY-CHIP-MODE" value="current &amp; voltage"/>
<attribute name="POE" value="PoE+"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="SHIELD-TABS" value="Yes"/>
<attribute name="TAB" value="Up"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="7499811420"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_10G_7499611420" prefix="T">
<description>&lt;b&gt;WE-RJ45 10G Transformer
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RJ45 connector with integrated transformer &amp; common mode choke
&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +85°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122818v209%20Family_WE-RJ45LAN_10G_7499611420_a.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122818v209%20Family_WE-RJ45LAN_10G_7499611420_a.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-RJ45-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-RJ45-10G&lt;/a&gt;&lt;p&gt;

Updated By Ella Wu 2026-01-29&lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499611420"/>
</gates>
<devices>
<device name="" package="7499611420">
<connects>
<connect gate="G$1" pin="CD1" pad="7"/>
<connect gate="G$1" pin="CD2" pad="1"/>
<connect gate="G$1" pin="CD3" pad="6"/>
<connect gate="G$1" pin="CD4" pad="12"/>
<connect gate="G$1" pin="D1+" pad="8"/>
<connect gate="G$1" pin="D1-" pad="9"/>
<connect gate="G$1" pin="D2+" pad="3"/>
<connect gate="G$1" pin="D2-" pad="2"/>
<connect gate="G$1" pin="D3+" pad="4"/>
<connect gate="G$1" pin="D3-" pad="5"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="10"/>
<connect gate="G$1" pin="LED1_G+" pad="14"/>
<connect gate="G$1" pin="LED1_G-" pad="13"/>
<connect gate="G$1" pin="LED2_G-" pad="17"/>
<connect gate="G$1" pin="LED2_Y+_G+" pad="16"/>
<connect gate="G$1" pin="LED2_Y-" pad="15"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10GBASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7499611420?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="LED" value="yellow/green-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7499611420"/>
<attribute name="PHY-CHIP-MODE" value="current &amp; voltage"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="SHIELD-TABS" value="Yes"/>
<attribute name="TAB" value="Up"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="7499611420"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_10G_7499611424" prefix="T">
<description>&lt;b&gt;WE-RJ45 10G Transformer
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RJ45 connector with integrated transformer &amp; common mode choke
&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +85°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122818v209%20Family_WE-RJ45LAN_10G_7499611420_a.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122818v209%20Family_WE-RJ45LAN_10G_7499611420_a.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-RJ45-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-RJ45-10G&lt;/a&gt;&lt;p&gt;

Create By Ella Wu  2020-10-26&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499611424"/>
</gates>
<devices>
<device name="" package="7499611424">
<connects>
<connect gate="G$1" pin="LED1_G+" pad="15"/>
<connect gate="G$1" pin="LED1_G+/Y-" pad="17"/>
<connect gate="G$1" pin="LED1_G-" pad="16"/>
<connect gate="G$1" pin="LED1_G-/Y+" pad="18"/>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P10" pad="10"/>
<connect gate="G$1" pin="P11" pad="11"/>
<connect gate="G$1" pin="P12" pad="12"/>
<connect gate="G$1" pin="P13" pad="13"/>
<connect gate="G$1" pin="P14" pad="14"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P4" pad="4"/>
<connect gate="G$1" pin="P5" pad="5"/>
<connect gate="G$1" pin="P6" pad="6"/>
<connect gate="G$1" pin="P7" pad="7"/>
<connect gate="G$1" pin="P8" pad="8"/>
<connect gate="G$1" pin="P9" pad="9"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10GBASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7499611424?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="LED" value="yellow/green-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7499611424"/>
<attribute name="PHY-CHIP-MODE" value="current &amp; voltage"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="SHIELD-TABS" value="Yes"/>
<attribute name="TAB" value="Up"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="7499611424"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_10G_7499611422" prefix="T">
<description>&lt;b&gt;WE-RJ45 10G Transformer
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;RJ45 connector with integrated transformer &amp; common mode choke
&lt;br&gt;10G Base-T
&lt;br&gt;PoE(+) over 4 pairs
&lt;br&gt;Compliant with IEEE standards: 802.3af, 802.3at, 802.3an and 802.3bt
&lt;br&gt;Suitable for industrial temperatures: -40°C up to +85°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Office and factory access points
&lt;br&gt;Gateways
&lt;br&gt;Servers
&lt;br&gt;High-speed routers and switches
&lt;br&gt;HDBaseT applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122818v209%20Family_WE-RJ45LAN_10G_7499611420_a.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122818v209%20Family_WE-RJ45LAN_10G_7499611420_a.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LAN-RJ45-10G/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LAN-RJ45-10G&lt;/a&gt;&lt;p&gt;

Create By Ella Wu  2020-10-26&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499611420"/>
</gates>
<devices>
<device name="" package="7499611422">
<connects>
<connect gate="G$1" pin="CD1" pad="7"/>
<connect gate="G$1" pin="CD2" pad="1"/>
<connect gate="G$1" pin="CD3" pad="6"/>
<connect gate="G$1" pin="CD4" pad="12"/>
<connect gate="G$1" pin="D1+" pad="8"/>
<connect gate="G$1" pin="D1-" pad="9"/>
<connect gate="G$1" pin="D2+" pad="3"/>
<connect gate="G$1" pin="D2-" pad="2"/>
<connect gate="G$1" pin="D3+" pad="4"/>
<connect gate="G$1" pin="D3-" pad="5"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="10"/>
<connect gate="G$1" pin="LED1_G+" pad="14"/>
<connect gate="G$1" pin="LED1_G-" pad="13"/>
<connect gate="G$1" pin="LED2_G-" pad="17"/>
<connect gate="G$1" pin="LED2_Y+_G+" pad="16"/>
<connect gate="G$1" pin="LED2_Y-" pad="15"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10GBASE-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7499611422?ae"/>
<attribute name="IMPROVED-CMRR" value="No"/>
<attribute name="LED" value="yellow/green-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PART-NUMBER" value="7499611422"/>
<attribute name="PHY-CHIP-MODE" value="current &amp; voltage"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value=" 1 "/>
<attribute name="SHIELD-TABS" value="Yes"/>
<attribute name="TAB" value="Down"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="7499611422"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
