<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<library>
<description>Würth Elektronik - Passive Components - Signal &amp; Communications - Filtered Connectors - WE-RJ45 LAN

Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, 
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. 
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. 
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. 

Please contact us for more information: libraries@we-online.com 

Würth Elektronik eiSos GmbH &amp; Co. KG
EMC &amp; Inductive Solutions
www.we-online.com

Fusion360, Library Revision 2026c, 2026-09-22
Copyright: Würth Elektronik</description>
<packages>
<package name="7499111221A">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="7499210001A">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="74981104400">
<description>WE-RJ45 LAN Through Hole Reflow
1000BASE-T, Ports:1x1, Tab:Up</description>
</package>
<package name="7498210220A">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="74990214400">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1x2, Tab:Up</description>
</package>
<package name="7499011222A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Down</description>
</package>
<package name="7498011122AR">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="74991104403">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Down</description>
</package>
<package name="7499111615">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="7498011001A">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Down</description>
</package>
<package name="7499110123">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Vertical</description>
</package>
<package name="7497011611A">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="74991104404">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="7499211125">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="74991114410">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Vertical</description>
</package>
<package name="74981102100">
<description>WE-RJ45 LAN Through Hole Reflow
10/100/1000BASE-T, Ports:1, Tab:Vertical</description>
</package>
<package name="7499210121A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Down</description>
</package>
<package name="74990111215A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Down</description>
</package>
<package name="7499511420">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="7499511440">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="7499211123A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Down</description>
</package>
<package name="7499511611A">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="7499011001A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Down</description>
</package>
<package name="74990101241">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Vertical</description>
</package>
<package name="7497111611A">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="74990101212">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Up</description>
</package>
<package name="7499010003A">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="74991114411">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Down</description>
</package>
<package name="7499010001A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Up</description>
</package>
<package name="7499031120A">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1x4, Tab:Down</description>
</package>
<package name="74982104400">
<description>WE-RJ45 LAN Through Hole Reflow
100BASE-TX, Ports:1x1, Tab:Up</description>
</package>
<package name="7499210123A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Vertical</description>
</package>
<package name="7498011008">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Down</description>
</package>
<package name="74990111217">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="7499211122A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Down</description>
</package>
<package name="7499211002A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Down</description>
</package>
<package name="7499110124">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1x1, Tab:Up</description>
</package>
<package name="7497110616">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="7499410221">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Vertical</description>
</package>
<package name="7499110122">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1x1, Tab:Down</description>
</package>
<package name="74980111212">
<description>WE-RJ45 LAN Through Hole Reflow
10/100BASE-TX, Ports:1, Tab:Down</description>
</package>
<package name="7499021125">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x2, Tab:Down</description>
</package>
<package name="7499010121A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Up</description>
</package>
<package name="7499011441A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Up</description>
</package>
<package name="74981104402">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Vertical</description>
</package>
<package name="7499010126A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Vertical</description>
</package>
<package name="7498010210A">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="7499410213">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Down</description>
</package>
<package name="7498111001A">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="7498111120AR">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="7498210003">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="7499011121A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Down</description>
</package>
<package name="74991204400">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1x2, Tab:Down</description>
</package>
<package name="7499111446">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1x1, Tab:Down</description>
</package>
<package name="7499111001A">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1x1, Tab:Down</description>
</package>
<package name="7499010211A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Down</description>
</package>
<package name="7499021002A">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1x2, Tab:Down</description>
</package>
<package name="74990100011A">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="7499011448">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Vertical</description>
</package>
<package name="7499010004A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Down</description>
</package>
<package name="74990100040">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Down</description>
</package>
<package name="74991214400">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1x2, Tab:Down</description>
</package>
<package name="7499511002A">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="7499411122A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1, Tab:Up</description>
</package>
<package name="7499211121A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Down</description>
</package>
<package name="74991114412">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="7499111614A">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="74990110030">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Up</description>
</package>
<package name="7499051002">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:2x1, Tab:Up/Down</description>
</package>
<package name="7498011211">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1, Tab:Down</description>
</package>
<package name="74980101200">
<description>WE-RJ45 LAN Through Hole Reflow
10/100BASE-TX, Ports:1, Tab:Vertical</description>
</package>
<package name="7498111123">
<description>WE-RJ45 LAN Through Hole Reflow
1000BASE-T, Ports:1, Tab:Down</description>
</package>
<package name="7499151120">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:2x1, Tab:Up/Down</description>
</package>
<package name="74990101210">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Vertical</description>
</package>
<package name="7499311614">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="74980104400">
<description>WE-RJ45 LAN Through Hole Reflow
100BASE-TX, Ports:1, Tab:Up</description>
</package>
<package name="74980111211">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="74980100000">
<description>WE-RJ45 LAN Through Hole Reflow
10/100BASE-TX, Ports:1, Tab:Vertical</description>
</package>
<package name="74990112116A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Up</description>
</package>
<package name="7499010441">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Down</description>
</package>
<package name="7499121211">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1x2, Tab:Down</description>
</package>
<package name="7499110120A">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1x1, Tab:Vertical</description>
</package>
<package name="74991104402">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Vertical</description>
</package>
<package name="7498111124">
<description>WE-RJ45 LAN Through Hole Reflow
1000BASE-T, Ports:1, Tab:Down</description>
</package>
<package name="7499111121A">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1x1, Tab:Down</description>
</package>
<package name="7498210002">
<description>WE-RJ45 LAN Transformer
10/100BASE-T, Ports:1, Tab:Down</description>
</package>
<package name="7499111447">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="7499111000A">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1, Tab:Up</description>
</package>
<package name="74990111211">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Down</description>
</package>
<package name="74984104401">
<description>WE-RJ45 LAN Through Hole Reflow
10/100BASE-TX, Ports:1, Tab:Vertical</description>
</package>
<package name="7499210124A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Up</description>
</package>
<package name="74980100001">
<description>WE-RJ45 LAN Through Hole Reflow
10/100BASE-TX, Ports:1, Tab:Down</description>
</package>
<package name="74984104400">
<description>WE-RJ45 LAN Through Hole Reflow
100BASE-TX, Ports:1x1, Tab:Up</description>
</package>
<package name="7499410443">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1</description>
</package>
<package name="7499510443">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1</description>
</package>
<package name="7499511443">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1</description>
</package>
<package name="7499411443">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1</description>
</package>
<package name="7498510213">
<description>WE-RJ45 LAN Transformer
1000BASE-T, Ports:1x1, Tab: Down</description>
</package>
<package name="7499011002A">
<description>WE-RJ45 LAN Transformer
100BASE-TX, Ports:1x1, Tab:Down</description>
</package>
</packages>
<symbols>
<symbol name="7499410440">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V4" direction="pas"/>
<pin name="V3" direction="pas"/>
<pin name="V1" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_G+/Y-" direction="pas"/>
<pin name="LED2_G-/Y+" direction="pas"/>
<pin name="LED1_Y-/G+" direction="pas"/>
<pin name="LED1_Y+/G-" direction="pas"/>
</symbol>
<symbol name="7499510440">
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V4" direction="pas"/>
<pin name="V3" direction="pas"/>
<pin name="V1" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="LED1_Y-/G+" direction="pas"/>
<pin name="LED1_Y+/G-" direction="pas"/>
<pin name="LED2_Y-/G+" direction="pas"/>
<pin name="LED2_Y+/G-" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="7499031001A">
<pin name="A1" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="B4" direction="pas"/>
<pin name="B5" direction="pas"/>
<pin name="B6" direction="pas"/>
<pin name="B8" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="B7" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C3" direction="pas"/>
<pin name="C4" direction="pas"/>
<pin name="C5" direction="pas"/>
<pin name="C6" direction="pas"/>
<pin name="C7" direction="pas"/>
<pin name="C8" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="D4" direction="pas"/>
<pin name="D5" direction="pas"/>
<pin name="D6" direction="pas"/>
<pin name="D7" direction="pas"/>
<pin name="D8" direction="pas"/>
</symbol>
<symbol name="7499411440">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V4" direction="pas"/>
<pin name="V3" direction="pas"/>
<pin name="V1" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_G+/Y-" direction="pas"/>
<pin name="LED2_G-/Y+" direction="pas"/>
<pin name="LED1_Y-/G+" direction="pas"/>
<pin name="LED1_Y+/G-" direction="pas"/>
</symbol>
<symbol name="7499011002A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499511441">
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V4" direction="pas"/>
<pin name="V3" direction="pas"/>
<pin name="V1" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="LED1_Y-/G+" direction="pas"/>
<pin name="LED1_Y+/G-" direction="pas"/>
<pin name="LED2_Y-/G+" direction="pas"/>
<pin name="LED2_Y+/G-" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="7499111221A">
<pin name="D4-" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="CD4" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="CD2" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="CD3" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="CD1" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
</symbol>
<symbol name="7498210220A">
<pin name="RD+" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CD" direction="pas"/>
<pin name="V1+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V1-" direction="pas"/>
<pin name="V2+" direction="pas"/>
<pin name="V2-" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
</symbol>
<symbol name="7498011122AR">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="74981104400">
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="LED1_G+/Y-" direction="pas"/>
<pin name="LED1_G-/Y+" direction="pas"/>
<pin name="LED2_G+/Y-" direction="pas"/>
<pin name="LED2_G-/Y+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="74990214400">
<pin name="A1" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="B4" direction="pas"/>
<pin name="B5" direction="pas"/>
<pin name="B6" direction="pas"/>
<pin name="B8" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="B7" direction="pas"/>
<pin name="A12" direction="pas"/>
<pin name="A11" direction="pas"/>
<pin name="A9" direction="pas"/>
<pin name="A10" direction="pas"/>
<pin name="B9" direction="pas"/>
<pin name="B10" direction="pas"/>
<pin name="B11" direction="pas"/>
<pin name="B12" direction="pas"/>
</symbol>
<symbol name="7499210001A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="V+" direction="pas"/>
</symbol>
<symbol name="7498011001A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499011222A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="74991104403">
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="LED1_Y-/G+" direction="pas"/>
<pin name="LED1_Y+/G-" direction="pas"/>
<pin name="LED2_Y-/G+" direction="pas"/>
<pin name="LED2_Y+/G-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
</symbol>
<symbol name="7499110123">
<pin name="D4-" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="LED1_G-/Y+" direction="pas"/>
<pin name="LED1_G+/Y-" direction="pas"/>
<pin name="LED2_Y-/G+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="LED2_Y+/G-" direction="pas"/>
</symbol>
<symbol name="74991104404">
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="LED1_Y-/G+" direction="pas"/>
<pin name="LED1_Y+/G-" direction="pas"/>
<pin name="LED2_Y-/G+" direction="pas"/>
<pin name="LED2_Y+/G-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
</symbol>
<symbol name="74990111215A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499111615">
<pin name="D2+" direction="pas"/>
<pin name="CD1" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="CD2" direction="pas"/>
<pin name="CD3" direction="pas"/>
<pin name="CD4" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="LED1_O-" direction="pas"/>
<pin name="LED1_O+/G+" direction="pas"/>
<pin name="LED2_Y-" direction="pas"/>
<pin name="LED2_Y+" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
</symbol>
<symbol name="7499210121A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="V+" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="NC@1" direction="pas"/>
</symbol>
<symbol name="74981102100">
<pin name="D3+" direction="pas"/>
<pin name="VCC&amp;GND" direction="pas"/>
<pin name="VCC&amp;GND1" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="LED2_Y-" direction="pas"/>
<pin name="LED2_Y+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D4-" direction="pas"/>
</symbol>
<symbol name="7497011611A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED2_G-/O+" direction="pas"/>
<pin name="LED2_G+/O-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="SHIELD3" direction="pas"/>
<pin name="SHIELD4" direction="pas"/>
</symbol>
<symbol name="7499511611A">
<pin name="D2+" direction="pas"/>
<pin name="CD1" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V4" direction="pas"/>
<pin name="V3" direction="pas"/>
<pin name="V1" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="CD2" direction="pas"/>
<pin name="CD3" direction="pas"/>
<pin name="CD4" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED2_O+/G-" direction="pas"/>
<pin name="LED2_O-/G+" direction="pas"/>
</symbol>
<symbol name="USB2.0">
<pin name="D-" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VCC" direction="pas"/>
</symbol>
<symbol name="7499211125">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="V+" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="LED2_Y+" direction="pas"/>
<pin name="LED2_Y-" direction="pas"/>
</symbol>
<symbol name="7499511420">
<pin name="D2+" direction="pas"/>
<pin name="CD1" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V4" direction="pas"/>
<pin name="V3" direction="pas"/>
<pin name="V1" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="CD2" direction="pas"/>
<pin name="CD3" direction="pas"/>
<pin name="CD4" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="LED2_G-/Y+" direction="pas"/>
<pin name="LED2_G+/Y-" direction="pas"/>
</symbol>
<symbol name="7499511440">
<pin name="D2+" direction="pas"/>
<pin name="CD1" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V4" direction="pas"/>
<pin name="V3" direction="pas"/>
<pin name="V1" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="CD2" direction="pas"/>
<pin name="CD3" direction="pas"/>
<pin name="CD4" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="LED1_G-/Y+" direction="pas"/>
<pin name="LED1_G+/Y-" direction="pas"/>
<pin name="LED2_G-/Y+" direction="pas"/>
<pin name="LED2_G+/Y-" direction="pas"/>
</symbol>
<symbol name="7499011001A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
</symbol>
<symbol name="74990101212">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_Y+" direction="pas"/>
<pin name="LED2_Y-" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499010003A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7497111611A">
<pin name="D4-" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="VDD" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="LED2_G+/O+" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
<pin name="LED2_O-" direction="pas"/>
</symbol>
<symbol name="74991114411">
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="LED1_Y-/G+" direction="pas"/>
<pin name="LED1_Y+/G-" direction="pas"/>
<pin name="LED2_Y-/G+" direction="pas"/>
<pin name="LED2_Y+/G-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
</symbol>
<symbol name="7499211123A">
<pin name="RD+" direction="pas"/>
<pin name="CD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V2-" direction="pas"/>
<pin name="V2+" direction="pas"/>
<pin name="V1+" direction="pas"/>
<pin name="V1-" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
</symbol>
<symbol name="74990101241">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="74991114410">
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="LED1_G+/Y-" direction="pas"/>
<pin name="LED1_G-/Y+" direction="pas"/>
<pin name="LED2_G+/Y-" direction="pas"/>
<pin name="LED2_G-/Y+" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="7499031120A">
<pin name="A1" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="B4" direction="pas"/>
<pin name="B5" direction="pas"/>
<pin name="B6" direction="pas"/>
<pin name="B8" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="B7" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C3" direction="pas"/>
<pin name="C4" direction="pas"/>
<pin name="C5" direction="pas"/>
<pin name="C6" direction="pas"/>
<pin name="C7" direction="pas"/>
<pin name="C8" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="D4" direction="pas"/>
<pin name="D5" direction="pas"/>
<pin name="D6" direction="pas"/>
<pin name="D7" direction="pas"/>
<pin name="D8" direction="pas"/>
<pin name="A9" direction="pas"/>
<pin name="A10" direction="pas"/>
<pin name="A11" direction="pas"/>
<pin name="A12" direction="pas"/>
<pin name="B9" direction="pas"/>
<pin name="B10" direction="pas"/>
<pin name="B11" direction="pas"/>
<pin name="B12" direction="pas"/>
<pin name="C9" direction="pas"/>
<pin name="C10" direction="pas"/>
<pin name="C11" direction="pas"/>
<pin name="C12" direction="pas"/>
<pin name="D9" direction="pas"/>
<pin name="D10" direction="pas"/>
<pin name="D11" direction="pas"/>
<pin name="D12" direction="pas"/>
<pin name="SHIELD3" direction="pas"/>
<pin name="SHIELD4" direction="pas"/>
<pin name="SHIELD5" direction="pas"/>
</symbol>
<symbol name="7499010001A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499210123A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="V+" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="NC@1" direction="pas"/>
</symbol>
<symbol name="74982104400">
<pin name="TD+" direction="pas"/>
<pin name="CD" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="RD+" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="V1+" direction="pas"/>
<pin name="V1-" direction="pas"/>
<pin name="LED1_G+/Y-" direction="pas"/>
<pin name="LED1_G-/Y+" direction="pas"/>
<pin name="LED2_G+/Y-" direction="pas"/>
<pin name="LED2_G-/Y+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="V2+" direction="pas"/>
<pin name="V2-" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
</symbol>
<symbol name="74990111217">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499211002A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V2-" direction="pas"/>
<pin name="V2+" direction="pas"/>
<pin name="V1+" direction="pas"/>
<pin name="V1-" direction="pas"/>
</symbol>
<symbol name="7499110124">
<pin name="D4-" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="LED2_G-/Y+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="LED2_G+/Y-" direction="pas"/>
</symbol>
<symbol name="7497110616">
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="VDD" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED2_G-/O+" direction="pas"/>
<pin name="LED2_G+/O-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="SHIELD3" direction="pas"/>
<pin name="SHIELD4" direction="pas"/>
<pin name="SHIELD5" direction="pas"/>
<pin name="SHIELD6" direction="pas"/>
<pin name="SHIELD7" direction="pas"/>
<pin name="SHIELD8" direction="pas"/>
</symbol>
<symbol name="USB3.0">
<pin name="D-" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="RX-" direction="pas"/>
<pin name="RX+" direction="pas"/>
<pin name="GND_SIG" direction="pas"/>
<pin name="TX-" direction="pas"/>
<pin name="TX+" direction="pas"/>
</symbol>
<symbol name="7499211122A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V2-" direction="pas"/>
<pin name="V2+" direction="pas"/>
<pin name="V1+" direction="pas"/>
<pin name="V1-" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
</symbol>
<symbol name="7498011008">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499110122">
<pin name="D4-" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
</symbol>
<symbol name="7499410221">
<pin name="RD+" direction="pas"/>
<pin name="CD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V2+" direction="pas"/>
<pin name="V2-" direction="pas"/>
<pin name="V1+" direction="pas"/>
<pin name="V1-" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
</symbol>
<symbol name="74980111212">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499021125">
<pin name="A1" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="B4" direction="pas"/>
<pin name="B5" direction="pas"/>
<pin name="B6" direction="pas"/>
<pin name="B8" direction="pas"/>
<pin name="SHIELD3" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="B7" direction="pas"/>
<pin name="A9" direction="pas"/>
<pin name="A10" direction="pas"/>
<pin name="A11" direction="pas"/>
<pin name="A12" direction="pas"/>
<pin name="B9" direction="pas"/>
<pin name="B10" direction="pas"/>
<pin name="B11" direction="pas"/>
<pin name="B12" direction="pas"/>
</symbol>
<symbol name="7499011441A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_G+/Y-" direction="pas"/>
<pin name="LED2_G-/Y+" direction="pas"/>
<pin name="LED1_G-/Y+" direction="pas"/>
<pin name="LED1_G+/Y-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499010121A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_Y+" direction="pas"/>
<pin name="LED2_Y-" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499010126A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499410213">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V2-" direction="pas"/>
<pin name="V2+" direction="pas"/>
<pin name="V1+" direction="pas"/>
<pin name="V1-" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="LED2_Y+" direction="pas"/>
<pin name="LED2_Y-" direction="pas"/>
</symbol>
<symbol name="7498010210A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="74981104402">
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="LED1_Y-/G+" direction="pas"/>
<pin name="LED1_Y+/G-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="LED2_Y+/G-" direction="pas"/>
<pin name="LED2_Y-/G+" direction="pas"/>
</symbol>
<symbol name="7498111001A">
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
</symbol>
<symbol name="7498111120AR">
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="LED2_Y-" direction="pas"/>
<pin name="LED2_Y+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
</symbol>
<symbol name="7499011121A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7498210003">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="V1+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V1-" direction="pas"/>
<pin name="V2+" direction="pas"/>
<pin name="V2-" direction="pas"/>
</symbol>
<symbol name="74991204400">
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="A11" direction="pas"/>
<pin name="A12" direction="pas"/>
<pin name="A13" direction="pas"/>
<pin name="A14" direction="pas"/>
<pin name="B11" direction="pas"/>
<pin name="B12" direction="pas"/>
<pin name="B13" direction="pas"/>
<pin name="B14" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="A9" direction="pas"/>
<pin name="A10" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="B4" direction="pas"/>
<pin name="B5" direction="pas"/>
<pin name="B6" direction="pas"/>
<pin name="B7" direction="pas"/>
<pin name="B8" direction="pas"/>
<pin name="B9" direction="pas"/>
<pin name="B10" direction="pas"/>
</symbol>
<symbol name="7499111446">
<pin name="D4-" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="LED1_Y-/G+" direction="pas"/>
<pin name="LED1_Y+/G-" direction="pas"/>
<pin name="LED2_Y-/G+" direction="pas"/>
<pin name="LED2_Y+/G-" direction="pas"/>
</symbol>
<symbol name="7499021002A">
<pin name="A1" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="B4" direction="pas"/>
<pin name="B5" direction="pas"/>
<pin name="B6" direction="pas"/>
<pin name="B8" direction="pas"/>
<pin name="SHIELD3" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="B7" direction="pas"/>
</symbol>
<symbol name="7499111001A">
<pin name="D4-" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
</symbol>
<symbol name="74990100011A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
</symbol>
<symbol name="7499010211A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_Y+" direction="pas"/>
<pin name="LED2_Y-" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499011448">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_G-/Y+" direction="pas"/>
<pin name="LED2_G+/Y-" direction="pas"/>
<pin name="LED1_Y+/G-" direction="pas"/>
<pin name="LED1_Y-/G+" direction="pas"/>
</symbol>
<symbol name="74991214400">
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="A11" direction="pas"/>
<pin name="A12" direction="pas"/>
<pin name="A13" direction="pas"/>
<pin name="A14" direction="pas"/>
<pin name="B11" direction="pas"/>
<pin name="B12" direction="pas"/>
<pin name="B13" direction="pas"/>
<pin name="B14" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="A9" direction="pas"/>
<pin name="A10" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="B4" direction="pas"/>
<pin name="B5" direction="pas"/>
<pin name="B6" direction="pas"/>
<pin name="B7" direction="pas"/>
<pin name="B8" direction="pas"/>
<pin name="B9" direction="pas"/>
<pin name="B10" direction="pas"/>
</symbol>
<symbol name="7499211121A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="V+" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="NC@1" direction="pas"/>
</symbol>
<symbol name="74980101200">
<pin name="8" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="RD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
</symbol>
<symbol name="7499010004A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499411122A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V2-" direction="pas"/>
<pin name="V2+" direction="pas"/>
<pin name="V1+" direction="pas"/>
<pin name="V1-" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="LED2_Y-" direction="pas"/>
<pin name="LED2_Y+" direction="pas"/>
<pin name="CRD" direction="pas"/>
</symbol>
<symbol name="74990100040">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="CRD" direction="pas"/>
</symbol>
<symbol name="7499511002A">
<pin name="D2+" direction="pas"/>
<pin name="CD1" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V4" direction="pas"/>
<pin name="V3" direction="pas"/>
<pin name="V1" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="CD2" direction="pas"/>
<pin name="CD3" direction="pas"/>
<pin name="CD4" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D4-" direction="pas"/>
</symbol>
<symbol name="74991104412">
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="LED1_Y-/G+" direction="pas"/>
<pin name="LED1_Y+/G-" direction="pas"/>
<pin name="LED2_Y-/G+" direction="pas"/>
<pin name="LED2_Y+/G-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
</symbol>
<symbol name="7499111614A">
<pin name="D4-" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="CD4" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="CD2" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="CD3" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="CD1" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED2_O+/G-" direction="pas"/>
<pin name="LED2_O-/G+" direction="pas"/>
</symbol>
<symbol name="7498111123">
<pin name="D3+" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D4-" direction="pas"/>
</symbol>
<symbol name="74990110030">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499151120">
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="A11" direction="pas"/>
<pin name="A12" direction="pas"/>
<pin name="A13" direction="pas"/>
<pin name="A14" direction="pas"/>
<pin name="B11" direction="pas"/>
<pin name="B12" direction="pas"/>
<pin name="B13" direction="pas"/>
<pin name="B14" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="A9" direction="pas"/>
<pin name="A10" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="B4" direction="pas"/>
<pin name="B5" direction="pas"/>
<pin name="B6" direction="pas"/>
<pin name="B7" direction="pas"/>
<pin name="B8" direction="pas"/>
<pin name="B9" direction="pas"/>
<pin name="B10" direction="pas"/>
<pin name="SHIELD3" direction="pas"/>
<pin name="SHIELD4" direction="pas"/>
</symbol>
<symbol name="7499051002">
<pin name="A1" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="B4" direction="pas"/>
<pin name="B5" direction="pas"/>
<pin name="B6" direction="pas"/>
<pin name="B8" direction="pas"/>
<pin name="SHIELD3" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="B7" direction="pas"/>
<pin name="SHIELD4" direction="pas"/>
</symbol>
<symbol name="7499311614">
<pin name="D2+" direction="pas"/>
<pin name="CD1" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V4" direction="pas"/>
<pin name="V3" direction="pas"/>
<pin name="V1" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="CD2" direction="pas"/>
<pin name="CD3" direction="pas"/>
<pin name="CD4" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="LED2_G-/O+" direction="pas"/>
<pin name="LED2_G+/O-" direction="pas"/>
</symbol>
<symbol name="74990101210">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7498011211">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_Y-" direction="pas"/>
<pin name="LED2_Y+" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
</symbol>
<symbol name="74980100000">
<pin name="TD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="RD+" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="74980104400">
<pin name="TD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="RD+" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="LED1_G+/Y-" direction="pas"/>
<pin name="LED1_G-/Y+" direction="pas"/>
<pin name="LED2_G+_Y-" direction="pas"/>
<pin name="LED2_G-_Y+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499010441">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_G-/Y+" direction="pas"/>
<pin name="LED2_G+/Y-" direction="pas"/>
<pin name="LED1_G-/Y+" direction="pas"/>
<pin name="LED1_G+/Y-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499121211">
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="A11" direction="pas"/>
<pin name="A12" direction="pas"/>
<pin name="A13" direction="pas"/>
<pin name="A14" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="A10" direction="pas"/>
<pin name="B11" direction="pas"/>
<pin name="B12" direction="pas"/>
<pin name="B13" direction="pas"/>
<pin name="B14" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B10" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="A9" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="B4" direction="pas"/>
<pin name="B5" direction="pas"/>
<pin name="B6" direction="pas"/>
<pin name="B7" direction="pas"/>
<pin name="B8" direction="pas"/>
<pin name="B9" direction="pas"/>
</symbol>
<symbol name="74980111211">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="LED2_Y+" direction="pas"/>
<pin name="LED2_Y-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="74991104402">
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="LED1_Y-/G+" direction="pas"/>
<pin name="LED1_Y+/G-" direction="pas"/>
<pin name="LED2_Y-/G+" direction="pas"/>
<pin name="LED2_Y+/G-" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="74990112116A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7499110120A">
<pin name="D4-" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
</symbol>
<symbol name="74990111211">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="7498111124">
<pin name="D3+" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="CGND" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D4-" direction="pas"/>
</symbol>
<symbol name="7499111121A">
<pin name="D4-" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="LED1_Y+" direction="pas"/>
<pin name="LED1_Y-" direction="pas"/>
<pin name="LED2_G+" direction="pas"/>
<pin name="LED2_G-" direction="pas"/>
</symbol>
<symbol name="7499111000A">
<pin name="D4-" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="CD4" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="CD2" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="CD3" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="CD1" direction="pas"/>
<pin name="D2+" direction="pas"/>
</symbol>
<symbol name="7499111447">
<pin name="D4-" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="V+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="LED1_Y-/G+" direction="pas"/>
<pin name="LED1_Y+/G-" direction="pas"/>
<pin name="LED2_Y-/G+" direction="pas"/>
<pin name="LED2_Y+/G-" direction="pas"/>
</symbol>
<symbol name="74980100001">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="74984104401">
<pin name="V+" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CD" direction="pas"/>
<pin name="RD+" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="LED1_Y+/G-" direction="pas"/>
<pin name="LED2_Y-/G+" direction="pas"/>
<pin name="LED2_Y+/G-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="LED1_Y-/G+" direction="pas"/>
<pin name="V1-" direction="pas"/>
<pin name="V2+" direction="pas"/>
<pin name="V2-" direction="pas"/>
</symbol>
<symbol name="7498210002">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V+" direction="pas"/>
</symbol>
<symbol name="7499210124A">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="CRD" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="V+" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="LED2_Y-" direction="pas"/>
<pin name="LED2_Y+" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="NC@1" direction="pas"/>
</symbol>
<symbol name="74984104400">
<pin name="TD+" direction="pas"/>
<pin name="CD" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="RD+" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="V1+" direction="pas"/>
<pin name="V1-" direction="pas"/>
<pin name="LED1_G+/Y-" direction="pas"/>
<pin name="LED1_G-/Y+" direction="pas"/>
<pin name="LED2_G+/Y-" direction="pas"/>
<pin name="LED2_G-/Y+" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="V2+" direction="pas"/>
<pin name="V2-" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
</symbol>
<symbol name="7499410443">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V4" direction="pas"/>
<pin name="V3" direction="pas"/>
<pin name="V1" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="LED1_G+/Y-" direction="pas"/>
<pin name="LED1_G-/Y+" direction="pas"/>
<pin name="LED2_Y+/G-" direction="pas"/>
<pin name="LED2_Y-/G+" direction="pas"/>
<pin name="CRD" direction="pas"/>
</symbol>
<symbol name="7499510443">
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V4" direction="pas"/>
<pin name="V3" direction="pas"/>
<pin name="V1" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="LED1_G+/Y-" direction="pas"/>
<pin name="LED1_G-/Y+" direction="pas"/>
<pin name="LED2_G+/Y-" direction="pas"/>
<pin name="LED2_G-/Y+" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="7499511443">
<pin name="D2+" direction="pas"/>
<pin name="D2-" direction="pas"/>
<pin name="D1+" direction="pas"/>
<pin name="D1-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V4" direction="pas"/>
<pin name="V3" direction="pas"/>
<pin name="V1" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="D3+" direction="pas"/>
<pin name="D3-" direction="pas"/>
<pin name="D4+" direction="pas"/>
<pin name="D4-" direction="pas"/>
<pin name="LED1_G+/Y-" direction="pas"/>
<pin name="LED1_G-/Y+" direction="pas"/>
<pin name="LED2_G+/Y-" direction="pas"/>
<pin name="LED2_G-/Y+" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="7499411443">
<pin name="RD+" direction="pas"/>
<pin name="CTD" direction="pas"/>
<pin name="RD-" direction="pas"/>
<pin name="TD+" direction="pas"/>
<pin name="TD-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V4" direction="pas"/>
<pin name="V3" direction="pas"/>
<pin name="V1" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="LED1_G+/Y-" direction="pas"/>
<pin name="LED1_G-/Y+" direction="pas"/>
<pin name="LED2_Y+/G-" direction="pas"/>
<pin name="LED2_Y-/G+" direction="pas"/>
<pin name="CRD" direction="pas"/>
</symbol>
<symbol name="7498510213">
<pin name="RD2+" direction="pas"/>
<pin name="RD2-" direction="pas"/>
<pin name="TD2+" direction="pas"/>
<pin name="TD2-" direction="pas"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="V4" direction="pas"/>
<pin name="V3" direction="pas"/>
<pin name="V1" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="TD1+" direction="pas"/>
<pin name="TD1-" direction="pas"/>
<pin name="RD1+" direction="pas"/>
<pin name="RD1-" direction="pas"/>
<pin name="LED1_G+" direction="pas"/>
<pin name="LED1_G-" direction="pas"/>
<pin name="LED2_Y+" direction="pas"/>
<pin name="LED2_Y-" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-RJ45_7499111221A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-03-27 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499111221A"/>
</gates>
<devices>
<device name="" package="7499111221A">
<connects>
<connect gate="G$1" pin="CD1" pad="12"/>
<connect gate="G$1" pin="CD2" pad="6"/>
<connect gate="G$1" pin="CD3" pad="1"/>
<connect gate="G$1" pin="CD4" pad="7"/>
<connect gate="G$1" pin="D1+" pad="11"/>
<connect gate="G$1" pin="D1-" pad="10"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="3"/>
<connect gate="G$1" pin="D3-" pad="2"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="LED1_G+" pad="14"/>
<connect gate="G$1" pin="LED1_G-" pad="13"/>
<connect gate="G$1" pin="LED2_G+" pad="16"/>
<connect gate="G$1" pin="LED2_G-" pad="15"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499111221A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499111221A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499111221A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499210001A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499210001A"/>
</gates>
<devices>
<device name="" package="7499210001A">
<connects>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="LED" value="No LED"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499210001A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499210001A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499210001A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74981104400" prefix="J">
<description>WE-RJ45 LAN Through Hole Reflow

Characteristics 

RJ45 designed to use for Pin-in-Paste soldering

High mechanical stability through THT pins

High Temperature LEDs

Extra high standoff for a good thermal airflow

Power over Ethernet up to 30 W

Compliant with standard: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45_THR

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74981104400"/>
</gates>
<devices>
<device name="" package="74981104400">
<connects>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="6"/>
<connect gate="G$1" pin="D3-" pad="7"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="LED1_G+/Y-" pad="11"/>
<connect gate="G$1" pin="LED1_G-/Y+" pad="12"/>
<connect gate="G$1" pin="LED2_G+/Y-" pad="13"/>
<connect gate="G$1" pin="LED2_G-/Y+" pad="14"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green/yellow - green/yellow"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Up"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="74981104400"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74981104400?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74981104400"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498210220A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2025-03-18 

2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498210220A"/>
</gates>
<devices>
<device name="" package="7498210220A">
<connects>
<connect gate="G$1" pin="CD" pad="5"/>
<connect gate="G$1" pin="LED1_G+" pad="1"/>
<connect gate="G$1" pin="LED1_G-" pad="2"/>
<connect gate="G$1" pin="LED2_G+" pad="13"/>
<connect gate="G$1" pin="LED2_G-" pad="14"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="7"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="3"/>
<connect gate="G$1" pin="TD-" pad="4"/>
<connect gate="G$1" pin="V1+" pad="9"/>
<connect gate="G$1" pin="V1-" pad="10"/>
<connect gate="G$1" pin="V2+" pad="11"/>
<connect gate="G$1" pin="V2-" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="LED" value="green-green"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="POE" value="PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7498210220A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7498210220A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7498210220A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499111615" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2022-01-18 

2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499111615"/>
</gates>
<devices>
<device name="" package="7499111615">
<connects>
<connect gate="G$1" pin="CD1" pad="12"/>
<connect gate="G$1" pin="CD2" pad="6"/>
<connect gate="G$1" pin="CD3" pad="1"/>
<connect gate="G$1" pin="CD4" pad="7"/>
<connect gate="G$1" pin="D1+" pad="11"/>
<connect gate="G$1" pin="D1-" pad="10"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="3"/>
<connect gate="G$1" pin="D3-" pad="2"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="LED1_G-" pad="17"/>
<connect gate="G$1" pin="LED1_O+/G+" pad="16"/>
<connect gate="G$1" pin="LED1_O-" pad="15"/>
<connect gate="G$1" pin="LED2_Y+" pad="14"/>
<connect gate="G$1" pin="LED2_Y-" pad="13"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green/orange-yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499111615"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499111615?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499111615"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990214400" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Created by Ella Wu 2020-10-27 

2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74990214400"/>
</gates>
<devices>
<device name="" package="74990214400">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B10" pad="B10"/>
<connect gate="G$1" pin="B11" pad="B11"/>
<connect gate="G$1" pin="B12" pad="B12"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="B5" pad="B5"/>
<connect gate="G$1" pin="B6" pad="B6"/>
<connect gate="G$1" pin="B7" pad="B7"/>
<connect gate="G$1" pin="B8" pad="B8"/>
<connect gate="G$1" pin="B9" pad="B9"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x2"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="74990214400"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74990214400?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74990214400"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499011222A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499011222A"/>
</gates>
<devices>
<device name="" package="7499011222A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="LED1_G+" pad="9"/>
<connect gate="G$1" pin="LED1_G-" pad="10"/>
<connect gate="G$1" pin="LED2_G+" pad="11"/>
<connect gate="G$1" pin="LED2_G-" pad="12"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="green-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499011222A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499011222A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499011222A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498011001A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2025-08-28 

2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498011001A"/>
</gates>
<devices>
<device name="" package="7498011001A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="No LED"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7498011001A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7498011001A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7498011001A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74991104403" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 
RJ45 Connector with integrated transformer / common mode choke
Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s
Available in SMD, THT and THT with USB
Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 
Suitable for industrial temperatures from –40 °C up to +85 °C
Compatible to Industrial Ethernet systems like EtherCAT or Profinet
Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2026-07-21
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74991104403"/>
</gates>
<devices>
<device name="" package="74991104403">
<connects>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="6"/>
<connect gate="G$1" pin="D3-" pad="7"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LED1_Y+/G-" pad="12"/>
<connect gate="G$1" pin="LED1_Y-/G+" pad="11"/>
<connect gate="G$1" pin="LED2_Y+/G-" pad="14"/>
<connect gate="G$1" pin="LED2_Y-/G+" pad="13"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="yellow/green-yellow/green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="74991104403"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74991104403?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74991104403"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498011122AR" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498011122AR"/>
</gates>
<devices>
<device name="" package="7498011122AR">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="LED1_Y+" pad="9"/>
<connect gate="G$1" pin="LED1_Y-" pad="10"/>
<connect gate="G$1" pin="LED2_G+" pad="11"/>
<connect gate="G$1" pin="LED2_G-" pad="12"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7498011122AR"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7498011122AR?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7498011122AR"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499110123" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499110123"/>
</gates>
<devices>
<device name="" package="7499110123">
<connects>
<connect gate="G$1" pin="D1+" pad="9"/>
<connect gate="G$1" pin="D1-" pad="8"/>
<connect gate="G$1" pin="D2+" pad="7"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="5"/>
<connect gate="G$1" pin="D3-" pad="4"/>
<connect gate="G$1" pin="D4+" pad="3"/>
<connect gate="G$1" pin="D4-" pad="2"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="LED1_G+/Y-" pad="12"/>
<connect gate="G$1" pin="LED1_G-/Y+" pad="11"/>
<connect gate="G$1" pin="LED2_Y+/G-" pad="14"/>
<connect gate="G$1" pin="LED2_Y-/G+" pad="13"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green-yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Vertical"/>
<attribute name="VALUE" value="7499110123"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499110123?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499110123"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7497011611A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella 2025-03-11

2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7497011611A"/>
<gate name="G$2" symbol="USB2.0"/>
</gates>
<devices>
<device name="" package="7497011611A">
<connects>
<connect gate="G$1" pin="CRD" pad="6"/>
<connect gate="G$1" pin="CTD" pad="1"/>
<connect gate="G$1" pin="LED1_Y+" pad="14"/>
<connect gate="G$1" pin="LED1_Y-" pad="13"/>
<connect gate="G$1" pin="LED2_G+/O-" pad="16"/>
<connect gate="G$1" pin="LED2_G-/O+" pad="15"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="5"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="SHIELD3" pad="S3"/>
<connect gate="G$1" pin="SHIELD4" pad="S4"/>
<connect gate="G$1" pin="TD+" pad="2"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$2" pin="D+" pad="U3"/>
<connect gate="G$2" pin="D-" pad="U2"/>
<connect gate="G$2" pin="GND" pad="U4"/>
<connect gate="G$2" pin="VCC" pad="U1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="green/orange-yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7497011611A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7497011611A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7497011611A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74991104404" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 
RJ45 Connector with integrated transformer / common mode choke
Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s
Available in SMD, THT and THT with USB
Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 
Suitable for industrial temperatures from –40 °C up to +85 °C
Compatible to Industrial Ethernet systems like EtherCAT or Profinet
Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2026-07-21
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74991104404"/>
</gates>
<devices>
<device name="" package="74991104404">
<connects>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="6"/>
<connect gate="G$1" pin="D3-" pad="7"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LED1_Y+/G-" pad="12"/>
<connect gate="G$1" pin="LED1_Y-/G+" pad="11"/>
<connect gate="G$1" pin="LED2_Y+/G-" pad="14"/>
<connect gate="G$1" pin="LED2_Y-/G+" pad="13"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="yellow/green-yellow/green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="74991104404"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74991104404?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74991104404"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74991114410" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Created by Ella Wu 2020-10-27 

2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74991114410"/>
</gates>
<devices>
<device name="" package="74991114410">
<connects>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="2"/>
<connect gate="G$1" pin="D2+" pad="3"/>
<connect gate="G$1" pin="D2-" pad="4"/>
<connect gate="G$1" pin="D3+" pad="7"/>
<connect gate="G$1" pin="D3-" pad="8"/>
<connect gate="G$1" pin="D4+" pad="9"/>
<connect gate="G$1" pin="D4-" pad="10"/>
<connect gate="G$1" pin="LED1_G+/Y-" pad="11"/>
<connect gate="G$1" pin="LED1_G-/Y+" pad="12"/>
<connect gate="G$1" pin="LED2_G+/Y-" pad="13"/>
<connect gate="G$1" pin="LED2_G-/Y+" pad="14"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="yellow/green-yellow/green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Vertical"/>
<attribute name="VALUE" value="74991114410"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74991114410?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74991114410"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499211125" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499211125"/>
</gates>
<devices>
<device name="" package="7499211125">
<connects>
<connect gate="G$1" pin="CRD" pad="3"/>
<connect gate="G$1" pin="CTD" pad="5"/>
<connect gate="G$1" pin="LED1_G+" pad="12"/>
<connect gate="G$1" pin="LED1_G-" pad="11"/>
<connect gate="G$1" pin="LED2_Y+" pad="13"/>
<connect gate="G$1" pin="LED2_Y-" pad="14"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="2"/>
<connect gate="G$1" pin="SHIELD1" pad="Z2"/>
<connect gate="G$1" pin="SHIELD2" pad="Z1"/>
<connect gate="G$1" pin="TD+" pad="4"/>
<connect gate="G$1" pin="TD-" pad="6"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499211125"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499211125?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499211125"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74981102100" prefix="J">
<description>WE-LAN RJ45 LAN Transformer

Characteristics
RJ45 Connector with integrated transformer / common mode choke
Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s
Available in SMT, THT and THT with USB
Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt
Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications
Suitable for industrial temperatures from –40 °C up to +85 °C
Compatible to Industrial Ethernet systems like EtherCAT or Profinet
Compliant with most IC’s for Ethernet applications such as Microchip, Broadcom, Marvell
Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella 2026-09-22
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74981102100"/>
</gates>
<devices>
<device name="" package="74981102100">
<connects>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="2"/>
<connect gate="G$1" pin="D2+" pad="3"/>
<connect gate="G$1" pin="D2-" pad="4"/>
<connect gate="G$1" pin="D3+" pad="7"/>
<connect gate="G$1" pin="D3-" pad="8"/>
<connect gate="G$1" pin="D4+" pad="9"/>
<connect gate="G$1" pin="D4-" pad="10"/>
<connect gate="G$1" pin="LED1_G+" pad="11"/>
<connect gate="G$1" pin="LED1_G-" pad="12"/>
<connect gate="G$1" pin="LED2_Y+" pad="14"/>
<connect gate="G$1" pin="LED2_Y-" pad="13"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="VCC&amp;GND" pad="6"/>
<connect gate="G$1" pin="VCC&amp;GND1" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000 Base-T"/>
<attribute name="LED" value="green-yellow"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Vertical"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="74981102100"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74981102100?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74981102100"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499210121A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499210121A"/>
</gates>
<devices>
<device name="" package="7499210121A">
<connects>
<connect gate="G$1" pin="CRD" pad="3"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="LED1_Y+" pad="11"/>
<connect gate="G$1" pin="LED1_Y-" pad="12"/>
<connect gate="G$1" pin="LED2_G+" pad="13"/>
<connect gate="G$1" pin="LED2_G-" pad="14"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="NC@1" pad="8"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="2"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="5"/>
<connect gate="G$1" pin="TD-" pad="6"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499210121A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499210121A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499210121A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990111215A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74990111215A"/>
</gates>
<devices>
<device name="" package="74990111215A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="LED1_Y+" pad="9"/>
<connect gate="G$1" pin="LED1_Y-" pad="10"/>
<connect gate="G$1" pin="LED2_G+" pad="11"/>
<connect gate="G$1" pin="LED2_G-" pad="12"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="74990111215A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74990111215A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74990111215A"/>
<attribute name="IMPROVED_CMRR" value="Yes"/>
<attribute name="OPERATING_TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499511420" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-03-27 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499511420"/>
</gates>
<devices>
<device name="" package="7499511420">
<connects>
<connect gate="G$1" pin="CD1" pad="12"/>
<connect gate="G$1" pin="CD2" pad="6"/>
<connect gate="G$1" pin="CD3" pad="1"/>
<connect gate="G$1" pin="CD4" pad="7"/>
<connect gate="G$1" pin="D1+" pad="10"/>
<connect gate="G$1" pin="D1-" pad="11"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="4"/>
<connect gate="G$1" pin="D3+" pad="2"/>
<connect gate="G$1" pin="D3-" pad="3"/>
<connect gate="G$1" pin="D4+" pad="9"/>
<connect gate="G$1" pin="D4-" pad="8"/>
<connect gate="G$1" pin="LED1_G+" pad="17"/>
<connect gate="G$1" pin="LED1_G-" pad="18"/>
<connect gate="G$1" pin="LED2_G+/Y-" pad="20"/>
<connect gate="G$1" pin="LED2_G-/Y+" pad="19"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="V1" pad="13"/>
<connect gate="G$1" pin="V2" pad="14"/>
<connect gate="G$1" pin="V3" pad="15"/>
<connect gate="G$1" pin="V4" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green/yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="4PPoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499511420"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499511420?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499511420"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499511440" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-03-27 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499511440"/>
</gates>
<devices>
<device name="" package="7499511440">
<connects>
<connect gate="G$1" pin="CD1" pad="12"/>
<connect gate="G$1" pin="CD2" pad="6"/>
<connect gate="G$1" pin="CD3" pad="1"/>
<connect gate="G$1" pin="CD4" pad="7"/>
<connect gate="G$1" pin="D1+" pad="11"/>
<connect gate="G$1" pin="D1-" pad="10"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="3"/>
<connect gate="G$1" pin="D3-" pad="2"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="LED1_G+/Y-" pad="18"/>
<connect gate="G$1" pin="LED1_G-/Y+" pad="17"/>
<connect gate="G$1" pin="LED2_G+/Y-" pad="20"/>
<connect gate="G$1" pin="LED2_G-/Y+" pad="19"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="V1" pad="13"/>
<connect gate="G$1" pin="V2" pad="14"/>
<connect gate="G$1" pin="V3" pad="15"/>
<connect gate="G$1" pin="V4" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green/yellow - green/yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE+"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499511440"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499511440?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499511440"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499011001A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499011001A"/>
</gates>
<devices>
<device name="" package="7499011001A">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="No LED"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499011001A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499011001A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499011001A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499211123A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499211123A"/>
</gates>
<devices>
<device name="" package="7499211123A">
<connects>
<connect gate="G$1" pin="CD" pad="3"/>
<connect gate="G$1" pin="LED1_Y+" pad="11"/>
<connect gate="G$1" pin="LED1_Y-" pad="12"/>
<connect gate="G$1" pin="LED2_G+" pad="13"/>
<connect gate="G$1" pin="LED2_G-" pad="14"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="5"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="G$1" pin="V1+" pad="7"/>
<connect gate="G$1" pin="V1-" pad="8"/>
<connect gate="G$1" pin="V2+" pad="9"/>
<connect gate="G$1" pin="V2-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499211123A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499211123A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499211123A"/>
<attribute name="IMPROVED_CMRR" value="Yes"/>
<attribute name="OPERATING_TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990101241" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74990101241"/>
</gates>
<devices>
<device name="" package="74990101241">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="LED1_Y+" pad="9"/>
<connect gate="G$1" pin="LED1_Y-" pad="10"/>
<connect gate="G$1" pin="LED2_G+" pad="11"/>
<connect gate="G$1" pin="LED2_G-" pad="12"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="LED" value="green-yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Vertical"/>
<attribute name="VALUE" value="74990101241"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74990101241?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74990101241"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74991114411" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 
RJ45 Connector with integrated transformer / common mode choke
Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s
Available in SMD, THT and THT with USB
Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 
Suitable for industrial temperatures from –40 °C up to +85 °C
Compatible to Industrial Ethernet systems like EtherCAT or Profinet
Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2026-07-21
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74991114411"/>
</gates>
<devices>
<device name="" package="74991114411">
<connects>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="6"/>
<connect gate="G$1" pin="D3-" pad="7"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LED1_Y+/G-" pad="12"/>
<connect gate="G$1" pin="LED1_Y-/G+" pad="11"/>
<connect gate="G$1" pin="LED2_Y+/G-" pad="14"/>
<connect gate="G$1" pin="LED2_Y-/G+" pad="13"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="yellow/green-yellow/green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="74991114411"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74991114411?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74991114411"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990101212" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74990101212"/>
</gates>
<devices>
<device name="" package="74990101212">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="LED1_G+" pad="10"/>
<connect gate="G$1" pin="LED1_G-" pad="9"/>
<connect gate="G$1" pin="LED2_Y+" pad="12"/>
<connect gate="G$1" pin="LED2_Y-" pad="11"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="74990101212"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74990101212?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74990101212"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499511611A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-03-27 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499511611A"/>
</gates>
<devices>
<device name="" package="7499511611A">
<connects>
<connect gate="G$1" pin="CD1" pad="12"/>
<connect gate="G$1" pin="CD2" pad="6"/>
<connect gate="G$1" pin="CD3" pad="1"/>
<connect gate="G$1" pin="CD4" pad="7"/>
<connect gate="G$1" pin="D1+" pad="11"/>
<connect gate="G$1" pin="D1-" pad="10"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="3"/>
<connect gate="G$1" pin="D3-" pad="2"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="LED1_Y+" pad="18"/>
<connect gate="G$1" pin="LED1_Y-" pad="17"/>
<connect gate="G$1" pin="LED2_O+/G-" pad="19"/>
<connect gate="G$1" pin="LED2_O-/G+" pad="20"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="V1" pad="13"/>
<connect gate="G$1" pin="V2" pad="14"/>
<connect gate="G$1" pin="V3" pad="15"/>
<connect gate="G$1" pin="V4" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green/orange-yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE+"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499511611A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499511611A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499511611A"/>
<attribute name="IMPROVED_CMRR" value="Yes"/>
<attribute name="OPERATING_TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499031120A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499031120A"/>
</gates>
<devices>
<device name="" package="7499031120A">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B10" pad="B10"/>
<connect gate="G$1" pin="B11" pad="B11"/>
<connect gate="G$1" pin="B12" pad="B12"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="B5" pad="B5"/>
<connect gate="G$1" pin="B6" pad="B6"/>
<connect gate="G$1" pin="B7" pad="B7"/>
<connect gate="G$1" pin="B8" pad="B8"/>
<connect gate="G$1" pin="B9" pad="B9"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C10" pad="C10"/>
<connect gate="G$1" pin="C11" pad="C11"/>
<connect gate="G$1" pin="C12" pad="C12"/>
<connect gate="G$1" pin="C2" pad="C2"/>
<connect gate="G$1" pin="C3" pad="C3"/>
<connect gate="G$1" pin="C4" pad="C4"/>
<connect gate="G$1" pin="C5" pad="C5"/>
<connect gate="G$1" pin="C6" pad="C6"/>
<connect gate="G$1" pin="C7" pad="C7"/>
<connect gate="G$1" pin="C8" pad="C8"/>
<connect gate="G$1" pin="C9" pad="C9"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="SHIELD3" pad="S3"/>
<connect gate="G$1" pin="SHIELD4" pad="S4"/>
<connect gate="G$1" pin="SHIELD5" pad="S5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x4"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499031120A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499031120A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499031120A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7497111611A" prefix="J">
<description>WE-LAN RJ45 LAN Transformer

Characteristics
RJ45 Connector with integrated transformer / common mode choke
Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s
Available in SMT, THT and THT with USB
Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt
Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications
Suitable for industrial temperatures from –40 °C up to +85 °C
Compatible to Industrial Ethernet systems like EtherCAT or Profinet
Compliant with most IC’s for Ethernet applications such as Microchip, Broadcom, Marvell
Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella 2026-09-22
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7497111611A"/>
<gate name="G$2" symbol="USB2.0"/>
<gate name="G$3" symbol="USB2.0"/>
</gates>
<devices>
<device name="" package="7497111611A">
<connects>
<connect gate="G$1" pin="D1+" pad="9"/>
<connect gate="G$1" pin="D1-" pad="10"/>
<connect gate="G$1" pin="D2+" pad="7"/>
<connect gate="G$1" pin="D2-" pad="8"/>
<connect gate="G$1" pin="D3+" pad="4"/>
<connect gate="G$1" pin="D3-" pad="5"/>
<connect gate="G$1" pin="D4+" pad="2"/>
<connect gate="G$1" pin="D4-" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LED1_Y+" pad="12"/>
<connect gate="G$1" pin="LED1_Y-" pad="11"/>
<connect gate="G$1" pin="LED2_G+/O+" pad="15"/>
<connect gate="G$1" pin="LED2_G-" pad="14"/>
<connect gate="G$1" pin="LED2_O-" pad="16"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4 S5 S6 S7 S8"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$2" pin="D+" pad="U3"/>
<connect gate="G$2" pin="D-" pad="U2"/>
<connect gate="G$2" pin="GND" pad="U4"/>
<connect gate="G$2" pin="VCC" pad="U1"/>
<connect gate="G$3" pin="D+" pad="U7"/>
<connect gate="G$3" pin="D-" pad="U6"/>
<connect gate="G$3" pin="GND" pad="U8"/>
<connect gate="G$3" pin="VCC" pad="U5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green/orange-yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7497111611A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7497111611A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7497111611A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499210123A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2024-09-20 

2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499210123A"/>
</gates>
<devices>
<device name="" package="7499210123A">
<connects>
<connect gate="G$1" pin="CRD" pad="3"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="LED1_Y+" pad="11"/>
<connect gate="G$1" pin="LED1_Y-" pad="12"/>
<connect gate="G$1" pin="LED2_G+" pad="13"/>
<connect gate="G$1" pin="LED2_G-" pad="14"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="NC@1" pad="8"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="2"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="5"/>
<connect gate="G$1" pin="TD-" pad="6"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="green-yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE (up to 350 mA)"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Vertical"/>
<attribute name="VALUE" value="7499210123A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499210123A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499210123A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499010001A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2024-03-22 

2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499010001A"/>
</gates>
<devices>
<device name="" package="7499010001A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="-"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499010001A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499010001A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499010001A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498011008" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2025-08-28 

2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498011008"/>
</gates>
<devices>
<device name="" package="7498011008">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="No LED"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7498011008"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7498011008?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7498011008"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74982104400" prefix="J">
<description>WE-RJ45 LAN Through Hole Reflow

Characteristics 

RJ45 designed to use for Pin-in-Paste soldering

High mechanical stability through THT pins

High Temperature LEDs

Extra high standoff for a good thermal airflow

Power over Ethernet up to 30 W

Compliant with standard: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45_THR

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74982104400"/>
</gates>
<devices>
<device name="" package="74982104400">
<connects>
<connect gate="G$1" pin="CD" pad="3"/>
<connect gate="G$1" pin="LED1_G+/Y-" pad="11"/>
<connect gate="G$1" pin="LED1_G-/Y+" pad="12"/>
<connect gate="G$1" pin="LED2_G+/Y-" pad="13"/>
<connect gate="G$1" pin="LED2_G-/Y+" pad="14"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="5"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="G$1" pin="V1+" pad="7"/>
<connect gate="G$1" pin="V1-" pad="8"/>
<connect gate="G$1" pin="V2+" pad="9"/>
<connect gate="G$1" pin="V2-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="green/yellow - green/yellow"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="POE" value="PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Up"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="74982104400"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74982104400?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74982104400"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499010003A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499010003A"/>
</gates>
<devices>
<device name="" package="7499010003A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="LED" value="-"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499010003A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499010003A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499010003A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990111217" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2021-09-17 

2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74990111217"/>
</gates>
<devices>
<device name="" package="74990111217">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="LED1_Y+" pad="9"/>
<connect gate="G$1" pin="LED1_Y-" pad="10"/>
<connect gate="G$1" pin="LED2_G+" pad="11"/>
<connect gate="G$1" pin="LED2_G-" pad="12"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="74990111217"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74990111217?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74990111217"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499110124" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499110124"/>
</gates>
<devices>
<device name="" package="7499110124">
<connects>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="2"/>
<connect gate="G$1" pin="D2+" pad="3"/>
<connect gate="G$1" pin="D2-" pad="4"/>
<connect gate="G$1" pin="D3+" pad="7"/>
<connect gate="G$1" pin="D3-" pad="8"/>
<connect gate="G$1" pin="D4+" pad="9"/>
<connect gate="G$1" pin="D4-" pad="10"/>
<connect gate="G$1" pin="LED1_G+" pad="11"/>
<connect gate="G$1" pin="LED1_G-" pad="12"/>
<connect gate="G$1" pin="LED2_G+/Y-" pad="14"/>
<connect gate="G$1" pin="LED2_G-/Y+" pad="13"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green-yellow/green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499110124"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499110124?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499110124"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499211002A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499211002A"/>
</gates>
<devices>
<device name="" package="7499211002A">
<connects>
<connect gate="G$1" pin="CTD" pad="3"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="5"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="G$1" pin="V1+" pad="7"/>
<connect gate="G$1" pin="V1-" pad="8"/>
<connect gate="G$1" pin="V2+" pad="9"/>
<connect gate="G$1" pin="V2-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="No LED"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499211002A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499211002A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499211002A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7497110616" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7497110616"/>
<gate name="G$2" symbol="USB3.0"/>
<gate name="G$3" symbol="USB3.0"/>
</gates>
<devices>
<device name="" package="7497110616">
<connects>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="6"/>
<connect gate="G$1" pin="D3-" pad="7"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="LED1_Y+" pad="12"/>
<connect gate="G$1" pin="LED1_Y-" pad="11"/>
<connect gate="G$1" pin="LED2_G+/O-" pad="14"/>
<connect gate="G$1" pin="LED2_G-/O+" pad="13"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
<connect gate="G$1" pin="SHIELD3" pad="Z3"/>
<connect gate="G$1" pin="SHIELD4" pad="Z4"/>
<connect gate="G$1" pin="SHIELD5" pad="Z5"/>
<connect gate="G$1" pin="SHIELD6" pad="Z6"/>
<connect gate="G$1" pin="SHIELD7" pad="Z7"/>
<connect gate="G$1" pin="SHIELD8" pad="Z8"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$2" pin="D+" pad="U3"/>
<connect gate="G$2" pin="D-" pad="U2"/>
<connect gate="G$2" pin="GND" pad="U4"/>
<connect gate="G$2" pin="GND_SIG" pad="U7"/>
<connect gate="G$2" pin="RX+" pad="U6"/>
<connect gate="G$2" pin="RX-" pad="U5"/>
<connect gate="G$2" pin="TX+" pad="U9"/>
<connect gate="G$2" pin="TX-" pad="U8"/>
<connect gate="G$2" pin="VCC" pad="U1"/>
<connect gate="G$3" pin="D+" pad="U12"/>
<connect gate="G$3" pin="D-" pad="U11"/>
<connect gate="G$3" pin="GND" pad="U13"/>
<connect gate="G$3" pin="GND_SIG" pad="U16"/>
<connect gate="G$3" pin="RX+" pad="U15"/>
<connect gate="G$3" pin="RX-" pad="U14"/>
<connect gate="G$3" pin="TX+" pad="U18"/>
<connect gate="G$3" pin="TX-" pad="U17"/>
<connect gate="G$3" pin="VCC" pad="U10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="yellow/green-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7497110616"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7497110616?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7497110616"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499211122A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499211122A"/>
</gates>
<devices>
<device name="" package="7499211122A">
<connects>
<connect gate="G$1" pin="CTD" pad="3"/>
<connect gate="G$1" pin="LED1_Y+" pad="11"/>
<connect gate="G$1" pin="LED1_Y-" pad="12"/>
<connect gate="G$1" pin="LED2_G+" pad="13"/>
<connect gate="G$1" pin="LED2_G-" pad="14"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="5"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="G$1" pin="V1+" pad="7"/>
<connect gate="G$1" pin="V1-" pad="8"/>
<connect gate="G$1" pin="V2+" pad="9"/>
<connect gate="G$1" pin="V2-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499211122A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499211122A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499211122A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499110122" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499110122"/>
</gates>
<devices>
<device name="" package="7499110122">
<connects>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="2"/>
<connect gate="G$1" pin="D2+" pad="3"/>
<connect gate="G$1" pin="D2-" pad="4"/>
<connect gate="G$1" pin="D3+" pad="7"/>
<connect gate="G$1" pin="D3-" pad="8"/>
<connect gate="G$1" pin="D4+" pad="9"/>
<connect gate="G$1" pin="D4-" pad="10"/>
<connect gate="G$1" pin="LED1_Y+" pad="11"/>
<connect gate="G$1" pin="LED1_Y-" pad="12"/>
<connect gate="G$1" pin="LED2_G+" pad="13"/>
<connect gate="G$1" pin="LED2_G-" pad="14"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499110122"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499110122?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499110122"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74980111212" prefix="J">
<description>WE-RJ45 LAN Transformer
 
Characteristics
 
RJ45 Connector with integrated transformer / common mode choke
 
Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s
 
Available in SMD, THT and THT with USB
 
Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt
 
Applications
 
Suitable for industrial temperatures from –40 °C up to +85 °C
 
Compatible to Industrial Ethernet systems like EtherCAT or Profinet
 
Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
 
Hubs, Routers, Switches, IP cameras, IoT applications
 
Details see: www.we-online.com/components/products/WE-LAN-RJ45
 
Updated by Ella Wu 2026-07-21
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74980111212"/>
</gates>
<devices>
<device name="" package="74980111212">
<connects>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="LED1_Y+" pad="9"/>
<connect gate="G$1" pin="LED1_Y-" pad="10"/>
<connect gate="G$1" pin="LED2_G+" pad="11"/>
<connect gate="G$1" pin="LED2_G-" pad="12"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Down"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="74980111212"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74980111212?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74980111212"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499010121A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499010121A"/>
</gates>
<devices>
<device name="" package="7499010121A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="LED1_G+" pad="10"/>
<connect gate="G$1" pin="LED1_G-" pad="9"/>
<connect gate="G$1" pin="LED2_Y+" pad="12"/>
<connect gate="G$1" pin="LED2_Y-" pad="11"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499010121A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499010121A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499010121A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499021125" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2020-11-13 

2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499021125"/>
</gates>
<devices>
<device name="" package="7499021125">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B10" pad="B10"/>
<connect gate="G$1" pin="B11" pad="B11"/>
<connect gate="G$1" pin="B12" pad="B12"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="B5" pad="B5"/>
<connect gate="G$1" pin="B6" pad="B6"/>
<connect gate="G$1" pin="B7" pad="B7"/>
<connect gate="G$1" pin="B8" pad="B8"/>
<connect gate="G$1" pin="B9" pad="B9"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
<connect gate="G$1" pin="SHIELD3" pad="Z3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x2"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499021125"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499021125?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499021125"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74981104402" prefix="J">
<description>WE-LAN RJ45 LAN Transformer

Characteristics
RJ45 Connector with integrated transformer / common mode choke
Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s
Available in SMT, THT and THT with USB
Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt
Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications
Suitable for industrial temperatures from –40 °C up to +85 °C
Compatible to Industrial Ethernet systems like EtherCAT or Profinet
Compliant with most IC’s for Ethernet applications such as Microchip, Broadcom, Marvell
Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella 2026-09-22
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74981104402"/>
</gates>
<devices>
<device name="" package="74981104402">
<connects>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="6"/>
<connect gate="G$1" pin="D3-" pad="7"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LED1_Y+/G-" pad="12"/>
<connect gate="G$1" pin="LED1_Y-/G+" pad="11"/>
<connect gate="G$1" pin="LED2_Y+/G-" pad="13"/>
<connect gate="G$1" pin="LED2_Y-/G+" pad="14"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="yellow/green-yellow/green"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Vertical"/>
<attribute name="VALUE" value="74981104402"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74981104402?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74981104402"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499011441A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2024-03-22 

2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499011441A"/>
</gates>
<devices>
<device name="" package="7499011441A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="LED1_G+/Y-" pad="10"/>
<connect gate="G$1" pin="LED1_G-/Y+" pad="9"/>
<connect gate="G$1" pin="LED2_G+/Y-" pad="12"/>
<connect gate="G$1" pin="LED2_G-/Y+" pad="11"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="green/yellow - green/yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499011441A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499011441A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499011441A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498010210A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498010210A"/>
</gates>
<devices>
<device name="" package="7498010210A">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="CRD" pad="6"/>
<connect gate="G$1" pin="CTD" pad="5"/>
<connect gate="G$1" pin="LED1_Y+" pad="1"/>
<connect gate="G$1" pin="LED1_Y-" pad="2"/>
<connect gate="G$1" pin="LED2_G+" pad="12"/>
<connect gate="G$1" pin="LED2_G-" pad="11"/>
<connect gate="G$1" pin="NC" pad="9"/>
<connect gate="G$1" pin="RD+" pad="7"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="3"/>
<connect gate="G$1" pin="TD-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="green-yellow"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7498010210A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7498010210A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7498010210A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498111001A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498111001A"/>
</gates>
<devices>
<device name="" package="7498111001A">
<connects>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="1"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="3"/>
<connect gate="G$1" pin="D3+" pad="6"/>
<connect gate="G$1" pin="D3-" pad="5"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="7"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
<connect gate="G$1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="No LED"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7498111001A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7498111001A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7498111001A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499010126A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2024-09-20 

2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499010126A"/>
</gates>
<devices>
<device name="" package="7499010126A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="LED1_Y+" pad="9"/>
<connect gate="G$1" pin="LED1_Y-" pad="10"/>
<connect gate="G$1" pin="LED2_G+" pad="11"/>
<connect gate="G$1" pin="LED2_G-" pad="12"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="green-yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Vertical"/>
<attribute name="VALUE" value="7499010126A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499010126A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499010126A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499410221" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499410221"/>
</gates>
<devices>
<device name="" package="7499410221">
<connects>
<connect gate="G$1" pin="CD" pad="2"/>
<connect gate="G$1" pin="LED1_G+" pad="12"/>
<connect gate="G$1" pin="LED1_G-" pad="11"/>
<connect gate="G$1" pin="LED2_G+" pad="14"/>
<connect gate="G$1" pin="LED2_G-" pad="13"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="5"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="V1+" pad="8"/>
<connect gate="G$1" pin="V1-" pad="7"/>
<connect gate="G$1" pin="V2+" pad="10"/>
<connect gate="G$1" pin="V2-" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="LED" value="green-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE+"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Vertical"/>
<attribute name="VALUE" value="7499410221"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499410221?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499410221"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498111120AR" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498111120AR"/>
</gates>
<devices>
<device name="" package="7498111120AR">
<connects>
<connect gate="G$1" pin="D1+" pad="3"/>
<connect gate="G$1" pin="D1-" pad="4"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="7"/>
<connect gate="G$1" pin="D3-" pad="8"/>
<connect gate="G$1" pin="D4+" pad="9"/>
<connect gate="G$1" pin="D4-" pad="10"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="LED1_G+" pad="2"/>
<connect gate="G$1" pin="LED1_G-" pad="1"/>
<connect gate="G$1" pin="LED2_Y+" pad="14"/>
<connect gate="G$1" pin="LED2_Y-" pad="13"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7498111120AR"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7498111120AR?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7498111120AR"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499410213" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499410213"/>
</gates>
<devices>
<device name="" package="7499410213">
<connects>
<connect gate="G$1" pin="CTD" pad="3"/>
<connect gate="G$1" pin="LED1_G+" pad="11"/>
<connect gate="G$1" pin="LED1_G-" pad="12"/>
<connect gate="G$1" pin="LED2_Y+" pad="13"/>
<connect gate="G$1" pin="LED2_Y-" pad="14"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="5"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="G$1" pin="V1+" pad="7"/>
<connect gate="G$1" pin="V1-" pad="8"/>
<connect gate="G$1" pin="V2+" pad="9"/>
<connect gate="G$1" pin="V2-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="green-yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE+"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499410213"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499410213?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499410213"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74991204400" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Created by Ella Wu 2021-09-06 

2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74991204400"/>
</gates>
<devices>
<device name="" package="74991204400">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A13" pad="A13"/>
<connect gate="G$1" pin="A14" pad="A14"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B10" pad="B10"/>
<connect gate="G$1" pin="B11" pad="B11"/>
<connect gate="G$1" pin="B12" pad="B12"/>
<connect gate="G$1" pin="B13" pad="B13"/>
<connect gate="G$1" pin="B14" pad="B14"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="B5" pad="B5"/>
<connect gate="G$1" pin="B6" pad="B6"/>
<connect gate="G$1" pin="B7" pad="B7"/>
<connect gate="G$1" pin="B8" pad="B8"/>
<connect gate="G$1" pin="B9" pad="B9"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="yellow/green-yellow/green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x2"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="74991204400"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74991204400?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74991204400"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498210003" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2025-04-25 

2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498210003"/>
</gates>
<devices>
<device name="" package="7498210003">
<connects>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="V1+" pad="9"/>
<connect gate="G$1" pin="V1-" pad="10"/>
<connect gate="G$1" pin="V2+" pad="11"/>
<connect gate="G$1" pin="V2-" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="LED" value="-"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="POE" value="PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7498210003"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7498210003?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7498210003"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499111446" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499111446"/>
</gates>
<devices>
<device name="" package="7499111446">
<connects>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="6"/>
<connect gate="G$1" pin="D3-" pad="7"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="LED1_Y+/G-" pad="12"/>
<connect gate="G$1" pin="LED1_Y-/G+" pad="11"/>
<connect gate="G$1" pin="LED2_Y+/G-" pad="14"/>
<connect gate="G$1" pin="LED2_Y-/G+" pad="13"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green/yellow - green/yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499111446"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499111446?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499111446"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499011121A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499011121A"/>
</gates>
<devices>
<device name="" package="7499011121A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="LED1_Y+" pad="9"/>
<connect gate="G$1" pin="LED1_Y-" pad="10"/>
<connect gate="G$1" pin="LED2_G+" pad="11"/>
<connect gate="G$1" pin="LED2_G-" pad="12"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499011121A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499011121A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499011121A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499111001A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499111001A"/>
</gates>
<devices>
<device name="" package="7499111001A">
<connects>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="2"/>
<connect gate="G$1" pin="D2+" pad="3"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="4"/>
<connect gate="G$1" pin="D3-" pad="5"/>
<connect gate="G$1" pin="D4+" pad="7"/>
<connect gate="G$1" pin="D4-" pad="8"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="No LED"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499111001A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499111001A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499111001A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499010211A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499010211A"/>
</gates>
<devices>
<device name="" package="7499010211A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="LED1_G+" pad="9"/>
<connect gate="G$1" pin="LED1_G-" pad="10"/>
<connect gate="G$1" pin="LED2_Y+" pad="12"/>
<connect gate="G$1" pin="LED2_Y-" pad="11"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="green-yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499010211A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499010211A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499010211A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499021002A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499021002A"/>
</gates>
<devices>
<device name="" package="7499021002A">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="B5" pad="B5"/>
<connect gate="G$1" pin="B6" pad="B6"/>
<connect gate="G$1" pin="B7" pad="B7"/>
<connect gate="G$1" pin="B8" pad="B8"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
<connect gate="G$1" pin="SHIELD3" pad="Z3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="LED" value="-"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x2"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499021002A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499021002A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499021002A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990100011A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74990100011A"/>
</gates>
<devices>
<device name="" package="74990100011A">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="LED" value="No LED"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="74990100011A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74990100011A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74990100011A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499011448" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Created by Ella Wu 2020-10-27 

2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499011448"/>
</gates>
<devices>
<device name="" package="7499011448">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="LED1_Y+/G-" pad="9"/>
<connect gate="G$1" pin="LED1_Y-/G+" pad="10"/>
<connect gate="G$1" pin="LED2_G+/Y-" pad="11"/>
<connect gate="G$1" pin="LED2_G-/Y+" pad="12"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="LED" value="yellow/green-yellow/green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Vertical"/>
<attribute name="VALUE" value="7499011448"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499011448?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499011448"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499010004A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499010004A"/>
</gates>
<devices>
<device name="" package="7499010004A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="No LED"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="7499010004A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499010004A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499010004A"/>
<attribute name="OPERATING_TEMPERATURE" value="0 °C up to +70 °C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74991214400" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45
Created by Ella Wu 2021-09-06 

2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74991214400"/>
</gates>
<devices>
<device name="" package="74991214400">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A13" pad="A13"/>
<connect gate="G$1" pin="A14" pad="A14"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B10" pad="B10"/>
<connect gate="G$1" pin="B11" pad="B11"/>
<connect gate="G$1" pin="B12" pad="B12"/>
<connect gate="G$1" pin="B13" pad="B13"/>
<connect gate="G$1" pin="B14" pad="B14"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="B5" pad="B5"/>
<connect gate="G$1" pin="B6" pad="B6"/>
<connect gate="G$1" pin="B7" pad="B7"/>
<connect gate="G$1" pin="B8" pad="B8"/>
<connect gate="G$1" pin="B9" pad="B9"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="yellow/green-yellow/green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x2"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="74991214400"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74991214400?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74991214400"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499511002A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-03-27 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499511002A"/>
</gates>
<devices>
<device name="" package="7499511002A">
<connects>
<connect gate="G$1" pin="CD1" pad="12"/>
<connect gate="G$1" pin="CD2" pad="6"/>
<connect gate="G$1" pin="CD3" pad="1"/>
<connect gate="G$1" pin="CD4" pad="7"/>
<connect gate="G$1" pin="D1+" pad="11"/>
<connect gate="G$1" pin="D1-" pad="10"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="3"/>
<connect gate="G$1" pin="D3-" pad="2"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="V1" pad="13"/>
<connect gate="G$1" pin="V2" pad="14"/>
<connect gate="G$1" pin="V3" pad="15"/>
<connect gate="G$1" pin="V4" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="No LED"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE+"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499511002A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499511002A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499511002A"/>
<attribute name="IMPROVED_CMRR" value="Yes"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990100040" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74990100040"/>
</gates>
<devices>
<device name="" package="74990100040">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="No LED"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="74990100040"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74990100040?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74990100040"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499211121A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499211121A"/>
</gates>
<devices>
<device name="" package="7499211121A">
<connects>
<connect gate="G$1" pin="CRD" pad="3"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="LED1_Y+" pad="11"/>
<connect gate="G$1" pin="LED1_Y-" pad="12"/>
<connect gate="G$1" pin="LED2_G+" pad="13"/>
<connect gate="G$1" pin="LED2_G-" pad="14"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="NC@1" pad="8"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="2"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="5"/>
<connect gate="G$1" pin="TD-" pad="6"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499211121A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499211121A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499211121A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499411122A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-03-27 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499411122A"/>
</gates>
<devices>
<device name="" package="7499411122A">
<connects>
<connect gate="G$1" pin="CRD" pad="6"/>
<connect gate="G$1" pin="CTD" pad="12"/>
<connect gate="G$1" pin="LED1_G+" pad="18"/>
<connect gate="G$1" pin="LED1_G-" pad="17"/>
<connect gate="G$1" pin="LED2_Y+" pad="20"/>
<connect gate="G$1" pin="LED2_Y-" pad="19"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="5"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="11"/>
<connect gate="G$1" pin="TD-" pad="10"/>
<connect gate="G$1" pin="V1+" pad="13"/>
<connect gate="G$1" pin="V1-" pad="14"/>
<connect gate="G$1" pin="V2+" pad="15"/>
<connect gate="G$1" pin="V2-" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE+"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499411122A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499411122A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499411122A"/>
<attribute name="IMPROVED_CMRR" value="Yes"/>
<attribute name="OPERATING_TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74991114412" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 
RJ45 Connector with integrated transformer / common mode choke
Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s
Available in SMD, THT and THT with USB
Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 
Suitable for industrial temperatures from –40 °C up to +85 °C
Compatible to Industrial Ethernet systems like EtherCAT or Profinet
Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2026-07-21
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74991104412"/>
</gates>
<devices>
<device name="" package="74991114412">
<connects>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="6"/>
<connect gate="G$1" pin="D3-" pad="7"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LED1_Y+/G-" pad="12"/>
<connect gate="G$1" pin="LED1_Y-/G+" pad="11"/>
<connect gate="G$1" pin="LED2_Y+/G-" pad="14"/>
<connect gate="G$1" pin="LED2_Y-/G+" pad="13"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="yellow/green-yellow/green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="74991114412"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74991114412?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74991114412"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499111614A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-03-27 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499111614A"/>
</gates>
<devices>
<device name="" package="7499111614A">
<connects>
<connect gate="G$1" pin="CD1" pad="12"/>
<connect gate="G$1" pin="CD2" pad="6"/>
<connect gate="G$1" pin="CD3" pad="1"/>
<connect gate="G$1" pin="CD4" pad="7"/>
<connect gate="G$1" pin="D1+" pad="11"/>
<connect gate="G$1" pin="D1-" pad="10"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="3"/>
<connect gate="G$1" pin="D3-" pad="2"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="LED1_Y+" pad="14"/>
<connect gate="G$1" pin="LED1_Y-" pad="13"/>
<connect gate="G$1" pin="LED2_O+/G-" pad="15"/>
<connect gate="G$1" pin="LED2_O-/G+" pad="16"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green/orange-yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499111614A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499111614A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499111614A"/>
<attribute name="IMPROVED_CMRR" value="Yes"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990110030" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2024-03-22 

2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74990110030"/>
</gates>
<devices>
<device name="" package="74990110030">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="-"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="74990110030"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74990110030?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74990110030"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499051002" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499051002"/>
</gates>
<devices>
<device name="" package="7499051002">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="B5" pad="B5"/>
<connect gate="G$1" pin="B6" pad="B6"/>
<connect gate="G$1" pin="B7" pad="B7"/>
<connect gate="G$1" pin="B8" pad="B8"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
<connect gate="G$1" pin="SHIELD3" pad="Z3"/>
<connect gate="G$1" pin="SHIELD4" pad="Z4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="LED" value="-"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="2x1"/>
<attribute name="TAB" value="Up/Down"/>
<attribute name="VALUE" value="7499051002"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499051002?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499051002"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498011211" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498011211"/>
</gates>
<devices>
<device name="" package="7498011211">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="LED1_G+" pad="1"/>
<connect gate="G$1" pin="LED1_G-" pad="2"/>
<connect gate="G$1" pin="LED2_Y+" pad="9"/>
<connect gate="G$1" pin="LED2_Y-" pad="10"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="3"/>
<connect gate="G$1" pin="TD-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="green-yellow"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7498011211"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7498011211?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7498011211"/>
<attribute name="IMPROVED_CMRR" value="Yes"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499151120" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella 2025-03-11

2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499151120"/>
</gates>
<devices>
<device name="" package="7499151120">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A13" pad="A13"/>
<connect gate="G$1" pin="A14" pad="A14"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B10" pad="B10"/>
<connect gate="G$1" pin="B11" pad="B11"/>
<connect gate="G$1" pin="B12" pad="B12"/>
<connect gate="G$1" pin="B13" pad="B13"/>
<connect gate="G$1" pin="B14" pad="B14"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="B5" pad="B5"/>
<connect gate="G$1" pin="B6" pad="B6"/>
<connect gate="G$1" pin="B7" pad="B7"/>
<connect gate="G$1" pin="B8" pad="B8"/>
<connect gate="G$1" pin="B9" pad="B9"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="SHIELD3" pad="S3"/>
<connect gate="G$1" pin="SHIELD4" pad="S4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="2x1"/>
<attribute name="TAB" value="Up/Down"/>
<attribute name="VALUE" value="7499151120"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499151120?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499151120"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74980101200" prefix="J">
<description>WE-LAN RJ45 LAN Transformer

Characteristics
RJ45 Connector with integrated transformer / common mode choke
Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s
Available in SMT, THT and THT with USB
Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt
Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications
Suitable for industrial temperatures from –40 °C up to +85 °C
Compatible to Industrial Ethernet systems like EtherCAT or Profinet
Compliant with most IC’s for Ethernet applications such as Microchip, Broadcom, Marvell
Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella 2026-09-22
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74980101200"/>
</gates>
<devices>
<device name="" package="74980101200">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="LED1_Y+" pad="9"/>
<connect gate="G$1" pin="LED1_Y-" pad="10"/>
<connect gate="G$1" pin="LED2_G+" pad="11"/>
<connect gate="G$1" pin="LED2_G-" pad="12"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-TX"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Vertical"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="74980101200"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74980101200?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74980101200"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498111123" prefix="J">
<description>WE-RJ45 LAN Through Hole Reflow

Characteristics 

RJ45 designed to use for Pin-in-Paste soldering

High mechanical stability through THT pins

High Temperature LEDs

Extra high standoff for a good thermal airflow

Power over Ethernet up to 30 W

Compliant with standard: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45_THR

Created by Ella Wu 2022-12-16 

2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498111123"/>
</gates>
<devices>
<device name="" package="7498111123">
<connects>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="2"/>
<connect gate="G$1" pin="D2+" pad="3"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="4"/>
<connect gate="G$1" pin="D3-" pad="5"/>
<connect gate="G$1" pin="D4+" pad="7"/>
<connect gate="G$1" pin="D4-" pad="8"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="LED1_Y+" pad="11"/>
<connect gate="G$1" pin="LED1_Y-" pad="12"/>
<connect gate="G$1" pin="LED2_G+" pad="13"/>
<connect gate="G$1" pin="LED2_G-" pad="14"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Down"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="7498111123"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7498111123?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7498111123"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499311614" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2021-06-08 

2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499311614"/>
</gates>
<devices>
<device name="" package="7499311614">
<connects>
<connect gate="G$1" pin="CD1" pad="12"/>
<connect gate="G$1" pin="CD2" pad="6"/>
<connect gate="G$1" pin="CD3" pad="1"/>
<connect gate="G$1" pin="CD4" pad="7"/>
<connect gate="G$1" pin="D1+" pad="10"/>
<connect gate="G$1" pin="D1-" pad="11"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="4"/>
<connect gate="G$1" pin="D3+" pad="2"/>
<connect gate="G$1" pin="D3-" pad="3"/>
<connect gate="G$1" pin="D4+" pad="9"/>
<connect gate="G$1" pin="D4-" pad="8"/>
<connect gate="G$1" pin="LED1_G+" pad="18"/>
<connect gate="G$1" pin="LED1_G-" pad="17"/>
<connect gate="G$1" pin="LED2_G+/O-" pad="20"/>
<connect gate="G$1" pin="LED2_G-/O+" pad="19"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="V1" pad="13"/>
<connect gate="G$1" pin="V2" pad="14"/>
<connect gate="G$1" pin="V3" pad="15"/>
<connect gate="G$1" pin="V4" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green/orange-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499311614"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499311614?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499311614"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990101210" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74990101210"/>
</gates>
<devices>
<device name="" package="74990101210">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="LED1_Y+" pad="9"/>
<connect gate="G$1" pin="LED1_Y-" pad="10"/>
<connect gate="G$1" pin="LED2_G+" pad="11"/>
<connect gate="G$1" pin="LED2_G-" pad="12"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-T"/>
<attribute name="LED" value="green-yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Vertical"/>
<attribute name="VALUE" value="74990101210"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74990101210?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74990101210"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74980104400" prefix="J">
<description>WE-RJ45 LAN Through Hole Reflow

Characteristics 

RJ45 designed to use for Pin-in-Paste soldering

High mechanical stability through THT pins

High Temperature LEDs

Extra high standoff for a good thermal airflow

Power over Ethernet up to 30 W

Compliant with standard: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45_THR

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74980104400"/>
</gates>
<devices>
<device name="" package="74980104400">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="LED1_G+/Y-" pad="9"/>
<connect gate="G$1" pin="LED1_G-/Y+" pad="10"/>
<connect gate="G$1" pin="LED2_G+_Y-" pad="11"/>
<connect gate="G$1" pin="LED2_G-_Y+" pad="12"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="green/yellow - green/yellow"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="74980104400"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74980104400?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74980104400"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74980111211" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke
Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s
Available in SMD, THT and THT with USB
Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C
Compatible to Industrial Ethernet systems like EtherCAT or Profinet
Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology
Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2026-07-01
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74980111211"/>
</gates>
<devices>
<device name="" package="74980111211">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="LED1_G+" pad="1"/>
<connect gate="G$1" pin="LED1_G-" pad="2"/>
<connect gate="G$1" pin="LED2_Y+" pad="12"/>
<connect gate="G$1" pin="LED2_Y-" pad="11"/>
<connect gate="G$1" pin="NC" pad="9"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="3"/>
<connect gate="G$1" pin="TD-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="74980111211"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74980111211?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74980111211"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74980100000" prefix="J">
<description>WE-LAN RJ45 LAN Transformer

Characteristics
RJ45 Connector with integrated transformer / common mode choke
Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s
Available in SMT, THT and THT with USB
Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt
Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications
Suitable for industrial temperatures from –40 °C up to +85 °C
Compatible to Industrial Ethernet systems like EtherCAT or Profinet
Compliant with most IC’s for Ethernet applications such as Microchip, Broadcom, Marvell
Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella 2026-09-22
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74980100000"/>
</gates>
<devices>
<device name="" package="74980100000">
<connects>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-TX"/>
<attribute name="LED" value="-"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Vertical"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="74980100000"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74980100000?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74980100000"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990112116A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2024-03-22 

2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74990112116A"/>
</gates>
<devices>
<device name="" package="74990112116A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="LED1_Y+" pad="10"/>
<connect gate="G$1" pin="LED1_Y-" pad="9"/>
<connect gate="G$1" pin="LED2_G+" pad="12"/>
<connect gate="G$1" pin="LED2_G-" pad="11"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="green-yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="74990112116A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74990112116A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74990112116A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499010441" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499010441"/>
</gates>
<devices>
<device name="" package="7499010441">
<connects>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="LED1_G+/Y-" pad="10"/>
<connect gate="G$1" pin="LED1_G-/Y+" pad="9"/>
<connect gate="G$1" pin="LED2_G+/Y-" pad="11"/>
<connect gate="G$1" pin="LED2_G-/Y+" pad="12"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="green/yellow - green/yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499010441"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499010441?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499010441"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499110120A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2024-09-20 

2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499110120A"/>
</gates>
<devices>
<device name="" package="7499110120A">
<connects>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="6"/>
<connect gate="G$1" pin="D3-" pad="7"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="LED1_Y+" pad="11"/>
<connect gate="G$1" pin="LED1_Y-" pad="12"/>
<connect gate="G$1" pin="LED2_G+" pad="13"/>
<connect gate="G$1" pin="LED2_G-" pad="14"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green-yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Vertical"/>
<attribute name="VALUE" value="7499110120A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499110120A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499110120A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499121211" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499121211"/>
</gates>
<devices>
<device name="" package="7499121211">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A13" pad="A13"/>
<connect gate="G$1" pin="A14" pad="A14"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B10" pad="B10"/>
<connect gate="G$1" pin="B11" pad="B11"/>
<connect gate="G$1" pin="B12" pad="B12"/>
<connect gate="G$1" pin="B13" pad="B13"/>
<connect gate="G$1" pin="B14" pad="B14"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="B5" pad="B5"/>
<connect gate="G$1" pin="B6" pad="B6"/>
<connect gate="G$1" pin="B7" pad="B7"/>
<connect gate="G$1" pin="B8" pad="B8"/>
<connect gate="G$1" pin="B9" pad="B9"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green-yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x2"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499121211"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499121211?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499121211"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74991104402" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Created by Ella Wu 2020-10-27 

2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74991104402"/>
</gates>
<devices>
<device name="" package="74991104402">
<connects>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="2"/>
<connect gate="G$1" pin="D2+" pad="3"/>
<connect gate="G$1" pin="D2-" pad="4"/>
<connect gate="G$1" pin="D3+" pad="7"/>
<connect gate="G$1" pin="D3-" pad="8"/>
<connect gate="G$1" pin="D4+" pad="9"/>
<connect gate="G$1" pin="D4-" pad="10"/>
<connect gate="G$1" pin="LED1_Y+/G-" pad="12"/>
<connect gate="G$1" pin="LED1_Y-/G+" pad="11"/>
<connect gate="G$1" pin="LED2_Y+/G-" pad="14"/>
<connect gate="G$1" pin="LED2_Y-/G+" pad="13"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="yellow/green-yellow/green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Vertical"/>
<attribute name="VALUE" value="74991104402"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74991104402?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74991104402"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498111124" prefix="J">
<description>WE-RJ45 LAN Through Hole Reflow

Characteristics 

RJ45 designed to use for Pin-in-Paste soldering

High mechanical stability through THT pins

High Temperature LEDs

Extra high standoff for a good thermal airflow

Power over Ethernet up to 30 W

Compliant with standard: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45_THR

Created by Ella Wu 2022-12-16 

2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498111124"/>
</gates>
<devices>
<device name="" package="7498111124">
<connects>
<connect gate="G$1" pin="CGND" pad="10"/>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="6"/>
<connect gate="G$1" pin="D3-" pad="7"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="LED1_Y+" pad="11"/>
<connect gate="G$1" pin="LED1_Y-" pad="12"/>
<connect gate="G$1" pin="LED2_G+" pad="13"/>
<connect gate="G$1" pin="LED2_G-" pad="14"/>
<connect gate="G$1" pin="SGND" pad="1"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Down"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="7498111124"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7498111124?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7498111124"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499111121A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499111121A"/>
</gates>
<devices>
<device name="" package="7499111121A">
<connects>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="2"/>
<connect gate="G$1" pin="D2+" pad="3"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="4"/>
<connect gate="G$1" pin="D3-" pad="5"/>
<connect gate="G$1" pin="D4+" pad="7"/>
<connect gate="G$1" pin="D4-" pad="8"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="LED1_Y+" pad="11"/>
<connect gate="G$1" pin="LED1_Y-" pad="12"/>
<connect gate="G$1" pin="LED2_G+" pad="13"/>
<connect gate="G$1" pin="LED2_G-" pad="14"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499111121A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499111121A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499111121A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498210002" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2025-08-28 

2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498210002"/>
</gates>
<devices>
<device name="" package="7498210002">
<connects>
<connect gate="G$1" pin="CRD" pad="4"/>
<connect gate="G$1" pin="CTD" pad="3"/>
<connect gate="G$1" pin="RD+" pad="5"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="No LED"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="POE" value="PoE+ (up to 600 mA)"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7498210002"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7498210002?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7498210002"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990111211" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74990111211"/>
</gates>
<devices>
<device name="" package="74990111211">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="LED1_Y+" pad="9"/>
<connect gate="G$1" pin="LED1_Y-" pad="10"/>
<connect gate="G$1" pin="LED2_G+" pad="11"/>
<connect gate="G$1" pin="LED2_G-" pad="12"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="74990111211"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74990111211?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74990111211"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499111000A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2023-03-27 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499111000A"/>
</gates>
<devices>
<device name="" package="7499111000A">
<connects>
<connect gate="G$1" pin="CD1" pad="12"/>
<connect gate="G$1" pin="CD2" pad="6"/>
<connect gate="G$1" pin="CD3" pad="1"/>
<connect gate="G$1" pin="CD4" pad="7"/>
<connect gate="G$1" pin="D1+" pad="11"/>
<connect gate="G$1" pin="D1-" pad="10"/>
<connect gate="G$1" pin="D2+" pad="4"/>
<connect gate="G$1" pin="D2-" pad="5"/>
<connect gate="G$1" pin="D3+" pad="3"/>
<connect gate="G$1" pin="D3-" pad="2"/>
<connect gate="G$1" pin="D4+" pad="8"/>
<connect gate="G$1" pin="D4-" pad="9"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value=" 0 "/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499111000A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499111000A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499111000A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499111447" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2019-08-05 

2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499111447"/>
</gates>
<devices>
<device name="" package="7499111447">
<connects>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="2"/>
<connect gate="G$1" pin="D2+" pad="3"/>
<connect gate="G$1" pin="D2-" pad="4"/>
<connect gate="G$1" pin="D3+" pad="7"/>
<connect gate="G$1" pin="D3-" pad="8"/>
<connect gate="G$1" pin="D4+" pad="9"/>
<connect gate="G$1" pin="D4-" pad="10"/>
<connect gate="G$1" pin="LED1_Y+/G-" pad="12"/>
<connect gate="G$1" pin="LED1_Y-/G+" pad="11"/>
<connect gate="G$1" pin="LED2_Y+/G-" pad="14"/>
<connect gate="G$1" pin="LED2_Y-/G+" pad="13"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green/yellow - green/yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499111447"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499111447?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499111447"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499210124A" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMD, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at, IEEE 802.3an and upcoming IEE 802.3bt

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella Wu 2024-03-22 

2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499210124A"/>
</gates>
<devices>
<device name="" package="7499210124A">
<connects>
<connect gate="G$1" pin="CRD" pad="3"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="LED1_G+" pad="12"/>
<connect gate="G$1" pin="LED1_G-" pad="11"/>
<connect gate="G$1" pin="LED2_Y+" pad="14"/>
<connect gate="G$1" pin="LED2_Y-" pad="13"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="NC@1" pad="8"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="2"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="5"/>
<connect gate="G$1" pin="TD-" pad="6"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Up"/>
<attribute name="VALUE" value="7499210124A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499210124A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499210124A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74980100001" prefix="J">
<description>WE-RJ45 LAN Through Hole Reflow

Characteristics 

RJ45 designed to use for Pin-in-Paste soldering

High mechanical stability through THT pins

High Temperature LEDs

Extra high standoff for a good thermal airflow

Power over Ethernet up to 30 W

Compliant with standard: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45_THR

Created by Ella Wu 2022-12-16 

2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74980100001"/>
</gates>
<devices>
<device name="" package="74980100001">
<connects>
<connect gate="G$1" pin="CRD" pad="6"/>
<connect gate="G$1" pin="CTD" pad="3"/>
<connect gate="G$1" pin="GND" pad="4 5"/>
<connect gate="G$1" pin="RD+" pad="7"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="SHIELD1" pad="Z1"/>
<connect gate="G$1" pin="SHIELD2" pad="Z2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-TX"/>
<attribute name="LED" value="-"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Down"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="74980100001"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74980100001?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74980100001"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74984104401" prefix="J">
<description>WE-LAN RJ45 LAN Transformer

Characteristics
RJ45 Connector with integrated transformer / common mode choke
Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s
Available in SMT, THT and THT with USB
Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt
Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications
Suitable for industrial temperatures from –40 °C up to +85 °C
Compatible to Industrial Ethernet systems like EtherCAT or Profinet
Compliant with most IC’s for Ethernet applications such as Microchip, Broadcom, Marvell
Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella 2026-09-22
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74984104401"/>
</gates>
<devices>
<device name="" package="74984104401">
<connects>
<connect gate="G$1" pin="CD" pad="2"/>
<connect gate="G$1" pin="LED1_Y+/G-" pad="12"/>
<connect gate="G$1" pin="LED1_Y-/G+" pad="11"/>
<connect gate="G$1" pin="LED2_Y+/G-" pad="14"/>
<connect gate="G$1" pin="LED2_Y-/G+" pad="13"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="5"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V1-" pad="8"/>
<connect gate="G$1" pin="V2+" pad="9"/>
<connect gate="G$1" pin="V2-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100BASE-TX"/>
<attribute name="LED" value="yellow/green-yellow/green"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="POE" value="PoE+"/>
<attribute name="PORTS" value="1"/>
<attribute name="TAB" value="Vertical"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="74984104401"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74984104401?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74984104401"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74984104400" prefix="J">
<description>WE-RJ45 LAN Through Hole Reflow

Characteristics 

RJ45 designed to use for Pin-in-Paste soldering

High mechanical stability through THT pins

High Temperature LEDs

Extra high standoff for a good thermal airflow

Power over Ethernet up to 30 W

Compliant with standard: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45_THR

Updated by Ella Wu 2023-08-16 

2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74984104400"/>
</gates>
<devices>
<device name="" package="74984104400">
<connects>
<connect gate="G$1" pin="CD" pad="3"/>
<connect gate="G$1" pin="LED1_G+/Y-" pad="11"/>
<connect gate="G$1" pin="LED1_G-/Y+" pad="12"/>
<connect gate="G$1" pin="LED2_G+/Y-" pad="13"/>
<connect gate="G$1" pin="LED2_G-/Y+" pad="14"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="5"/>
<connect gate="G$1" pin="SHIELD1" pad="S1" route="any"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="G$1" pin="V1+" pad="7"/>
<connect gate="G$1" pin="V1-" pad="8"/>
<connect gate="G$1" pin="V2+" pad="9"/>
<connect gate="G$1" pin="V2-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="green/yellow - green/yellow"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="POE" value="PoE+"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Up"/>
<attribute name="USB" value="No"/>
<attribute name="VALUE" value="74984104400"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74984104400?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="74984104400"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499410443" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMT, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt

Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Created by Ella Wu 2026-05-20 

2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499410443"/>
</gates>
<devices>
<device name="" package="7499410443">
<connects>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="LED1_G+/Y-" pad="15"/>
<connect gate="G$1" pin="LED1_G-/Y+" pad="16"/>
<connect gate="G$1" pin="LED2_Y+/G-" pad="17"/>
<connect gate="G$1" pin="LED2_Y-/G+" pad="18"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="V1" pad="11"/>
<connect gate="G$1" pin="V2" pad="12"/>
<connect gate="G$1" pin="V3" pad="13"/>
<connect gate="G$1" pin="V4" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="green/yellow - green/yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE+"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499410443"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499410443?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499410443"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499510443" prefix="J">
<description>WE-LAN RJ45 LAN Transformer

Characteristics
RJ45 Connector with integrated transformer / common mode choke
Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s
Available in SMT, THT and THT with USB
Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt
Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications
Suitable for industrial temperatures from –40 °C up to +85 °C
Compatible to Industrial Ethernet systems like EtherCAT or Profinet
Compliant with most IC’s for Ethernet applications such as Microchip, Broadcom, Marvell
Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Updated by Ella 2026-09-22
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499510443"/>
</gates>
<devices>
<device name="" package="7499510443">
<connects>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="2"/>
<connect gate="G$1" pin="D2+" pad="3"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="7"/>
<connect gate="G$1" pin="D3-" pad="8"/>
<connect gate="G$1" pin="D4+" pad="9"/>
<connect gate="G$1" pin="D4-" pad="10"/>
<connect gate="G$1" pin="LED1_G+/Y-" pad="15"/>
<connect gate="G$1" pin="LED1_G-/Y+" pad="16"/>
<connect gate="G$1" pin="LED2_G+/Y-" pad="17"/>
<connect gate="G$1" pin="LED2_G-/Y+" pad="18"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="V1" pad="11"/>
<connect gate="G$1" pin="V2" pad="12"/>
<connect gate="G$1" pin="V3" pad="13"/>
<connect gate="G$1" pin="V4" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green/yellow - green/yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE+"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499510443"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499510443?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499510443"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499511443" prefix="J">
<description>WE-LAN RJ45 LAN Transformer

Characteristics
RJ45 Connector with integrated transformer / common mode choke
Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s
Available in SMT, THT and THT with USB
Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt
Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications
Suitable for industrial temperatures from –40 °C up to +85 °C
Compatible to Industrial Ethernet systems like EtherCAT or Profinet
Compliant with most IC’s for Ethernet applications such as Microchip, Broadcom, Marvell
Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Created by Ella 2026-09-22
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499511443"/>
</gates>
<devices>
<device name="" package="7499511443">
<connects>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="2"/>
<connect gate="G$1" pin="D2+" pad="3"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="7"/>
<connect gate="G$1" pin="D3-" pad="8"/>
<connect gate="G$1" pin="D4+" pad="9"/>
<connect gate="G$1" pin="D4-" pad="10"/>
<connect gate="G$1" pin="LED1_G+/Y-" pad="15"/>
<connect gate="G$1" pin="LED1_G-/Y+" pad="16"/>
<connect gate="G$1" pin="LED2_G+/Y-" pad="17"/>
<connect gate="G$1" pin="LED2_G-/Y+" pad="18"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="V1" pad="11"/>
<connect gate="G$1" pin="V2" pad="12"/>
<connect gate="G$1" pin="V3" pad="13"/>
<connect gate="G$1" pin="V4" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green/yellow - green/yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE+"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499511443"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499511443?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499511443"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499411443" prefix="J">
<description>WE-RJ45 LAN Transformer

Characteristics 

RJ45 Connector with integrated transformer / common mode choke

Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s

Available in SMT, THT and THT with USB

Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt

Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications 

Suitable for industrial temperatures from –40 °C up to +85 °C

Compatible to Industrial Ethernet systems like EtherCAT or Profinet

Compliant with most IC’s for Ethernet applications such as Microchip, Texas Instruments, Broadcom, Linear Technology

Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Created by Ella Wu 2026-05-20 

2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499411443"/>
</gates>
<devices>
<device name="" package="7499411443">
<connects>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="LED1_G+/Y-" pad="15"/>
<connect gate="G$1" pin="LED1_G-/Y+" pad="16"/>
<connect gate="G$1" pin="LED2_Y+/G-" pad="17"/>
<connect gate="G$1" pin="LED2_Y-/G+" pad="18"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="V1" pad="11"/>
<connect gate="G$1" pin="V2" pad="12"/>
<connect gate="G$1" pin="V3" pad="13"/>
<connect gate="G$1" pin="V4" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="green/yellow - green/yellow"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="PoE+"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499411443"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499411443?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499411443"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498510213" prefix="J">
<description>WE-LAN RJ45 LAN Transformer

Characteristics
RJ45 Connector with integrated transformer / common mode choke
Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s
Available in SMT, THT and THT with USB
Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt
Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications
Suitable for industrial temperatures from –40 °C up to +85 °C
Compatible to Industrial Ethernet systems like EtherCAT or Profinet
Compliant with most IC’s for Ethernet applications such as Microchip, Broadcom, Marvell
Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Created by Ella 2026-09-22
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498510213"/>
</gates>
<devices>
<device name="" package="7498510213">
<connects>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="LED1_G+" pad="15"/>
<connect gate="G$1" pin="LED1_G-" pad="16"/>
<connect gate="G$1" pin="LED2_Y+" pad="17"/>
<connect gate="G$1" pin="LED2_Y-" pad="18"/>
<connect gate="G$1" pin="RD1+" pad="3"/>
<connect gate="G$1" pin="RD1-" pad="6"/>
<connect gate="G$1" pin="RD2+" pad="9"/>
<connect gate="G$1" pin="RD2-" pad="10"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD1+" pad="1"/>
<connect gate="G$1" pin="TD1-" pad="2"/>
<connect gate="G$1" pin="TD2+" pad="7"/>
<connect gate="G$1" pin="TD2-" pad="8"/>
<connect gate="G$1" pin="V1" pad="11"/>
<connect gate="G$1" pin="V2" pad="12"/>
<connect gate="G$1" pin="V3" pad="13"/>
<connect gate="G$1" pin="V4" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="1000BASE-T"/>
<attribute name="LED" value="green-yellow"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="POE" value="PoE+"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7498510213"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7498510213?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7498510213"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PHY_CHIP_MODE" value="current"/>
<attribute name="SHIELD_TABS" value="No"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499011002A" prefix="J">
<description>WE-LAN RJ45 LAN Transformer

Characteristics
RJ45 Connector with integrated transformer / common mode choke
Power over Ethernet up to 50 Watt and speeds up to 10 Gbit/s
Available in SMT, THT and THT with USB
Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt
Improved Common Mode Rejection (CMRR) due to additional NiZn cores

Applications
Suitable for industrial temperatures from –40 °C up to +85 °C
Compatible to Industrial Ethernet systems like EtherCAT or Profinet
Compliant with most IC’s for Ethernet applications such as Microchip, Broadcom, Marvell
Hubs, Routers, Switches, IP cameras, IoT applications

Details see: www.we-online.com/components/products/WE-LAN-RJ45

Created by Ella 2026-09-22
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499011002A"/>
</gates>
<devices>
<device name="" package="7499011002A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD1" pad="S1"/>
<connect gate="G$1" pin="SHIELD2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="100BASE-TX"/>
<attribute name="LED" value="No LED"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="POE" value="non-PoE"/>
<attribute name="PORTS" value="1x1"/>
<attribute name="TAB" value="Down"/>
<attribute name="VALUE" value="7499011002A"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7499011002A?ae"/>
<attribute name="CATEGORY" value="Filtered Connectors"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7499011002A"/>
<attribute name="IMPROVED_CMRR" value="No"/>
<attribute name="OPERATING_TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="PHY_CHIP_MODE" value="current &amp; voltage"/>
<attribute name="SHIELD_TABS" value="Yes"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
