<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - EMC Components - ESD Protection - WE-TVS&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2026a, 2026-02-12&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-TVS_DFN2020-2L">
<description>&lt;b&gt;WE-TVS TVS Diode
&lt;br&gt;&lt;/b&gt;Size:  DFN2020-2L
&lt;BR&gt;L X W X H = 2mm X2mm X 0.5mm</description>
</package>
<package name="WE-TVS_DFN3810-9L">
<description>&lt;b&gt;WE-TVS TVS Diode
&lt;br&gt;&lt;/b&gt;Size:  DFN3810-9L
&lt;BR&gt;L X W X H = 3.8mm X 1mm X 0.5mm</description>
</package>
<package name="WE-TVS_SOT23-6L">
<description>&lt;b&gt;WE-TVS TVS Diode
&lt;br&gt;&lt;/b&gt;Size:  SOT23-6L
&lt;BR&gt;L X W X H = 2.8mm X 2.9mm X 1.45mm</description>
</package>
<package name="WE-TVS_SC70-6L">
<description>&lt;b&gt;WE-TVS TVS Diode
&lt;br&gt;&lt;/b&gt;Size:  SC70-6L
&lt;BR&gt;L X W X H = 2mm X2.1mm X 1mm</description>
</package>
<package name="WE-TVS_DFN1610-2L">
<description>&lt;b&gt;WE-TVS TVS Diode
&lt;br&gt;&lt;/b&gt;Size:  DFN1610-2L
&lt;BR&gt;L X W X H = 1.6mm X1mm X 0.5mm</description>
</package>
<package name="WE-TVS_DFN1210-6L">
<description>&lt;b&gt;WE-TVS TVS Diode
&lt;br&gt;&lt;/b&gt;Size:  DFN1210-6L
&lt;BR&gt;L X W X H = 1.2mm X 1.0mm X 0.45mm</description>
</package>
<package name="WE-TVS_MSOP-10L">
<description>&lt;b&gt;WE-TVS TVS Diode
&lt;br&gt;&lt;/b&gt;Size:  MSOP-10L
&lt;BR&gt;L X W X H = 4.9mm X 3mm X 0.975mm</description>
</package>
<package name="WE-TVS_SOT23-3L">
<description>&lt;b&gt;WE-TVS TVS Diode
&lt;br&gt;&lt;/b&gt;Size:  SOT23-3L
&lt;BR&gt;L X W X H = 2.9mm X 2.4mm X 1.04mm</description>
</package>
<package name="WE-TVS_MSOP-8L">
<description>&lt;b&gt;WE-TVS TVS Diode
&lt;br&gt;&lt;/b&gt;Size:  MSOP-8L
&lt;BR&gt;L X W X H = 4.9mm X 3mm X 0.975mm</description>
</package>
<package name="WE-TVS_SOT143-4L">
<description>&lt;b&gt;WE-TVS TVS Diode
&lt;br&gt;&lt;/b&gt;Size:  SOT143-4L
&lt;BR&gt;L X W X H = 2.92mm X2.4mm X 1.06mm</description>
</package>
<package name="WE-TVS_SOT23-5L">
<description>&lt;b&gt;WE-TVS TVS Diode
&lt;br&gt;&lt;/b&gt;Size:  SOT23-5L
&lt;BR&gt;L X W X H = 2.9mm X2.8mm X 1.16mm</description>
</package>
<package name="WE-TVS_SC70-5L">
<description>&lt;b&gt;WE-TVS TVS Diode
&lt;br&gt;&lt;/b&gt;Size:  SC70-5L
&lt;BR&gt;L X W X H = 2mm X2.2mm X 1mm</description>
</package>
<package name="WE-TVS_SOT563">
<description>&lt;b&gt;WE-TVS TVS Diode
&lt;br&gt;&lt;/b&gt;Size:  SOT563
&lt;BR&gt;L X W X H = 1.6mm X1.6mm X 0.55mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-TVS_DFN2020-2L_UNI">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WE-TVS_DFN3810-9L">
<pin name="9" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="WE-TVS_6RTR4">
<pin name="6" direction="pas"/>
<pin name="VDD" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="WE-TVS_6RTR4D">
<pin name="4" direction="pas"/>
<pin name="VDD" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="WE-TVS_6ESD5">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WE-TVS_DFN-2L_BI">
<pin name="I/O" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="WE-TVS_MSOP-10L">
<pin name="GND" direction="pas"/>
<pin name="VDD" direction="pas"/>
<pin name="I/O1" direction="pas"/>
<pin name="I/O2" direction="pas"/>
<pin name="I/O3" direction="pas"/>
<pin name="I/O4" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-TVS_DFN1210-6L">
<pin name="I/O1" direction="pas"/>
<pin name="I/O2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="NC1" direction="pas"/>
<pin name="NC2" direction="pas"/>
</symbol>
<symbol name="WE-TVS_SOT23-3L_BI">
<pin name="I/O2" direction="pas"/>
<pin name="I/O1" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="WE-TVS_MSOP-8L">
<pin name="GND" direction="pas"/>
<pin name="I/O1" direction="pas"/>
<pin name="I/O2" direction="pas"/>
<pin name="I/O6" direction="pas"/>
<pin name="I/O3" direction="pas"/>
<pin name="I/O4" direction="pas"/>
<pin name="I/O5" direction="pas"/>
<pin name="VDD" direction="pas"/>
</symbol>
<symbol name="WE-TVS_SOT143-4L">
<pin name="VDD" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="WE-TVS_6ESD4">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="GND@1" direction="pas"/>
</symbol>
<symbol name="WE-TVS_DFN-2L_UNI">
<pin name="I/O" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="WE-TVS_SOT23-5L">
<pin name="I/O2" direction="pas"/>
<pin name="I/O1" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VDD" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="WE-TVS_SC70-5L">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WE-TVS_SOT23-3L_UNI">
<pin name="I/O2" direction="pas"/>
<pin name="I/O1" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="WE-TVS_6RTR4FD">
<pin name="VDD" direction="pas"/>
<pin name="I/O1" direction="pas"/>
<pin name="I/O2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="I/O3" direction="pas"/>
<pin name="I/O4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-TVS-SS_DFN3810-9L_824014885" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Super Speed Series
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;Very low capacitance
&lt;br&gt;Rail to Rail protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94-V0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Super Speed data lines
&lt;br&gt;HDMI 1.3/1.4/2.0, DVI
&lt;br&gt;DisplayPort
&lt;br&gt;USB 3.1 Gen 1 (5Gb/s)
&lt;br&gt;SATA and eSATA
&lt;br&gt;GBit LAN
&lt;br&gt;Thunderbolt
&lt;br&gt;LVDS
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;&lt;b&gt;SS = Super Speed
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106434v209%20Family_WE-TVS-SuperSpeed.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106434v209%20Family_WE-TVS-SuperSpeed.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS-SUPER-SPEED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS-SUPER-SPEED&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_DFN3810-9L"/>
</gates>
<devices>
<device name="" package="WE-TVS_DFN3810-9L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="0.5pF"/>
<attribute name="CHANNELS" value="8"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824014885?ae"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IPEAK" value="5A"/>
<attribute name="LENGTH" value="3.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824014885"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="DFN3810-9L"/>
<attribute name="VALUE" value="824014885"/>
<attribute name="VBR-MIN" value="6V"/>
<attribute name="VCH-CLAMP-ESD" value="10.5V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="15kV"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS-HS_SOT23-6L_824015" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – High Speed Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low clamping voltage
&lt;br&gt;Sturdy design
&lt;br&gt;Very low capacitance
&lt;br&gt;Flow Thru Design for a simple layout
&lt;br&gt;Rail to Rail protection
&lt;br&gt;Epoxy flame resistant UL94-V0
&lt;br&gt;RoHS, REACH and free of halogens

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Very fast data lines
&lt;br&gt;USB 2.0
&lt;br&gt;Ethernet
&lt;br&gt;PoE
&lt;br&gt;VGA
&lt;br&gt;Sim Cards
&lt;br&gt;Keypads
&lt;br&gt;&lt;br&gt;&lt;B&gt;HS = High Speed
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;&lt;/b&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CAIR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS-HS&lt;/a&gt;&lt;p&gt;

Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6RTR4"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-6L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="1pF"/>
<attribute name="CHANNELS" value="4+1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824015?ae"/>
<attribute name="HEIGHT" value="1.16mm"/>
<attribute name="IPEAK" value="12A"/>
<attribute name="LENGTH" value="2.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824015"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="SOT23-6L"/>
<attribute name="VALUE" value="824015"/>
<attribute name="VBR-MIN" value="6.1V"/>
<attribute name="VCH-CLAMP-ESD" value="13V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="12kV"/>
<attribute name="WIDTH" value="2.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS-SS_DFN3810-9L_824014883" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Super Speed Series
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;Very low capacitance
&lt;br&gt;Rail to Rail protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94-V0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Super Speed data lines
&lt;br&gt;HDMI 1.3/1.4/2.0, DVI
&lt;br&gt;DisplayPort
&lt;br&gt;USB 3.1 Gen 1 (5Gb/s)
&lt;br&gt;SATA and eSATA
&lt;br&gt;GBit LAN
&lt;br&gt;Thunderbolt
&lt;br&gt;LVDS
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;&lt;b&gt;SS = Super Speed
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106434v209%20Family_WE-TVS-SuperSpeed.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106434v209%20Family_WE-TVS-SuperSpeed.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS-SUPER-SPEED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS-SUPER-SPEED&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_DFN3810-9L"/>
</gates>
<devices>
<device name="" package="WE-TVS_DFN3810-9L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="0.5pF"/>
<attribute name="CHANNELS" value="8"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824014883?ae"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IPEAK" value="5A"/>
<attribute name="LENGTH" value="3.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824014883"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="DFN3810-9L"/>
<attribute name="VALUE" value="824014883"/>
<attribute name="VBR-MIN" value="4.5V"/>
<attribute name="VCH-CLAMP-ESD" value="9V"/>
<attribute name="VCH-MAX" value="3.3V"/>
<attribute name="VESD-CONTACT" value="12kV"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_SC70-6L_82402375" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Standard Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;High ESD withstand voltage
&lt;br&gt;Uni- or bidirectional protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC power supply
&lt;br&gt;USB Power Delivery (PD)
&lt;br&gt;Headsets and accessories
&lt;br&gt;PDAs
&lt;br&gt;Digital cameras
&lt;br&gt;MP3-Player
&lt;br&gt;Touch Panels
&lt;br&gt;Notebooks
&lt;br&gt;ESD, EFT and Surge Protection
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6ESD5"/>
</gates>
<devices>
<device name="" package="WE-TVS_SC70-6L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="13pF"/>
<attribute name="CHANNELS" value=" 5 "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/82402375?ae"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IPEAK" value="6A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="82402375"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="SC70-6L"/>
<attribute name="VALUE" value="82402375"/>
<attribute name="VBR-MIN" value="6V"/>
<attribute name="VCH-CLAMP-ESD" value="8V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="10kV"/>
<attribute name="WIDTH" value="2.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS-SS_SOT23-6L_824014" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Super Speed Series
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;Very low capacitance
&lt;br&gt;Rail to Rail protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94-V0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Super Speed data lines
&lt;br&gt;HDMI 1.3/1.4/2.0, DVI
&lt;br&gt;DisplayPort
&lt;br&gt;USB 3.1 Gen 1 (5Gb/s)
&lt;br&gt;SATA and eSATA
&lt;br&gt;GBit LAN
&lt;br&gt;Thunderbolt
&lt;br&gt;LVDS
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;&lt;b&gt;SS = Super Speed
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106434v209%20Family_WE-TVS-SuperSpeed.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106434v209%20Family_WE-TVS-SuperSpeed.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS-SUPER-SPEED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS-SUPER-SPEED&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6RTR4D"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-6L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="0.55pF"/>
<attribute name="CHANNELS" value="4+1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824014?ae"/>
<attribute name="HEIGHT" value="1.16mm"/>
<attribute name="IPEAK" value="4A"/>
<attribute name="LENGTH" value="2.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824014"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="SOT23-6L"/>
<attribute name="VALUE" value="824014"/>
<attribute name="VBR-MIN" value="6V"/>
<attribute name="VCH-CLAMP-ESD" value="12V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="10kV"/>
<attribute name="WIDTH" value="2.9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS-HS_SOT23-6L_824001" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – High Speed Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low clamping voltage
&lt;br&gt;Sturdy design
&lt;br&gt;Very low capacitance
&lt;br&gt;Flow Thru Design for a simple layout
&lt;br&gt;Rail to Rail protection
&lt;br&gt;Epoxy flame resistant UL94-V0
&lt;br&gt;RoHS, REACH and free of halogens

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Very fast data lines
&lt;br&gt;USB 2.0
&lt;br&gt;Ethernet
&lt;br&gt;PoE
&lt;br&gt;VGA
&lt;br&gt;Sim Cards
&lt;br&gt;Keypads
&lt;br&gt;&lt;br&gt;&lt;B&gt;HS = High Speed
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;&lt;/b&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CAIR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS-HS&lt;/a&gt;&lt;p&gt;

Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6RTR4"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-6L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="1pF"/>
<attribute name="CHANNELS" value="4+1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824001?ae"/>
<attribute name="HEIGHT" value="1.16mm"/>
<attribute name="IPEAK" value="5A"/>
<attribute name="LENGTH" value="2.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824001"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="SOT23-6L"/>
<attribute name="VALUE" value="824001"/>
<attribute name="VBR-MIN" value="6.2V"/>
<attribute name="VCH-CLAMP-ESD" value="14V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="8kV"/>
<attribute name="WIDTH" value="2.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS-HS_SOT23-6L_82400102" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – High Speed Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low clamping voltage
&lt;br&gt;Sturdy design
&lt;br&gt;Very low capacitance
&lt;br&gt;Flow Thru Design for a simple layout
&lt;br&gt;Rail to Rail protection
&lt;br&gt;Epoxy flame resistant UL94-V0
&lt;br&gt;RoHS, REACH and free of halogens

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Very fast data lines
&lt;br&gt;USB 2.0
&lt;br&gt;Ethernet
&lt;br&gt;PoE
&lt;br&gt;VGA
&lt;br&gt;Sim Cards
&lt;br&gt;Keypads
&lt;br&gt;&lt;br&gt;&lt;B&gt;HS = High Speed
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;&lt;/b&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CAIR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS-HS&lt;/a&gt;&lt;p&gt;

Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6RTR4FD"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-6L">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I/O1" pad="1"/>
<connect gate="G$1" pin="I/O2" pad="3"/>
<connect gate="G$1" pin="I/O3" pad="6"/>
<connect gate="G$1" pin="I/O4" pad="4"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="2pF"/>
<attribute name="CHANNELS" value="2+1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/82400102?ae"/>
<attribute name="HEIGHT" value="1.16mm"/>
<attribute name="IPEAK" value="7A"/>
<attribute name="LENGTH" value="2.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="82400102"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="SOT23-6L"/>
<attribute name="VALUE" value="82400102"/>
<attribute name="VBR-MIN" value="6V"/>
<attribute name="VCH-CLAMP-ESD" value="10V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="8kV"/>
<attribute name="WIDTH" value="2.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_SOT23-6L_82402305" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Standard Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;High ESD withstand voltage
&lt;br&gt;Uni- or bidirectional protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC power supply
&lt;br&gt;USB Power Delivery (PD)
&lt;br&gt;Headsets and accessories
&lt;br&gt;PDAs
&lt;br&gt;Digital cameras
&lt;br&gt;MP3-Player
&lt;br&gt;Touch Panels
&lt;br&gt;Notebooks
&lt;br&gt;ESD, EFT and Surge Protection
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6ESD5"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-6L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="13pF"/>
<attribute name="CHANNELS" value=" 5 "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/82402305?ae"/>
<attribute name="HEIGHT" value="1.16mm"/>
<attribute name="IPEAK" value="6A"/>
<attribute name="LENGTH" value="2.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="82402305"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="SOT23-6L"/>
<attribute name="VALUE" value="82402305"/>
<attribute name="VBR-MIN" value="6V"/>
<attribute name="VCH-CLAMP-ESD" value="8V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="10kV"/>
<attribute name="WIDTH" value="2.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_DFN1610-2L_824045810" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Standard Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;High ESD withstand voltage
&lt;br&gt;Uni- or bidirectional protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC power supply
&lt;br&gt;USB Power Delivery (PD)
&lt;br&gt;Headsets and accessories
&lt;br&gt;PDAs
&lt;br&gt;Digital cameras
&lt;br&gt;MP3-Player
&lt;br&gt;Touch Panels
&lt;br&gt;Notebooks
&lt;br&gt;ESD, EFT and Surge Protection
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_DFN-2L_UNI"/>
</gates>
<devices>
<device name="" package="WE-TVS_DFN1610-2L">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I/O" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="240pF"/>
<attribute name="CHANNELS" value=" 1 "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824045810?ae"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IPEAK" value="24A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824045810"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="DFN1610-2L"/>
<attribute name="VALUE" value="824045810"/>
<attribute name="VBR-MIN" value="22.8V"/>
<attribute name="VCH-CLAMP-ESD" value="25.5V"/>
<attribute name="VCH-MAX" value="20V"/>
<attribute name="VESD-CONTACT" value="30kV"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS-SS_MSOP-10L_82401444" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Super Speed Series
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;Very low capacitance
&lt;br&gt;Rail to Rail protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94-V0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Super Speed data lines
&lt;br&gt;HDMI 1.3/1.4/2.0, DVI
&lt;br&gt;DisplayPort
&lt;br&gt;USB 3.1 Gen 1 (5Gb/s)
&lt;br&gt;SATA and eSATA
&lt;br&gt;GBit LAN
&lt;br&gt;Thunderbolt
&lt;br&gt;LVDS
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;&lt;b&gt;SS = Super Speed
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106434v209%20Family_WE-TVS-SuperSpeed.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106434v209%20Family_WE-TVS-SuperSpeed.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS-SUPER-SPEED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS-SUPER-SPEED&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_MSOP-10L"/>
</gates>
<devices>
<device name="" package="WE-TVS_MSOP-10L">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="I/O1" pad="1"/>
<connect gate="G$1" pin="I/O2" pad="2"/>
<connect gate="G$1" pin="I/O3" pad="4"/>
<connect gate="G$1" pin="I/O4" pad="5"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="0.55pF"/>
<attribute name="CHANNELS" value="4+1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/82401444?ae"/>
<attribute name="HEIGHT" value="0.975mm"/>
<attribute name="IPEAK" value="5A"/>
<attribute name="LENGTH" value="4.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="82401444"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="MSOP-10L"/>
<attribute name="VALUE" value="82401444"/>
<attribute name="VBR-MIN" value="6V"/>
<attribute name="VCH-CLAMP-ESD" value="12V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="10kV"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS-SS_DFN1210-6L_824012823" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Super Speed Series
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;Very low capacitance
&lt;br&gt;Rail to Rail protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94-V0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Super Speed data lines
&lt;br&gt;HDMI 1.3/1.4/2.0, DVI
&lt;br&gt;DisplayPort
&lt;br&gt;USB 3.1 Gen 1 (5Gb/s)
&lt;br&gt;SATA and eSATA
&lt;br&gt;GBit LAN
&lt;br&gt;Thunderbolt
&lt;br&gt;LVDS
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;&lt;b&gt;SS = Super Speed
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106434v209%20Family_WE-TVS-SuperSpeed.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106434v209%20Family_WE-TVS-SuperSpeed.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS-SUPER-SPEED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS-SUPER-SPEED&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_DFN1210-6L"/>
</gates>
<devices>
<device name="" package="WE-TVS_DFN1210-6L">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I/O1" pad="1"/>
<connect gate="G$1" pin="I/O2" pad="2"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="NC1" pad="5"/>
<connect gate="G$1" pin="NC2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="0.18pF"/>
<attribute name="CHANNELS" value="2"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824012823?ae"/>
<attribute name="HEIGHT" value="0.45mm"/>
<attribute name="IPEAK" value="3A"/>
<attribute name="LENGTH" value="1.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824012823"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="DFN1210-6L"/>
<attribute name="VALUE" value="824012823"/>
<attribute name="VBR-MIN" value="4.5V"/>
<attribute name="VCH-CLAMP-ESD" value="13V"/>
<attribute name="VCH-MAX" value="3.3V"/>
<attribute name="VESD-CONTACT" value="8kV"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS-HS_SOT23-6L_824015043" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – High Speed Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low clamping voltage
&lt;br&gt;Sturdy design
&lt;br&gt;Very low capacitance
&lt;br&gt;Flow Thru Design for a simple layout
&lt;br&gt;Rail to Rail protection
&lt;br&gt;Epoxy flame resistant UL94-V0
&lt;br&gt;RoHS, REACH and free of halogens

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Very fast data lines
&lt;br&gt;USB 2.0
&lt;br&gt;Ethernet
&lt;br&gt;PoE
&lt;br&gt;VGA
&lt;br&gt;Sim Cards
&lt;br&gt;Keypads
&lt;br&gt;&lt;br&gt;&lt;B&gt;HS = High Speed
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;&lt;/b&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CAIR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS-HS&lt;/a&gt;&lt;p&gt;

Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6RTR4"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-6L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="2pF"/>
<attribute name="CHANNELS" value="4+1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824015043?ae"/>
<attribute name="HEIGHT" value="1.16mm"/>
<attribute name="IPEAK" value="30A"/>
<attribute name="LENGTH" value="2.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824015043"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="SOT23-6L"/>
<attribute name="VALUE" value="824015043"/>
<attribute name="VBR-MIN" value="4.5V"/>
<attribute name="VCH-CLAMP-ESD" value="7.5V"/>
<attribute name="VCH-MAX" value="3.3V"/>
<attribute name="VESD-CONTACT" value="30kV"/>
<attribute name="WIDTH" value="2.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS-HS_SC70-6L_82400274" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – High Speed Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low clamping voltage
&lt;br&gt;Sturdy design
&lt;br&gt;Very low capacitance
&lt;br&gt;Flow Thru Design for a simple layout
&lt;br&gt;Rail to Rail protection
&lt;br&gt;Epoxy flame resistant UL94-V0
&lt;br&gt;RoHS, REACH and free of halogens

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Very fast data lines
&lt;br&gt;USB 2.0
&lt;br&gt;Ethernet
&lt;br&gt;PoE
&lt;br&gt;VGA
&lt;br&gt;Sim Cards
&lt;br&gt;Keypads
&lt;br&gt;&lt;br&gt;&lt;B&gt;HS = High Speed
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;&lt;/b&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CAIR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS-HS&lt;/a&gt;&lt;p&gt;

Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6RTR4"/>
</gates>
<devices>
<device name="" package="WE-TVS_SC70-6L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="1.2pF"/>
<attribute name="CHANNELS" value="4+1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/82400274?ae"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IPEAK" value="6A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="82400274"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="SC70-6L"/>
<attribute name="VALUE" value="82400274"/>
<attribute name="VBR-MIN" value="6V"/>
<attribute name="VCH-CLAMP-ESD" value="12.5V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="12kV"/>
<attribute name="WIDTH" value="2.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_DFN1610-2L_824045812" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Standard Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;High ESD withstand voltage
&lt;br&gt;Uni- or bidirectional protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC power supply
&lt;br&gt;USB Power Delivery (PD)
&lt;br&gt;Headsets and accessories
&lt;br&gt;PDAs
&lt;br&gt;Digital cameras
&lt;br&gt;MP3-Player
&lt;br&gt;Touch Panels
&lt;br&gt;Notebooks
&lt;br&gt;ESD, EFT and Surge Protection
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_DFN-2L_UNI"/>
</gates>
<devices>
<device name="" package="WE-TVS_DFN1610-2L">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I/O" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="440pF"/>
<attribute name="CHANNELS" value=" 1 "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824045812?ae"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IPEAK" value="38A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824045812"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="DFN1610-2L"/>
<attribute name="VALUE" value="824045812"/>
<attribute name="VBR-MIN" value="13.3V"/>
<attribute name="VCH-CLAMP-ESD" value="15V"/>
<attribute name="VCH-MAX" value="12V"/>
<attribute name="VESD-CONTACT" value="30kV"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_SOT23-6L_82402304" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Standard Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;High ESD withstand voltage
&lt;br&gt;Uni- or bidirectional protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC power supply
&lt;br&gt;USB Power Delivery (PD)
&lt;br&gt;Headsets and accessories
&lt;br&gt;PDAs
&lt;br&gt;Digital cameras
&lt;br&gt;MP3-Player
&lt;br&gt;Touch Panels
&lt;br&gt;Notebooks
&lt;br&gt;ESD, EFT and Surge Protection
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6ESD4"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-6L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="13pF"/>
<attribute name="CHANNELS" value=" 4 "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/82402304?ae"/>
<attribute name="HEIGHT" value="1.16mm"/>
<attribute name="IPEAK" value="6A"/>
<attribute name="LENGTH" value="2.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="82402304"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="SOT23-6L"/>
<attribute name="VALUE" value="82402304"/>
<attribute name="VBR-MIN" value="6V"/>
<attribute name="VCH-CLAMP-ESD" value="8.5V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="10kV"/>
<attribute name="WIDTH" value="2.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_SOT23-3L_824022" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Standard Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;High ESD withstand voltage
&lt;br&gt;Uni- or bidirectional protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC power supply
&lt;br&gt;USB Power Delivery (PD)
&lt;br&gt;Headsets and accessories
&lt;br&gt;PDAs
&lt;br&gt;Digital cameras
&lt;br&gt;MP3-Player
&lt;br&gt;Touch Panels
&lt;br&gt;Notebooks
&lt;br&gt;ESD, EFT and Surge Protection
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Ella Wu  2021-12-16&lt;br&gt;
&lt;/b&gt;2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_SOT23-3L_BI"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-3L">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I/O1" pad="1"/>
<connect gate="G$1" pin="I/O2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="12pF"/>
<attribute name="CHANNELS" value=" 2 "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824022?ae"/>
<attribute name="HEIGHT" value="1.04mm"/>
<attribute name="IPEAK" value="8A"/>
<attribute name="LENGTH" value="2.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824022"/>
<attribute name="POLARITY" value="Bidirectional"/>
<attribute name="SIZE" value="SOT23-3L"/>
<attribute name="VALUE" value="824022"/>
<attribute name="VBR-MIN" value="6.1V"/>
<attribute name="VCH-CLAMP-ESD" value="9V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="12kV"/>
<attribute name="WIDTH" value="2.4mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_SOT23-3L_824021" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Standard Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;High ESD withstand voltage
&lt;br&gt;Uni- or bidirectional protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC power supply
&lt;br&gt;USB Power Delivery (PD)
&lt;br&gt;Headsets and accessories
&lt;br&gt;PDAs
&lt;br&gt;Digital cameras
&lt;br&gt;MP3-Player
&lt;br&gt;Touch Panels
&lt;br&gt;Notebooks
&lt;br&gt;ESD, EFT and Surge Protection
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_SOT23-3L_UNI"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-3L">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I/O1" pad="1"/>
<connect gate="G$1" pin="I/O2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="55pF"/>
<attribute name="CHANNELS" value=" 2 "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824021?ae"/>
<attribute name="HEIGHT" value="1.04mm"/>
<attribute name="IPEAK" value="15A"/>
<attribute name="LENGTH" value="2.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824021"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="SOT23-3L"/>
<attribute name="VALUE" value="824021"/>
<attribute name="VBR-MIN" value="6.1V"/>
<attribute name="VCH-CLAMP-ESD" value="10V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="18kV"/>
<attribute name="WIDTH" value="2.4mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_DFN1610-2L_824045817" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Standard Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;High ESD withstand voltage
&lt;br&gt;Uni- or bidirectional protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC power supply
&lt;br&gt;USB Power Delivery (PD)
&lt;br&gt;Headsets and accessories
&lt;br&gt;PDAs
&lt;br&gt;Digital cameras
&lt;br&gt;MP3-Player
&lt;br&gt;Touch Panels
&lt;br&gt;Notebooks
&lt;br&gt;ESD, EFT and Surge Protection
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_DFN-2L_UNI"/>
</gates>
<devices>
<device name="" package="WE-TVS_DFN1610-2L">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I/O" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="830pF"/>
<attribute name="CHANNELS" value=" 1 "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824045817?ae"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IPEAK" value="60A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824045817"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="DFN1610-2L"/>
<attribute name="VALUE" value="824045817"/>
<attribute name="VBR-MIN" value="7.8V"/>
<attribute name="VCH-CLAMP-ESD" value="10V"/>
<attribute name="VCH-MAX" value="7V"/>
<attribute name="VESD-CONTACT" value="30kV"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS-SS_MSOP-8L_82401646" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Super Speed Series
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;Very low capacitance
&lt;br&gt;Rail to Rail protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94-V0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Super Speed data lines
&lt;br&gt;HDMI 1.3/1.4/2.0, DVI
&lt;br&gt;DisplayPort
&lt;br&gt;USB 3.1 Gen 1 (5Gb/s)
&lt;br&gt;SATA and eSATA
&lt;br&gt;GBit LAN
&lt;br&gt;Thunderbolt
&lt;br&gt;LVDS
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;&lt;b&gt;SS = Super Speed
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106434v209%20Family_WE-TVS-SuperSpeed.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106434v209%20Family_WE-TVS-SuperSpeed.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS-SUPER-SPEED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS-SUPER-SPEED&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Ella Wu  2021-12-16&lt;br&gt;
&lt;/b&gt;2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_MSOP-8L"/>
</gates>
<devices>
<device name="" package="WE-TVS_MSOP-8L">
<connects>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="I/O1" pad="1"/>
<connect gate="G$1" pin="I/O2" pad="2"/>
<connect gate="G$1" pin="I/O3" pad="3"/>
<connect gate="G$1" pin="I/O4" pad="4"/>
<connect gate="G$1" pin="I/O5" pad="5"/>
<connect gate="G$1" pin="I/O6" pad="6"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CHANNELS" value="6+1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/82401646?ae"/>
<attribute name="HEIGHT" value="0.975mm"/>
<attribute name="IPEAK" value="-"/>
<attribute name="LENGTH" value="4.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="82401646"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="MSOP-8L"/>
<attribute name="VALUE" value="82401646"/>
<attribute name="VBR-MIN" value="6V"/>
<attribute name="VCH-CLAMP-ESD" value="13V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="8kV"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_DFN1610-2L_824032815" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Standard Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;High ESD withstand voltage
&lt;br&gt;Uni- or bidirectional protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC power supply
&lt;br&gt;USB Power Delivery (PD)
&lt;br&gt;Headsets and accessories
&lt;br&gt;PDAs
&lt;br&gt;Digital cameras
&lt;br&gt;MP3-Player
&lt;br&gt;Touch Panels
&lt;br&gt;Notebooks
&lt;br&gt;ESD, EFT and Surge Protection
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_DFN-2L_BI"/>
</gates>
<devices>
<device name="" package="WE-TVS_DFN1610-2L">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I/O" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="140pF"/>
<attribute name="CHANNELS" value=" 1 "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824032815?ae"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IPEAK" value="100A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824032815"/>
<attribute name="POLARITY" value="Bidirectional"/>
<attribute name="SIZE" value="DFN1610-2L"/>
<attribute name="VALUE" value="824032815"/>
<attribute name="VBR-MIN" value="6V"/>
<attribute name="VCH-CLAMP-ESD" value="6V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="30kV"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_DFN1610-2L_824031815" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Standard Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;High ESD withstand voltage
&lt;br&gt;Uni- or bidirectional protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC power supply
&lt;br&gt;USB Power Delivery (PD)
&lt;br&gt;Headsets and accessories
&lt;br&gt;PDAs
&lt;br&gt;Digital cameras
&lt;br&gt;MP3-Player
&lt;br&gt;Touch Panels
&lt;br&gt;Notebooks
&lt;br&gt;ESD, EFT and Surge Protection
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_DFN-2L_UNI"/>
</gates>
<devices>
<device name="" package="WE-TVS_DFN1610-2L">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I/O" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="250pF"/>
<attribute name="CHANNELS" value=" 1 "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824031815?ae"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IPEAK" value="80A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824031815"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="DFN1610-2L"/>
<attribute name="VALUE" value="824031815"/>
<attribute name="VBR-MIN" value="6V"/>
<attribute name="VCH-CLAMP-ESD" value="6V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="30kV"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS-HS_SOT143-4L_8240136" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – High Speed Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low clamping voltage
&lt;br&gt;Sturdy design
&lt;br&gt;Very low capacitance
&lt;br&gt;Flow Thru Design for a simple layout
&lt;br&gt;Rail to Rail protection
&lt;br&gt;Epoxy flame resistant UL94-V0
&lt;br&gt;RoHS, REACH and free of halogens

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Very fast data lines
&lt;br&gt;USB 2.0
&lt;br&gt;Ethernet
&lt;br&gt;PoE
&lt;br&gt;VGA
&lt;br&gt;Sim Cards
&lt;br&gt;Keypads
&lt;br&gt;&lt;br&gt;&lt;B&gt;HS = High Speed
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;&lt;/b&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CAIR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS-HS&lt;/a&gt;&lt;p&gt;

Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_SOT143-4L"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT143-4L">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="3pF"/>
<attribute name="CHANNELS" value="2+1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8240136?ae"/>
<attribute name="HEIGHT" value="1.06mm"/>
<attribute name="IPEAK" value="12A"/>
<attribute name="LENGTH" value="2.92mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="8240136"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="SOT143-4L"/>
<attribute name="VALUE" value="8240136"/>
<attribute name="VBR-MIN" value="4.5V"/>
<attribute name="VCH-CLAMP-ESD" value="9V"/>
<attribute name="VCH-MAX" value="3.3V"/>
<attribute name="VESD-CONTACT" value="24kV"/>
<attribute name="WIDTH" value="2.4mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS-HS_SOT143-4L_8240116" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – High Speed Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low clamping voltage
&lt;br&gt;Sturdy design
&lt;br&gt;Very low capacitance
&lt;br&gt;Flow Thru Design for a simple layout
&lt;br&gt;Rail to Rail protection
&lt;br&gt;Epoxy flame resistant UL94-V0
&lt;br&gt;RoHS, REACH and free of halogens

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Very fast data lines
&lt;br&gt;USB 2.0
&lt;br&gt;Ethernet
&lt;br&gt;PoE
&lt;br&gt;VGA
&lt;br&gt;Sim Cards
&lt;br&gt;Keypads
&lt;br&gt;&lt;br&gt;&lt;B&gt;HS = High Speed
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;&lt;/b&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CAIR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS-HS&lt;/a&gt;&lt;p&gt;

Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_SOT143-4L"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT143-4L">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="2pF"/>
<attribute name="CHANNELS" value="2+1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8240116?ae"/>
<attribute name="HEIGHT" value="1.06mm"/>
<attribute name="IPEAK" value="12A"/>
<attribute name="LENGTH" value="2.92mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="8240116"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="SOT143-4L"/>
<attribute name="VALUE" value="8240116"/>
<attribute name="VBR-MIN" value="6.1V"/>
<attribute name="VCH-CLAMP-ESD" value="13V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="12kV"/>
<attribute name="WIDTH" value="2.4mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS-HS_SOT143-4L_8240026" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – High Speed Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low clamping voltage
&lt;br&gt;Sturdy design
&lt;br&gt;Very low capacitance
&lt;br&gt;Flow Thru Design for a simple layout
&lt;br&gt;Rail to Rail protection
&lt;br&gt;Epoxy flame resistant UL94-V0
&lt;br&gt;RoHS, REACH and free of halogens

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Very fast data lines
&lt;br&gt;USB 2.0
&lt;br&gt;Ethernet
&lt;br&gt;PoE
&lt;br&gt;VGA
&lt;br&gt;Sim Cards
&lt;br&gt;Keypads
&lt;br&gt;&lt;br&gt;&lt;B&gt;HS = High Speed
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;&lt;/b&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CAIR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS-HS&lt;/a&gt;&lt;p&gt;

Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_SOT143-4L"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT143-4L">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="1.2pF"/>
<attribute name="CHANNELS" value="2+1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8240026?ae"/>
<attribute name="HEIGHT" value="1.06mm"/>
<attribute name="IPEAK" value="6A"/>
<attribute name="LENGTH" value="2.92mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="8240026"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="SOT143-4L"/>
<attribute name="VALUE" value="8240026"/>
<attribute name="VBR-MIN" value="6V"/>
<attribute name="VCH-CLAMP-ESD" value="12.5V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="12kV"/>
<attribute name="WIDTH" value="2.4mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS-HS_SOT23-5L_824011" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – High Speed Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low clamping voltage
&lt;br&gt;Sturdy design
&lt;br&gt;Very low capacitance
&lt;br&gt;Flow Thru Design for a simple layout
&lt;br&gt;Rail to Rail protection
&lt;br&gt;Epoxy flame resistant UL94-V0
&lt;br&gt;RoHS, REACH and free of halogens

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Very fast data lines
&lt;br&gt;USB 2.0
&lt;br&gt;Ethernet
&lt;br&gt;PoE
&lt;br&gt;VGA
&lt;br&gt;Sim Cards
&lt;br&gt;Keypads
&lt;br&gt;&lt;br&gt;&lt;B&gt;HS = High Speed
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;&lt;/b&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CAIR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS-HS&lt;/a&gt;&lt;p&gt;

Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_SOT23-5L"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-5L">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I/O1" pad="3"/>
<connect gate="G$1" pin="I/O2" pad="4"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="2pF"/>
<attribute name="CHANNELS" value="2+1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824011?ae"/>
<attribute name="HEIGHT" value="1.16mm"/>
<attribute name="IPEAK" value="13A"/>
<attribute name="LENGTH" value="2.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824011"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="SOT23-5L"/>
<attribute name="VALUE" value="824011"/>
<attribute name="VBR-MIN" value="6.1V"/>
<attribute name="VCH-CLAMP-ESD" value="13V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="16kV"/>
<attribute name="WIDTH" value="2.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_SOT23-3L_824094024" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Standard Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;High ESD withstand voltage
&lt;br&gt;Uni- or bidirectional protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC power supply
&lt;br&gt;USB Power Delivery (PD)
&lt;br&gt;Headsets and accessories
&lt;br&gt;PDAs
&lt;br&gt;Digital cameras
&lt;br&gt;MP3-Player
&lt;br&gt;Touch Panels
&lt;br&gt;Notebooks
&lt;br&gt;ESD, EFT and Surge Protection
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created  by  Ella Wu  2021-12-15&lt;br&gt;
&lt;/b&gt;2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_SOT23-3L_BI"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-3L">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I/O1" pad="1"/>
<connect gate="G$1" pin="I/O2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="38pF"/>
<attribute name="CHANNELS" value=" 2 "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824094024?ae"/>
<attribute name="HEIGHT" value="1.04mm"/>
<attribute name="ICH-LEAK-MAX" value="100V"/>
<attribute name="IPEAK" value="6A"/>
<attribute name="LENGTH" value="2.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824094024"/>
<attribute name="POLARITY" value="Bidirectional"/>
<attribute name="SIZE" value="SOT23-3L"/>
<attribute name="VALUE" value="824094024"/>
<attribute name="VBR-MIN" value="26.2V"/>
<attribute name="VCH-CLAMP-ESD" value="31V"/>
<attribute name="VCH-MAX" value="24V"/>
<attribute name="VESD-CONTACT" value="30kV"/>
<attribute name="WIDTH" value="2.4mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_SC70-5L_82402374" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Standard Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;High ESD withstand voltage
&lt;br&gt;Uni- or bidirectional protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC power supply
&lt;br&gt;USB Power Delivery (PD)
&lt;br&gt;Headsets and accessories
&lt;br&gt;PDAs
&lt;br&gt;Digital cameras
&lt;br&gt;MP3-Player
&lt;br&gt;Touch Panels
&lt;br&gt;Notebooks
&lt;br&gt;ESD, EFT and Surge Protection
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_SC70-5L"/>
</gates>
<devices>
<device name="" package="WE-TVS_SC70-5L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="13pF"/>
<attribute name="CHANNELS" value=" 4 "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/82402374?ae"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IPEAK" value="6A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="82402374"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="SC70-5L"/>
<attribute name="VALUE" value="82402374"/>
<attribute name="VBR-MIN" value="6V"/>
<attribute name="VCH-CLAMP-ESD" value="8.5V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="10kV"/>
<attribute name="WIDTH" value="2.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_DFN1610-2L_824032813" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – Standard Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast turn-on
&lt;br&gt;Low clamping voltage
&lt;br&gt;High ESD withstand voltage
&lt;br&gt;Uni- or bidirectional protection
&lt;br&gt;Small package
&lt;br&gt;Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC power supply
&lt;br&gt;USB Power Delivery (PD)
&lt;br&gt;Headsets and accessories
&lt;br&gt;PDAs
&lt;br&gt;Digital cameras
&lt;br&gt;MP3-Player
&lt;br&gt;Touch Panels
&lt;br&gt;Notebooks
&lt;br&gt;ESD, EFT and Surge Protection
&lt;br&gt;ESD protection in accordance with EN 61000-4-2 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106433v209%20Family_WE-TVS_Standard.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TVS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_DFN-2L_BI"/>
</gates>
<devices>
<device name="" package="WE-TVS_DFN1610-2L">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I/O" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="280pF"/>
<attribute name="CHANNELS" value=" 1 "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/824032813?ae"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IPEAK" value="180A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="824032813"/>
<attribute name="POLARITY" value="Bidirectional"/>
<attribute name="SIZE" value="DFN1610-2L"/>
<attribute name="VALUE" value="824032813"/>
<attribute name="VBR-MIN" value="4V"/>
<attribute name="VCH-CLAMP-ESD" value="4.7V"/>
<attribute name="VCH-MAX" value="3.3V"/>
<attribute name="VESD-CONTACT" value="30kV"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS-HS_SOT563_82400152" prefix="D">
<description>&lt;b&gt;WE-TVS TVS Diode – High Speed Series
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low clamping voltage
&lt;br&gt;Sturdy design
&lt;br&gt;Very low capacitance
&lt;br&gt;Flow Thru Design for a simple layout
&lt;br&gt;Rail to Rail protection
&lt;br&gt;Epoxy flame resistant UL94-V0
&lt;br&gt;RoHS, REACH and free of halogens

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Very fast data lines
&lt;br&gt;USB 2.0
&lt;br&gt;Ethernet
&lt;br&gt;PoE
&lt;br&gt;VGA
&lt;br&gt;Sim Cards
&lt;br&gt;Keypads
&lt;br&gt;&lt;br&gt;&lt;B&gt;HS = High Speed
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14883v209%20Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;&lt;/b&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-CAIR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-TVS-HS&lt;/a&gt;&lt;p&gt;

Updated  by  Ella Wu  2019-07-12&lt;br&gt;
&lt;/b&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6RTR4FD"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT563">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I/O1" pad="1"/>
<connect gate="G$1" pin="I/O2" pad="3"/>
<connect gate="G$1" pin="I/O3" pad="6"/>
<connect gate="G$1" pin="I/O4" pad="4"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CCH-TYP" value="2pF"/>
<attribute name="CHANNELS" value="2+1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/82400152?ae"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="IPEAK" value="6A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="82400152"/>
<attribute name="POLARITY" value="Unidirectional"/>
<attribute name="SIZE" value="SOT563"/>
<attribute name="VALUE" value="82400152"/>
<attribute name="VBR-MIN" value="6V"/>
<attribute name="VCH-CLAMP-ESD" value="10V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VESD-CONTACT" value="8kV"/>
<attribute name="WE-NUMBE" value=""/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
