<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - Common Mode Chokes for Low Voltage and Data Lines - WE-UCF&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-05-12&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-UCF_4TURNS">
<description>&lt;b&gt;WE-UCF SMT Common Mode Line Filter
&lt;br&gt;16.6mm X 12.5mm X 9.3mm, SMT</description>
</package>
<package name="WE-UCF_2TURNS">
<description>&lt;b&gt;WE-UCF SMT Common Mode Line Filter
&lt;br&gt;16.6mm X 12.5mm X 9.3mm, SMT</description>
</package>
</packages>
<symbols>
<symbol name="CM2W-H">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-UCF_4TURNS" prefix="L">
<description>&lt;B&gt;WE-UCF SMT Common Mode Line Filter
&lt;Br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High inductance range
&lt;br&gt;High current range
&lt;br&gt;Small package
&lt;br&gt;Low profile
&lt;br&gt;Surface mount technology
&lt;br&gt;Wide range of filtering spectrum
&lt;br&gt;Climatic category 40/125/21
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;Br&gt;&lt;/b&gt; Filtering
&lt;br&gt;DC power lines
&lt;br&gt;Buck-/ Boost Converter filtering
&lt;br&gt;Data lines with low bitrate
&lt;br&gt;Heavily influenced lines
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14886v209%20Family_WE-UCF.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14886v209%20Family_WE-UCF.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-UCF"&gt;https://www.we-online.com/catalog/en/WE-UCF&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Ella Wu 2021-05-12&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-UCF_4TURNS">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="2" pad="9 10"/>
<connect gate="G$1" pin="3" pad="4 5"/>
<connect gate="G$1" pin="4" pad="6 7"/>
</connects>
<technologies>
<technology name="_744290121">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744290121.pdf"/>
<attribute name="IR" value="5.5A"/>
<attribute name="LS" value="680nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744290121 "/>
<attribute name="RDC" value="0.0105Ohm"/>
<attribute name="VALUE" value="0.12mH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="WINDING-STYLE" value="sectional"/>
</technology>
<technology name="_744290130">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744290130.pdf"/>
<attribute name="IR" value="10A"/>
<attribute name="LS" value="110nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744290130 "/>
<attribute name="RDC" value="0.0027Ohm"/>
<attribute name="VALUE" value="0.013mH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="WINDING-STYLE" value="sectional"/>
</technology>
<technology name="_744290560">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744290560.pdf"/>
<attribute name="IR" value="7A"/>
<attribute name="LS" value="330nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744290560 "/>
<attribute name="RDC" value="0.0047Ohm"/>
<attribute name="VALUE" value="0.056mH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="WINDING-STYLE" value="sectional"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UCF_2TURNS" prefix="L">
<description>&lt;B&gt;WE-UCF SMT Common Mode Line Filter
&lt;Br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High inductance range
&lt;br&gt;High current range
&lt;br&gt;Small package
&lt;br&gt;Low profile
&lt;br&gt;Surface mount technology
&lt;br&gt;Wide range of filtering spectrum
&lt;br&gt;Climatic category 40/125/21
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;Br&gt;&lt;/b&gt; Filtering
&lt;br&gt;DC power lines
&lt;br&gt;Buck-/ Boost Converter filtering
&lt;br&gt;Data lines with low bitrate
&lt;br&gt;Heavily influenced lines
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14886v209%20Family_WE-UCF.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14886v209%20Family_WE-UCF.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-UCF"&gt;https://www.we-online.com/catalog/en/WE-UCF&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Ella Wu 2021-05-12&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-UCF_2TURNS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="10"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="6"/>
</connects>
<technologies>
<technology name="_744290103">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744290103.pdf"/>
<attribute name="IR" value="0.5A"/>
<attribute name="LS" value="83000nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744290103 "/>
<attribute name="RDC" value="0.92Ohm"/>
<attribute name="VALUE" value="10mH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="WINDING-STYLE" value="sectional"/>
</technology>
<technology name="_744290104">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744290104.pdf"/>
<attribute name="IR" value="0.15A"/>
<attribute name="LS" value="780000nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744290104 "/>
<attribute name="RDC" value="8.5Ohm"/>
<attribute name="VALUE" value="100mH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="WINDING-STYLE" value="sectional"/>
</technology>
<technology name="_744290152">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744290152.pdf"/>
<attribute name="IR" value="1.5A"/>
<attribute name="LS" value="13000nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744290152 "/>
<attribute name="RDC" value="0.12Ohm"/>
<attribute name="VALUE" value="1.5mH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="WINDING-STYLE" value="sectional"/>
</technology>
<technology name="_744290283">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744290283.pdf"/>
<attribute name="IR" value="0.3A"/>
<attribute name="LS" value="220000nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744290283 "/>
<attribute name="RDC" value="2.8Ohm"/>
<attribute name="VALUE" value="28mH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="WINDING-STYLE" value="sectional"/>
</technology>
<technology name="_744290321">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744290321.pdf"/>
<attribute name="IR" value="3.25A"/>
<attribute name="LS" value="2200nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744290321 "/>
<attribute name="RDC" value="0.029Ohm"/>
<attribute name="VALUE" value="0.32mH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="WINDING-STYLE" value="sectional"/>
</technology>
<technology name="_744290472">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744290472.pdf"/>
<attribute name="IR" value="0.75A"/>
<attribute name="LS" value="25000nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744290472 "/>
<attribute name="RDC" value="0.52Ohm"/>
<attribute name="VALUE" value="4.7mH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="WINDING-STYLE" value="sectional"/>
</technology>
<technology name="_744290473">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744290473.pdf"/>
<attribute name="IR" value="0.25A"/>
<attribute name="LS" value="460000nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744290473 "/>
<attribute name="RDC" value="4Ohm"/>
<attribute name="VALUE" value="47mH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="WINDING-STYLE" value="sectional"/>
</technology>
<technology name="_744290683">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744290683.pdf"/>
<attribute name="IR" value="0.2A"/>
<attribute name="LS" value="960000nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744290683 "/>
<attribute name="RDC" value="5Ohm"/>
<attribute name="VALUE" value="68mH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="WINDING-STYLE" value="sectional"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
