<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - Ferrites For PCB Assembly - WE-UKW&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-UKW_7427501">
<description>&lt;B&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_7427502">
<description>&lt;B&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_7427504">
<description>&lt;B&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275043">
<description>&lt;B&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275013">
<description>&lt;B&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275143">
<description>&lt;B&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275010">
<description>&lt;B&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275223">
<description>&lt;B&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275123">
<description>&lt;B&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275011">
<description>&lt;B&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275046">
<description>&lt;B&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275023">
<description>&lt;B&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275243">
<description>&lt;B&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275022">
<description>&lt;B&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_742750421">
<description>&lt;B&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_7427503">
<description>&lt;B&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CM2W-H">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-UKW_2SW" prefix="L">
<description>&lt;b&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Impedance will increase with more turns, available in 1 to 3 turns
&lt;br&gt; 4 different materials available for perfect interference suppression
&lt;br&gt; Also available ready-bent or in individual length
&lt;br&gt; Maximum current capability is 3 A / 5 A (short-time)
&lt;br&gt; Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Protection against radio frequency interferences
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14887v209%20Family_WE-UKW_6LOCH.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14887v209%20Family_WE-UKW_6LOCH.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-UKW/S"&gt;http://katalog.we-online.de/en/pbs/WE-UKW/S&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created  by Ella Wu  2019-01-02&lt;br&gt;
&lt;/b&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="_742750421" package="WE-UKW_742750421">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/742750421.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 742750421 "/>
<attribute name="TYPE" value="2x1 turn vertical"/>
<attribute name="VALUE" value="230Ohm@100MHz"/>
<attribute name="Z" value="145Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_74275022" package="WE-UKW_74275022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74275022.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74275022 "/>
<attribute name="TYPE" value="2x1.5 turns horizontal"/>
<attribute name="VALUE" value="512Ohm@100MHz"/>
<attribute name="Z" value="320Ohm@25MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UKW_1SW" prefix="L">
<description>&lt;b&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Impedance will increase with more turns, available in 1 to 3 turns
&lt;br&gt; 4 different materials available for perfect interference suppression
&lt;br&gt; Also available ready-bent or in individual length
&lt;br&gt; Maximum current capability is 3 A / 5 A (short-time)
&lt;br&gt; Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Protection against radio frequency interferences
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14887v209%20Family_WE-UKW_6LOCH.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14887v209%20Family_WE-UKW_6LOCH.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-UKW/S"&gt;http://katalog.we-online.de/en/pbs/WE-UKW/S&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created  by Ella Wu  2019-01-02&lt;br&gt;
&lt;/b&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_7427501" package="WE-UKW_7427501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/7427501.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7427501 "/>
<attribute name="TYPE" value="2.5 turns horizontal"/>
<attribute name="VALUE" value="800Ohm@100MHz"/>
<attribute name="Z" value="598Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_7427502" package="WE-UKW_7427502">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/7427502.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7427502 "/>
<attribute name="TYPE" value="2.5 turns horizontal"/>
<attribute name="VALUE" value="976Ohm@100MHz"/>
<attribute name="Z" value="670Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_7427503" package="WE-UKW_7427503">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/7427503.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7427503 "/>
<attribute name="TYPE" value="2.5 turns horizontal"/>
<attribute name="VALUE" value="938Ohm@100MHz"/>
<attribute name="Z" value="489Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_7427504" package="WE-UKW_7427504">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/7427504.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7427504 "/>
<attribute name="TYPE" value="2.5 turns horizontal"/>
<attribute name="VALUE" value="773Ohm@100MHz"/>
<attribute name="Z" value="702Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_74275010" package="WE-UKW_74275010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74275010.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74275010 "/>
<attribute name="TYPE" value="2.5 turns vertical"/>
<attribute name="VALUE" value="860Ohm@100MHz"/>
<attribute name="Z" value="623Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_74275011" package="WE-UKW_74275011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74275011.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74275011 "/>
<attribute name="TYPE" value="2.5 turns horizontal"/>
<attribute name="VALUE" value="800Ohm@100MHz"/>
<attribute name="Z" value="598Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_74275013" package="WE-UKW_74275013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74275013.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74275013 "/>
<attribute name="TYPE" value="3 turns vertical"/>
<attribute name="VALUE" value="950Ohm@100MHz"/>
<attribute name="Z" value="650Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_74275023" package="WE-UKW_74275023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74275023.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74275023 "/>
<attribute name="TYPE" value="3 turns vertical"/>
<attribute name="VALUE" value="1240Ohm@100MHz"/>
<attribute name="Z" value="720Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_74275043" package="WE-UKW_74275043">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74275043.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74275043 "/>
<attribute name="TYPE" value="3 turns vertical"/>
<attribute name="VALUE" value="961Ohm@100MHz"/>
<attribute name="Z" value="920Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_74275046" package="WE-UKW_74275046">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74275046.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74275046 "/>
<attribute name="TYPE" value="2.5 turns horizontal"/>
<attribute name="VALUE" value="773Ohm@100MHz"/>
<attribute name="Z" value="702Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_74275143" package="WE-UKW_74275143">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74275143.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74275143 "/>
<attribute name="TYPE" value="3 turns vertical"/>
<attribute name="VALUE" value="961Ohm@100MHz"/>
<attribute name="Z" value="920Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_74275223" package="WE-UKW_74275223">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74275223.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74275223 "/>
<attribute name="TYPE" value="3 turns vertical"/>
<attribute name="VALUE" value="1240Ohm@100MHz"/>
<attribute name="Z" value="720Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_74275243" package="WE-UKW_74275243">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74275243.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74275243 "/>
<attribute name="TYPE" value="3 turns vertical"/>
<attribute name="VALUE" value="961Ohm@100MHz"/>
<attribute name="Z" value="920Ohm@25MHz"/>
</technology>
</technologies>
</device>
<device name="_74275123" package="WE-UKW_74275123">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/74275123.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74275123 "/>
<attribute name="TYPE" value="3 turns vertical"/>
<attribute name="VALUE" value="1240Ohm@100MHz"/>
<attribute name="Z" value="720Ohm@25MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
