<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - EMC Components - ESD Protection - WE-VE ULC&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2026a, 2026-02-24&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-VE_ULC_0603">
<description>&lt;B&gt;WE-VE ULC ESD Suppressor
&lt;BR&gt;&lt;/B&gt;Size : 0603
&lt;br&gt;L X W X H = 1.6mm X 0.85mm X 0.51mm</description>
</package>
<package name="WE-VE_ULC_0402">
<description>&lt;B&gt;WE-VE ULC ESD Suppressor
&lt;BR&gt;&lt;/B&gt;Size : 0402
&lt;br&gt;L X W X H = 1mm X 0.5mm X 0.34mm</description>
</package>
</packages>
<symbols>
<symbol name="VARISTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-VE_ULC_0603" prefix="RV">
<description>&lt;b&gt; WE-VE ULC ESD Suppressor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Fast response time
&lt;br&gt;No leakage current
&lt;br&gt;Low clamping voltage
&lt;br&gt;Almost no energy consumption in stand-by mode
&lt;br&gt;Excellent absorption for ESD-impulses
&lt;br&gt;Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;Nickel barrier
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Protection of data lines
&lt;br&gt;Protection of bus systems
&lt;br&gt;Protection of semiconductors
&lt;br&gt;ESD protection in accordance with EN 61000-4-2: 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14892v209%20Family_WE-VE_ULC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14892v209%20Family_WE-VE_ULC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-VE-ULC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-VE-ULC&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-02-24&lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="VARISTOR"/>
</gates>
<devices>
<device name="" package="WE-VE_ULC_0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_82306050029">
<attribute name="CCH" value="0.2pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/82306050029?ae"/>
<attribute name="HEIGHT" value="0.51mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 82306050029 "/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="5V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VCH-MIN" value="-5V"/>
<attribute name="VESD-CONTACT" value="8kV"/>
<attribute name="VTRIG-ESD" value="150V"/>
<attribute name="WIDTH" value="0.85mm"/>
</technology>
<technology name="_82306120029">
<attribute name="CCH" value="0.2pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/82306120029?ae"/>
<attribute name="HEIGHT" value="0.51mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 82306120029 "/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="12V"/>
<attribute name="VCH-MAX" value="12V"/>
<attribute name="VCH-MIN" value="-12V"/>
<attribute name="VESD-CONTACT" value="8kV"/>
<attribute name="VTRIG-ESD" value="150V"/>
<attribute name="WIDTH" value="0.85mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VE_ULC_0402" prefix="RV">
<description>&lt;b&gt; WE-VE ULC ESD Suppressor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Fast response time
&lt;br&gt;No leakage current
&lt;br&gt;Low clamping voltage
&lt;br&gt;Almost no energy consumption in stand-by mode
&lt;br&gt;Excellent absorption for ESD-impulses
&lt;br&gt;Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;Nickel barrier
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Protection of data lines
&lt;br&gt;Protection of bus systems
&lt;br&gt;Protection of semiconductors
&lt;br&gt;ESD protection in accordance with EN 61000-4-2: 
&lt;br&gt;– 8 kV contact discharge 
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14892v209%20Family_WE-VE_ULC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14892v209%20Family_WE-VE_ULC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-VE-ULC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-VE-ULC&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-02-24&lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="VARISTOR"/>
</gates>
<devices>
<device name="" package="WE-VE_ULC_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_82307050029">
<attribute name="CCH" value="0.2pF"/>
<attribute name="CCH-MAX" value="0.8pF"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/82307050029?ae"/>
<attribute name="HEIGHT" value="0.34mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 82307050029 "/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="5V"/>
<attribute name="VCH-MAX" value="5V"/>
<attribute name="VCH-MIN" value="-5V"/>
<attribute name="VCLAMP" value="17V"/>
<attribute name="VESD-CONTACT" value="8kV"/>
<attribute name="VTRIG-ESD" value="100V"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
