<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - ESD Protection - WE-VEA&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-VEA_0508">
<description>&lt;B&gt;WE-VEA ESD Suppressor-Array
&lt;BR&gt;&lt;/B&gt;Size : 0508</description>
</package>
<package name="WE-VEA_0612">
<description>&lt;B&gt;WE-VEA ESD Suppressor-Array
&lt;BR&gt;&lt;/B&gt;Size : 0612</description>
</package>
</packages>
<symbols>
<symbol name="WE-VEA">
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-VEA_0508" prefix="D">
<description>&lt;b&gt;WE-VEA ESD Suppressor-Array
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; &lt;br&gt;Fast response time (1 ns)
&lt;br&gt;Low signal insertion loss
&lt;br&gt;No leakage current
&lt;br&gt;Low clamping voltage
&lt;br&gt;Almost no energy consumption in stand-by mode
&lt;br&gt;Excellent absorption for ESD-impulses
&lt;br&gt;Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Protection of data lines
&lt;br&gt;Protection of bus systems
&lt;br&gt;Protection of video transmission lines
&lt;br&gt;Protection of semiconductors
&lt;br&gt;ESD protection in accordance with EN 61000-4-2
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14893v209%20Family_WE-VEA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14893v209%20Family_WE-VEA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-VEA"&gt;https://katalog.we-online.de/en/pbs/WE-VEA&lt;/a&gt;&lt;p&gt;

Updated  by  Ella Wu  2019-07-04&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-VEA"/>
</gates>
<devices>
<device name="" package="WE-VEA_0508">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="7"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="4"/>
<connect gate="G$1" pin="8" pad="2"/>
</connects>
<technologies>
<technology name="_82380050100">
<attribute name="CHANNELS" value=" 4 "/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/82380050100.pdf"/>
<attribute name="ILEAK" value="0.1uA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 82380050100 "/>
<attribute name="RISO" value="10  MOhm "/>
<attribute name="VALUE" value="5V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VEA_0612" prefix="D">
<description>&lt;b&gt;WE-VEA ESD Suppressor-Array
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; &lt;br&gt;Fast response time (1 ns)
&lt;br&gt;Low signal insertion loss
&lt;br&gt;No leakage current
&lt;br&gt;Low clamping voltage
&lt;br&gt;Almost no energy consumption in stand-by mode
&lt;br&gt;Excellent absorption for ESD-impulses
&lt;br&gt;Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Protection of data lines
&lt;br&gt;Protection of bus systems
&lt;br&gt;Protection of video transmission lines
&lt;br&gt;Protection of semiconductors
&lt;br&gt;ESD protection in accordance with EN 61000-4-2
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14893v209%20Family_WE-VEA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14893v209%20Family_WE-VEA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-VEA"&gt;https://katalog.we-online.de/en/pbs/WE-VEA&lt;/a&gt;&lt;p&gt;

Updated  by  Ella Wu  2019-07-04&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-VEA"/>
</gates>
<devices>
<device name="" package="WE-VEA_0612">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="7"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="4"/>
<connect gate="G$1" pin="8" pad="2"/>
</connects>
<technologies>
<technology name="_82380180121">
<attribute name="CHANNELS" value=" 4 "/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pbs/datasheet/82380180121.pdf"/>
<attribute name="ILEAK" value="1uA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 82380180121 "/>
<attribute name="RISO" value="10  MOhm "/>
<attribute name="VALUE" value="18V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
