<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Automotive - Single Coil Power Inductors - WE-XHMA&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-06-11&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-XHMA_1090">
<description>&lt;b&gt;WE-XHMA SMD Power Inductor
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;1090, SMT, 2pins
&lt;br&gt;L X W X H = 11.6mm X 10.5mm X 9.1mm</description>
</package>
<package name="WE-XHMA_8080">
<description>&lt;b&gt;WE-XHMA SMD Power Inductor
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;8080, SMT, 2pins
&lt;br&gt;L X W X H = 8.8mm X 8.3mm X 8mm</description>
</package>
<package name="WE-XHMA_6060">
<description>&lt;b&gt;WE-XHMA SMD Power Inductor
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;6060, SMT, 2pins
&lt;br&gt;L X W X H = 6.65mm X 6.45mm X 6.1mm</description>
</package>
<package name="WE-XHMA_1510">
<description>&lt;b&gt;WE-XHMA SMD Power Inductor
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;1510, SMT, 2pins
&lt;br&gt;L X W X H = 16.4mm X 15.4mm X 10mm</description>
</package>
<package name="WE-XHMA_6030">
<description>&lt;b&gt;WE-XHMA SMD Power Inductor
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;6030, SMT, 2pins
&lt;br&gt;L X W X H = 6.65mm X 6.45mm X 3.3mm</description>
</package>
</packages>
<symbols>
<symbol name="L_POINT_GAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-XHMA_1090" prefix="L">
<description>&lt;b&gt;WE-XHMA SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flat wire coil for low copper losses
&lt;br&gt;Composite core material allows high saturation currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low leakage flux noise
&lt;br&gt;Operating temperature: -40°C up to +125°C
&lt;br&gt;AEC-Q200
&lt;br&gt;Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;Power supplies for mobile devices
&lt;br&gt;POL-converters
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Filter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o496382v209%20family-we-xhma-7843xxxxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o496382v209%20family-we-xhma-7843xxxxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMA&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-02-10&lt;br&gt;
2022 (C) Würth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMA_1090">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78439369022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439369022?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="9.1mm"/>
<attribute name="IR" value="16A@40K"/>
<attribute name="IRP" value="32.05A@40K"/>
<attribute name="ISAT" value="32.1A@30%"/>
<attribute name="ISAT2" value="15.65A@10%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439369022"/>
<attribute name="RDC-TYP" value="2.2mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_78439369033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439369033?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="HEIGHT" value="9.1mm"/>
<attribute name="IR" value="15A@40K"/>
<attribute name="IRP" value="24.95A@40K"/>
<attribute name="ISAT" value="34A@30%"/>
<attribute name="ISAT2" value="15.6A@10%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439369033"/>
<attribute name="RDC-TYP" value="3.4mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_78439369047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439369047?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="HEIGHT" value="9.1mm"/>
<attribute name="IR" value="13.5A@40K"/>
<attribute name="IRP" value="20A@40K"/>
<attribute name="ISAT" value="28.05A@30%"/>
<attribute name="ISAT2" value="13.6A@10%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439369047"/>
<attribute name="RDC-TYP" value="5mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_78439369056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439369056?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="HEIGHT" value="9.1mm"/>
<attribute name="IR" value="11.5A@40K"/>
<attribute name="IRP" value="18.15A@40K"/>
<attribute name="ISAT" value="24.45A@30%"/>
<attribute name="ISAT2" value="11.1A@10%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439369056"/>
<attribute name="RDC-TYP" value="5.9mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_78439369068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439369068?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="HEIGHT" value="9.1mm"/>
<attribute name="IR" value="10.5A@40K"/>
<attribute name="IRP" value="16.3A@40K"/>
<attribute name="ISAT" value="23.25A@30%"/>
<attribute name="ISAT2" value="10.7A@10%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439369068"/>
<attribute name="RDC-TYP" value="7.16mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_78439369082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439369082?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="HEIGHT" value="9.1mm"/>
<attribute name="IR" value="9.8A@40K"/>
<attribute name="IRP" value="13.4A@40K"/>
<attribute name="ISAT" value="20.45A@30%"/>
<attribute name="ISAT2" value="9.4A@10%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439369082"/>
<attribute name="RDC-TYP" value="10mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_78439369100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439369100?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="9.1mm"/>
<attribute name="IR" value="9.4A@40K"/>
<attribute name="IRP" value="12.7A@40K"/>
<attribute name="ISAT" value="20.3A@30%"/>
<attribute name="ISAT2" value="9.2A@10%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439369100"/>
<attribute name="RDC-TYP" value="11mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_78439369150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439369150?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="HEIGHT" value="9.1mm"/>
<attribute name="IR" value="8.3A@40K"/>
<attribute name="IRP" value="10.75A@40K"/>
<attribute name="ISAT" value="16.95A@30%"/>
<attribute name="ISAT2" value="7.2A@10%"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439369150"/>
<attribute name="RDC-TYP" value="14.8mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMA_8080" prefix="L">
<description>&lt;b&gt;WE-XHMA SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flat wire coil for low copper losses
&lt;br&gt;Composite core material allows high saturation currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low leakage flux noise
&lt;br&gt;Operating temperature: -40°C up to +125°C
&lt;br&gt;AEC-Q200
&lt;br&gt;Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;Power supplies for mobile devices
&lt;br&gt;POL-converters
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Filter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o496382v209%20family-we-xhma-7843xxxxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o496382v209%20family-we-xhma-7843xxxxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMA&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-02-10&lt;br&gt;
2022 (C) Würth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMA_8080">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78439358010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439358010?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="HEIGHT" value="8mm"/>
<attribute name="IR" value="17A@40K"/>
<attribute name="IRP" value="30.25A@40K"/>
<attribute name="ISAT" value="38.15A@30%"/>
<attribute name="ISAT2" value="18.15A@10%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="8.8mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439358010"/>
<attribute name="RDC-TYP" value="2.1mOhm"/>
<attribute name="SIZE" value="8080"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="8.3mm"/>
</technology>
<technology name="_78439358022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439358022?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="HEIGHT" value="8mm"/>
<attribute name="IR" value="13A@40K"/>
<attribute name="IRP" value="21.85A@40K"/>
<attribute name="ISAT" value="26.45A@30%"/>
<attribute name="ISAT2" value="12.55A@10%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="8.8mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439358022"/>
<attribute name="RDC-TYP" value="3.7mOhm"/>
<attribute name="SIZE" value="8080"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="8.3mm"/>
</technology>
<technology name="_78439358047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439358047?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="8mm"/>
<attribute name="IR" value="9.5A@40K"/>
<attribute name="IRP" value="13.35A@40K"/>
<attribute name="ISAT" value="16.65A@30%"/>
<attribute name="ISAT2" value="7.5A@10%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="8.8mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439358047"/>
<attribute name="RDC-TYP" value="8.65mOhm"/>
<attribute name="SIZE" value="8080"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="8.3mm"/>
</technology>
<technology name="_78439358068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439358068?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="8mm"/>
<attribute name="IR" value="7.2A@40K"/>
<attribute name="IRP" value="10.55A@40K"/>
<attribute name="ISAT" value="17.6A@30%"/>
<attribute name="ISAT2" value="8.5A@10%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="8.8mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439358068"/>
<attribute name="RDC-TYP" value="13mOhm"/>
<attribute name="SIZE" value="8080"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="8.3mm"/>
</technology>
<technology name="_78439358100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439358100?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="HEIGHT" value="8mm"/>
<attribute name="IR" value="5.8A@40K"/>
<attribute name="IRP" value="8.5A@40K"/>
<attribute name="ISAT" value="13.5A@30%"/>
<attribute name="ISAT2" value="6.3A@10%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="8.8mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439358100"/>
<attribute name="RDC-TYP" value="19mOhm"/>
<attribute name="SIZE" value="8080"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="8.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMA_6060" prefix="L">
<description>&lt;b&gt;WE-XHMA SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flat wire coil for low copper losses
&lt;br&gt;Composite core material allows high saturation currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low leakage flux noise
&lt;br&gt;Operating temperature: -40°C up to +125°C
&lt;br&gt;AEC-Q200
&lt;br&gt;Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;Power supplies for mobile devices
&lt;br&gt;POL-converters
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Filter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o496382v209%20family-we-xhma-7843xxxxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o496382v209%20family-we-xhma-7843xxxxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMA&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-06-11br&gt;
2025 (C) Würth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMA_6060">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78439346047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439346047?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IR" value="7.4A@40K"/>
<attribute name="IRP" value="9.6A@40K"/>
<attribute name="ISAT" value="13A@30%"/>
<attribute name="ISAT2" value="6.5A@10%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439346047"/>
<attribute name="RDC-TYP" value="13mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_78439346056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439346056?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IR" value="6.9A@40K"/>
<attribute name="IRP" value="8.9A@40K"/>
<attribute name="ISAT" value="12.1A@30%"/>
<attribute name="ISAT2" value="5.8A@10%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439346056"/>
<attribute name="RDC-TYP" value="15mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_78439346068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439346068?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IR" value="6.5A@40K"/>
<attribute name="IRP" value="8.1A@40K"/>
<attribute name="ISAT" value="11.3A@30%"/>
<attribute name="ISAT2" value="5.65A@10%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439346068"/>
<attribute name="RDC-TYP" value="17.6mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_78439346082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439346082?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IR" value="5.3A@40K"/>
<attribute name="IRP" value="6.95A@40K"/>
<attribute name="ISAT" value="9.3A@30%"/>
<attribute name="ISAT2" value="4.6A@10%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439346082"/>
<attribute name="RDC-TYP" value="23mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_78439346100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439346100?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IR" value="5A@40K"/>
<attribute name="IRP" value="6.4A@40K"/>
<attribute name="ISAT" value="9.7A@30%"/>
<attribute name="ISAT2" value="5.05A@10%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439346100"/>
<attribute name="RDC-TYP" value="26.5mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_78439346150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439346150?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IR" value="4.2A@40K"/>
<attribute name="IRP" value="4.9A@40K"/>
<attribute name="ISAT" value="7.4A@30%"/>
<attribute name="ISAT2" value="3.65A@10%"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439346150"/>
<attribute name="RDC-TYP" value="42mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMA_6030" prefix="L">
<description>&lt;b&gt;WE-XHMA SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flat wire coil for low copper losses
&lt;br&gt;Composite core material allows high saturation currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low leakage flux noise
&lt;br&gt;Operating temperature: -40°C up to +125°C
&lt;br&gt;AEC-Q200
&lt;br&gt;Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;Power supplies for mobile devices
&lt;br&gt;POL-converters
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Filter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o496382v209%20family-we-xhma-7843xxxxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o496382v209%20family-we-xhma-7843xxxxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMA&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-02-10&lt;br&gt;
2022 (C) Würth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMA_6030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784393440018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784393440018?ae"/>
<attribute name="FRES" value="169MHz"/>
<attribute name="HEIGHT" value="3.3mm"/>
<attribute name="IR" value="20A@40K"/>
<attribute name="IRP" value="35.65A@40K"/>
<attribute name="ISAT" value="50.6A@30%"/>
<attribute name="ISAT2" value="24.9A@10%"/>
<attribute name="L" value="0.18uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784393440018"/>
<attribute name="RDC-TYP" value="1.32mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="0.18uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_784393440033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784393440033?ae"/>
<attribute name="FRES" value="113MHz"/>
<attribute name="HEIGHT" value="3.3mm"/>
<attribute name="IR" value="16.5A@40K"/>
<attribute name="IRP" value="27.35A@40K"/>
<attribute name="ISAT" value="42.9A@30%"/>
<attribute name="ISAT2" value="20A@10%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784393440033"/>
<attribute name="RDC-TYP" value="2.1mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_784393440056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784393440056?ae"/>
<attribute name="FRES" value="77MHz"/>
<attribute name="HEIGHT" value="3.3mm"/>
<attribute name="IR" value="16A@40K"/>
<attribute name="IRP" value="22.75A@40K"/>
<attribute name="ISAT" value="30.8A@30%"/>
<attribute name="ISAT2" value="14.5A@10%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784393440056"/>
<attribute name="RDC-TYP" value="2.9mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_78439344010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439344010?ae"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="HEIGHT" value="3.3mm"/>
<attribute name="IR" value="12A@40K"/>
<attribute name="IRP" value="15.75A@40K"/>
<attribute name="ISAT" value="24.95A@30%"/>
<attribute name="ISAT2" value="11A@10%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439344010"/>
<attribute name="RDC-TYP" value="5.5mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_78439344012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439344012?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="HEIGHT" value="3.3mm"/>
<attribute name="IR" value="10.3A@40K"/>
<attribute name="IRP" value="14.45A@40K"/>
<attribute name="ISAT" value="21.6A@30%"/>
<attribute name="ISAT2" value="7.7A@10%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439344012"/>
<attribute name="RDC-TYP" value="6.4mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_78439344022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439344022?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="HEIGHT" value="3.3mm"/>
<attribute name="IR" value="8A@40K"/>
<attribute name="IRP" value="10.85A@40K"/>
<attribute name="ISAT" value="16.25A@30%"/>
<attribute name="ISAT2" value="7.5A@10%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439344022"/>
<attribute name="RDC-TYP" value="10.5mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_78439344033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439344033?ae"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="HEIGHT" value="3.3mm"/>
<attribute name="IR" value="6A@40K"/>
<attribute name="IRP" value="7.65A@40K"/>
<attribute name="ISAT" value="14.5A@30%"/>
<attribute name="ISAT2" value="6.7A@10%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439344033"/>
<attribute name="RDC-TYP" value="19.2mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_78439344047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439344047?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="3.3mm"/>
<attribute name="IR" value="4.7A@40K"/>
<attribute name="IRP" value="5.8A@40K"/>
<attribute name="ISAT" value="10.5A@30%"/>
<attribute name="ISAT2" value="3.7A@10%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439344047"/>
<attribute name="RDC-TYP" value="31mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMA_1510" prefix="L">
<description>&lt;b&gt;WE-XHMA SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Flat wire coil for low copper losses
&lt;br&gt;Composite core material allows high saturation currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low leakage flux noise
&lt;br&gt;Operating temperature: -40°C up to +125°C
&lt;br&gt;AEC-Q200
&lt;br&gt;Automotive approved
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;Power supplies for mobile devices
&lt;br&gt;POL-converters
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Filter
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o496382v209%20family-we-xhma-7843xxxxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o496382v209%20family-we-xhma-7843xxxxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMA&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2022-02-10&lt;br&gt;
2022 (C) Würth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMA_1510">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78439370047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439370047?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IR" value="17A@40K"/>
<attribute name="IRP" value="29.37A@40K"/>
<attribute name="ISAT" value="47.4A@30%"/>
<attribute name="ISAT2" value="20.9A@10%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439370047"/>
<attribute name="RDC-TYP" value="3.1mOhm"/>
<attribute name="SIZE" value="1510"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="15.4mm"/>
</technology>
<technology name="_78439370068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439370068?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IR" value="15A@40K"/>
<attribute name="IRP" value="25.3A@40K"/>
<attribute name="ISAT" value="40.05A@30%"/>
<attribute name="ISAT2" value="17.8A@10%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439370068"/>
<attribute name="RDC-TYP" value="4.1mOhm"/>
<attribute name="SIZE" value="1510"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="15.4mm"/>
</technology>
<technology name="_78439370082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439370082?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IR" value="13A@40K"/>
<attribute name="IRP" value="21.35A@40K"/>
<attribute name="ISAT" value="36.4A@30%"/>
<attribute name="ISAT2" value="15A@10%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439370082"/>
<attribute name="RDC-TYP" value="5.5mOhm"/>
<attribute name="SIZE" value="1510"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="15.4mm"/>
</technology>
<technology name="_78439370100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439370100?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IR" value="11.5A@40K"/>
<attribute name="IRP" value="19.6A@40K"/>
<attribute name="ISAT" value="31.2A@30%"/>
<attribute name="ISAT2" value="12.9A@10%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439370100"/>
<attribute name="RDC-TYP" value="6.4mOhm"/>
<attribute name="SIZE" value="1510"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="15.4mm"/>
</technology>
<technology name="_78439370150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439370150?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IR" value="10A@40K"/>
<attribute name="IRP" value="14.7A@40K"/>
<attribute name="ISAT" value="26.1A@30%"/>
<attribute name="ISAT2" value="10.25A@10%"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439370150"/>
<attribute name="RDC-TYP" value="10.5mOhm"/>
<attribute name="SIZE" value="1510"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="WIDTH" value="15.4mm"/>
</technology>
<technology name="_78439370220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439370220?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IR" value="8A@40K"/>
<attribute name="IRP" value="13.35A@40K"/>
<attribute name="ISAT" value="22.35A@30%"/>
<attribute name="ISAT2" value="9.1A@10%"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439370220"/>
<attribute name="RDC-TYP" value="12.5mOhm"/>
<attribute name="SIZE" value="1510"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="WIDTH" value="15.4mm"/>
</technology>
<technology name="_78439370330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78439370330?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IR" value="8.5A@40K"/>
<attribute name="IRP" value="10.8A@40K"/>
<attribute name="ISAT" value="18.15A@30%"/>
<attribute name="ISAT2" value="6.8A@10%"/>
<attribute name="L" value="33uH"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="MATERIAL" value="Hyperflux"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78439370330"/>
<attribute name="RDC-TYP" value="18mOhm"/>
<attribute name="SIZE" value="1510"/>
<attribute name="VALUE" value="33uH"/>
<attribute name="WIDTH" value="15.4mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
