<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Single Coil Power Inductors - WE-XHMI&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025b, 2025-06-13&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-XHMI_1510">
<description>&lt;b&gt;WE-XHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;1510, SMT, 2pins
&lt;br&gt;L X W X H = 16.4mm X 15.4mm X 10mm</description>
</package>
<package name="WE-XHMI_6060P">
<description>&lt;b&gt;WE-XHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;6060P, SMT, 2pins
&lt;br&gt;L X W X H = 6.6mm X 6.4mm X 3.1mm</description>
</package>
<package name="WE-XHMI_5020">
<description>&lt;b&gt;WE-XHMI SMD Power Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size: 5020, SMT, 2pins
&lt;br&gt;LXWXH=5.55X5.35X2mm</description>
</package>
<package name="WE-XHMI_1090">
<description>&lt;b&gt;WE-XHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;1090, SMT, 2pins
&lt;br&gt;L X W X H = 11.6mm X 10.5mm X 8.8mm</description>
</package>
<package name="WE-XHMI_6030">
<description>&lt;b&gt;WE-XHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;6030, SMT, 2pins
&lt;br&gt;L X W X H = 6.65mm X 6.45mm X 2.75mm</description>
</package>
<package name="WE-XHMI_1010P">
<description>&lt;b&gt;WE-XHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;1010P, SMT, 2pins
&lt;br&gt;L X W X H = 11.3mm X 10mm X 10mm</description>
</package>
<package name="WE-XHMI_6030P">
<description>&lt;b&gt;WE-XHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;6030P, SMT, 2pins
&lt;br&gt;L X W X H = 6.6mm X 6.4mm X 3.1mm</description>
</package>
<package name="WE-XHMI_4020">
<description>&lt;b&gt;WE-XHMI SMD Power Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size: 4020, SMT, 2pins
&lt;br&gt;LXWXH=4.3X4.3X2mm</description>
</package>
<package name="WE-XHMI_7070">
<description>&lt;b&gt;WE-XHMI SMD Power Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size: 7070, SMT, 2pins
&lt;br&gt;LXWXH=7.9X7.6X7.1mm</description>
</package>
<package name="WE-XHMI_1060P">
<description>&lt;b&gt;WE-XHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;1060P, SMT, 2pins
&lt;br&gt;L X W X H = 11.3mm X 10mm X 6mm</description>
</package>
<package name="WE-XHMI_4030">
<description>&lt;b&gt;WE-XHMI SMD Power Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size: 4030, SMT, 2pins
&lt;br&gt;LXWXH=4.3X4.3X3mm</description>
</package>
<package name="WE-XHMI_5050">
<description>&lt;b&gt;WE-XHMI SMD Power Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size: 5050, SMT, 2pins
&lt;br&gt;LXWXH=5.55X5.35X5.1mm</description>
</package>
<package name="WE-XHMI_8080">
<description>&lt;b&gt;WE-XHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;8080, SMT, 2pins
&lt;br&gt;L X W X H = 8.8mm X 8.3mm X 7.8mm</description>
</package>
<package name="WE-XHMI_7030">
<description>&lt;b&gt;WE-XHMI SMD Power Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size: 7070, SMT, 2pins
&lt;br&gt;LXWXH=7.9X7.6X3.0mm</description>
</package>
<package name="WE-XHMI_4040">
<description>&lt;b&gt;WE-XHMI SMD Power Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size: 4040, SMT, 2pins
&lt;br&gt;LXWXH=4.3X4.3X4.1mm</description>
</package>
<package name="WE-XHMI_5030">
<description>&lt;b&gt;WE-XHMI SMD Power Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size: 5030, SMT, 2pins
&lt;br&gt;LXWXH=5.55X5.35X3mm</description>
</package>
<package name="WE-XHMI_6060">
<description>&lt;b&gt;WE-XHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;6060, SMT, 2pins
&lt;br&gt;L X W X H = 6.65mm X 6.45mm X 5.8mm</description>
</package>
</packages>
<symbols>
<symbol name="L_POINT_GAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-XHMI_1510" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-09-18&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_1510">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74439370033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439370033?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="33.8A@40K"/>
<attribute name="ISAT" value="43A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439370033"/>
<attribute name="RDC-MAX" value="2.97mOhm"/>
<attribute name="RDC-TYP" value="2.6mOhm"/>
<attribute name="SIZE" value="1510"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="15.4mm"/>
</technology>
<technology name="_74439370047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439370047?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="29.7A@40K"/>
<attribute name="ISAT" value="47.4A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439370047"/>
<attribute name="RDC-MAX" value="3.41mOhm"/>
<attribute name="RDC-TYP" value="3.1mOhm"/>
<attribute name="SIZE" value="1510"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="15.4mm"/>
</technology>
<technology name="_74439370056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439370056?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="29.6A@40K"/>
<attribute name="ISAT" value="40.1A@30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439370056"/>
<attribute name="RDC-MAX" value="3.96mOhm"/>
<attribute name="RDC-TYP" value="3.5mOhm"/>
<attribute name="SIZE" value="1510"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="15.4mm"/>
</technology>
<technology name="_74439370068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439370068?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="25.3A@40K"/>
<attribute name="ISAT" value="40.05A@30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439370068"/>
<attribute name="RDC-MAX" value="4.51mOhm"/>
<attribute name="RDC-TYP" value="4.1mOhm"/>
<attribute name="SIZE" value="1510"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="15.4mm"/>
</technology>
<technology name="_74439370082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439370082?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="21.35A@40K"/>
<attribute name="ISAT" value="36.4A@30%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439370082"/>
<attribute name="RDC-MAX" value="6.05mOhm"/>
<attribute name="RDC-TYP" value="5.5mOhm"/>
<attribute name="SIZE" value="1510"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="15.4mm"/>
</technology>
<technology name="_74439370100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439370100?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="19.6A@40K"/>
<attribute name="ISAT" value="31.2A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439370100"/>
<attribute name="RDC-MAX" value="7.04mOhm"/>
<attribute name="RDC-TYP" value="6.4mOhm"/>
<attribute name="SIZE" value="1510"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="15.4mm"/>
</technology>
<technology name="_74439370150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439370150?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="14.7A@40K"/>
<attribute name="ISAT" value="26.1A@30%"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439370150"/>
<attribute name="RDC-MAX" value="11.55mOhm"/>
<attribute name="RDC-TYP" value="10.5mOhm"/>
<attribute name="SIZE" value="1510"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="WIDTH" value="15.4mm"/>
</technology>
<technology name="_74439370220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439370220?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="13.35A@40K"/>
<attribute name="ISAT" value="22.35A@30%"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439370220"/>
<attribute name="RDC-MAX" value="13.75mOhm"/>
<attribute name="RDC-TYP" value="12.5mOhm"/>
<attribute name="SIZE" value="1510"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="WIDTH" value="15.4mm"/>
</technology>
<technology name="_74439370330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439370330?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="10.8A@40K"/>
<attribute name="ISAT" value="18.15A@30%"/>
<attribute name="L" value="33uH"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439370330"/>
<attribute name="RDC-MAX" value="19.8mOhm"/>
<attribute name="RDC-TYP" value="18mOhm"/>
<attribute name="SIZE" value="1510"/>
<attribute name="VALUE" value="33uH"/>
<attribute name="WIDTH" value="15.4mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_6060P" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-04-14&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_6060P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443934650022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443934650022?ae"/>
<attribute name="FRES" value="125MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="54A@40K"/>
<attribute name="ISAT" value="70.6A@30%"/>
<attribute name="L" value="0.22uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443934650022"/>
<attribute name="RDC-MAX" value="1.3mOhm"/>
<attribute name="RDC-TYP" value="1.1mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_7443934650047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443934650047?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="45A@40K"/>
<attribute name="ISAT" value="40.6A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443934650047"/>
<attribute name="RDC-MAX" value="1.5mOhm"/>
<attribute name="RDC-TYP" value="1.4mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_7443934650068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443934650068?ae"/>
<attribute name="FRES" value="62MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="40.6A@40K"/>
<attribute name="ISAT" value="29.4A@30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443934650068"/>
<attribute name="RDC-MAX" value="2.1mOhm"/>
<attribute name="RDC-TYP" value="1.7mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393465010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393465010?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="32.3A@40K"/>
<attribute name="ISAT" value="26.2A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393465010"/>
<attribute name="RDC-MAX" value="2.5mOhm"/>
<attribute name="RDC-TYP" value="2.2mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393465012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393465012?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="30.9A@40K"/>
<attribute name="ISAT" value="22.7A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393465012"/>
<attribute name="RDC-MAX" value="3.4mOhm"/>
<attribute name="RDC-TYP" value="2.6mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393465015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393465015?ae"/>
<attribute name="FRES" value="32MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="30.6A@40K"/>
<attribute name="ISAT" value="22A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393465015"/>
<attribute name="RDC-MAX" value="3.8mOhm"/>
<attribute name="RDC-TYP" value="3mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393465018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393465018?ae"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="25.7A@40K"/>
<attribute name="ISAT" value="21.5A@30%"/>
<attribute name="L" value="1.8uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393465018"/>
<attribute name="RDC-MAX" value="4mOhm"/>
<attribute name="RDC-TYP" value="3.5mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393465022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393465022?ae"/>
<attribute name="FRES" value="29MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="22.3A@40K"/>
<attribute name="ISAT" value="18.6A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393465022"/>
<attribute name="RDC-MAX" value="4.5mOhm"/>
<attribute name="RDC-TYP" value="3.9mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393465033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393465033?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="20.4A@40K"/>
<attribute name="ISAT" value="15.6A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393465033"/>
<attribute name="RDC-MAX" value="6.5mOhm"/>
<attribute name="RDC-TYP" value="6mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393465047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393465047?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="14.6A@40K"/>
<attribute name="ISAT" value="14.4A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393465047"/>
<attribute name="RDC-MAX" value="10.1mOhm"/>
<attribute name="RDC-TYP" value="9.4mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393465056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393465056?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="13.7A@40K"/>
<attribute name="ISAT" value="12A@30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393465056"/>
<attribute name="RDC-MAX" value="11.7mOhm"/>
<attribute name="RDC-TYP" value="10.9mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393465068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393465068?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="13.4A@40K"/>
<attribute name="ISAT" value="10.9A@30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393465068"/>
<attribute name="RDC-MAX" value="14mOhm"/>
<attribute name="RDC-TYP" value="12.5mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393465082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393465082?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="13.1A@40K"/>
<attribute name="ISAT" value="10.1A@30%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393465082"/>
<attribute name="RDC-MAX" value="16.8mOhm"/>
<attribute name="RDC-TYP" value="14.6mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393465100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393465100?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="10A@40K"/>
<attribute name="ISAT" value="9.9A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393465100"/>
<attribute name="RDC-MAX" value="19.4mOhm"/>
<attribute name="RDC-TYP" value="18mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393465120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393465120?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="8.9A@40K"/>
<attribute name="ISAT" value="9.8A@30%"/>
<attribute name="L" value="12uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393465120"/>
<attribute name="RDC-MAX" value="24.2mOhm"/>
<attribute name="RDC-TYP" value="22.8mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="12uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393465150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393465150?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="8.5A@40K"/>
<attribute name="ISAT" value="7.8A@30%"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393465150"/>
<attribute name="RDC-MAX" value="31.1mOhm"/>
<attribute name="RDC-TYP" value="28.6mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393465180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393465180?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="7.2A@40K"/>
<attribute name="ISAT" value="6.8A@30%"/>
<attribute name="L" value="18uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393465180"/>
<attribute name="RDC-MAX" value="37.3mOhm"/>
<attribute name="RDC-TYP" value="34.5mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="18uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393465220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393465220?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="5.3A@40K"/>
<attribute name="ISAT" value="6.7A@30%"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393465220"/>
<attribute name="RDC-MAX" value="46.9mOhm"/>
<attribute name="RDC-TYP" value="42mOhm"/>
<attribute name="SIZE" value="6060P"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_5020" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-11&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_5020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744393330016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393330016?ae"/>
<attribute name="FRES" value="190MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="24.7A@40K"/>
<attribute name="ISAT" value="41.5A@30%"/>
<attribute name="L" value="0.16uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393330016"/>
<attribute name="RDC-MAX" value="3.13mOhm"/>
<attribute name="RDC-TYP" value="2.2mOhm"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="0.16uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_744393330033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393330033?ae"/>
<attribute name="FRES" value="105MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="20.8A@40K"/>
<attribute name="ISAT" value="27A@30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393330033"/>
<attribute name="RDC-MAX" value="4.25mOhm"/>
<attribute name="RDC-TYP" value="3mOhm"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_744393330056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393330056?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="15.4A@40K"/>
<attribute name="ISAT" value="21.6A@30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393330056"/>
<attribute name="RDC-MAX" value="8mOhm"/>
<attribute name="RDC-TYP" value="5.2mOhm"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_744393330068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393330068?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="13.3A@40K"/>
<attribute name="ISAT" value="17.2A@30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393330068"/>
<attribute name="RDC-MAX" value="9.38mOhm"/>
<attribute name="RDC-TYP" value="6.7mOhm"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_74439333010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439333010?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="11.4A@40K"/>
<attribute name="ISAT" value="14.4A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439333010"/>
<attribute name="RDC-MAX" value="10.92mOhm"/>
<attribute name="RDC-TYP" value="9.5mOhm"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_74439333012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439333012?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="10.7A@40K"/>
<attribute name="ISAT" value="11.6A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439333012"/>
<attribute name="RDC-MAX" value="15mOhm"/>
<attribute name="RDC-TYP" value="10.8mOhm"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_1090" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-09-18&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_1090">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74439369010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369010?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="8.8mm"/>
<attribute name="IRP" value="48.2A@40K"/>
<attribute name="ISAT" value="55.3A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439369010"/>
<attribute name="RDC-MAX" value="1.61mOhm"/>
<attribute name="RDC-TYP" value="1.4mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_74439369015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369015?ae"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="HEIGHT" value="8.8mm"/>
<attribute name="IRP" value="40.6A@40K"/>
<attribute name="ISAT" value="38.55A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439369015"/>
<attribute name="RDC-MAX" value="1.76mOhm"/>
<attribute name="RDC-TYP" value="1.46mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_74439369022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369022?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="8.8mm"/>
<attribute name="IRP" value="32.05A@40K"/>
<attribute name="ISAT" value="32.1A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439369022"/>
<attribute name="RDC-MAX" value="2.42mOhm"/>
<attribute name="RDC-TYP" value="2.2mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_74439369033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369033?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="HEIGHT" value="8.8mm"/>
<attribute name="IRP" value="24.95A@40K"/>
<attribute name="ISAT" value="34A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439369033"/>
<attribute name="RDC-MAX" value="3.74mOhm"/>
<attribute name="RDC-TYP" value="3.4mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_74439369047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369047?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="HEIGHT" value="8.8mm"/>
<attribute name="IRP" value="20A@40K"/>
<attribute name="ISAT" value="28.05A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439369047"/>
<attribute name="RDC-MAX" value="5.5mOhm"/>
<attribute name="RDC-TYP" value="5mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_74439369056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369056?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="HEIGHT" value="8.8mm"/>
<attribute name="IRP" value="18.15A@40K"/>
<attribute name="ISAT" value="24.45A@30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439369056"/>
<attribute name="RDC-MAX" value="6.49mOhm"/>
<attribute name="RDC-TYP" value="5.9mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_74439369068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369068?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="HEIGHT" value="8.8mm"/>
<attribute name="IRP" value="16.3A@40K"/>
<attribute name="ISAT" value="23.25A@30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439369068"/>
<attribute name="RDC-MAX" value="7.88mOhm"/>
<attribute name="RDC-TYP" value="7.16mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_74439369082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369082?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="HEIGHT" value="8.8mm"/>
<attribute name="IRP" value="13.4A@40K"/>
<attribute name="ISAT" value="20.45A@30%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439369082"/>
<attribute name="RDC-MAX" value="11mOhm"/>
<attribute name="RDC-TYP" value="10mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_74439369100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369100?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="8.8mm"/>
<attribute name="IRP" value="12.7A@40K"/>
<attribute name="ISAT" value="20.3A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439369100"/>
<attribute name="RDC-MAX" value="12.1mOhm"/>
<attribute name="RDC-TYP" value="11mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_74439369150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369150?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="HEIGHT" value="8.8mm"/>
<attribute name="IRP" value="10.75A@40K"/>
<attribute name="ISAT" value="16.95A@30%"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439369150"/>
<attribute name="RDC-MAX" value="16.28mOhm"/>
<attribute name="RDC-TYP" value="14.8mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_74439369220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369220?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="HEIGHT" value="8.8mm"/>
<attribute name="IRP" value="9.7A@40K"/>
<attribute name="ISAT" value="13.8A@30%"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439369220"/>
<attribute name="RDC-MAX" value="23.65mOhm"/>
<attribute name="RDC-TYP" value="21mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_74439369330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369330?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="HEIGHT" value="8.8mm"/>
<attribute name="IRP" value="7.1A@40K"/>
<attribute name="ISAT" value="11.7A@30%"/>
<attribute name="L" value="33uH"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439369330"/>
<attribute name="RDC-MAX" value="39.6mOhm"/>
<attribute name="RDC-TYP" value="36.2mOhm"/>
<attribute name="SIZE" value="1090"/>
<attribute name="VALUE" value="33uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_6030" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-09-18&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_6030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744393440015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393440015?ae"/>
<attribute name="FRES" value="191MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="37A@40K"/>
<attribute name="ISAT" value="56A@30%"/>
<attribute name="L" value="0.15uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393440015"/>
<attribute name="RDC-MAX" value="1.49mOhm"/>
<attribute name="RDC-TYP" value="1.24mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="0.15uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_744393440018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393440018?ae"/>
<attribute name="FRES" value="169MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="35.65A@40K"/>
<attribute name="ISAT" value="50.6A@30%"/>
<attribute name="L" value="0.18uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393440018"/>
<attribute name="RDC-MAX" value="1.45mOhm"/>
<attribute name="RDC-TYP" value="1.32mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="0.18uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_744393440033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393440033?ae"/>
<attribute name="FRES" value="113MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="27.35A@40K"/>
<attribute name="ISAT" value="42.9A@30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393440033"/>
<attribute name="RDC-MAX" value="2.31mOhm"/>
<attribute name="RDC-TYP" value="2.1mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_744393440047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393440047?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="27.3A@40K"/>
<attribute name="ISAT" value="34A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393440047"/>
<attribute name="RDC-MAX" value="3.14mOhm"/>
<attribute name="RDC-TYP" value="2.8mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_744393440056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393440056?ae"/>
<attribute name="FRES" value="77MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="22.75A@40K"/>
<attribute name="ISAT" value="30.8A@30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393440056"/>
<attribute name="RDC-MAX" value="3.19mOhm"/>
<attribute name="RDC-TYP" value="2.9mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_744393440068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393440068?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="21.7A@40K"/>
<attribute name="ISAT" value="27.7A@30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393440068"/>
<attribute name="RDC-MAX" value="4.4mOhm"/>
<attribute name="RDC-TYP" value="3.8mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439344010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439344010?ae"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="15.75A@40K"/>
<attribute name="ISAT" value="24.95A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439344010"/>
<attribute name="RDC-MAX" value="6.05mOhm"/>
<attribute name="RDC-TYP" value="5.5mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439344012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439344012?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="14.45A@40K"/>
<attribute name="ISAT" value="21.6A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439344012"/>
<attribute name="RDC-MAX" value="7.04mOhm"/>
<attribute name="RDC-TYP" value="6.4mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439344018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439344018?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="14.4A@40K"/>
<attribute name="ISAT" value="17.6A@30%"/>
<attribute name="L" value="1.8uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439344018"/>
<attribute name="RDC-MAX" value="10.45mOhm"/>
<attribute name="RDC-TYP" value="9.7mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439344022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439344022?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="10.85A@40K"/>
<attribute name="ISAT" value="16.25A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439344022"/>
<attribute name="RDC-MAX" value="11.55mOhm"/>
<attribute name="RDC-TYP" value="10.5mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439344033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439344033?ae"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="7.65A@40K"/>
<attribute name="ISAT" value="14.5A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439344033"/>
<attribute name="RDC-MAX" value="21.12mOhm"/>
<attribute name="RDC-TYP" value="19.2mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439344047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439344047?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="5.8A@40K"/>
<attribute name="ISAT" value="10.5A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439344047"/>
<attribute name="RDC-MAX" value="34.1mOhm"/>
<attribute name="RDC-TYP" value="31mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_1010P" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-04-14&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_1010P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443936050022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443936050022?ae"/>
<attribute name="FRES" value="115MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="96.6A@40K"/>
<attribute name="ISAT" value="114A@30%"/>
<attribute name="L" value="0.22uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443936050022"/>
<attribute name="RDC-MAX" value="0.5mOhm"/>
<attribute name="RDC-TYP" value="0.37mOhm"/>
<attribute name="SIZE" value="1010P"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7443936050068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443936050068?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="61.1A@40K"/>
<attribute name="ISAT" value="68.5A@30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443936050068"/>
<attribute name="RDC-MAX" value="0.91mOhm"/>
<attribute name="RDC-TYP" value="0.77mOhm"/>
<attribute name="SIZE" value="1010P"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393605010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393605010?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="45.6A@40K"/>
<attribute name="ISAT" value="57A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393605010"/>
<attribute name="RDC-MAX" value="1.1mOhm"/>
<attribute name="RDC-TYP" value="0.97mOhm"/>
<attribute name="SIZE" value="1010P"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393605015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393605015?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="41.9A@40K"/>
<attribute name="ISAT" value="55A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393605015"/>
<attribute name="RDC-MAX" value="1.7mOhm"/>
<attribute name="RDC-TYP" value="1.4mOhm"/>
<attribute name="SIZE" value="1010P"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393605022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393605022?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="29.5A@40K"/>
<attribute name="ISAT" value="42.5A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393605022"/>
<attribute name="RDC-MAX" value="2.6mOhm"/>
<attribute name="RDC-TYP" value="1.9mOhm"/>
<attribute name="SIZE" value="1010P"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393605033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393605033?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="28.7A@40K"/>
<attribute name="ISAT" value="41.5A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393605033"/>
<attribute name="RDC-MAX" value="3.4mOhm"/>
<attribute name="RDC-TYP" value="2.7mOhm"/>
<attribute name="SIZE" value="1010P"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393605047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393605047?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="27.9A@40K"/>
<attribute name="ISAT" value="28A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393605047"/>
<attribute name="RDC-MAX" value="4.5mOhm"/>
<attribute name="RDC-TYP" value="3.8mOhm"/>
<attribute name="SIZE" value="1010P"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393605056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393605056?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="25.2A@40K"/>
<attribute name="ISAT" value="26A@30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393605056"/>
<attribute name="RDC-MAX" value="5.9mOhm"/>
<attribute name="RDC-TYP" value="5mOhm"/>
<attribute name="SIZE" value="1010P"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393605068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393605068?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="20A@40K"/>
<attribute name="ISAT" value="23.5A@30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393605068"/>
<attribute name="RDC-MAX" value="7mOhm"/>
<attribute name="RDC-TYP" value="5.9mOhm"/>
<attribute name="SIZE" value="1010P"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393605082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393605082?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="19.2A@40K"/>
<attribute name="ISAT" value="21.5A@30%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393605082"/>
<attribute name="RDC-MAX" value="8.7mOhm"/>
<attribute name="RDC-TYP" value="7.1mOhm"/>
<attribute name="SIZE" value="1010P"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393605100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393605100?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="17.2A@40K"/>
<attribute name="ISAT" value="21A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393605100"/>
<attribute name="RDC-MAX" value="9.7mOhm"/>
<attribute name="RDC-TYP" value="8.5mOhm"/>
<attribute name="SIZE" value="1010P"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393605150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393605150?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="14.9A@40K"/>
<attribute name="ISAT" value="20.5A@30%"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393605150"/>
<attribute name="RDC-MAX" value="15.2mOhm"/>
<attribute name="RDC-TYP" value="12.9mOhm"/>
<attribute name="SIZE" value="1010P"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393605220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393605220?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="IRP" value="11.6A@40K"/>
<attribute name="ISAT" value="15.5A@30%"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393605220"/>
<attribute name="RDC-MAX" value="22mOhm"/>
<attribute name="RDC-TYP" value="18.7mOhm"/>
<attribute name="SIZE" value="1010P"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_6030P" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;


Created by Ella Wu 2025-04-14&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_6030P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443934450015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443934450015?ae"/>
<attribute name="FRES" value="160MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="56.8A@40K"/>
<attribute name="ISAT" value="48A@30%"/>
<attribute name="L" value="0.15uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443934450015"/>
<attribute name="RDC-MAX" value="1.2mOhm"/>
<attribute name="RDC-TYP" value="0.9mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="0.15uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_7443934450022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443934450022?ae"/>
<attribute name="FRES" value="125MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="51.6A@40K"/>
<attribute name="ISAT" value="37.9A@30%"/>
<attribute name="L" value="0.22uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443934450022"/>
<attribute name="RDC-MAX" value="1.5mOhm"/>
<attribute name="RDC-TYP" value="1.2mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_7443934450033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443934450033?ae"/>
<attribute name="FRES" value="87MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="42.5A@40K"/>
<attribute name="ISAT" value="33.7A@30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443934450033"/>
<attribute name="RDC-MAX" value="2mOhm"/>
<attribute name="RDC-TYP" value="1.6mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_7443934450047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443934450047?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="40.7A@40K"/>
<attribute name="ISAT" value="33.2A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443934450047"/>
<attribute name="RDC-MAX" value="2.7mOhm"/>
<attribute name="RDC-TYP" value="2.1mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_7443934450056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443934450056?ae"/>
<attribute name="FRES" value="68MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="31.4A@40K"/>
<attribute name="ISAT" value="32.7A@30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443934450056"/>
<attribute name="RDC-MAX" value="3.4mOhm"/>
<attribute name="RDC-TYP" value="2.7mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_7443934450068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443934450068?ae"/>
<attribute name="FRES" value="57MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="30A@40K"/>
<attribute name="ISAT" value="22.3A@30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443934450068"/>
<attribute name="RDC-MAX" value="3.4mOhm"/>
<attribute name="RDC-TYP" value="2.8mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_7443934450082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443934450082?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="28.7A@40K"/>
<attribute name="ISAT" value="21.9A@30%"/>
<attribute name="L" value="0.82uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443934450082"/>
<attribute name="RDC-MAX" value="4mOhm"/>
<attribute name="RDC-TYP" value="3.4mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="0.82uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393445010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393445010?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="25.1A@40K"/>
<attribute name="ISAT" value="21.4A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393445010"/>
<attribute name="RDC-MAX" value="4.9mOhm"/>
<attribute name="RDC-TYP" value="4.2mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393445012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393445012?ae"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="24.8A@40K"/>
<attribute name="ISAT" value="20.6A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393445012"/>
<attribute name="RDC-MAX" value="5.2mOhm"/>
<attribute name="RDC-TYP" value="4.3mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393445015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393445015?ae"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="22A@40K"/>
<attribute name="ISAT" value="19.9A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393445015"/>
<attribute name="RDC-MAX" value="7mOhm"/>
<attribute name="RDC-TYP" value="5.8mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393445018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393445018?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="21.8A@40K"/>
<attribute name="ISAT" value="18.1A@30%"/>
<attribute name="L" value="1.8uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393445018"/>
<attribute name="RDC-MAX" value="8mOhm"/>
<attribute name="RDC-TYP" value="6.8mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393445022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393445022?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="19.2A@40K"/>
<attribute name="ISAT" value="17.7A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393445022"/>
<attribute name="RDC-MAX" value="10.3mOhm"/>
<attribute name="RDC-TYP" value="8.3mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393445033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393445033?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="13.9A@40K"/>
<attribute name="ISAT" value="12.5A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393445033"/>
<attribute name="RDC-MAX" value="15.4mOhm"/>
<attribute name="RDC-TYP" value="14.3mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393445047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393445047?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="13A@40K"/>
<attribute name="ISAT" value="10.8A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393445047"/>
<attribute name="RDC-MAX" value="21mOhm"/>
<attribute name="RDC-TYP" value="16.7mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393445056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393445056?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="11.7A@40K"/>
<attribute name="ISAT" value="10.6A@30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393445056"/>
<attribute name="RDC-MAX" value="24.1mOhm"/>
<attribute name="RDC-TYP" value="19.9mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393445068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393445068?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="9.8A@40K"/>
<attribute name="ISAT" value="9.3A@30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393445068"/>
<attribute name="RDC-MAX" value="28mOhm"/>
<attribute name="RDC-TYP" value="24.4mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393445082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393445082?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="7.8A@40K"/>
<attribute name="ISAT" value="8.8A@30%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393445082"/>
<attribute name="RDC-MAX" value="38mOhm"/>
<attribute name="RDC-TYP" value="36mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393445100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393445100?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="7.5A@40K"/>
<attribute name="ISAT" value="7.4A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393445100"/>
<attribute name="RDC-MAX" value="44mOhm"/>
<attribute name="RDC-TYP" value="40.3mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393445120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393445120?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="6.6A@40K"/>
<attribute name="ISAT" value="7A@30%"/>
<attribute name="L" value="12uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393445120"/>
<attribute name="RDC-MAX" value="53mOhm"/>
<attribute name="RDC-TYP" value="48.5mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="12uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393445150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393445150?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="5.9A@40K"/>
<attribute name="ISAT" value="6.5A@30%"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393445150"/>
<attribute name="RDC-MAX" value="72mOhm"/>
<attribute name="RDC-TYP" value="61.8mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
<technology name="_744393445180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393445180?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="5A@40K"/>
<attribute name="ISAT" value="5.6A@30%"/>
<attribute name="L" value="18uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393445180"/>
<attribute name="RDC-MAX" value="77mOhm"/>
<attribute name="RDC-TYP" value="68.3mOhm"/>
<attribute name="SIZE" value="6030P"/>
<attribute name="VALUE" value="18uH"/>
<attribute name="WIDTH" value="6.4mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_4020" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-09-18&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_4020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744393230011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393230011?ae"/>
<attribute name="FRES" value="295MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="23.7A@40K"/>
<attribute name="ISAT" value="41.5A@30%"/>
<attribute name="L" value="0.11uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393230011"/>
<attribute name="RDC-MAX" value="2.44mOhm"/>
<attribute name="RDC-TYP" value="2mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="0.11uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_744393230022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393230022?ae"/>
<attribute name="FRES" value="160MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="20A@40K"/>
<attribute name="ISAT" value="24.2A@30%"/>
<attribute name="L" value="0.22uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393230022"/>
<attribute name="RDC-MAX" value="3.78mOhm"/>
<attribute name="RDC-TYP" value="3.05mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_744393230047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393230047?ae"/>
<attribute name="FRES" value="95MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="14.5A@40K"/>
<attribute name="ISAT" value="12.8A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393230047"/>
<attribute name="RDC-MAX" value="6.69mOhm"/>
<attribute name="RDC-TYP" value="5.25mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_744393230056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393230056?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="12.7A@40K"/>
<attribute name="ISAT" value="12A@30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393230056"/>
<attribute name="RDC-MAX" value="8mOhm"/>
<attribute name="RDC-TYP" value="6.3mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_744393230068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393230068?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="12.6A@40K"/>
<attribute name="ISAT" value="11.8A@30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393230068"/>
<attribute name="RDC-MAX" value="9.63mOhm"/>
<attribute name="RDC-TYP" value="6.6mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_744393230082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393230082?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="10.8A@40K"/>
<attribute name="ISAT" value="11.6A@30%"/>
<attribute name="L" value="0.82uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393230082"/>
<attribute name="RDC-MAX" value="11mOhm"/>
<attribute name="RDC-TYP" value="9.3mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="0.82uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74439323010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439323010?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="10A@40K"/>
<attribute name="ISAT" value="10.2A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439323010"/>
<attribute name="RDC-MAX" value="13.44mOhm"/>
<attribute name="RDC-TYP" value="10.7mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74439323012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439323012?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="8.9A@40K"/>
<attribute name="ISAT" value="8.6A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439323012"/>
<attribute name="RDC-MAX" value="16.08mOhm"/>
<attribute name="RDC-TYP" value="12.5mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74439323015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439323015?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="7.8A@40K"/>
<attribute name="ISAT" value="8.4A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439323015"/>
<attribute name="RDC-MAX" value="18.48mOhm"/>
<attribute name="RDC-TYP" value="16.3mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74439323022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439323022?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="7.2A@40K"/>
<attribute name="ISAT" value="6.3A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439323022"/>
<attribute name="RDC-MAX" value="23.52mOhm"/>
<attribute name="RDC-TYP" value="20.2mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_7070" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-01-11&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_7070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74439387033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439387033?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="HEIGHT" value="7.1mm"/>
<attribute name="IRP" value="18.2A@40K"/>
<attribute name="ISAT" value="18.6A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="7.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439387033"/>
<attribute name="RDC-MAX" value="8.76mOhm"/>
<attribute name="RDC-TYP" value="6.4mOhm"/>
<attribute name="SIZE" value="7070"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="7.6mm"/>
</technology>
<technology name="_74439387047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439387047?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="HEIGHT" value="7.1mm"/>
<attribute name="IRP" value="15A@40K"/>
<attribute name="ISAT" value="16A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="7.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439387047"/>
<attribute name="RDC-MAX" value="11.52mOhm"/>
<attribute name="RDC-TYP" value="9.2mOhm"/>
<attribute name="SIZE" value="7070"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="7.6mm"/>
</technology>
<technology name="_74439387056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439387056?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="HEIGHT" value="7.1mm"/>
<attribute name="IRP" value="14.8A@40K"/>
<attribute name="ISAT" value="13.9A@30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="7.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439387056"/>
<attribute name="RDC-MAX" value="13.32mOhm"/>
<attribute name="RDC-TYP" value="12.4mOhm"/>
<attribute name="SIZE" value="7070"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="7.6mm"/>
</technology>
<technology name="_74439387068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439387068?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="HEIGHT" value="7.1mm"/>
<attribute name="IRP" value="12.5A@40K"/>
<attribute name="ISAT" value="13.7A@30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="7.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439387068"/>
<attribute name="RDC-MAX" value="16.8mOhm"/>
<attribute name="RDC-TYP" value="12.4mOhm"/>
<attribute name="SIZE" value="7070"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="7.6mm"/>
</technology>
<technology name="_74439387082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439387082?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="7.1mm"/>
<attribute name="IRP" value="11.2A@40K"/>
<attribute name="ISAT" value="12.7A@30%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="7.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439387082"/>
<attribute name="RDC-MAX" value="19.5mOhm"/>
<attribute name="RDC-TYP" value="14.5mOhm"/>
<attribute name="SIZE" value="7070"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="7.6mm"/>
</technology>
<technology name="_74439387100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439387100?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="HEIGHT" value="7.1mm"/>
<attribute name="IRP" value="9.6A@40K"/>
<attribute name="ISAT" value="12.6A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="7.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439387100"/>
<attribute name="RDC-MAX" value="22.92mOhm"/>
<attribute name="RDC-TYP" value="19mOhm"/>
<attribute name="SIZE" value="7070"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="7.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_1060P" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-04-14&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_1060P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744393665010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393665010?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IRP" value="48.1A@40K"/>
<attribute name="ISAT" value="55A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393665010"/>
<attribute name="RDC-MAX" value="1.9mOhm"/>
<attribute name="RDC-TYP" value="1.5mOhm"/>
<attribute name="SIZE" value="1060P"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393665012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393665012?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IRP" value="43A@40K"/>
<attribute name="ISAT" value="52A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393665012"/>
<attribute name="RDC-MAX" value="2.2mOhm"/>
<attribute name="RDC-TYP" value="1.8mOhm"/>
<attribute name="SIZE" value="1060P"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393665015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393665015?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IRP" value="39.4A@40K"/>
<attribute name="ISAT" value="47A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393665015"/>
<attribute name="RDC-MAX" value="2.2mOhm"/>
<attribute name="RDC-TYP" value="2.1mOhm"/>
<attribute name="SIZE" value="1060P"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393665022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393665022?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IRP" value="33A@40K"/>
<attribute name="ISAT" value="38A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393665022"/>
<attribute name="RDC-MAX" value="4mOhm"/>
<attribute name="RDC-TYP" value="3.1mOhm"/>
<attribute name="SIZE" value="1060P"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393665033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393665033?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IRP" value="27.9A@40K"/>
<attribute name="ISAT" value="30A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393665033"/>
<attribute name="RDC-MAX" value="5.6mOhm"/>
<attribute name="RDC-TYP" value="4.6mOhm"/>
<attribute name="SIZE" value="1060P"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393665047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393665047?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IRP" value="24.7A@40K"/>
<attribute name="ISAT" value="26.5A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393665047"/>
<attribute name="RDC-MAX" value="7.3mOhm"/>
<attribute name="RDC-TYP" value="5.7mOhm"/>
<attribute name="SIZE" value="1060P"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393665056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393665056?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IRP" value="23.9A@40K"/>
<attribute name="ISAT" value="21.5A@30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393665056"/>
<attribute name="RDC-MAX" value="8mOhm"/>
<attribute name="RDC-TYP" value="6.4mOhm"/>
<attribute name="SIZE" value="1060P"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393665068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393665068?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IRP" value="22.2A@40K"/>
<attribute name="ISAT" value="20A@30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393665068"/>
<attribute name="RDC-MAX" value="9mOhm"/>
<attribute name="RDC-TYP" value="7.1mOhm"/>
<attribute name="SIZE" value="1060P"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393665082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393665082?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IRP" value="19.4A@40K"/>
<attribute name="ISAT" value="19.5A@30%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393665082"/>
<attribute name="RDC-MAX" value="13mOhm"/>
<attribute name="RDC-TYP" value="10.7mOhm"/>
<attribute name="SIZE" value="1060P"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_744393665100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393665100?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IRP" value="15.3A@40K"/>
<attribute name="ISAT" value="18.5A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393665100"/>
<attribute name="RDC-MAX" value="15.4mOhm"/>
<attribute name="RDC-TYP" value="12.6mOhm"/>
<attribute name="SIZE" value="1060P"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_4030" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-09-18&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_4030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744393240033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393240033?ae"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="19.4A@40K"/>
<attribute name="ISAT" value="20A@30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393240033"/>
<attribute name="RDC-MAX" value="4mOhm"/>
<attribute name="RDC-TYP" value="3.1mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_744393240047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393240047?ae"/>
<attribute name="FRES" value="105MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="17.1A@40K"/>
<attribute name="ISAT" value="19.2A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393240047"/>
<attribute name="RDC-MAX" value="4.5mOhm"/>
<attribute name="RDC-TYP" value="3.9mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_744393240056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393240056?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="16.4A@40K"/>
<attribute name="ISAT" value="17A@30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393240056"/>
<attribute name="RDC-MAX" value="5.63mOhm"/>
<attribute name="RDC-TYP" value="4.1mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_744393240064">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393240064?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="15.2A@40K"/>
<attribute name="ISAT" value="17A@30%"/>
<attribute name="L" value="0.64uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393240064"/>
<attribute name="RDC-MAX" value="5.81mOhm"/>
<attribute name="RDC-TYP" value="4.8mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="0.64uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_744393240090">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393240090?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="14A@40K"/>
<attribute name="ISAT" value="15.6A@30%"/>
<attribute name="L" value="0.9uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393240090"/>
<attribute name="RDC-MAX" value="8.5mOhm"/>
<attribute name="RDC-TYP" value="6.1mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="0.9uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74439324010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439324010?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="11.1A@40K"/>
<attribute name="ISAT" value="12A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439324010"/>
<attribute name="RDC-MAX" value="10.32mOhm"/>
<attribute name="RDC-TYP" value="8.7mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74439324012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439324012?ae"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="10.9A@40K"/>
<attribute name="ISAT" value="11.8A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439324012"/>
<attribute name="RDC-MAX" value="10.8mOhm"/>
<attribute name="RDC-TYP" value="8.9mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74439324015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439324015?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="10.6A@40K"/>
<attribute name="ISAT" value="11.6A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439324015"/>
<attribute name="RDC-MAX" value="12.9mOhm"/>
<attribute name="RDC-TYP" value="10.1mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74439324022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439324022?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="7.8A@40K"/>
<attribute name="ISAT" value="10.5A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439324022"/>
<attribute name="RDC-MAX" value="19.8mOhm"/>
<attribute name="RDC-TYP" value="16.6mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74439324033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439324033?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="7.1A@40K"/>
<attribute name="ISAT" value="8.2A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439324033"/>
<attribute name="RDC-MAX" value="25.5mOhm"/>
<attribute name="RDC-TYP" value="20.2mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74439324047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439324047?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="5.3A@40K"/>
<attribute name="ISAT" value="5.8A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439324047"/>
<attribute name="RDC-MAX" value="36.96mOhm"/>
<attribute name="RDC-TYP" value="31.3mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_5050" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-06-13&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_5050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744393305033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393305033?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="HEIGHT" value="5.1mm"/>
<attribute name="IRP" value="9.2A@40K"/>
<attribute name="ISAT" value="12.3A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393305033"/>
<attribute name="RDC-MAX" value="16.6mOhm"/>
<attribute name="RDC-TYP" value="13.2mOhm"/>
<attribute name="SIZE" value="5050"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_744393305056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393305056?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="HEIGHT" value="5.1mm"/>
<attribute name="IRP" value="6.7A@40K"/>
<attribute name="ISAT" value="9.7A@30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393305056"/>
<attribute name="RDC-MAX" value="25.44mOhm"/>
<attribute name="RDC-TYP" value="21.8mOhm"/>
<attribute name="SIZE" value="5050"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_744393305068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393305068?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="HEIGHT" value="5.1mm"/>
<attribute name="IRP" value="6.6A@40K"/>
<attribute name="ISAT" value="6.9A@30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393305068"/>
<attribute name="RDC-MAX" value="29.28mOhm"/>
<attribute name="RDC-TYP" value="23.7mOhm"/>
<attribute name="SIZE" value="5050"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_744393305082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393305082?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="HEIGHT" value="5.1mm"/>
<attribute name="IRP" value="5.9A@40K"/>
<attribute name="ISAT" value="6.2A@30%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393305082"/>
<attribute name="RDC-MAX" value="34.68mOhm"/>
<attribute name="RDC-TYP" value="29.3mOhm"/>
<attribute name="SIZE" value="5050"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_744393305100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393305100?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="5.1mm"/>
<attribute name="IRP" value="5A@40K"/>
<attribute name="ISAT" value="6A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393305100"/>
<attribute name="RDC-MAX" value="43.08mOhm"/>
<attribute name="RDC-TYP" value="35.4mOhm"/>
<attribute name="SIZE" value="5050"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_744393305150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393305150?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="HEIGHT" value="5.1mm"/>
<attribute name="IRP" value="4A@40K"/>
<attribute name="ISAT" value="4.9A@30%"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393305150"/>
<attribute name="RDC-MAX" value="70.8mOhm"/>
<attribute name="RDC-TYP" value="56.8mOhm"/>
<attribute name="SIZE" value="5050"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_744393305220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393305220?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="HEIGHT" value="5.1mm"/>
<attribute name="IRP" value="3.5A@40K"/>
<attribute name="ISAT" value="4A@30%"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393305220"/>
<attribute name="RDC-MAX" value="90mOhm"/>
<attribute name="RDC-TYP" value="75mOhm"/>
<attribute name="SIZE" value="5050"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_8080" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-09-18&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_8080">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744393580068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393580068?ae"/>
<attribute name="FRES" value="62MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IRP" value="38A@40K"/>
<attribute name="ISAT" value="52.2A@30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="8.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393580068"/>
<attribute name="RDC-MAX" value="1.69mOhm"/>
<attribute name="RDC-TYP" value="1.41mOhm"/>
<attribute name="SIZE" value="8080"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="8.3mm"/>
</technology>
<technology name="_74439358010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439358010?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IRP" value="30.25A@40K"/>
<attribute name="ISAT" value="38.15A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="8.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439358010"/>
<attribute name="RDC-MAX" value="2.32mOhm"/>
<attribute name="RDC-TYP" value="2.1mOhm"/>
<attribute name="SIZE" value="8080"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="8.3mm"/>
</technology>
<technology name="_74439358015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439358015?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IRP" value="25.1A@40K"/>
<attribute name="ISAT" value="32A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="8.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439358015"/>
<attribute name="RDC-MAX" value="3.5mOhm"/>
<attribute name="RDC-TYP" value="2.91mOhm"/>
<attribute name="SIZE" value="8080"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="8.3mm"/>
</technology>
<technology name="_74439358022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439358022?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IRP" value="21.85A@40K"/>
<attribute name="ISAT" value="26.45A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="8.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439358022"/>
<attribute name="RDC-MAX" value="4.07mOhm"/>
<attribute name="RDC-TYP" value="3.7mOhm"/>
<attribute name="SIZE" value="8080"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="8.3mm"/>
</technology>
<technology name="_74439358033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439358033?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IRP" value="17.9A@40K"/>
<attribute name="ISAT" value="20.3A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="8.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439358033"/>
<attribute name="RDC-MAX" value="7.48mOhm"/>
<attribute name="RDC-TYP" value="6.8mOhm"/>
<attribute name="SIZE" value="8080"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="8.3mm"/>
</technology>
<technology name="_74439358047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439358047?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IRP" value="13.35A@40K"/>
<attribute name="ISAT" value="16.65A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="8.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439358047"/>
<attribute name="RDC-MAX" value="9.51mOhm"/>
<attribute name="RDC-TYP" value="8.65mOhm"/>
<attribute name="SIZE" value="8080"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="8.3mm"/>
</technology>
<technology name="_74439358068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439358068?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IRP" value="10.55A@40K"/>
<attribute name="ISAT" value="17.6A@30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="8.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439358068"/>
<attribute name="RDC-MAX" value="14.3mOhm"/>
<attribute name="RDC-TYP" value="13mOhm"/>
<attribute name="SIZE" value="8080"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="8.3mm"/>
</technology>
<technology name="_74439358100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439358100?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IRP" value="8.5A@40K"/>
<attribute name="ISAT" value="13.5A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="8.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439358100"/>
<attribute name="RDC-MAX" value="20.9mOhm"/>
<attribute name="RDC-TYP" value="19mOhm"/>
<attribute name="SIZE" value="8080"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="8.3mm"/>
</technology>
<technology name="_74439358150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439358150?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IRP" value="7.25A@40K"/>
<attribute name="ISAT" value="10.7A@30%"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="8.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439358150"/>
<attribute name="RDC-MAX" value="27.5mOhm"/>
<attribute name="RDC-TYP" value="25mOhm"/>
<attribute name="SIZE" value="8080"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="WIDTH" value="8.3mm"/>
</technology>
<technology name="_74439358220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439358220?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IRP" value="7.1A@40K"/>
<attribute name="ISAT" value="8.3A@30%"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="8.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439358220"/>
<attribute name="RDC-MAX" value="34.1mOhm"/>
<attribute name="RDC-TYP" value="30.7mOhm"/>
<attribute name="SIZE" value="8080"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="WIDTH" value="8.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_7030" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2024-01-11&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_7030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74439384010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439384010?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="23.7A@40K"/>
<attribute name="ISAT" value="25A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="7.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439384010"/>
<attribute name="RDC-MAX" value="5.16mOhm"/>
<attribute name="RDC-TYP" value="3.9mOhm"/>
<attribute name="SIZE" value="7030"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="7.6mm"/>
</technology>
<technology name="_74439384012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439384012?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="23.6A@40K"/>
<attribute name="ISAT" value="21.9A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="7.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439384012"/>
<attribute name="RDC-MAX" value="5.4mOhm"/>
<attribute name="RDC-TYP" value="4.2mOhm"/>
<attribute name="SIZE" value="7030"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="7.6mm"/>
</technology>
<technology name="_74439384015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439384015?ae"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="20.1A@40K"/>
<attribute name="ISAT" value="18.8A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="7.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439384015"/>
<attribute name="RDC-MAX" value="6.6mOhm"/>
<attribute name="RDC-TYP" value="5.1mOhm"/>
<attribute name="SIZE" value="7030"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="7.6mm"/>
</technology>
<technology name="_74439384022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439384022?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="16.7A@40K"/>
<attribute name="ISAT" value="13.8A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="7.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439384022"/>
<attribute name="RDC-MAX" value="10.56mOhm"/>
<attribute name="RDC-TYP" value="7.9mOhm"/>
<attribute name="SIZE" value="7030"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="7.6mm"/>
</technology>
<technology name="_74439384033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439384033?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="11.4A@40K"/>
<attribute name="ISAT" value="13.6A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="7.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439384033"/>
<attribute name="RDC-MAX" value="19.08mOhm"/>
<attribute name="RDC-TYP" value="14.4mOhm"/>
<attribute name="SIZE" value="7030"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="7.6mm"/>
</technology>
<technology name="_74439384047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439384047?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="9.5A@40K"/>
<attribute name="ISAT" value="11A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="7.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439384047"/>
<attribute name="RDC-MAX" value="24.96mOhm"/>
<attribute name="RDC-TYP" value="19.8mOhm"/>
<attribute name="SIZE" value="7030"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="7.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_4040" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-11&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_4040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74439325033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439325033?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="4.1mm"/>
<attribute name="IRP" value="7.2A@40K"/>
<attribute name="ISAT" value="7.9A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439325033"/>
<attribute name="RDC-MAX" value="25mOhm"/>
<attribute name="RDC-TYP" value="20.4mOhm"/>
<attribute name="SIZE" value="4040"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74439325047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439325047?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="4.1mm"/>
<attribute name="IRP" value="5.7A@40K"/>
<attribute name="ISAT" value="5.7A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439325047"/>
<attribute name="RDC-MAX" value="34.8mOhm"/>
<attribute name="RDC-TYP" value="26.5mOhm"/>
<attribute name="SIZE" value="4040"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74439325056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439325056?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="HEIGHT" value="4.1mm"/>
<attribute name="IRP" value="5.1A@40K"/>
<attribute name="ISAT" value="5.5A@30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439325056"/>
<attribute name="RDC-MAX" value="44.4mOhm"/>
<attribute name="RDC-TYP" value="34.2mOhm"/>
<attribute name="SIZE" value="4040"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74439325068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439325068?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="HEIGHT" value="4.1mm"/>
<attribute name="IRP" value="4.1A@40K"/>
<attribute name="ISAT" value="4.9A@30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439325068"/>
<attribute name="RDC-MAX" value="55mOhm"/>
<attribute name="RDC-TYP" value="42.3mOhm"/>
<attribute name="SIZE" value="4040"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_6060" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-05-12&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_6060">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74439346010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346010?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="20.95A@40K"/>
<attribute name="ISAT" value="24A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439346010"/>
<attribute name="RDC-MAX" value="4.07mOhm"/>
<attribute name="RDC-TYP" value="3.39mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439346012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346012?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="20.5A@40K"/>
<attribute name="ISAT" value="20A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439346012"/>
<attribute name="RDC-MAX" value="4.38mOhm"/>
<attribute name="RDC-TYP" value="3.65mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439346015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346015?ae"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="19.35A@40K"/>
<attribute name="ISAT" value="20.5A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439346015"/>
<attribute name="RDC-MAX" value="4.68mOhm"/>
<attribute name="RDC-TYP" value="3.9mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439346018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346018?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="17.35A@40K"/>
<attribute name="ISAT" value="18.3A@30%"/>
<attribute name="L" value="1.8uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439346018"/>
<attribute name="RDC-MAX" value="5.64mOhm"/>
<attribute name="RDC-TYP" value="4.7mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439346022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346022?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="15.75A@40K"/>
<attribute name="ISAT" value="19.5A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439346022"/>
<attribute name="RDC-MAX" value="6.69mOhm"/>
<attribute name="RDC-TYP" value="5.58mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439346033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346033?ae"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="10.7A@40K"/>
<attribute name="ISAT" value="15A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439346033"/>
<attribute name="RDC-MAX" value="12.99mOhm"/>
<attribute name="RDC-TYP" value="10.83mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439346047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346047?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="9.6A@40K"/>
<attribute name="ISAT" value="13A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439346047"/>
<attribute name="RDC-MAX" value="14.3mOhm"/>
<attribute name="RDC-TYP" value="13mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439346056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346056?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="8.9A@40K"/>
<attribute name="ISAT" value="12.1A@30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439346056"/>
<attribute name="RDC-MAX" value="16.5mOhm"/>
<attribute name="RDC-TYP" value="15mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439346068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346068?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="8.1A@40K"/>
<attribute name="ISAT" value="11.3A@30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439346068"/>
<attribute name="RDC-MAX" value="19.36mOhm"/>
<attribute name="RDC-TYP" value="17.6mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439346082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346082?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="6.95A@40K"/>
<attribute name="ISAT" value="9.3A@30%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439346082"/>
<attribute name="RDC-MAX" value="25.3mOhm"/>
<attribute name="RDC-TYP" value="23mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439346100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346100?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="6.4A@40K"/>
<attribute name="ISAT" value="9.7A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439346100"/>
<attribute name="RDC-MAX" value="29.15mOhm"/>
<attribute name="RDC-TYP" value="26.5mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
<technology name="_74439346150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346150?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="6.1mm"/>
<attribute name="IRP" value="4.9A@40K"/>
<attribute name="ISAT" value="7.4A@30%"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="6.65mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439346150"/>
<attribute name="RDC-MAX" value="46.2mOhm"/>
<attribute name="RDC-TYP" value="42mOhm"/>
<attribute name="SIZE" value="6060"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="WIDTH" value="6.45mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_5030" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI Performance:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -55°C up to +150°C
&lt;br&gt;Optimized for ultra low RDC and AC losses to enhance efficiency and minimize self-heating
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WE-XHMI:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;Reliable inductor featuring a balanced combination of low losses and high current capability
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20FAMILY-WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-09-18&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744393340016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393340016?ae"/>
<attribute name="FRES" value="195MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="24.2A@40K"/>
<attribute name="ISAT" value="39.9A@30%"/>
<attribute name="L" value="0.16uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393340016"/>
<attribute name="RDC-MAX" value="2.75mOhm"/>
<attribute name="RDC-TYP" value="2.1mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="0.16uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_744393340033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393340033?ae"/>
<attribute name="FRES" value="105MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="21.2A@40K"/>
<attribute name="ISAT" value="33.3A@30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393340033"/>
<attribute name="RDC-MAX" value="3.88mOhm"/>
<attribute name="RDC-TYP" value="3.01mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_744393340056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393340056?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="18.3A@40K"/>
<attribute name="ISAT" value="24.4A@30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393340056"/>
<attribute name="RDC-MAX" value="4.81mOhm"/>
<attribute name="RDC-TYP" value="3.99mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_744393340068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393340068?ae"/>
<attribute name="FRES" value="62MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="15.7A@40K"/>
<attribute name="ISAT" value="17.7A@30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744393340068"/>
<attribute name="RDC-MAX" value="4.88mOhm"/>
<attribute name="RDC-TYP" value="4.09mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_74439334010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439334010?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="14.7A@40K"/>
<attribute name="ISAT" value="13.4A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439334010"/>
<attribute name="RDC-MAX" value="8.4mOhm"/>
<attribute name="RDC-TYP" value="6.3mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_74439334012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439334012?ae"/>
<attribute name="FRES" value="46MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="13.6A@40K"/>
<attribute name="ISAT" value="13.3A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439334012"/>
<attribute name="RDC-MAX" value="8.76mOhm"/>
<attribute name="RDC-TYP" value="6.6mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_74439334015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439334015?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="12A@40K"/>
<attribute name="ISAT" value="13A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439334015"/>
<attribute name="RDC-MAX" value="20.56mOhm"/>
<attribute name="RDC-TYP" value="8mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_74439334018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439334018?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="10.8A@40K"/>
<attribute name="ISAT" value="12.9A@30%"/>
<attribute name="L" value="1.8uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439334018"/>
<attribute name="RDC-MAX" value="10.8mOhm"/>
<attribute name="RDC-TYP" value="9.1mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_74439334022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439334022?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="10.3A@40K"/>
<attribute name="ISAT" value="12.8A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439334022"/>
<attribute name="RDC-MAX" value="14.52mOhm"/>
<attribute name="RDC-TYP" value="11.3mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_74439334033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439334033?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="8.2A@40K"/>
<attribute name="ISAT" value="8A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439334033"/>
<attribute name="RDC-MAX" value="19.92mOhm"/>
<attribute name="RDC-TYP" value="16.3mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
<technology name="_74439334047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439334047?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IRP" value="6.8A@40K"/>
<attribute name="ISAT" value="7.5A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="5.55mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74439334047"/>
<attribute name="RDC-MAX" value="27.96mOhm"/>
<attribute name="RDC-TYP" value="22.9mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="5.35mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
