<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Optoelectronic Components - IC LEDs - WL-ICLED&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024b, 2024-09-10&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-ILED_5050_PLCC6">
</package>
<package name="1311610030140">
</package>
<package name="1315050930002">
<description>&lt;b&gt;WL-ICLED Integrated Controller within LED
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
Size: PLCC 4 5050, SMT, 4pins
&lt;br&gt;LXWXH=5.4X5X1.58mm</description>
</package>
<package name="1313210530000">
<description>&lt;b&gt;WL-ICLED Integrated Controller within LED
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
Size: Side View 3210, SMT, 4pins
&lt;br&gt;LXWXH=3.2X1.5X1mm</description>
</package>
<package name="1312121320437">
<description>&lt;b&gt;WL-ICLED Integrated Controller within LED
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
Size: PLCC 6 2121, SMT, 6pins
&lt;br&gt;LXWXH=2.2X2.2X1.1mm</description>
</package>
<package name="1312020030000">
<description>&lt;b&gt;WL-ICLED Integrated Controller within LED
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
Size: Chip LED 2020, SMT, 4pins
&lt;br&gt;LXWXH=2X2X0.9mm</description>
</package>
</packages>
<symbols>
<symbol name="1311610030140">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="1315050930002">
<pin name="VDD" direction="pas"/>
<pin name="DOUT" direction="pas"/>
<pin name="DIN" direction="pas"/>
<pin name="VSS" direction="pas"/>
</symbol>
<symbol name="1312020030000">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="1315050930246">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="1313210530000">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="1312121320437">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="1315050930246" prefix="D">
<description>&lt;b&gt;WL-ICLED Integrated Controller within LED&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Compatible with open source libraries such as FastLED
&lt;br&gt;Ready to use with pre-programmed IC
&lt;br&gt;0% to 100% digital dimming via command
&lt;br&gt;Individual pixel colour and brightness control
&lt;br&gt;Full RGB spectrum
&lt;br&gt;Signal control system

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Signal control system
&lt;br&gt;Full-color matrix display
&lt;br&gt;Audio and gaming systems
&lt;br&gt;Indoor illumination
&lt;br&gt;E-mobility
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o752565v209%20Family-WL-ICLED.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o752565v209%20Family-WL-ICLED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-ICLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WL-ICLED&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-09-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1315050930246"/>
</gates>
<devices>
<device name="" package="WL-ILED_5050_PLCC6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1315050930246?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="470nm &amp; 525nm &amp; 625nm"/>
<attribute name="EMITTING-COLOR" value="Blue &amp; Green &amp; Red"/>
<attribute name="FPWM" value="20kHz"/>
<attribute name="IC-OUTPUT-CURRENT" value="21mA"/>
<attribute name="LUMINOUS-INTENSITY" value="400mcd &amp; 1800mcd &amp; 800mcd"/>
<attribute name="PART-NUMBER" value=" 1315050930246 "/>
<attribute name="PEAK-WAVELENGTH" value="465nm &amp; 520nm &amp; 630nm"/>
<attribute name="VALUE" value=" 1315050930246 "/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1311610030140" prefix="D">
<description>&lt;b&gt;WL-ICLED Integrated Controller within LED&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Compatible with open source libraries such as FastLED
&lt;br&gt;Ready to use with pre-programmed IC
&lt;br&gt;0% to 100% digital dimming via command
&lt;br&gt;Individual pixel colour and brightness control
&lt;br&gt;Full RGB spectrum
&lt;br&gt;Signal control system

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Signal control system
&lt;br&gt;Full-color matrix display
&lt;br&gt;Audio and gaming systems
&lt;br&gt;Indoor illumination
&lt;br&gt;E-mobility
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o752565v209%20Family-WL-ICLED.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o752565v209%20Family-WL-ICLED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-ICLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WL-ICLED&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-09-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1311610030140"/>
</gates>
<devices>
<device name="" package="1311610030140">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1311610030140?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="470nm &amp; 525nm &amp; 625nm"/>
<attribute name="EMITTING-COLOR" value="Green &amp; Blue &amp; Red"/>
<attribute name="FPWM" value="20kHz"/>
<attribute name="IC-OUTPUT-CURRENT" value="6mA"/>
<attribute name="LUMINOUS-INTENSITY" value="50mcd &amp; 120mcd &amp; 80mcd"/>
<attribute name="PART-NUMBER" value=" 1311610030140 "/>
<attribute name="PEAK-WAVELENGTH" value="465nm &amp; 520nm &amp; 630nm"/>
<attribute name="VALUE" value=" 1311610030140 "/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1315050930002" prefix="D">
<description>&lt;b&gt;WL-ICLED Integrated Controller within LED&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Compatible with open source libraries such as FastLED
&lt;br&gt;Ready to use with pre-programmed IC
&lt;br&gt;0% to 100% digital dimming via command
&lt;br&gt;Individual pixel colour and brightness control
&lt;br&gt;Full RGB spectrum
&lt;br&gt;Signal control system

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Signal control system
&lt;br&gt;Full-color matrix display
&lt;br&gt;Audio and gaming systems
&lt;br&gt;Indoor illumination
&lt;br&gt;E-mobility
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o752565v209%20Family-WL-ICLED.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o752565v209%20Family-WL-ICLED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-ICLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WL-ICLED&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-02-23 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1315050930002"/>
</gates>
<devices>
<device name="" package="1315050930002">
<connects>
<connect gate="G$1" pin="DIN" pad="2"/>
<connect gate="G$1" pin="DOUT" pad="4"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1315050930002?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="470nm &amp; 525nm &amp; 625nm"/>
<attribute name="EMITTING-COLOR" value="Green &amp; Red &amp; Blue"/>
<attribute name="FPWM" value="2.5kHz"/>
<attribute name="IC-OUTPUT-CURRENT" value="13mA"/>
<attribute name="LUMINOUS-INTENSITY" value="260mcd &amp; 1300mcd &amp; 450mcd"/>
<attribute name="PART-NUMBER" value=" 1315050930002 "/>
<attribute name="PEAK-WAVELENGTH" value="465nm &amp; 520nm &amp; 630nm"/>
<attribute name="VALUE" value=" 1315050930002 "/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1312121320437" prefix="D">
<description>&lt;b&gt;WL-ICLED Integrated Controller within LED&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Compatible with open source libraries such as FastLED
&lt;br&gt;Ready to use with pre-programmed IC
&lt;br&gt;0% to 100% digital dimming via command
&lt;br&gt;Individual pixel colour and brightness control
&lt;br&gt;Full RGB spectrum
&lt;br&gt;Signal control system

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Signal control system
&lt;br&gt;Full-color matrix display
&lt;br&gt;Audio and gaming systems
&lt;br&gt;Indoor illumination
&lt;br&gt;E-mobility
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o752565v209%20Family-WL-ICLED.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o752565v209%20Family-WL-ICLED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-ICLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WL-ICLED&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-02-23 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1312121320437"/>
</gates>
<devices>
<device name="" package="1312121320437">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1312121320437?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="470nm &amp; 525nm &amp; 625nm"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Green &amp; Blue"/>
<attribute name="FPWM" value="0.6kHz"/>
<attribute name="IC-OUTPUT-CURRENT" value="20mA"/>
<attribute name="LUMINOUS-INTENSITY" value="240mcd &amp; 1000mcd &amp; 600mcd"/>
<attribute name="PART-NUMBER" value=" 1312121320437 "/>
<attribute name="PEAK-WAVELENGTH" value="465nm &amp; 520nm &amp; 630nm"/>
<attribute name="VALUE" value=" 1312121320437 "/>
<attribute name="VIEWING-ANGLE" value="110°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1313210530000" prefix="D">
<description>&lt;b&gt;WL-ICLED Integrated Controller within LED&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Compatible with open source libraries such as FastLED
&lt;br&gt;Ready to use with pre-programmed IC
&lt;br&gt;0% to 100% digital dimming via command
&lt;br&gt;Individual pixel colour and brightness control
&lt;br&gt;Full RGB spectrum
&lt;br&gt;Signal control system

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Signal control system
&lt;br&gt;Full-color matrix display
&lt;br&gt;Audio and gaming systems
&lt;br&gt;Indoor illumination
&lt;br&gt;E-mobility
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o752565v209%20Family-WL-ICLED.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o752565v209%20Family-WL-ICLED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-ICLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WL-ICLED&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-02-23 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1313210530000"/>
</gates>
<devices>
<device name="" package="1313210530000">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1313210530000?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="470nm &amp; 525nm &amp; 625nm"/>
<attribute name="EMITTING-COLOR" value="Green &amp; Red &amp; Blue"/>
<attribute name="FPWM" value="5kHz"/>
<attribute name="IC-OUTPUT-CURRENT" value="5.5mA"/>
<attribute name="LUMINOUS-INTENSITY" value="50mcd &amp; 120mcd &amp; 80mcd"/>
<attribute name="PART-NUMBER" value=" 1313210530000 "/>
<attribute name="PEAK-WAVELENGTH" value="465nm &amp; 520nm &amp; 630nm"/>
<attribute name="VALUE" value=" 1313210530000 "/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1312020030000" prefix="D">
<description>&lt;b&gt;WL-ICLED Integrated Controller within LED&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Compatible with open source libraries such as FastLED
&lt;br&gt;Ready to use with pre-programmed IC
&lt;br&gt;0% to 100% digital dimming via command
&lt;br&gt;Individual pixel colour and brightness control
&lt;br&gt;Full RGB spectrum
&lt;br&gt;Signal control system

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Signal control system
&lt;br&gt;Full-color matrix display
&lt;br&gt;Audio and gaming systems
&lt;br&gt;Indoor illumination
&lt;br&gt;E-mobility
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o752565v209%20Family-WL-ICLED.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o752565v209%20Family-WL-ICLED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-ICLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WL-ICLED&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-02-23 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1312020030000"/>
</gates>
<devices>
<device name="" package="1312020030000">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1312020030000?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="470nm &amp; 525nm &amp; 625nm"/>
<attribute name="EMITTING-COLOR" value="Green &amp; Red &amp; Blue"/>
<attribute name="FPWM" value="5kHz"/>
<attribute name="IC-OUTPUT-CURRENT" value="5.5mA"/>
<attribute name="LUMINOUS-INTENSITY" value="50mcd &amp; 120mcd &amp; 80mcd"/>
<attribute name="PART-NUMBER" value=" 1312020030000 "/>
<attribute name="PEAK-WAVELENGTH" value="465nm &amp; 520nm &amp; 630nm"/>
<attribute name="VALUE" value=" 1312020030000 "/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
