<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Optoelectronic Components - Optocoupler - Optocoupler Darlington - WL-OCDA&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt;

&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-06-20&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-OCDA_SOP4">
<description>&lt;b&gt; WL-OCDA Optocoupler Darlington

&lt;/b&gt;&lt;br&gt;Size : SOP4, SMT, 4pins</description>
</package>
<package name="WL-OCDA_DIP4_SL-TYPE">
<description>&lt;b&gt; WL-OCDA Optocoupler Darlington

&lt;/b&gt;&lt;br&gt;Size : DIP 4 SL-Type, SMT, 4pins</description>
</package>
<package name="WL-OCDA_DIP4_S-TYPE">
<description>&lt;b&gt; WL-OCDA Optocoupler Darlington

&lt;/b&gt;&lt;br&gt;Size : DIP 4 S-Type, SMT, 4pins</description>
</package>
<package name="WL-OCDA_DIP4_M-TYPE">
<description>&lt;b&gt; WL-OCDA Optocoupler Darlington

&lt;/b&gt;&lt;br&gt;Size : DIP 4 M-Type, THT, 4pins</description>
</package>
<package name="WL-OCDA_DIP4_STANDARD">
<description>&lt;b&gt; WL-OCDA Optocoupler Darlington

&lt;/b&gt;&lt;br&gt;Size : DIP 4 Standard, THT, 4pins</description>
</package>
<package name="WL-OCDA_DIP4_SLM-TYPE">
<description>&lt;b&gt; WL-OCDA Optocoupler Darlington
 
&lt;/b&gt;&lt;br&gt;Size : DIP 4 SLM-Type, SMT, 4pins</description>
</package>
</packages>
<symbols>
<symbol name="WL-OCDA_SERIES_355">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WL-OCDA_SERIES_815">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WL-OCDA_SERIES_352">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-OCDA_SERIES_352" prefix="Q">
<description>&lt;b&gt;WL-OCDA Optocoupler Darlington 
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristics
&lt;br&gt;&lt;/b&gt;&lt;br&gt;High isolation Voltage
&lt;br&gt; Good stability of inner isolation
&lt;br&gt; Stable CTR in full operation
&lt;br&gt; Different leadframe options

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
 
&lt;b&gt;Applications
&lt;br&gt;&lt;/b&gt;&lt;br&gt;Power Supply, charger 
&lt;br&gt;Computers &amp; Microprocessors 
&lt;br&gt;Office equipment 
&lt;br&gt;Instrumental applications, machines 
&lt;br&gt;Ammeter, Smart Meter 

&lt;/b&gt;&lt;br&gt;         
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o495458v209%20Group_815%2B352.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o495458v209%20Group_815%2B352.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-OCDA_OPTOCOUPLER_PHOTOTRANSISTOR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-OCDA_OPTOCOUPLER_PHOTOTRANSISTOR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu, 2022-06-21
 &lt;br&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCDA_SERIES_352"/>
</gates>
<devices>
<device name="" package="WL-OCDA_SOP4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_141352145000">
<attribute name="CTR-MAX" value=" 150 "/>
<attribute name="CTR-MIN" value="1000%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/141352145000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 141352145000 "/>
<attribute name="TC-CTR" value="IF = 1mA,VCE = 2 V"/>
<attribute name="VALUE" value=" 141352145000 "/>
<attribute name="VCE" value="350V"/>
<attribute name="VISO" value="3750(V(RMS))"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-OCDA_SERIES_355" prefix="Q">
<description>&lt;b&gt;WL-OCDA Optocoupler Darlington 
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristics
&lt;br&gt;&lt;/b&gt;&lt;br&gt;High isolation Voltage
&lt;br&gt; Good stability of inner isolation
&lt;br&gt; Stable CTR in full operation
&lt;br&gt; Different leadframe options

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
 
&lt;b&gt;Applications
&lt;br&gt;&lt;/b&gt;&lt;br&gt;Power Supply, charger 
&lt;br&gt;Computers &amp; Microprocessors 
&lt;br&gt;Office equipment 
&lt;br&gt;Instrumental applications, machines 
&lt;br&gt;Ammeter, Smart Meter 

&lt;/b&gt;&lt;br&gt;         
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o495458v209%20Group_815%2B352.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o495458v209%20Group_815%2B352.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-OCDA_OPTOCOUPLER_PHOTOTRANSISTOR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-OCDA_OPTOCOUPLER_PHOTOTRANSISTOR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu, 2022-06-21
 &lt;br&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCDA_SERIES_355"/>
</gates>
<devices>
<device name="" package="WL-OCDA_SOP4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_141355145000">
<attribute name="CTR-MAX" value=" 75 "/>
<attribute name="CTR-MIN" value="600%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/141355145000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 141355145000 "/>
<attribute name="TC-CTR" value="IF = 1mA,VCE = 2 V"/>
<attribute name="VALUE" value=" 141355145000 "/>
<attribute name="VCE" value="40V"/>
<attribute name="VISO" value="3750(V(RMS))"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-OCDA_SERIES_815" prefix="Q">
<description>&lt;b&gt;WL-OCDA Optocoupler Darlington 
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristics
&lt;br&gt;&lt;/b&gt;&lt;br&gt;High isolation Voltage
&lt;br&gt; Good stability of inner isolation
&lt;br&gt; Stable CTR in full operation
&lt;br&gt; Different leadframe options

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
 
&lt;b&gt;Applications
&lt;br&gt;&lt;/b&gt;&lt;br&gt;Power Supply, charger 
&lt;br&gt;Computers &amp; Microprocessors 
&lt;br&gt;Office equipment 
&lt;br&gt;Instrumental applications, machines 
&lt;br&gt;Ammeter, Smart Meter 

&lt;/b&gt;&lt;br&gt;         
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o495458v209%20Group_815%2B352.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o495458v209%20Group_815%2B352.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-OCDA_OPTOCOUPLER_PHOTOTRANSISTOR/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-OCDA_OPTOCOUPLER_PHOTOTRANSISTOR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu, 2022-06-21
 &lt;br&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCDA_SERIES_815"/>
</gates>
<devices>
<device name="_DIP4_M-TYPE" package="WL-OCDA_DIP4_M-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_141815141010">
<attribute name="CTR-MAX" value=" 75 "/>
<attribute name="CTR-MIN" value="600%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/141815141010?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 141815141010 "/>
<attribute name="TC-CTR" value="IF = 1mA,VCE = 2 V"/>
<attribute name="VALUE" value=" 141815141010 "/>
<attribute name="VCE" value="40V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP4_SLM-TYPE" package="WL-OCDA_DIP4_SLM-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_141815144000">
<attribute name="CTR-MAX" value=" 75 "/>
<attribute name="CTR-MIN" value="600%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/141815144000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 141815144000 "/>
<attribute name="TC-CTR" value="IF = 1mA,VCE = 2 V"/>
<attribute name="VALUE" value=" 141815144000 "/>
<attribute name="VCE" value="40V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP4_SL-TYPE" package="WL-OCDA_DIP4_SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_141815143000">
<attribute name="CTR-MAX" value=" 75 "/>
<attribute name="CTR-MIN" value="600%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/141815143000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 141815143000 "/>
<attribute name="TC-CTR" value="IF = 1mA,VCE = 2 V"/>
<attribute name="VALUE" value=" 141815143000 "/>
<attribute name="VCE" value="40V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP4_STANDARD" package="WL-OCDA_DIP4_STANDARD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_141815140010">
<attribute name="CTR-MAX" value=" 75 "/>
<attribute name="CTR-MIN" value="600%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/141815140010?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 141815140010 "/>
<attribute name="TC-CTR" value="IF = 1mA,VCE = 2 V"/>
<attribute name="VALUE" value=" 141815140010 "/>
<attribute name="VCE" value="40V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP4_S-TYPE" package="WL-OCDA_DIP4_S-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_141815142000">
<attribute name="CTR-MAX" value=" 75 "/>
<attribute name="CTR-MIN" value="600%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/141815142000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 141815142000 "/>
<attribute name="TC-CTR" value="IF = 1mA,VCE = 2 V"/>
<attribute name="VALUE" value=" 141815142000 "/>
<attribute name="VCE" value="40V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
