<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>Würth Elektronik - Optoelectronic Components - Optocoupler - WL-OCHS Optocoupler High Speed

Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, 
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. 
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. 
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. 

Please contact us for more information: libraries@we-online.com 

Würth Elektronik eiSos GmbH &amp; Co. KG
EMC &amp; Inductive Solutions
www.we-online.com

Fusion360, Library Revision 2026a, 2026-08-06
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-OCHS_SOP5-SL-TYPE">
<description>WL-OCHS Optocoupler High Speed

Size: SOP-5 SL-Type, SMT, 5pins
LXWXH=4.55X4.1X2.1mm</description>
</package>
<package name="WL-OCHS_SOP8-SL-TYPE">
<description>WL-OCHS Optocoupler High Speed

Size: SOP-8 SL-Type, SMT, 8pins
LXWXH=4.05X5.08X3.18mm</description>
</package>
<package name="WL-OCHS_DIP8_STANDARD">
<description>WL-OCHS Optocoupler High Speed

Size: DIP-8 STANDARD, THT, 8pins
LXWXH=6.5X9.68X3.5mm</description>
</package>
<package name="WL-OCHS_DIP8_SL-TYPE">
<description>WL-OCHS Optocoupler High Speed

Size: DIP-8 SL-Type, SMT, 8pins
LXWXH=8.57X9.68X4.46mm</description>
</package>
</packages>
<symbols>
<symbol name="WL-OCHS_SOP5_1436X1155110">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WL-OCHS_SOP8_14363X285210">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="WL-OCHS_SOP5_1435X1155110">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WL-OCHS_SOP8_14353X285110">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="WL-OCPT_DIP8_14313X18X1X0">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="WL-OCHS_SOP8_143501185110">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="WL-OCHS_SOP8_1436X1185210">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="WL-OCPT_DIP8_14313718X2X0">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="143601155210" prefix="Q">
<description>WL-OCHS SOP-5

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-SOP-5
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCHS_SOP5_1436X1155110"/>
</gates>
<devices>
<device name="" package="WL-OCHS_SOP5-SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="5 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143601155210?ae"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="ITH-TYP" value="2.5 mA"/>
<attribute name="LENGTH" value="4.55mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="MPN" value="143601155210"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PACKAGE-TYPE" value="SOP5"/>
<attribute name="TPLH" value="41 nsV"/>
<attribute name="VALUE" value="143601155210"/>
<attribute name="VISO" value="3750 V (RMS)"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="143611155210" prefix="Q">
<description>WL-OCHS SOP-5

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-SOP-5
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCHS_SOP5_1436X1155110"/>
</gates>
<devices>
<device name="" package="WL-OCHS_SOP5-SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="20 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143611155210?ae"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="ITH-TYP" value="2.5 mA"/>
<attribute name="LENGTH" value="4.55mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="MPN" value="143611155210"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PACKAGE-TYPE" value="SOP5"/>
<attribute name="TPLH" value="41 nsV"/>
<attribute name="VALUE" value="143611155210"/>
<attribute name="VISO" value="3750 V (RMS)"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="143501185110" prefix="Q">
<description>WL-OCHS SOP-8

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-SOP-8
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCHS_SOP8_143501185110"/>
</gates>
<devices>
<device name="" package="WL-OCHS_SOP8-SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="5 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143501185110?ae"/>
<attribute name="HEIGHT" value="3.18mm"/>
<attribute name="LENGTH" value="4.05mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="MPN" value="143501185110"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +110 °C"/>
<attribute name="PACKAGE-TYPE" value="SOP8"/>
<attribute name="TPLH" value="150 nsV"/>
<attribute name="VALUE" value="143501185110"/>
<attribute name="VISO" value="3750 V (RMS)"/>
<attribute name="WIDTH" value="5.08mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="143531285110" prefix="Q">
<description>WL-OCHS SOP-8

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-SOP-8
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCHS_SOP8_14353X285110"/>
</gates>
<devices>
<device name="" package="WL-OCHS_SOP8-SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="1 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143531285110?ae"/>
<attribute name="HEIGHT" value="3.18mm"/>
<attribute name="LENGTH" value="4.05mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="MPN" value="143531285110"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +110 °C"/>
<attribute name="PACKAGE-TYPE" value="SOP8"/>
<attribute name="TPLH" value="600 nsV"/>
<attribute name="VALUE" value="143531285110"/>
<attribute name="VISO" value="3750 V (RMS)"/>
<attribute name="WIDTH" value="5.08mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="143630285210" prefix="Q">
<description>WL-OCHS SOP-8

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-SOP-8
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCHS_SOP8_14363X285210"/>
</gates>
<devices>
<device name="" package="WL-OCHS_SOP8-SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="5 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143630285210?ae"/>
<attribute name="HEIGHT" value="3.18mm"/>
<attribute name="ITH-TYP" value="2.4 mA"/>
<attribute name="LENGTH" value="4.05mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="MPN" value="143630285210"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PACKAGE-TYPE" value="SOP8"/>
<attribute name="TPLH" value="48 nsV"/>
<attribute name="VALUE" value="143630285210"/>
<attribute name="VISO" value="3750 V (RMS)"/>
<attribute name="WIDTH" value="5.08mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="143136180100" prefix="Q">
<description>WL-OCHS DIP-8

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-DIP-8
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCPT_DIP8_14313X18X1X0"/>
</gates>
<devices>
<device name="" package="WL-OCHS_DIP8_STANDARD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="1 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143136180100?ae"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="MPN" value="143136180100"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +110 °C"/>
<attribute name="PACKAGE-TYPE" value="DIP 8, Standard"/>
<attribute name="TPLH" value="600 nsV"/>
<attribute name="VALUE" value="143136180100"/>
<attribute name="VISO" value="5000 V (RMS)"/>
<attribute name="WIDTH" value="9.68mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="143501155110" prefix="Q">
<description>WL-OCHS SOP-5

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-SOP-5
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCHS_SOP5_1435X1155110"/>
</gates>
<devices>
<device name="" package="WL-OCHS_SOP5-SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="5 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143501155110?ae"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.55mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="MPN" value="143501155110"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +110 °C"/>
<attribute name="PACKAGE-TYPE" value="SOP5"/>
<attribute name="TPLH" value="150 nsV"/>
<attribute name="VALUE" value="143501155110"/>
<attribute name="VISO" value="3750 V (RMS)"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="143137180200" prefix="Q">
<description>WL-OCHS DIP-8

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-DIP-8
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCPT_DIP8_14313718X2X0"/>
</gates>
<devices>
<device name="" package="WL-OCHS_DIP8_STANDARD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="5 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143137180200?ae"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="ITH-TYP" value="3 mA"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="MPN" value="143137180200"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PACKAGE-TYPE" value="DIP 8, Standard"/>
<attribute name="TPLH" value="41 nsV"/>
<attribute name="VALUE" value="143137180200"/>
<attribute name="VISO" value="5000 V (RMS)"/>
<attribute name="WIDTH" value="9.68mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="143511155110" prefix="Q">
<description>WL-OCHS SOP-5

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-SOP-5
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCHS_SOP5_1435X1155110"/>
</gates>
<devices>
<device name="" package="WL-OCHS_SOP5-SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="15 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143511155110?ae"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.55mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="MPN" value="143511155110"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +110 °C"/>
<attribute name="PACKAGE-TYPE" value="SOP5"/>
<attribute name="TPLH" value="150 nsV"/>
<attribute name="VALUE" value="143511155110"/>
<attribute name="VISO" value="3750 V (RMS)"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="143601185210" prefix="Q">
<description>WL-OCHS SOP-8

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-SOP-8
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCHS_SOP8_1436X1185210"/>
</gates>
<devices>
<device name="" package="WL-OCHS_SOP8-SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="5 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143601185210?ae"/>
<attribute name="HEIGHT" value="3.18mm"/>
<attribute name="ITH-TYP" value="3 mA"/>
<attribute name="LENGTH" value="4.05mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="MPN" value="143601185210"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGE-TYPE" value="SOP8"/>
<attribute name="TPLH" value="41 nsV"/>
<attribute name="VALUE" value="143601185210"/>
<attribute name="VISO" value="3750 V (RMS)"/>
<attribute name="WIDTH" value="5.08mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="143530285110" prefix="Q">
<description>WL-OCHS SOP-8

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-SOP-8
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCHS_SOP8_14353X285110"/>
</gates>
<devices>
<device name="" package="WL-OCHS_SOP8-SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="1 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143530285110?ae"/>
<attribute name="HEIGHT" value="3.18mm"/>
<attribute name="LENGTH" value="4.05mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="MPN" value="143530285110"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +110 °C"/>
<attribute name="PACKAGE-TYPE" value="SOP8"/>
<attribute name="TPLH" value="600 nsV"/>
<attribute name="VALUE" value="143530285110"/>
<attribute name="VISO" value="3750 V (RMS)"/>
<attribute name="WIDTH" value="5.08mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="143631285210" prefix="Q">
<description>WL-OCHS SOP-8

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-SOP-8
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCHS_SOP8_14363X285210"/>
</gates>
<devices>
<device name="" package="WL-OCHS_SOP8-SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="10 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143631285210?ae"/>
<attribute name="HEIGHT" value="3.18mm"/>
<attribute name="ITH-TYP" value="2.4 mA"/>
<attribute name="LENGTH" value="4.05mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="MPN" value="143631285210"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PACKAGE-TYPE" value="SOP8"/>
<attribute name="TPLH" value="48 nsV"/>
<attribute name="VALUE" value="143631285210"/>
<attribute name="VISO" value="3750 V (RMS)"/>
<attribute name="WIDTH" value="5.08mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="143135180100" prefix="Q">
<description>WL-OCHS DIP-8

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-DIP-8
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCPT_DIP8_14313X18X1X0"/>
</gates>
<devices>
<device name="" package="WL-OCHS_DIP8_STANDARD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="1 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143135180100?ae"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="LENGTH" value="6.5mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="MPN" value="143135180100"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +110 °C"/>
<attribute name="PACKAGE-TYPE" value="DIP 8, Standard"/>
<attribute name="TPLH" value="1300 nsV"/>
<attribute name="VALUE" value="143135180100"/>
<attribute name="VISO" value="5000 V (RMS)"/>
<attribute name="WIDTH" value="9.68mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="143611185210" prefix="Q">
<description>WL-OCHS SOP-8

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-SOP-8
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCHS_SOP8_1436X1185210"/>
</gates>
<devices>
<device name="" package="WL-OCHS_SOP8-SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="20 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143611185210?ae"/>
<attribute name="HEIGHT" value="3.18mm"/>
<attribute name="ITH-TYP" value="3 mA"/>
<attribute name="LENGTH" value="4.05mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="MPN" value="143611185210"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PACKAGE-TYPE" value="SOP8"/>
<attribute name="TPLH" value="41 nsV"/>
<attribute name="VALUE" value="143611185210"/>
<attribute name="VISO" value="3750 V (RMS)"/>
<attribute name="WIDTH" value="5.08mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="143136183110" prefix="Q">
<description>WL-OCHS DIP-8

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-DIP-8
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCPT_DIP8_14313X18X1X0"/>
</gates>
<devices>
<device name="" package="WL-OCHS_DIP8_SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="1 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143136183110?ae"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="LENGTH" value="8.57mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="MPN" value="143136183110"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +110 °C"/>
<attribute name="PACKAGE-TYPE" value="DIP 8, SL-Type"/>
<attribute name="TPLH" value="600 nsV"/>
<attribute name="VALUE" value="143136183110"/>
<attribute name="VISO" value="5000 V (RMS)"/>
<attribute name="WIDTH" value="9.68mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="143135183110" prefix="Q">
<description>WL-OCHS DIP-8

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-DIP-8
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCPT_DIP8_14313X18X1X0"/>
</gates>
<devices>
<device name="" package="WL-OCHS_DIP8_SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="1 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143135183110?ae"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="LENGTH" value="8.57mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="MPN" value="143135183110"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +110 °C"/>
<attribute name="PACKAGE-TYPE" value="DIP 8, SL-Type"/>
<attribute name="TPLH" value="1300 nsV"/>
<attribute name="VALUE" value="143135183110"/>
<attribute name="VISO" value="5000 V (RMS)"/>
<attribute name="WIDTH" value="9.68mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="143137183210" prefix="Q">
<description>WL-OCHS DIP-8

Characteristics
Very high transmission speed - MHz to Mbit/s range
Precise shifting without much delay thanks to fast switching times
High insulation voltage VISO = 3750 &amp; 5000 VRMS
High immunity to interference (EMC)

Applications
High-speed digital signal transmission
Interface isolation (e.g., UART, SPI, RS-232, RS-485)
Switching power supplies and power electronics
Industrial controls and automation
Microcontroller and embedded systems

Details see: www.we-online.com/en/components/products/WL-OCHS-DIP-8
 
Created by Ella 2026-08-06
2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCPT_DIP8_14313718X2X0"/>
</gates>
<devices>
<device name="" package="WL-OCHS_DIP8_SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Optocoupler"/>
<attribute name="CMTILH" value="5 kV/µsmA"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/143137183210?ae"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="ITH-TYP" value="3 mA"/>
<attribute name="LENGTH" value="8.57mm"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="MPN" value="143137183210"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="PACKAGE-TYPE" value="DIP 8, SL-Type"/>
<attribute name="TPLH" value="41 nsV"/>
<attribute name="VALUE" value="143137183210"/>
<attribute name="VISO" value="5000 V (RMS)"/>
<attribute name="WIDTH" value="9.68mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
