<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Optoelectronic Components - 7 Segments Display - WL-S7DS&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-01-17&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-S7DS_0.3INCH">
<description>&lt;b&gt;WL-S7DS 7 Segments Display SMT Single Digit 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
Size: 0.3inch, SMT, 10pins
&lt;br&gt;L X W X H=12mm X 7.3mm X 3.75mm</description>
</package>
<package name="WL-S7DS_0.39INCH">
<description>&lt;b&gt;WL-S7DS 7 Segments Display SMT Single Digit 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
Size: 0.39inch, SMT, 10pins
&lt;br&gt;L X W X H=15mm X 9.8mm X 3.75mm</description>
</package>
<package name="WL-S7DS_0.56INCH">
<description>&lt;b&gt;WL-S7DS 7 Segments Display SMT Single Digit 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
Size: 0.56inch, SMT, 10pins
&lt;br&gt;L X W X H=19mm X 12.4mm X 3.75mm</description>
</package>
<package name="WL-S7DS_0.2INCH">
<description>&lt;b&gt;WL-S7DS 7 Segments Display SMT Single Digit 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
Size: 0.2inch, SMT, 10pins
&lt;br&gt;L X W X H=10mm X 6.9mm X 3mm</description>
</package>
</packages>
<symbols>
<symbol name="COMMON_CATHODE">
<pin name="7" direction="pas"/>
<pin name="-" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="COMMON_ANODE">
<pin name="7" direction="pas"/>
<pin name="+" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-S7DS_0.3INCH_COMMON-ANODE" prefix="D">
<description>&lt;b&gt;WL-S7DS 7 Segments Display SMT Single Digit 
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial standard size and schematic
&lt;br&gt; Low power consumption
&lt;br&gt; Grey surface
&lt;br&gt; Milky / Diffuesed segments
&lt;br&gt; Driving with DC current in forward direction only
&lt;br&gt; Suitable for high peak current upto 100 mA

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Audio / measure equipment
&lt;br&gt; Instrument panels
 &lt;br&gt;Digital read out display
&lt;br&gt; Control units

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o335301v209%20WL-S7DS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o335301v209%20WL-S7DS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL_S7DS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL_S7DS&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2022-09-14&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="COMMON_ANODE"/>
</gates>
<devices>
<device name="" package="WL-S7DS_0.3INCH">
<connects>
<connect gate="G$1" pin="+" pad="3 8"/>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_157112B12800">
<attribute name="CIRCUITRY" value="Common Anode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157112B12800?ae"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="3V"/>
<attribute name="HEIGHT" value="3.75mm"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="32mcd"/>
<attribute name="PART-NUMBER" value="157112B12800"/>
<attribute name="VALUE" value="157112B12800"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_157112S12800">
<attribute name="CIRCUITRY" value="Common Anode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157112S12800?ae"/>
<attribute name="EMITTING-COLOR" value="Super Red"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="2V"/>
<attribute name="HEIGHT" value="3.75mm"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="28mcd"/>
<attribute name="PART-NUMBER" value="157112S12800"/>
<attribute name="VALUE" value="157112S12800"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_157112V12800">
<attribute name="CIRCUITRY" value="Common Anode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157112V12800?ae"/>
<attribute name="EMITTING-COLOR" value="Bright Green"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="2V"/>
<attribute name="HEIGHT" value="3.75mm"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="21mcd"/>
<attribute name="PART-NUMBER" value="157112V12800"/>
<attribute name="VALUE" value="157112V12800"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-S7DS_0.39INCH_COMMON-ANODE" prefix="D">
<description>&lt;b&gt;WL-S7DS 7 Segments Display SMT Single Digit 
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial standard size and schematic
&lt;br&gt; Low power consumption
&lt;br&gt; Grey surface
&lt;br&gt; Milky / Diffuesed segments
&lt;br&gt; Driving with DC current in forward direction only
&lt;br&gt; Suitable for high peak current upto 100 mA

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Audio / measure equipment
&lt;br&gt; Instrument panels
 &lt;br&gt;Digital read out display
&lt;br&gt; Control units

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o335301v209%20WL-S7DS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o335301v209%20WL-S7DS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL_S7DS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL_S7DS&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2022-05-12&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="COMMON_ANODE"/>
</gates>
<devices>
<device name="" package="WL-S7DS_0.39INCH">
<connects>
<connect gate="G$1" pin="+" pad="3 8"/>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CIRCUITRY" value=""/>
<attribute name="DATASHEET-URL" value=""/>
<attribute name="EMITTING-COLOR" value=""/>
<attribute name="FORWARD-VOLTAGE-TYP" value=""/>
<attribute name="HEIGHT" value=""/>
<attribute name="LENGTH" value=""/>
<attribute name="LUMINOUS-INTENSITY-TYP" value=""/>
<attribute name="PART-NUMBER" value=""/>
<attribute name="VALUE" value=""/>
<attribute name="WIDTH" value=""/>
</technology>
<technology name="_157121S12800">
<attribute name="CIRCUITRY" value="Common Anode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157121S12800?ae"/>
<attribute name="EMITTING-COLOR" value="Super Red"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="2V"/>
<attribute name="HEIGHT" value="3.75mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="38mcd"/>
<attribute name="PART-NUMBER" value="157121S12800"/>
<attribute name="VALUE" value="157121S12800"/>
<attribute name="WIDTH" value="9.8mm"/>
</technology>
<technology name="_157121V12800">
<attribute name="CIRCUITRY" value="Common Anode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157121V12800?ae"/>
<attribute name="EMITTING-COLOR" value="Bright Green"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="2V"/>
<attribute name="HEIGHT" value="3.75mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="35mcd"/>
<attribute name="PART-NUMBER" value="157121V12800"/>
<attribute name="VALUE" value="157121V12800"/>
<attribute name="WIDTH" value="9.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-S7DS_0.3INCH_COMMON-CATHODE" prefix="D">
<description>&lt;b&gt;WL-S7DS 7 Segments Display SMT Single Digit 
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial standard size and schematic
&lt;br&gt; Low power consumption
&lt;br&gt; Grey surface
&lt;br&gt; Milky / Diffuesed segments
&lt;br&gt; Driving with DC current in forward direction only
&lt;br&gt; Suitable for high peak current upto 100 mA

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Audio / measure equipment
&lt;br&gt; Instrument panels
 &lt;br&gt;Digital read out display
&lt;br&gt; Control units

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o335301v209%20WL-S7DS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o335301v209%20WL-S7DS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL_S7DS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL_S7DS&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2022-05-12&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="COMMON_CATHODE"/>
</gates>
<devices>
<device name="" package="WL-S7DS_0.3INCH">
<connects>
<connect gate="G$1" pin="-" pad="3 8"/>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_157112B12700">
<attribute name="CIRCUITRY" value="Common Cathode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157112B12700?ae"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="3V"/>
<attribute name="HEIGHT" value="3.75mm"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="32mcd"/>
<attribute name="PART-NUMBER" value="157112B12700"/>
<attribute name="VALUE" value="157112B12700"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_157112S12700">
<attribute name="CIRCUITRY" value="Common Cathode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157112S12700?ae"/>
<attribute name="EMITTING-COLOR" value="Super Red"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="2V"/>
<attribute name="HEIGHT" value="3.75mm"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="28mcd"/>
<attribute name="PART-NUMBER" value="157112S12700"/>
<attribute name="VALUE" value="157112S12700"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_157112V12700">
<attribute name="CIRCUITRY" value="Common Cathode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157112V12700?ae"/>
<attribute name="EMITTING-COLOR" value="Bright Green"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="2V"/>
<attribute name="HEIGHT" value="3.75mm"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="21mcd"/>
<attribute name="PART-NUMBER" value="157112V12700"/>
<attribute name="VALUE" value="157112V12700"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-S7DS_0.56INCH_COMMON-ANODE" prefix="D">
<description>&lt;b&gt;WL-S7DS 7 Segments Display SMT Single Digit 
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial standard size and schematic
&lt;br&gt; Low power consumption
&lt;br&gt; Grey surface
&lt;br&gt; Milky / Diffuesed segments
&lt;br&gt; Driving with DC current in forward direction only
&lt;br&gt; Suitable for high peak current upto 100 mA

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Audio / measure equipment
&lt;br&gt; Instrument panels
 &lt;br&gt;Digital read out display
&lt;br&gt; Control units

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o335301v209%20WL-S7DS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o335301v209%20WL-S7DS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL_S7DS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL_S7DS&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu, 2022-05-12&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="COMMON_ANODE"/>
</gates>
<devices>
<device name="" package="WL-S7DS_0.56INCH">
<connects>
<connect gate="G$1" pin="+" pad="3 8"/>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_157143B12800">
<attribute name="CIRCUITRY" value="Common Anode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157143B12800?ae"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="3V"/>
<attribute name="HEIGHT" value="3.75mm"/>
<attribute name="LENGTH" value="19mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="32mcd"/>
<attribute name="PART-NUMBER" value="157143B12800"/>
<attribute name="VALUE" value="157143B12800"/>
<attribute name="WIDTH" value="12.4mm"/>
</technology>
<technology name="_157143S12800">
<attribute name="CIRCUITRY" value="Common Anode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157143S12800?ae"/>
<attribute name="EMITTING-COLOR" value="Super Red"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="2V"/>
<attribute name="HEIGHT" value="3.75mm"/>
<attribute name="LENGTH" value="19mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="28mcd"/>
<attribute name="PART-NUMBER" value="157143S12800"/>
<attribute name="VALUE" value="157143S12800"/>
<attribute name="WIDTH" value="12.4mm"/>
</technology>
<technology name="_157143V12800">
<attribute name="CIRCUITRY" value="Common Anode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157143V12800?ae"/>
<attribute name="EMITTING-COLOR" value="Bright Green"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="2V"/>
<attribute name="HEIGHT" value="3.75mm"/>
<attribute name="LENGTH" value="19mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="35mcd"/>
<attribute name="PART-NUMBER" value="157143V12800"/>
<attribute name="VALUE" value="157143V12800"/>
<attribute name="WIDTH" value="12.4mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-S7DS_0.56INCH_COMMON-CATHODE" prefix="D">
<description>&lt;b&gt;WL-S7DS 7 Segments Display SMT Single Digit 
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial standard size and schematic
&lt;br&gt; Low power consumption
&lt;br&gt; Grey surface
&lt;br&gt; Milky / Diffuesed segments
&lt;br&gt; Driving with DC current in forward direction only
&lt;br&gt; Suitable for high peak current upto 100 mA

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Audio / measure equipment
&lt;br&gt; Instrument panels
 &lt;br&gt;Digital read out display
&lt;br&gt; Control units

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o335301v209%20WL-S7DS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o335301v209%20WL-S7DS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL_S7DS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL_S7DS&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2022-05-12&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="COMMON_CATHODE"/>
</gates>
<devices>
<device name="" package="WL-S7DS_0.56INCH">
<connects>
<connect gate="G$1" pin="-" pad="3 8"/>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_157143S12700">
<attribute name="CIRCUITRY" value="Common Cathode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157143S12700?ae"/>
<attribute name="EMITTING-COLOR" value="Super Red"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="2V"/>
<attribute name="HEIGHT" value="3.75mm"/>
<attribute name="LENGTH" value="19mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="28mcd"/>
<attribute name="PART-NUMBER" value="157143S12700"/>
<attribute name="VALUE" value="157143S12700"/>
<attribute name="WIDTH" value="12.4mm"/>
</technology>
<technology name="_157143V12700">
<attribute name="CIRCUITRY" value="Common Cathode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157143V12700?ae"/>
<attribute name="EMITTING-COLOR" value="Bright Green"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="2V"/>
<attribute name="HEIGHT" value="3.75mm"/>
<attribute name="LENGTH" value="19mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="35mcd"/>
<attribute name="PART-NUMBER" value="157143V12700"/>
<attribute name="VALUE" value="157143V12700"/>
<attribute name="WIDTH" value="12.4mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-S7DS_0.2INCH_COMMON-ANODE" prefix="D">
<description>&lt;b&gt;WL-S7DS 7 Segments Display SMT Single Digit 
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial standard size and schematic
&lt;br&gt; Low power consumption
&lt;br&gt; Grey surface
&lt;br&gt; Milky / Diffuesed segments
&lt;br&gt; Driving with DC current in forward direction only
&lt;br&gt; Suitable for high peak current upto 100 mA

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Audio / measure equipment
&lt;br&gt; Instrument panels
 &lt;br&gt;Digital read out display
&lt;br&gt; Control units

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o335301v209%20WL-S7DS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o335301v209%20WL-S7DS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL_S7DS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL_S7DS&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2023-01-17&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="COMMON_ANODE"/>
</gates>
<devices>
<device name="" package="WL-S7DS_0.2INCH">
<connects>
<connect gate="G$1" pin="+" pad="3 8"/>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_157102B12800">
<attribute name="CIRCUITRY" value="Common Anode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157102B12800?ae"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="3V"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="24mcd"/>
<attribute name="PART-NUMBER" value="157102B12800"/>
<attribute name="VALUE" value="157102B12800"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_157102S12800">
<attribute name="CIRCUITRY" value="Common Anode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157102S12800?ae"/>
<attribute name="EMITTING-COLOR" value="Super Red"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="2V"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="16mcd"/>
<attribute name="PART-NUMBER" value="157102S12800"/>
<attribute name="VALUE" value="157102S12800"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_157102V12800">
<attribute name="CIRCUITRY" value="Common Anode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157102V12800?ae"/>
<attribute name="EMITTING-COLOR" value="Bright Green"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="2V"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="17mcd"/>
<attribute name="PART-NUMBER" value="157102V12800"/>
<attribute name="VALUE" value="157102V12800"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-S7DS_0.2INCH_COMMON-CATHODE" prefix="D">
<description>&lt;b&gt;WL-S7DS 7 Segments Display SMT Single Digit 
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial standard size and schematic
&lt;br&gt; Low power consumption
&lt;br&gt; Grey surface
&lt;br&gt; Milky / Diffuesed segments
&lt;br&gt; Driving with DC current in forward direction only
&lt;br&gt; Suitable for high peak current upto 100 mA

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Audio / measure equipment
&lt;br&gt; Instrument panels
 &lt;br&gt;Digital read out display
&lt;br&gt; Control units

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o335301v209%20WL-S7DS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o335301v209%20WL-S7DS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL_S7DS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL_S7DS&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2023-01-17&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="COMMON_CATHODE"/>
</gates>
<devices>
<device name="" package="WL-S7DS_0.2INCH">
<connects>
<connect gate="G$1" pin="-" pad="3 8"/>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_157102B12700">
<attribute name="CIRCUITRY" value="Common Cathode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157102B12700?ae"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="3V"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="24mcd"/>
<attribute name="PART-NUMBER" value="157102B12700"/>
<attribute name="VALUE" value="157102B12700"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_157102S12700">
<attribute name="CIRCUITRY" value="Common Cathode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157102S12700?ae"/>
<attribute name="EMITTING-COLOR" value="Super Red"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="2V"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="15mcd"/>
<attribute name="PART-NUMBER" value="157102S12700"/>
<attribute name="VALUE" value="157102S12700"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
<technology name="_157102V12700">
<attribute name="CIRCUITRY" value="Common Cathode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157102V12700?ae"/>
<attribute name="EMITTING-COLOR" value="Bright Green"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="2V"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="17mcd"/>
<attribute name="PART-NUMBER" value="157102V12700"/>
<attribute name="VALUE" value="157102V12700"/>
<attribute name="WIDTH" value="6.9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-S7DS_0.39INCH_COMMON-CATHODE" prefix="D">
<description>&lt;b&gt;WL-S7DS 7 Segments Display SMT Single Digit 
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial standard size and schematic
&lt;br&gt; Low power consumption
&lt;br&gt; Grey surface
&lt;br&gt; Milky / Diffuesed segments
&lt;br&gt; Driving with DC current in forward direction only
&lt;br&gt; Suitable for high peak current upto 100 mA

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Audio / measure equipment
&lt;br&gt; Instrument panels
 &lt;br&gt;Digital read out display
&lt;br&gt; Control units

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o335301v209%20WL-S7DS_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o335301v209%20WL-S7DS_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL_S7DS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL_S7DS&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2022-05-12&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="COMMON_CATHODE"/>
</gates>
<devices>
<device name="" package="WL-S7DS_0.39INCH">
<connects>
<connect gate="G$1" pin="-" pad="3 8"/>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_157121B12700">
<attribute name="CIRCUITRY" value="Common Cathode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157121B12700?ae"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="3V"/>
<attribute name="HEIGHT" value="3.75mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="32mcd"/>
<attribute name="PART-NUMBER" value="157121B12700"/>
<attribute name="VALUE" value="157121B12700"/>
<attribute name="WIDTH" value="9.8mm"/>
</technology>
<technology name="_157121S12700">
<attribute name="CIRCUITRY" value="Common Cathode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157121S12700?ae"/>
<attribute name="EMITTING-COLOR" value="Super Red"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="2V"/>
<attribute name="HEIGHT" value="3.75mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="38mcd"/>
<attribute name="PART-NUMBER" value="157121S12700"/>
<attribute name="VALUE" value="157121S12700"/>
<attribute name="WIDTH" value="9.8mm"/>
</technology>
<technology name="_157121V12700">
<attribute name="CIRCUITRY" value="Common Cathode"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/157121V12700?ae"/>
<attribute name="EMITTING-COLOR" value="Bright Green"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="2V"/>
<attribute name="HEIGHT" value="3.75mm"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="LUMINOUS-INTENSITY-TYP" value="35mcd"/>
<attribute name="PART-NUMBER" value="157121V12700"/>
<attribute name="VALUE" value="157121V12700"/>
<attribute name="WIDTH" value="9.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
