<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Optoelectronic Components - Infrared - Infrared LEDs - WL-SICW&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-08-27&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-SICW_0603_15406085BA300">
<description>&lt;B&gt;WL-SICW SMT Chip LED Infrared Waterclear
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Size: 0603, SMT, 2pins
&lt;BR&gt;LXWXH=1.6x0.8x0.6mm</description>
</package>
<package name="WL-SICW_0603_15406094BA500">
<description>&lt;B&gt;WL-SICW SMT Chip LED Infrared Waterclear
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Size: 0603, SMT, 2pins
&lt;BR&gt;LXWXH=1.6x0.8x0.6mm</description>
</package>
<package name="WL-SICW_0603_154060XXBA400A">
<description>&lt;B&gt;WL-SICW SMT Chip LED Infrared Waterclear
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Size:0603, SMT, 2pins
&lt;BR&gt;LXWXH=1.6x0.8x0.88mm</description>
</package>
<package name="WL-SICW_0805">
<description>&lt;B&gt;WL-SICW SMT Chip LED Infrared Waterclear
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Size: 0805, SMT, 2pins
&lt;BR&gt;LXWXH=2x1.3x0.8mm</description>
</package>
<package name="WL-SICW_0603_LENS_15406085B6000">
<description>&lt;B&gt;WL-SICW SMT Chip LED Infrared Waterclear
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Size:0603 Lens, SMT, 2pins
&lt;BR&gt;LXWXH=1.6x0.8x0.93mm</description>
</package>
<package name="WL-SICW_1206_15412094BA400">
<description>&lt;B&gt;WL-SICW SMT Chip LED Infrared Waterclear
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Size: 1206, SMT, 2pins
&lt;BR&gt;LXWXH=3.2x1.6x1.1mm</description>
</package>
<package name="WL-SICW_0603_LENS_15406094B6000">
<description>&lt;B&gt;WL-SICW SMT Chip LED Infrared Waterclear
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Size:0603 Lens, SMT, 2pins
&lt;BR&gt;LXWXH=1.6x0.8x0.93mm</description>
</package>
<package name="WL-SICW_0402">
<description>&lt;B&gt;WL-SICW SMT Chip LED Infrared Waterclear
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Size: 0402, SMT, 2pins
&lt;BR&gt;&lt;BR&gt;LXWXH=1x0.5x0.5mm</description>
</package>
<package name="WL-SICW_1206_15412085BA400">
<description>&lt;B&gt;WL-SICW SMT Chip LED Infrared Waterclear
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Size: 1206, SMT, 2pins
&lt;BR&gt;LXWXH=3.2x1.6x1.1mm</description>
</package>
<package name="WL-SICW_1206_154120XXA9000">
<description>&lt;B&gt;WL-SICW SMT Chip LED Infrared Waterclear
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;Size: 1206, SMT, 2pins
&lt;BR&gt;LXWXH=3x1.5x1.21mm</description>
</package>
</packages>
<symbols>
<symbol name="LED">
<description>LED</description>
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-SICW_0603" prefix="D" uservalue="yes">
<description>&lt;b&gt;WL-SICW SMD Chip LED Infrared Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low energy consumption
&lt;br&gt;High reliability
&lt;br&gt;Low current requirement
&lt;br&gt;Fast switching
&lt;br&gt;IR Emitter
&lt;br&gt;standard size 0603
&lt;br&gt;Compact package outline
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Infrared sensor
&lt;br&gt;Distance measure
&lt;br&gt;Remote control
&lt;br&gt;Smoke detector
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135757v209%20WL-SICW_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135757v209%20WL-SICW_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SICW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL-SICW&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-08-27&lt;br&gt;
&lt;/b&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="_15406085BA300" package="WL-SICW_0603_15406085BA300">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15406085BA300?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="1.4V"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LAMDA-CENTROLD-TYP" value="845nm"/>
<attribute name="LAMDA-PEAK-TYP" value="850nm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="15406085BA300"/>
<attribute name="RADIANT-INTENSITY-TYP" value="2mW/sr"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VIEWING-ANGLE" value="130°"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_15406094BA500" package="WL-SICW_0603_15406094BA500">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15406094BA500?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="1.2V"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LAMDA-CENTROLD-TYP" value="940nm"/>
<attribute name="LAMDA-PEAK-TYP" value="940nm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="15406094BA500"/>
<attribute name="RADIANT-INTENSITY-TYP" value="0.8mW/sr"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VIEWING-ANGLE" value="150°"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_154060XXBA400A" package="WL-SICW_0603_154060XXBA400A">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_15406085BA400A">
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15406085BA400A?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="1.4V"/>
<attribute name="HEIGHT" value="0.88mm"/>
<attribute name="LAMDA-CENTROLD-TYP" value="845nm"/>
<attribute name="LAMDA-PEAK-TYP" value="850nm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="15406085BA400A"/>
<attribute name="RADIANT-INTENSITY-TYP" value="1.2mW/sr"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VIEWING-ANGLE" value="140°"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_15406094BA400A">
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15406094BA400A?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="1.2V"/>
<attribute name="HEIGHT" value="0.88mm"/>
<attribute name="LAMDA-CENTROLD-TYP" value="940nm"/>
<attribute name="LAMDA-PEAK-TYP" value="940nm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="15406094BA400A"/>
<attribute name="RADIANT-INTENSITY-TYP" value="1mW/sr"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VIEWING-ANGLE" value="140°"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SICW_0805" prefix="D" uservalue="yes">
<description>&lt;b&gt;WL-SICW SMD Chip LED Infrared Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low energy consumption
&lt;br&gt;High reliability
&lt;br&gt;Low current requirement
&lt;br&gt;Fast switching
&lt;br&gt;IR Emitter
&lt;br&gt;standard size 0603
&lt;br&gt;Compact package outline
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Infrared sensor
&lt;br&gt;Distance measure
&lt;br&gt;Remote control
&lt;br&gt;Smoke detector
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135757v209%20WL-SICW_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135757v209%20WL-SICW_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SICW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL-SICW&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-08-27&lt;br&gt;
&lt;/b&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="WL-SICW_0805">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_15408085BA400">
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15408085BA400?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="1.4V"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LAMDA-CENTROLD-TYP" value="845nm"/>
<attribute name="LAMDA-PEAK-TYP" value="850nm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="15408085BA400"/>
<attribute name="RADIANT-INTENSITY-TYP" value="1.5mW/sr"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VIEWING-ANGLE" value="140°"/>
<attribute name="WIDTH" value="1.3mm"/>
</technology>
<technology name="_15408094BA400">
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15408094BA400?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="1.2V"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LAMDA-CENTROLD-TYP" value="940nm"/>
<attribute name="LAMDA-PEAK-TYP" value="940nm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="15408094BA400"/>
<attribute name="RADIANT-INTENSITY-TYP" value="1mW/sr"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VIEWING-ANGLE" value="140°"/>
<attribute name="WIDTH" value="1.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SICW_0402" prefix="D" uservalue="yes">
<description>&lt;b&gt;WL-SICW SMD Chip LED Infrared Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low energy consumption
&lt;br&gt;High reliability
&lt;br&gt;Low current requirement
&lt;br&gt;Fast switching
&lt;br&gt;IR Emitter
&lt;br&gt;standard size 0603
&lt;br&gt;Compact package outline
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Infrared sensor
&lt;br&gt;Distance measure
&lt;br&gt;Remote control
&lt;br&gt;Smoke detector
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135757v209%20WL-SICW_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135757v209%20WL-SICW_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SICW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL-SICW&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-08-27&lt;br&gt;
&lt;/b&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="WL-SICW_0402">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_15404085BA420">
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15404085BA420?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="1.6V"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LAMDA-CENTROLD-TYP" value="845nm"/>
<attribute name="LAMDA-PEAK-TYP" value="850nm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="15404085BA420"/>
<attribute name="RADIANT-INTENSITY-TYP" value="6mW/sr"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VIEWING-ANGLE" value="140°"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_15404094BA420">
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15404094BA420?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="1.4V"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LAMDA-CENTROLD-TYP" value="940nm"/>
<attribute name="LAMDA-PEAK-TYP" value="940nm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="15404094BA420"/>
<attribute name="RADIANT-INTENSITY-TYP" value="5mW/sr"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VIEWING-ANGLE" value="140°"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SICW_0603_LENS" prefix="D" uservalue="yes">
<description>&lt;b&gt;WL-SICW SMD Chip LED Infrared Waterclear
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard size 0603
&lt;br&gt;Compact package outline
&lt;br&gt;Low energy consumption
&lt;br&gt;High reliability
&lt;br&gt;Low current requirement
&lt;br&gt;Fast switching
&lt;br&gt;Infrered Emitter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Infrared sensor
&lt;br&gt;Distance measure
&lt;br&gt;Remote control 
&lt;br&gt;Smoke detector
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135757v209%20Family_WL-SICW_0402_1206.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135757v209%20Family_WL-SICW_0402_1206.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WL-SICW/"&gt;https://www.we-online.com/catalog/en/WL-SICW/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated By Yingchun Shan 2020-03-24&lt;br&gt;
&lt;/b&gt;2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="_15406085B6000" package="WL-SICW_0603_LENS_15406085B6000">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15406085B6000?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="1.4V"/>
<attribute name="HEIGHT" value="0.93mm"/>
<attribute name="LAMDA-CENTROLD-TYP" value="845nm"/>
<attribute name="LAMDA-PEAK-TYP" value="850nm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="15406085B6000"/>
<attribute name="RADIANT-INTENSITY-TYP" value="5mW/sr"/>
<attribute name="SIZE" value="0603 Lens"/>
<attribute name="VIEWING-ANGLE" value="60°"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_15406094B6000" package="WL-SICW_0603_LENS_15406094B6000">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15406094B6000?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="1.2V"/>
<attribute name="HEIGHT" value="0.93mm"/>
<attribute name="LAMDA-CENTROLD-TYP" value="940nm"/>
<attribute name="LAMDA-PEAK-TYP" value="940nm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="15406094B6000"/>
<attribute name="RADIANT-INTENSITY-TYP" value="2mW/sr"/>
<attribute name="SIZE" value="0603 Lens"/>
<attribute name="VIEWING-ANGLE" value="60°"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SICW_1206" prefix="D" uservalue="yes">
<description>&lt;b&gt;WL-SICW SMD Chip LED Infrared Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low energy consumption
&lt;br&gt;High reliability
&lt;br&gt;Low current requirement
&lt;br&gt;Fast switching
&lt;br&gt;IR Emitter
&lt;br&gt;standard size 0603
&lt;br&gt;Compact package outline
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Infrared sensor
&lt;br&gt;Distance measure
&lt;br&gt;Remote control
&lt;br&gt;Smoke detector
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135757v209%20WL-SICW_Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135757v209%20WL-SICW_Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SICW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL-SICW&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-08-27&lt;br&gt;
&lt;/b&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="_15412094BA400" package="WL-SICW_1206_15412094BA400">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15412094BA400?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="1.2V"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="LAMDA-CENTROLD-TYP" value="940nm"/>
<attribute name="LAMDA-PEAK-TYP" value="940nm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="15412094BA400"/>
<attribute name="RADIANT-INTENSITY-TYP" value="1mW/sr"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VIEWING-ANGLE" value="140°"/>
<attribute name="WIDTH" value="1.5mm"/>
</technology>
</technologies>
</device>
<device name="_15412085BA400" package="WL-SICW_1206_15412085BA400">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15412085BA400?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="1.4V"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="LAMDA-CENTROLD-TYP" value="850nm"/>
<attribute name="LAMDA-PEAK-TYP" value="850nm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="15412085BA400"/>
<attribute name="RADIANT-INTENSITY-TYP" value="2.5mW/sr"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VIEWING-ANGLE" value="140°"/>
<attribute name="WIDTH" value="1.5mm"/>
</technology>
</technologies>
</device>
<device name="_154120XXA9000" package="WL-SICW_1206_154120XXA9000">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_15412085A9000">
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15412085A9000?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="1.4V"/>
<attribute name="HEIGHT" value="1.21mm"/>
<attribute name="LAMDA-CENTROLD-TYP" value="845nm"/>
<attribute name="LAMDA-PEAK-TYP" value="850nm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="15412085A9000"/>
<attribute name="RADIANT-INTENSITY-TYP" value="5mW/sr"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VIEWING-ANGLE" value="90°"/>
<attribute name="WIDTH" value="1.5mm"/>
</technology>
<technology name="_15412094A9000">
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/15412094A9000?ae"/>
<attribute name="FORWARD-VOLTAGE-TYP" value="1.2V"/>
<attribute name="HEIGHT" value="1.21mm"/>
<attribute name="LAMDA-CENTROLD-TYP" value="940nm"/>
<attribute name="LAMDA-PEAK-TYP" value="940nm"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="15412094A9000"/>
<attribute name="RADIANT-INTENSITY-TYP" value="5.5mW/sr"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VIEWING-ANGLE" value="90°"/>
<attribute name="WIDTH" value="1.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
