<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Infrared - Infrared LEDs - WL-SISW&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-24&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-SISW_1206">
<description>&lt;b&gt;WL-SISW&lt;/b&gt;&lt;br&gt; SMT Infrared Sideview LED Waterclear,Size 1206:3.2x1.6x2.55mm(LXWXH)</description>
</package>
<package name="WL-SISW_1104_15411485AA370">
<description>&lt;b&gt;WL-SISW&lt;/b&gt;&lt;br&gt; SMT Infrared Sideview LED Waterclear,Size 1104:3x1.0x2.0mm(LXWXH)</description>
</package>
<package name="WL-SISW_1104_15411494AA570">
<description>&lt;b&gt;WL-SISW&lt;/b&gt;&lt;br&gt; SMT Infrared Sideview LED Waterclear,Size 1104:3x1.0x2.0mm(LXWXH)</description>
</package>
<package name="WL-SISW_1106">
<description>&lt;b&gt;WL-SISW&lt;/b&gt;&lt;br&gt; SMT Infrared Sideview LED Waterclear,Size 1106:3x1.6x2.34mm(LXWXH)</description>
</package>
<package name="WL-SISW_1002_15410285AA170">
<description>&lt;b&gt;WL-SISW&lt;/b&gt;&lt;br&gt; SMT Infrared Sideview LED Waterclear,Size 1002:2.4x0.6x1.39mm(LXWXH)</description>
</package>
<package name="WL-SISW_1002_15410294AA570">
<description>&lt;b&gt;WL-SISW&lt;/b&gt;&lt;br&gt; SMT Infrared Sideview LED Waterclear,Size 1002:2.4x0.6x1.39mm(LXWXH)</description>
</package>
<package name="WL-SISW_0402">
<description>&lt;b&gt;WL-SISW&lt;/b&gt;&lt;br&gt; SMT Infrared Sideview LED Waterclear,Size 0402:1x0.3x0.55mm(LXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="LED">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="LED-1">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-SISW_1104_AA370" prefix="D" uservalue="yes">
<description>&lt;b&gt;WL-SISW SMD Infrared Sideview LED Waterclear
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard size 1104
&lt;br&gt;Compact package outline
&lt;br&gt;Low energy consumption
&lt;br&gt;High reliability
&lt;br&gt;Low current requirement
&lt;br&gt;Fast switching
&lt;br&gt;Infrared Emitter - Side view
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Infrared sensor
&lt;br&gt;Distance measure
&lt;br&gt;Remote control 
&lt;br&gt;IR Lightbarrier


&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o149232v209%20Family_WL-SISW_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o149232v209%20Family_WL-SISW_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/led/WL-SISW/"&gt;https://katalog.we-online.de/en/led/WL-SISW/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated By Yingchun Shan,2020-03-24&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="WL-SISW_1104_15411485AA370">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_15411485AA370">
<attribute name="ABSTRAHLWINKEL" value="130°"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15411485AA370.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="H" value="1mm"/>
<attribute name="I-E-MIN" value="1mW/sr"/>
<attribute name="I-E-TYP" value="2mW/sr"/>
<attribute name="LAMDA-CENTROLD-TYP" value="845nm"/>
<attribute name="LAMDA-PEAK-TYP" value="850nm"/>
<attribute name="PART-NUMBER" value="15411485AA370"/>
<attribute name="V-F-MAX" value="2V"/>
<attribute name="V-F-TYP" value="1.4V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SISW_1206" prefix="D" uservalue="yes">
<description>&lt;b&gt;WL-SISW SMD Infrared Sideview LED Waterclear
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard size 1104
&lt;br&gt;Compact package outline
&lt;br&gt;Low energy consumption
&lt;br&gt;High reliability
&lt;br&gt;Low current requirement
&lt;br&gt;Fast switching
&lt;br&gt;Infrared Emitter - Side view
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Infrared sensor
&lt;br&gt;Distance measure
&lt;br&gt;Remote control 
&lt;br&gt;IR Lightbarrier


&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o149232v209%20Family_WL-SISW_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o149232v209%20Family_WL-SISW_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/led/WL-SISW/"&gt;https://katalog.we-online.de/en/led/WL-SISW/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated By Yingchun Shan,2020-03-24&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="LED-1"/>
</gates>
<devices>
<device name="" package="WL-SISW_1206">
<connects>
<connect gate="G$1" pin="+" pad="3/4"/>
<connect gate="G$1" pin="-" pad="1/2"/>
</connects>
<technologies>
<technology name="_15412085A2070">
<attribute name="ABSTRAHLWINKEL" value="20°"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15412085A2070.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="H" value="2.55mm"/>
<attribute name="I-E-MIN" value="7mW/sr"/>
<attribute name="I-E-TYP" value="12mW/sr"/>
<attribute name="LAMDA-CENTROLD-TYP" value="845nm"/>
<attribute name="LAMDA-PEAK-TYP" value="850nm"/>
<attribute name="PART-NUMBER" value="15412085A2070"/>
<attribute name="V-F-MAX" value="2V"/>
<attribute name="V-F-TYP" value="1.4V"/>
</technology>
<technology name="_15412094A2070">
<attribute name="ABSTRAHLWINKEL" value="20°"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15412094A2070.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="H" value="2.55mm"/>
<attribute name="I-E-MIN" value="3mW/sr"/>
<attribute name="I-E-TYP" value="6mW/sr"/>
<attribute name="LAMDA-CENTROLD-TYP" value="940nm"/>
<attribute name="LAMDA-PEAK-TYP" value="940nm"/>
<attribute name="PART-NUMBER" value="15412094A2070"/>
<attribute name="V-F-MAX" value="2V"/>
<attribute name="V-F-TYP" value="1.2V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SISW_1106" prefix="D" uservalue="yes">
<description>&lt;b&gt;WL-SISW SMD Infrared Sideview LED Waterclear
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard size 1104
&lt;br&gt;Compact package outline
&lt;br&gt;Low energy consumption
&lt;br&gt;High reliability
&lt;br&gt;Low current requirement
&lt;br&gt;Fast switching
&lt;br&gt;Infrared Emitter - Side view
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Infrared sensor
&lt;br&gt;Distance measure
&lt;br&gt;Remote control 
&lt;br&gt;IR Lightbarrier


&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o149232v209%20Family_WL-SISW_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o149232v209%20Family_WL-SISW_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/led/WL-SISW/"&gt;https://katalog.we-online.de/en/led/WL-SISW/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated By Yingchun Shan,2020-03-24&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="WL-SISW_1106">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_15411085A4570">
<attribute name="ABSTRAHLWINKEL" value="45°"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15411085A4570.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="H" value="2.34mm"/>
<attribute name="I-E-MIN" value="6mW/sr"/>
<attribute name="I-E-TYP" value="11mW/sr"/>
<attribute name="LAMDA-CENTROLD-TYP" value="845nm"/>
<attribute name="LAMDA-PEAK-TYP" value="850nm"/>
<attribute name="PART-NUMBER" value="15411085A4570"/>
<attribute name="V-F-MAX" value="1.8V"/>
<attribute name="V-F-TYP" value="1.4V"/>
</technology>
<technology name="_15411094A6070">
<attribute name="ABSTRAHLWINKEL" value="60°"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15411094A6070.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="H" value="2.34mm"/>
<attribute name="I-E-MIN" value="4mW/sr"/>
<attribute name="I-E-TYP" value="6mW/sr"/>
<attribute name="LAMDA-CENTROLD-TYP" value="940nm"/>
<attribute name="LAMDA-PEAK-TYP" value="940nm"/>
<attribute name="PART-NUMBER" value="15411094A6070"/>
<attribute name="V-F-MAX" value="1.8V"/>
<attribute name="V-F-TYP" value="1.2V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SISW_1104_AA570" prefix="D" uservalue="yes">
<description>&lt;b&gt;WL-SISW SMD Infrared Sideview LED Waterclear
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard size 1104
&lt;br&gt;Compact package outline
&lt;br&gt;Low energy consumption
&lt;br&gt;High reliability
&lt;br&gt;Low current requirement
&lt;br&gt;Fast switching
&lt;br&gt;Infrared Emitter - Side view
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Infrared sensor
&lt;br&gt;Distance measure
&lt;br&gt;Remote control 
&lt;br&gt;IR Lightbarrier


&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o149232v209%20Family_WL-SISW_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o149232v209%20Family_WL-SISW_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/led/WL-SISW/"&gt;https://katalog.we-online.de/en/led/WL-SISW/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated By Yingchun Shan,2020-03-24&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="LED-1"/>
</gates>
<devices>
<device name="" package="WL-SISW_1104_15411494AA570">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_15411494AA570">
<attribute name="ABSTRAHLWINKEL" value="150°"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15411494AA570.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="H" value="1mm"/>
<attribute name="I-E-MIN" value="0.5mW/sr"/>
<attribute name="I-E-TYP" value="1mW/sr"/>
<attribute name="LAMDA-CENTROLD-TYP" value="940nm"/>
<attribute name="LAMDA-PEAK-TYP" value="940nm"/>
<attribute name="PART-NUMBER" value="15411494AA570"/>
<attribute name="V-F-MAX" value="1.7V"/>
<attribute name="V-F-TYP" value="1.2V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SISW_1002_AA570" prefix="D" uservalue="yes">
<description>&lt;b&gt;WL-SISW SMD Infrared Sideview LED Waterclear
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard size 1104
&lt;br&gt;Compact package outline
&lt;br&gt;Low energy consumption
&lt;br&gt;High reliability
&lt;br&gt;Low current requirement
&lt;br&gt;Fast switching
&lt;br&gt;Infrared Emitter - Side view
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Infrared sensor
&lt;br&gt;Distance measure
&lt;br&gt;Remote control 
&lt;br&gt;IR Lightbarrier


&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o149232v209%20Family_WL-SISW_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o149232v209%20Family_WL-SISW_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/led/WL-SISW/"&gt;https://katalog.we-online.de/en/led/WL-SISW/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated By Yingchun Shan,2020-03-24&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="LED-1"/>
</gates>
<devices>
<device name="" package="WL-SISW_1002_15410294AA570">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_15410294AA570">
<attribute name="ABSTRAHLWINKEL" value="150°"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15410294AA570.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="H" value="1.39mm"/>
<attribute name="I-E-MIN" value="1mW/sr"/>
<attribute name="I-E-TYP" value="1.5mW/sr"/>
<attribute name="LAMDA-CENTROLD-TYP" value="940nm"/>
<attribute name="LAMDA-PEAK-TYP" value="940nm"/>
<attribute name="PART-NUMBER" value="15410294AA570"/>
<attribute name="V-F-MAX" value="1.8V"/>
<attribute name="V-F-TYP" value="1.2V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SISW_1002_AA170" prefix="D" uservalue="yes">
<description>&lt;b&gt;WL-SISW SMD Infrared Sideview LED Waterclear
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard size 1104
&lt;br&gt;Compact package outline
&lt;br&gt;Low energy consumption
&lt;br&gt;High reliability
&lt;br&gt;Low current requirement
&lt;br&gt;Fast switching
&lt;br&gt;Infrared Emitter - Side view
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Infrared sensor
&lt;br&gt;Distance measure
&lt;br&gt;Remote control 
&lt;br&gt;IR Lightbarrier


&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o149232v209%20Family_WL-SISW_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o149232v209%20Family_WL-SISW_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/led/WL-SISW/"&gt;https://katalog.we-online.de/en/led/WL-SISW/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated By Yingchun Shan,2020-03-24&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="WL-SISW_1002_15410285AA170">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_15410285AA170">
<attribute name="ABSTRAHLWINKEL" value="110°"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15410285AA170.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="H" value="1.39mm"/>
<attribute name="I-E-MIN" value="2mW/sr"/>
<attribute name="I-E-TYP" value="5mW/sr"/>
<attribute name="LAMDA-CENTROLD-TYP" value="845nm"/>
<attribute name="LAMDA-PEAK-TYP" value="850nm"/>
<attribute name="PART-NUMBER" value="15410285AA170"/>
<attribute name="V-F-MAX" value="1.8V"/>
<attribute name="V-F-TYP" value="1.4V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SISW_0402" prefix="D" uservalue="yes">
<description>&lt;b&gt;WL-SISW SMD Infrared Sideview LED Waterclear
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Standard size 1104
&lt;br&gt;Compact package outline
&lt;br&gt;Low energy consumption
&lt;br&gt;High reliability
&lt;br&gt;Low current requirement
&lt;br&gt;Fast switching
&lt;br&gt;Infrared Emitter - Side view
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Infrared sensor
&lt;br&gt;Distance measure
&lt;br&gt;Remote control 
&lt;br&gt;IR Lightbarrier


&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o149232v209%20Family_WL-SISW_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o149232v209%20Family_WL-SISW_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/led/WL-SISW/"&gt;https://katalog.we-online.de/en/led/WL-SISW/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated By Yingchun Shan,2020-03-24&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="LED-1"/>
</gates>
<devices>
<device name="" package="WL-SISW_0402">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_15404085BA470">
<attribute name="ABSTRAHLWINKEL" value="140°"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15404085BA470.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="H" value="0.55mm"/>
<attribute name="I-E-MIN" value="0.1mW/sr"/>
<attribute name="I-E-TYP" value="1.5mW/sr"/>
<attribute name="LAMDA-CENTROLD-TYP" value="845nm"/>
<attribute name="LAMDA-PEAK-TYP" value="850nm"/>
<attribute name="PART-NUMBER" value="15404085BA470"/>
<attribute name="V-F-MAX" value="2V"/>
<attribute name="V-F-TYP" value="1.6V"/>
</technology>
<technology name="_15404094BA470">
<attribute name="ABSTRAHLWINKEL" value="140°"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15404094BA470.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="H" value="0.55mm"/>
<attribute name="I-E-MIN" value="0.1mW/sr"/>
<attribute name="I-E-TYP" value="1mW/sr"/>
<attribute name="LAMDA-CENTROLD-TYP" value="940nm"/>
<attribute name="LAMDA-PEAK-TYP" value="940nm"/>
<attribute name="PART-NUMBER" value="15404094BA470"/>
<attribute name="V-F-MAX" value="2V"/>
<attribute name="V-F-TYP" value="1.4V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
