<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<library>
<description>Würth Elektronik - Active Components - Power Modules (MagI³C Series) - Isolated Converter - MagI³C-FISM

Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, 
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. 
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. 
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. 

Please contact us for more information: libraries@we-online.com 

Würth Elektronik eiSos GmbH &amp; Co. KG
EMC &amp; Inductive Solutions
www.we-online.com

Fusion360, Library Revision 2026b, 2026-09-16
Copyright: Würth Elektronik</description>
<packages>
<package name="WPME-FISM_SIP-7_1779205341">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SIP-7, THT, 4pins

LXWXH = 19.5X6X10mm</description>
</package>
<package name="WPME-FISM_SIP-7_L19.65W7.05H10.16">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SIP-7, THT, 4pins

LXWXH = 19.65X7.05X10.16mm</description>
</package>
<package name="WPME-FISM_SIP-7_L19.6W7.05H10.2">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SIP-7, THT, 4pins

LXWXH = 19.6X7.05X10.2mm</description>
</package>
<package name="WPME-FISM_SIP-7_1779205141">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SIP-7, THT, 4pins

LXWXH = 19.5X6X10mm</description>
</package>
<package name="WPME-FISM_SIP-7_1779205241">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SIP-7, THT, 4pins

LXWXH = 19.5X6X10mm</description>
</package>
<package name="WPME-FISM_SIP-4_1779205211">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SIP-4, THT, 4pins

LXWXH = 11.5X6X10mm</description>
</package>
<package name="WPME-FISM_SIP-4_1779205011">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SIP-4, THT, 4pins

LXWXH = 11.5X6X10mm</description>
</package>
<package name="WPME-FISM_SIP-4_1779205311">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SIP-4, THT, 4pins

LXWXH = 11.5X6X10mm</description>
</package>
<package name="WPME-FISM_SIP-4_1779205111">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SIP-4, THT, 4pins

LXWXH = 11.5X6X10mm</description>
</package>
<package name="WPME-FISM_SIP-4_L11.5W6H10">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SIP-4, THT, 4pins

LXWXH = 11.5X6X10mm</description>
</package>
<package name="WPME-FISM_SMT-8_1769205141">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SMT-8, THT, 5pins

LXWXH = 12.7X11.05X6.25mm</description>
</package>
<package name="WPME-FISM_SMT-8_1769205341">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SMT-8, THT, 5pins

LXWXH = 12.8X11.1X6.9mm</description>
</package>
<package name="WPME-FISM_SMT-8_1768812141">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SMT-8, THT, 5pins

LXWXH = 12.7X11.05X6.25mm</description>
</package>
<package name="WPME-FISM_SMT-8_L12.75W10.7H6.95">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SMT-8, THT, 5pins

LXWXH = 12.75X10.7X6.95mm</description>
</package>
<package name="WPME-FISM_SMT-8_1769405241">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SMT-8, THT, 5pins

LXWXH = 12.7X11.05X6.25mm</description>
</package>
<package name="WPME-FISM_SMT-8_1769205041">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SMT-8, THT, 5pins

LXWXH = 12.7X11.05X6.25mm</description>
</package>
<package name="WPME-FISM_SMT-8_1769405341">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SMT-8, THT, 5pins

LXWXH = 12.8X11.1X6.9mm</description>
</package>
<package name="WPME-FISM_SMT-8_1768812241">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SMT-8, THT, 5pins

LXWXH = 12.7X11.05X6.25mm</description>
</package>
<package name="WPME-FISM_SMT-8_1769205241">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SMT-8, THT, 5pins

LXWXH = 12.7X11.05X6.25mm</description>
</package>
<package name="WPME-FISM_SMT-8_1768812341">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SMT-8, THT, 5pins

LXWXH = 12.8X11.1X6.9mm</description>
</package>
<package name="WPME-FISM_SMT-8_1769405141">
<description>MagI³C-FISM Fixed Isolated SIP Module

Size : SMT-8, THT, 5pins

LXWXH = 12.7X11.05X6.25mm</description>
</package>
</packages>
<symbols>
<symbol name="WPME-FISM_SIP-7">
<pin name="-VIN" direction="in"/>
<pin name="+VIN" direction="in"/>
<pin name="-VOUT" direction="out"/>
<pin name="+VOUT" direction="out"/>
</symbol>
<symbol name="WPME-FISM_SIP-4">
<pin name="-VIN" direction="in"/>
<pin name="+VIN" direction="in"/>
<pin name="-VOUT" direction="out"/>
<pin name="+VOUT" direction="out"/>
</symbol>
<symbol name="WPME-FISM_SMT-8">
<pin name="-VIN" direction="in"/>
<pin name="+VIN" direction="in"/>
<pin name="-VOUT" direction="out"/>
<pin name="+VOUT" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WPME-FISM_SIP-7" prefix="U">
<description>MagI³C-FISM Fixed Isolated SIP / SMT Module

Unregulated output voltage

Characteristics

Simple design (no transformer design know how required)

Leaded through-hole package for easy manufacturing and prototyping

Stand-alone solution (CIN and COUT integrated, no external components)

Simple functional isolation for overvoltage protection, avoiding ground loops, ground shift and noise in signal path or sensor systems

Industrial standard package and pin configuration

Low conducted and radiated EMI (compliant to EN55022 class B)

UL60950 certified

Applications

Data acquisition

Test and measurement systems

Interface and microcontroller supply

Industrial control

Details see: www.we-online.com/en/components/products/MAGIC-FISM

Updated by Ella 2025-01-21

2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-FISM_SIP-7"/>
</gates>
<devices>
<device name="_L19.6W7.05H10.2" package="WPME-FISM_SIP-7_L19.6W7.05H10.2">
<connects>
<connect gate="G$1" pin="+VIN" pad="1"/>
<connect gate="G$1" pin="+VOUT" pad="7"/>
<connect gate="G$1" pin="-VIN" pad="2"/>
<connect gate="G$1" pin="-VOUT" pad="5"/>
</connects>
<technologies>
<technology name="_177920514">
<attribute name="HEIGHT" value="10.2 mm"/>
<attribute name="LENGTH" value="19.6 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SIP-7"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="WIDTH" value="7.05 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="177920514"/>
<attribute name="INPUT_VOLTAGE" value="4.5 - 5.5V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="4000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/177920514?ae"/>
</technology>
<technology name="_177920524">
<attribute name="HEIGHT" value="10.2 mm"/>
<attribute name="LENGTH" value="19.6 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SIP-7"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="WIDTH" value="7.05 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="177920524"/>
<attribute name="INPUT_VOLTAGE" value="10.8 - 13.2V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="4000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/177920524?ae"/>
</technology>
</technologies>
</device>
<device name="_L19.65W7.05H10.16" package="WPME-FISM_SIP-7_L19.65W7.05H10.16">
<connects>
<connect gate="G$1" pin="+VIN" pad="1"/>
<connect gate="G$1" pin="+VOUT" pad="7"/>
<connect gate="G$1" pin="-VIN" pad="2"/>
<connect gate="G$1" pin="-VOUT" pad="5"/>
</connects>
<technologies>
<technology name="_1779405141">
<attribute name="HEIGHT" value="10.16 mm"/>
<attribute name="LENGTH" value="19.65 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-7"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="WIDTH" value="7.05 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1779405141"/>
<attribute name="INPUT_VOLTAGE" value="4.5 - 5.5V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="2 W"/>
<attribute name="ISOLATION_VOLTAGE" value="3000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1779405141?ae"/>
</technology>
<technology name="_1779405241">
<attribute name="HEIGHT" value="10.16 mm"/>
<attribute name="LENGTH" value="19.65 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-7"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="WIDTH" value="7.05 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1779405241"/>
<attribute name="INPUT_VOLTAGE" value="10.8 - 13.2V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="2 W"/>
<attribute name="ISOLATION_VOLTAGE" value="3000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1779405241?ae"/>
</technology>
<technology name="_1779405341">
<attribute name="HEIGHT" value="10.16 mm"/>
<attribute name="LENGTH" value="19.65 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-7"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="21.6 - 26.4Vin, 5Vout"/>
<attribute name="WIDTH" value="7.05 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1779405341"/>
<attribute name="INPUT_VOLTAGE" value="21.6 - 26.4V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="2 W"/>
<attribute name="ISOLATION_VOLTAGE" value="3000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1779405341?ae"/>
</technology>
</technologies>
</device>
<device name="_1779205241" package="WPME-FISM_SIP-7_1779205241">
<connects>
<connect gate="G$1" pin="+VIN" pad="1"/>
<connect gate="G$1" pin="+VOUT" pad="7"/>
<connect gate="G$1" pin="-VIN" pad="2"/>
<connect gate="G$1" pin="-VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="10.2 mm"/>
<attribute name="LENGTH" value="19.6 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-7"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="WIDTH" value="7.05 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1779205241"/>
<attribute name="INPUT_VOLTAGE" value="10.8 - 13.2V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="4000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1779205241?ae"/>
</technology>
</technologies>
</device>
<device name="_1779205141" package="WPME-FISM_SIP-7_1779205141">
<connects>
<connect gate="G$1" pin="+VIN" pad="1"/>
<connect gate="G$1" pin="+VOUT" pad="7"/>
<connect gate="G$1" pin="-VIN" pad="2"/>
<connect gate="G$1" pin="-VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="10.2 mm"/>
<attribute name="LENGTH" value="19.6 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-7"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="WIDTH" value="7.05 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1779205141"/>
<attribute name="INPUT_VOLTAGE" value="4.5 - 5.5V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="4000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1779205141?ae"/>
</technology>
</technologies>
</device>
<device name="_1779205341" package="WPME-FISM_SIP-7_1779205341">
<connects>
<connect gate="G$1" pin="+VIN" pad="1"/>
<connect gate="G$1" pin="+VOUT" pad="7"/>
<connect gate="G$1" pin="-VIN" pad="2"/>
<connect gate="G$1" pin="-VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="10.2 mm"/>
<attribute name="LENGTH" value="19.6 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-7"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="21.6 - 26.4Vin, 5Vout"/>
<attribute name="WIDTH" value="7.05 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1779205341"/>
<attribute name="INPUT_VOLTAGE" value="21.6 - 26.4V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="3000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1779205341?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WPME-FISM_SIP-4" prefix="U">
<description>MagI³C-FISM Fixed Isolated SIP / SMT Module

Unregulated output voltage

Characteristics

Simple design (no transformer design know how required)

Leaded through-hole package for easy manufacturing and prototyping

Stand-alone solution (CIN and COUT integrated, no external components)

Simple functional isolation for overvoltage protection, avoiding ground loops, ground shift and noise in signal path or sensor systems

Industrial standard package and pin configuration

Low conducted and radiated EMI (compliant to EN55022 class B)

UL60950 certified

Applications

Data acquisition

Test and measurement systems

Interface and microcontroller supply

Industrial control

Details see: www.we-online.com/en/components/products/MAGIC-FISM

Updated by Ella 2026-04-27

2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-FISM_SIP-4"/>
</gates>
<devices>
<device name="_L11.5W6H10" package="WPME-FISM_SIP-4_L11.5W6H10">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="4"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="3"/>
</connects>
<technologies>
<technology name="_177920501">
<attribute name="HEIGHT" value="10 mm"/>
<attribute name="LENGTH" value="11.5 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="2.97 - 3.63Vin, 5Vout"/>
<attribute name="WIDTH" value="6 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="177920501"/>
<attribute name="INPUT_VOLTAGE" value="2.97 - 3.63V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="1000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/177920501?ae"/>
</technology>
<technology name="_177920511">
<attribute name="HEIGHT" value="10 mm"/>
<attribute name="LENGTH" value="11.5 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="WIDTH" value="6 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="177920511"/>
<attribute name="INPUT_VOLTAGE" value="4.5 - 5.5V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="1000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/177920511?ae"/>
</technology>
<technology name="_177920521">
<attribute name="HEIGHT" value="10 mm"/>
<attribute name="LENGTH" value="11.5 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="WIDTH" value="6 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="177920521"/>
<attribute name="INPUT_VOLTAGE" value="10.8 - 13.2V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="1000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/177920521?ae"/>
</technology>
<technology name="_177920531">
<attribute name="HEIGHT" value="10 mm"/>
<attribute name="LENGTH" value="11.5 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="21.6 - 26.4Vin, 5Vout"/>
<attribute name="WIDTH" value="6 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="177920531"/>
<attribute name="INPUT_VOLTAGE" value="21.6 - 26.4V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="1000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/177920531?ae"/>
</technology>
<technology name="_1779405111">
<attribute name="HEIGHT" value="10 mm"/>
<attribute name="LENGTH" value="11.5 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="WIDTH" value="6 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1779405111"/>
<attribute name="INPUT_VOLTAGE" value="4.5 - 5.5V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="2 W"/>
<attribute name="ISOLATION_VOLTAGE" value="1500 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1779405111?ae"/>
</technology>
<technology name="_1779405211">
<attribute name="HEIGHT" value="10 mm"/>
<attribute name="LENGTH" value="11.5 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="WIDTH" value="6 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1779405211"/>
<attribute name="INPUT_VOLTAGE" value="10.8 - 13.2V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="2 W"/>
<attribute name="ISOLATION_VOLTAGE" value="1500 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1779405211?ae"/>
</technology>
<technology name="_1779405311">
<attribute name="HEIGHT" value="10 mm"/>
<attribute name="LENGTH" value="11.5 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="21.6 - 26.4Vin, 5Vout"/>
<attribute name="WIDTH" value="6 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1779405311"/>
<attribute name="INPUT_VOLTAGE" value="21.6 - 26.4V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="2 W"/>
<attribute name="ISOLATION_VOLTAGE" value="1500 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1779405311?ae"/>
</technology>
</technologies>
</device>
<device name="_1779205311" package="WPME-FISM_SIP-4_1779205311">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="4"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="10 mm"/>
<attribute name="LENGTH" value="11.5 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="21.6 - 26.4Vin, 5Vout"/>
<attribute name="WIDTH" value="6 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1779205311"/>
<attribute name="INPUT_VOLTAGE" value="21.6 - 26.4V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="1500 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1779205311?ae"/>
</technology>
</technologies>
</device>
<device name="_1779205111" package="WPME-FISM_SIP-4_1779205111">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="4"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="10 mm"/>
<attribute name="LENGTH" value="11.5 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="WIDTH" value="6 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1779205111"/>
<attribute name="INPUT_VOLTAGE" value="4.5 - 5.5V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="3000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1779205111?ae"/>
</technology>
</technologies>
</device>
<device name="_1779205211" package="WPME-FISM_SIP-4_1779205211">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="4"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="10 mm"/>
<attribute name="LENGTH" value="11.5 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="WIDTH" value="6 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1779205211"/>
<attribute name="INPUT_VOLTAGE" value="10.8 - 13.2V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="3000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1779205211?ae"/>
</technology>
</technologies>
</device>
<device name="_1779205011" package="WPME-FISM_SIP-4_1779205011">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="4"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="10 mm"/>
<attribute name="LENGTH" value="11.5 mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="2.79 - 3.63Vin, 5Vout"/>
<attribute name="WIDTH" value="6 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1779205011"/>
<attribute name="INPUT_VOLTAGE" value="2.79 - 3.63V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="3000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1779205011?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WPME-FISM_SMT-8" prefix="U">
<description>MagI³C-FISM Fixed Isolated SIP / SMT Module

Unregulated output voltage

Characteristics

Simple design (no transformer design know how required)

Leaded through-hole package for easy manufacturing and prototyping

Stand-alone solution (CIN and COUT integrated, no external components)

Simple functional isolation for overvoltage protection, avoiding ground loops, ground shift and noise in signal path or sensor systems

Industrial standard package and pin configuration

Low conducted and radiated EMI (compliant to EN55022 class B)

UL60950 certified

Applications

Data acquisition

Test and measurement systems

Interface and microcontroller supply

Industrial control

Details see: www.we-online.com/en/components/products/MAGIC-FISM

Updated by Ella 2026-04-27

2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-FISM_SMT-8"/>
</gates>
<devices>
<device name="_L12.75W10.7H6.95" package="WPME-FISM_SMT-8_L12.75W10.7H6.95">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="5"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="4"/>
</connects>
<technologies>
<technology name="_176920502">
<attribute name="HEIGHT" value="6.7 mm"/>
<attribute name="LENGTH" value="12.75 mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="2.97 - 3.63Vin, 5Vout"/>
<attribute name="WIDTH" value="10.7 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="176920502"/>
<attribute name="INPUT_VOLTAGE" value="2.97 - 3.63V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="2000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/176920502?ae"/>
</technology>
<technology name="_176920512">
<attribute name="HEIGHT" value="6.7 mm"/>
<attribute name="LENGTH" value="12.75 mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="WIDTH" value="10.7 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="176920512"/>
<attribute name="INPUT_VOLTAGE" value="4.5 - 5.5V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="2000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/176920512?ae"/>
</technology>
<technology name="_176920522">
<attribute name="HEIGHT" value="6.7 mm"/>
<attribute name="LENGTH" value="12.75 mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="WIDTH" value="10.7 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="176920522"/>
<attribute name="INPUT_VOLTAGE" value="10.8 - 13.2V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="2000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/176920522?ae"/>
</technology>
</technologies>
</device>
<device name="_1769205141" package="WPME-FISM_SMT-8_1769205141">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="5"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="6.25 mm"/>
<attribute name="LENGTH" value="12.7 mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="WIDTH" value="11.05 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1769205141"/>
<attribute name="INPUT_VOLTAGE" value="4.5 - 5.5V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="4000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1769205141?ae"/>
</technology>
</technologies>
</device>
<device name="_1769205241" package="WPME-FISM_SMT-8_1769205241">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="5"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="6.25 mm"/>
<attribute name="LENGTH" value="12.7 mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="WIDTH" value="11.05 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1769205241"/>
<attribute name="INPUT_VOLTAGE" value="10.8 - 13.2V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="4000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1769205241?ae"/>
</technology>
</technologies>
</device>
<device name="_1769205041" package="WPME-FISM_SMT-8_1769205041">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="5"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="6.25 mm"/>
<attribute name="LENGTH" value="12.7 mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="2.97 - 3.63Vin, 5Vout"/>
<attribute name="WIDTH" value="11.05 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1769205041"/>
<attribute name="INPUT_VOLTAGE" value="2.97 - 3.63V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="4000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1769205041?ae"/>
</technology>
</technologies>
</device>
<device name="_1769205341" package="WPME-FISM_SMT-8_1769205341">
<connects>
<connect gate="G$1" pin="+VIN" pad="3"/>
<connect gate="G$1" pin="+VOUT" pad="8"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="6.9 mm"/>
<attribute name="LENGTH" value="12.8 mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="21.6 - 26.4Vin, 5Vout"/>
<attribute name="WIDTH" value="11.1 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1769205341"/>
<attribute name="INPUT_VOLTAGE" value="21.6 - 26.4V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="3000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1769205341?ae"/>
</technology>
</technologies>
</device>
<device name="_1769405141" package="WPME-FISM_SMT-8_1769405141">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="5"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="6.25 mm"/>
<attribute name="LENGTH" value="12.7 mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="WIDTH" value="11.05 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1769405141"/>
<attribute name="INPUT_VOLTAGE" value="4.5 - 5.5V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="2 W"/>
<attribute name="ISOLATION_VOLTAGE" value="4000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1769405141?ae"/>
</technology>
</technologies>
</device>
<device name="_1769405241" package="WPME-FISM_SMT-8_1769405241">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="5"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="6.25 mm"/>
<attribute name="LENGTH" value="12.7 mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="WIDTH" value="11.05 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1769405241"/>
<attribute name="INPUT_VOLTAGE" value="10.8 - 13.2V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="2 W"/>
<attribute name="ISOLATION_VOLTAGE" value="4000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1769405241?ae"/>
</technology>
</technologies>
</device>
<device name="_1769405341" package="WPME-FISM_SMT-8_1769405341">
<connects>
<connect gate="G$1" pin="+VIN" pad="3"/>
<connect gate="G$1" pin="+VOUT" pad="8"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="6.9 mm"/>
<attribute name="LENGTH" value="12.8 mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="21.6 - 26.4Vin, 5Vout"/>
<attribute name="WIDTH" value="11.1 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1769405341"/>
<attribute name="INPUT_VOLTAGE" value="21.6 - 26.4V"/>
<attribute name="OUTPUT_VOLTAGE" value="5V"/>
<attribute name="OUTPUT_POWER" value="2 W"/>
<attribute name="ISOLATION_VOLTAGE" value="3000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1769405341?ae"/>
</technology>
</technologies>
</device>
<device name="_1768812141" package="WPME-FISM_SMT-8_1768812141">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="5"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="6.25 mm"/>
<attribute name="LENGTH" value="12.7 mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 12Vout"/>
<attribute name="WIDTH" value="11.05 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1768812141"/>
<attribute name="INPUT_VOLTAGE" value="4.5 - 5.5V"/>
<attribute name="OUTPUT_VOLTAGE" value="12V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="4000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1768812141?ae"/>
</technology>
</technologies>
</device>
<device name="_1768812241" package="WPME-FISM_SMT-8_1768812241">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="5"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="6.25 mm"/>
<attribute name="LENGTH" value="12.7 mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 12Vout"/>
<attribute name="WIDTH" value="11.05 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1768812241"/>
<attribute name="INPUT_VOLTAGE" value="10.8 - 13.2V"/>
<attribute name="OUTPUT_VOLTAGE" value="12V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="4000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1768812241?ae"/>
</technology>
</technologies>
</device>
<device name="_1768812341" package="WPME-FISM_SMT-8_1768812341">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="5"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="HEIGHT" value="6.9 mm"/>
<attribute name="LENGTH" value="12.8 mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="21.6 - 26.4Vin, 12Vout"/>
<attribute name="WIDTH" value="11.1 mm"/>
<attribute name="CATEGORY" value="Power Modules"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="1768812341"/>
<attribute name="INPUT_VOLTAGE" value="21.6 - 26.4V"/>
<attribute name="OUTPUT_VOLTAGE" value="12V"/>
<attribute name="OUTPUT_POWER" value="1 W"/>
<attribute name="ISOLATION_VOLTAGE" value="4000 V"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/1768812341?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
