<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Modules (MagI³C Series) - Step Down Converter - Variable Output Voltage - WPME-VDLM &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-07-30&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WPME-VDLM_LGA-16EP">
<description>&lt;b&gt;MagI³C-VDLM Variable Step Down LGA Module
&lt;br&gt;&lt;/b&gt;Size : LGA-16EP, SMT
&lt;BR&gt;LxWxH=9mm x 9mm x 3mm</description>
</package>
<package name="WPME-VDLM_LGA-12EP">
<description>&lt;b&gt;MagI³C-VDLM Variable Step Down LGA Module
&lt;br&gt;&lt;/b&gt;Size : LGA-12EP, SMT
&lt;BR&gt;LxWxH=10mm x 6mm x 3.1mm</description>
</package>
<package name="WPME-VDLM_LGA-26">
<description>&lt;b&gt;MagI³C-VDLM Variable Step Down LGA Module
&lt;br&gt;&lt;/b&gt;Size : LGA-26, SMT
&lt;BR&gt;LxWxH=10mm x 6mm x 3.1mm</description>
</package>
</packages>
<symbols>
<symbol name="WPME-VDLM_1710X3601">
<pin name="VIN" direction="pwr"/>
<pin name="EN/SYNC" direction="in"/>
<pin name="PG" direction="out"/>
<pin name="AGND" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="VOUT" direction="pwr"/>
<pin name="PGND" direction="pwr"/>
<pin name="FSW" direction="in"/>
<pin name="BIAS" direction="in"/>
</symbol>
<symbol name="WPME-VDLM_1710X3801">
<pin name="VIN" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="PG" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="VOUT" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="FSW" direction="pas"/>
<pin name="VCC" direction="pas"/>
</symbol>
<symbol name="WPME-VDLM_1710X3802">
<pin name="VIN" direction="pas"/>
<pin name="EN/SYNC" direction="pas"/>
<pin name="PG" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="VOUT" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="FSW" direction="pas"/>
<pin name="VCC" direction="pas"/>
</symbol>
<symbol name="WPME-VDLM_LGA-16EP">
<pin name="13FB" direction="in"/>
<pin name="16EN" direction="in"/>
<pin name="VIN1" direction="pwr"/>
<pin name="VIN2" direction="pwr"/>
<pin name="VIN3" direction="pwr"/>
<pin name="VIN4" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="10VOUT" direction="pwr"/>
<pin name="11VOUT" direction="pwr"/>
<pin name="12VOUT" direction="pwr"/>
<pin name="9VOUT" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="171031801" prefix="U">
<description>&lt;b&gt;MagI³C-VDLM Variable Step Down LGA Module &lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-12EP&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-26&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Sync function for custom switching frequencies
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Test and measurement equipment
&lt;br&gt;Medical equipment
&lt;br&gt;Interface supply
&lt;br&gt;Supply of microcontrollers, microprocessors, DSPs, FPGAs
&lt;br&gt;Industrial electronics
&lt;br&gt;Telecommunications

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDLM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDLM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2024-11-12&lt;br&gt;
&lt;/b&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDLM_LGA-16EP"/>
</gates>
<devices>
<device name="" package="WPME-VDLM_LGA-16EP">
<connects>
<connect gate="G$1" pin="10VOUT" pad="10"/>
<connect gate="G$1" pin="11VOUT" pad="11"/>
<connect gate="G$1" pin="12VOUT" pad="12"/>
<connect gate="G$1" pin="13FB" pad="13"/>
<connect gate="G$1" pin="16EN" pad="16"/>
<connect gate="G$1" pin="9VOUT" pad="9"/>
<connect gate="G$1" pin="GND" pad="EP1 EP2 EP3 EP4"/>
<connect gate="G$1" pin="VIN1" pad="1"/>
<connect gate="G$1" pin="VIN2" pad="2"/>
<connect gate="G$1" pin="VIN3" pad="3"/>
<connect gate="G$1" pin="VIN4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171031801?ae"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="I-OUTPUT" value="3A"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171031801"/>
<attribute name="SIZE" value="LGA-16EP"/>
<attribute name="V-INPUT" value="4 - 18Vin"/>
<attribute name="V-OUTPUT" value="0.8 - 17Vout"/>
<attribute name="VALUE" value="4 - 18Vin, 0.8 - 17Vout, 3A"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171021801" prefix="U">
<description>&lt;b&gt;MagI³C-VDLM Variable Step Down LGA Module &lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-12EP&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-26&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Sync function for custom switching frequencies
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Test and measurement equipment
&lt;br&gt;Medical equipment
&lt;br&gt;Interface supply
&lt;br&gt;Supply of microcontrollers, microprocessors, DSPs, FPGAs
&lt;br&gt;Industrial electronics
&lt;br&gt;Telecommunications

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDLM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDLM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2024-11-12&lt;br&gt;
&lt;/b&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDLM_LGA-16EP"/>
</gates>
<devices>
<device name="" package="WPME-VDLM_LGA-16EP">
<connects>
<connect gate="G$1" pin="10VOUT" pad="10"/>
<connect gate="G$1" pin="11VOUT" pad="11"/>
<connect gate="G$1" pin="12VOUT" pad="12"/>
<connect gate="G$1" pin="13FB" pad="13"/>
<connect gate="G$1" pin="16EN" pad="16"/>
<connect gate="G$1" pin="9VOUT" pad="9"/>
<connect gate="G$1" pin="GND" pad="EP1 EP2 EP3 EP4"/>
<connect gate="G$1" pin="VIN1" pad="1"/>
<connect gate="G$1" pin="VIN2" pad="2"/>
<connect gate="G$1" pin="VIN3" pad="3"/>
<connect gate="G$1" pin="VIN4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171021801?ae"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="I-OUTPUT" value="2A"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171021801"/>
<attribute name="SIZE" value="LGA-16EP"/>
<attribute name="V-INPUT" value="4 - 18Vin"/>
<attribute name="V-OUTPUT" value="0.8 - 17Vout"/>
<attribute name="VALUE" value="4 - 18Vin, 0.8 - 17Vout, 2A"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171011801" prefix="U">
<description>&lt;b&gt;MagI³C-VDLM Variable Step Down LGA Module &lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-12EP&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-26&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Sync function for custom switching frequencies
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Test and measurement equipment
&lt;br&gt;Medical equipment
&lt;br&gt;Interface supply
&lt;br&gt;Supply of microcontrollers, microprocessors, DSPs, FPGAs
&lt;br&gt;Industrial electronics
&lt;br&gt;Telecommunications

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDLM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDLM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2024-11-12&lt;br&gt;
&lt;/b&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDLM_LGA-16EP"/>
</gates>
<devices>
<device name="" package="WPME-VDLM_LGA-16EP">
<connects>
<connect gate="G$1" pin="10VOUT" pad="10"/>
<connect gate="G$1" pin="11VOUT" pad="11"/>
<connect gate="G$1" pin="12VOUT" pad="12"/>
<connect gate="G$1" pin="13FB" pad="13"/>
<connect gate="G$1" pin="16EN" pad="16"/>
<connect gate="G$1" pin="9VOUT" pad="9"/>
<connect gate="G$1" pin="GND" pad="EP1 EP2 EP3 EP4"/>
<connect gate="G$1" pin="VIN1" pad="1"/>
<connect gate="G$1" pin="VIN2" pad="2"/>
<connect gate="G$1" pin="VIN3" pad="3"/>
<connect gate="G$1" pin="VIN4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171011801?ae"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="I-OUTPUT" value="1A"/>
<attribute name="LENGTH" value="9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171011801"/>
<attribute name="SIZE" value="LGA-16EP"/>
<attribute name="V-INPUT" value="4 - 18Vin"/>
<attribute name="V-OUTPUT" value="0.8 - 17Vout"/>
<attribute name="VALUE" value="4 - 18Vin, 0.8 - 17Vout, 1A"/>
<attribute name="WIDTH" value="9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171033801" prefix="U">
<description>&lt;b&gt;MagI³C-VDLM Variable Step Down LGA Module &lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-12EP&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-26&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Sync function for custom switching frequencies
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Test and measurement equipment
&lt;br&gt;Medical equipment
&lt;br&gt;Interface supply
&lt;br&gt;Supply of microcontrollers, microprocessors, DSPs, FPGAs
&lt;br&gt;Industrial electronics
&lt;br&gt;Telecommunications

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDLM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDLM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2024-11-12&lt;br&gt;
&lt;/b&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDLM_1710X3801"/>
</gates>
<devices>
<device name="" package="WPME-VDLM_LGA-12EP">
<connects>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="EN" pad="12"/>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="FSW" pad="1"/>
<connect gate="G$1" pin="PG" pad="11"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VIN" pad="4 5 9" route="any"/>
<connect gate="G$1" pin="VOUT" pad="6 7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171033801?ae"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="I-OUTPUT" value="3A"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171033801"/>
<attribute name="SIZE" value="LGA-12EP"/>
<attribute name="V-INPUT" value="3.5 - 38Vin"/>
<attribute name="V-OUTPUT" value="0.85 - 6Vout"/>
<attribute name="VALUE" value="3.5 - 38Vin, 0.85 - 6Vout, 3A"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171013802" prefix="U">
<description>&lt;b&gt;MagI³C-VDLM Variable Step Down LGA Module &lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-12EP&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-26&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Sync function for custom switching frequencies
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Test and measurement equipment
&lt;br&gt;Medical equipment
&lt;br&gt;Interface supply
&lt;br&gt;Supply of microcontrollers, microprocessors, DSPs, FPGAs
&lt;br&gt;Industrial electronics
&lt;br&gt;Telecommunications

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDLM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDLM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2024-11-12&lt;br&gt;
&lt;/b&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDLM_1710X3802"/>
</gates>
<devices>
<device name="" package="WPME-VDLM_LGA-12EP">
<connects>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="EN/SYNC" pad="12"/>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="FSW" pad="1"/>
<connect gate="G$1" pin="PG" pad="11"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VIN" pad="4 5 9"/>
<connect gate="G$1" pin="VOUT" pad="6 7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171013802?ae"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="I-OUTPUT" value="1A"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171013802"/>
<attribute name="SIZE" value="LGA-12EP"/>
<attribute name="V-INPUT" value="3.5 - 38Vin"/>
<attribute name="V-OUTPUT" value="0.85 - 13Vout"/>
<attribute name="VALUE" value="3.5 - 38Vin, 0.85 - 13Vout, 1A"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171023802" prefix="U">
<description>&lt;b&gt;MagI³C-VDLM Variable Step Down LGA Module &lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-12EP&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-26&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Sync function for custom switching frequencies
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Test and measurement equipment
&lt;br&gt;Medical equipment
&lt;br&gt;Interface supply
&lt;br&gt;Supply of microcontrollers, microprocessors, DSPs, FPGAs
&lt;br&gt;Industrial electronics
&lt;br&gt;Telecommunications

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDLM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDLM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2024-11-12&lt;br&gt;
&lt;/b&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDLM_1710X3802"/>
</gates>
<devices>
<device name="" package="WPME-VDLM_LGA-12EP">
<connects>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="EN/SYNC" pad="12"/>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="FSW" pad="1"/>
<connect gate="G$1" pin="PG" pad="11"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VIN" pad="4 5 9"/>
<connect gate="G$1" pin="VOUT" pad="6 7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171023802?ae"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="I-OUTPUT" value="2A"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171023802"/>
<attribute name="SIZE" value="LGA-12EP"/>
<attribute name="V-INPUT" value="3.5 - 38Vin"/>
<attribute name="V-OUTPUT" value="0.85 - 13Vout"/>
<attribute name="VALUE" value="3.5 - 38Vin, 0.85 - 13Vout, 2A"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171033802" prefix="U">
<description>&lt;b&gt;MagI³C-VDLM Variable Step Down LGA Module &lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-12EP&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-26&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Sync function for custom switching frequencies
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Test and measurement equipment
&lt;br&gt;Medical equipment
&lt;br&gt;Interface supply
&lt;br&gt;Supply of microcontrollers, microprocessors, DSPs, FPGAs
&lt;br&gt;Industrial electronics
&lt;br&gt;Telecommunications

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDLM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDLM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2024-11-12&lt;br&gt;
&lt;/b&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDLM_1710X3802"/>
</gates>
<devices>
<device name="" package="WPME-VDLM_LGA-12EP">
<connects>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="EN/SYNC" pad="12"/>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="FSW" pad="1"/>
<connect gate="G$1" pin="PG" pad="11"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VIN" pad="4 5 9"/>
<connect gate="G$1" pin="VOUT" pad="6 7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171033802?ae"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="I-OUTPUT" value="3A"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171033802"/>
<attribute name="SIZE" value="LGA-12EP"/>
<attribute name="V-INPUT" value="3.5 - 38Vin"/>
<attribute name="V-OUTPUT" value="0.85 - 6Vout"/>
<attribute name="VALUE" value="3.5 - 38Vin, 0.85 - 6Vout, 3A"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171053601" prefix="U">
<description>&lt;b&gt;MagI³C-VDLM Variable Step Down LGA Module &lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-12EP&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-26&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Sync function for custom switching frequencies
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Test and measurement equipment
&lt;br&gt;Medical equipment
&lt;br&gt;Interface supply
&lt;br&gt;Supply of microcontrollers, microprocessors, DSPs, FPGAs
&lt;br&gt;Industrial electronics
&lt;br&gt;Telecommunications

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDLM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDLM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2025-07-30&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDLM_1710X3601"/>
</gates>
<devices>
<device name="" package="WPME-VDLM_LGA-26">
<connects>
<connect gate="G$1" pin="AGND" pad="B4"/>
<connect gate="G$1" pin="BIAS" pad="A4"/>
<connect gate="G$1" pin="EN/SYNC" pad="C1"/>
<connect gate="G$1" pin="FB" pad="A1"/>
<connect gate="G$1" pin="FSW" pad="C4"/>
<connect gate="G$1" pin="PG" pad="B1"/>
<connect gate="G$1" pin="PGND" pad="E1 E2 E3 E4 F1 F2 F3 F4"/>
<connect gate="G$1" pin="VIN" pad="D1 D2 D3 D4"/>
<connect gate="G$1" pin="VOUT" pad="G1 G2 G3 G4 H1 H2 H3 H4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171053601?ae"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="I-OUTPUT" value="5A"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171053601"/>
<attribute name="SIZE" value="LGA-26"/>
<attribute name="V-INPUT" value="4 - 36Vin"/>
<attribute name="V-OUTPUT" value="1 - 6Vout"/>
<attribute name="VALUE" value="4 - 36Vin, 1 - 6Vout, 5A"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171043601" prefix="U">
<description>&lt;b&gt;MagI³C-VDLM Variable Step Down LGA Module &lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-12EP&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-26&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Sync function for custom switching frequencies
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Test and measurement equipment
&lt;br&gt;Medical equipment
&lt;br&gt;Interface supply
&lt;br&gt;Supply of microcontrollers, microprocessors, DSPs, FPGAs
&lt;br&gt;Industrial electronics
&lt;br&gt;Telecommunications

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDLM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDLM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu 2025-07-30&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDLM_1710X3601"/>
</gates>
<devices>
<device name="" package="WPME-VDLM_LGA-26">
<connects>
<connect gate="G$1" pin="AGND" pad="B4"/>
<connect gate="G$1" pin="BIAS" pad="A4"/>
<connect gate="G$1" pin="EN/SYNC" pad="C1"/>
<connect gate="G$1" pin="FB" pad="A1"/>
<connect gate="G$1" pin="FSW" pad="C4"/>
<connect gate="G$1" pin="PG" pad="B1"/>
<connect gate="G$1" pin="PGND" pad="E1 E2 E3 E4 F1 F2 F3 F4"/>
<connect gate="G$1" pin="VIN" pad="D1 D2 D3 D4"/>
<connect gate="G$1" pin="VOUT" pad="G1 G2 G3 G4 H1 H2 H3 H4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171043601?ae"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="I-OUTPUT" value="4A"/>
<attribute name="LENGTH" value="11mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171043601"/>
<attribute name="SIZE" value="LGA-26"/>
<attribute name="V-INPUT" value="4 - 36Vin"/>
<attribute name="V-OUTPUT" value="1 - 6Vout"/>
<attribute name="VALUE" value="4 - 36Vin, 1 - 6Vout, 4A"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171023801" prefix="U">
<description>&lt;b&gt;MagI³C-VDLM Variable Step Down LGA Module &lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-12EP&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-26&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Sync function for custom switching frequencies
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Test and measurement equipment
&lt;br&gt;Medical equipment
&lt;br&gt;Interface supply
&lt;br&gt;Supply of microcontrollers, microprocessors, DSPs, FPGAs
&lt;br&gt;Industrial electronics
&lt;br&gt;Telecommunications

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDLM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDLM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2024-11-12&lt;br&gt;
&lt;/b&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDLM_1710X3801"/>
</gates>
<devices>
<device name="" package="WPME-VDLM_LGA-12EP">
<connects>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="EN" pad="12"/>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="FSW" pad="1"/>
<connect gate="G$1" pin="PG" pad="11"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VIN" pad="4 5 9" route="any"/>
<connect gate="G$1" pin="VOUT" pad="6 7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171023801?ae"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="I-OUTPUT" value="2A"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171023801"/>
<attribute name="SIZE" value="LGA-12EP"/>
<attribute name="V-INPUT" value="3.5 - 38Vin"/>
<attribute name="V-OUTPUT" value="0.85 - 13Vout"/>
<attribute name="VALUE" value="3.5 - 38Vin, 0.85 - 13Vout, 2A"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="171013801" prefix="U">
<description>&lt;b&gt;MagI³C-VDLM Variable Step Down LGA Module &lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-12EP&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported

&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-26&lt;/b&gt;
&lt;br&gt;For direct connection to 24 V industrial voltage network
&lt;br&gt;Sync function for custom switching frequencies
&lt;br&gt;Low profile LGA-package
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Point-of-Load DC-DC applications from 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Test and measurement equipment
&lt;br&gt;Medical equipment
&lt;br&gt;Interface supply
&lt;br&gt;Supply of microcontrollers, microprocessors, DSPs, FPGAs
&lt;br&gt;Industrial electronics
&lt;br&gt;Telecommunications

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o683498v209%20Family_Magic-VDLM_171013801_171011801.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-VDLM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-VDLM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2024-11-12&lt;br&gt;
&lt;/b&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-VDLM_1710X3801"/>
</gates>
<devices>
<device name="" package="WPME-VDLM_LGA-12EP">
<connects>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="EN" pad="12"/>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="FSW" pad="1"/>
<connect gate="G$1" pin="PG" pad="11"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VIN" pad="4 5 9" route="any"/>
<connect gate="G$1" pin="VOUT" pad="6 7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/171013801?ae"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="I-OUTPUT" value="1A"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="171013801"/>
<attribute name="SIZE" value="LGA-12EP"/>
<attribute name="V-INPUT" value="3.5 - 38Vin"/>
<attribute name="V-OUTPUT" value="0.85 - 13Vout"/>
<attribute name="VALUE" value="3.5 - 38Vin, 0.85 - 13Vout, 1A"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
