<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Circular Connectors - WR-CIRC &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-06-10&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="643250100305">
<description>&lt;b&gt;WR-CIRCM12 Panel Connector PCB Metal M12&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="643280100305">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector Angled 90° Female Metal M12&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="643230100405">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Angled 90° Plastic M16&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="643220100608">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="643260100605">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector Female Metal PG9&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="643250100304">
<description>&lt;b&gt;WR-CIRCM12 Panel Connector PCB Metal M12&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="643250100608">
<description>&lt;b&gt;WR-CIRCM12 Panel Connector PCB Metal M12&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="643220100408">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="643220100605">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="643220100405">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="643210100605">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="643280100304">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector Angled 90° Female Metal M12&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="643240100405">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Female Angled 90° Plastic M16&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="643240100408">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Female Angled 90° Plastic M16&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="643260100608">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector Female Metal PG9&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="643210100405">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic M16&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="643250100308">
<description>&lt;b&gt;WR-CIRCM12 Panel Connector PCB Metal M12&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="643210100404">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic M16&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="643210100608">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="643210100408">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic M16&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="643280100308">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector Angled 90° Female Metal M12&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="643230100404">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Angled 90° Plastic M16&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="643270100304">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Angled 90° Metal M12&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="643220100604">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="643250100604">
<description>&lt;b&gt;WR-CIRCM12 Panel Connector PCB Metal M12&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="643270100308">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Angled 90° Metal M12&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="643260100604">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector Female Metal PG9&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="643260100405">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Female Metal M16&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="643220110004">
<description>&lt;b&gt;WR-CIRCM12 A Shieldingless socket Female THT&lt;/b&gt;
&lt;br&gt;&lt;br&gt;THT, 4pins</description>
</package>
<package name="643240100404">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Female Angled 90° Plastic M16&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="643220110005">
<description>&lt;b&gt;WR-CIRCM12 A Shieldingless socket Female THT&lt;/b&gt;
&lt;br&gt;&lt;br&gt;THT, 5pins</description>
</package>
<package name="643260100408">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Female Metal M16&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="643270100305">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Angled 90° Metal M12&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="643260100404">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Female Metal M16&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="643250100605">
<description>&lt;b&gt;WR-CIRCM12 Panel Connector PCB Metal M12&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="643250100405">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Metal M16&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="643230100408">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Angled 90° Plastic M16&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="643210100604">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="643250100404">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Metal M16&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="643250100408">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Metal M16&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="643220100404">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;br&gt;
&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
</packages>
<symbols>
<symbol name="MALE_5PINS">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="FEMALE_5PINS">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="FEMALE_8PINS">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="MALE_4PINS">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="MALE_8PINS">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="FEMALE_5PINS_SHIELD">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="FEMALE_4PINS_SHIELD">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="FEMALE_8PINS_SHIELD">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="MALE_4PINS_SHIELD">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="FEMALE_4PINS">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="MALE_8PINS_SHIELD">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="MALE_5PINS_SHIELD">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="643250100305" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Panel Connector PCB Metal M12&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722357v209%20family-wr-circm12-6432501003xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722357v209%20family-wr-circm12-6432501003xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_M12"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_M12&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_5PINS"/>
</gates>
<devices>
<device name="" package="643250100305">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643250100305?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643250100305"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643250100305"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1000V"/>
<attribute name="WORKING-VOLTAGE" value="60V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643280100305" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector Angled 90° Female Metal M12&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Female
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;nsulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722386v209%20family-wr-circ-m12a-6432801003xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722386v209%20family-wr-circ-m12a-6432801003xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_ANGLED_90_FEMALE_METAL_M12"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_ANGLED_90_FEMALE_METAL_M12&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_5PINS_SHIELD"/>
</gates>
<devices>
<device name="" package="643280100305">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="SHIELD" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643280100305?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643280100305"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643280100305"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1000V"/>
<attribute name="WORKING-VOLTAGE" value="60V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643230100405" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Angled 90° Plastic M16&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722353v209%20family-wr-circm12-6432301004xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722353v209%20family-wr-circm12-6432301004xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_ANGLED_PLASTICM16"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_ANGLED_PLASTICM16&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-03-14&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_5PINS"/>
</gates>
<devices>
<device name="" package="643230100405">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643230100405?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643230100405"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643230100405"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1000V"/>
<attribute name="WORKING-VOLTAGE" value="60V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643220100608" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Female
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722376v209%20family-wr-circm12-6432201006xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722376v209%20family-wr-circm12-6432201006xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_PLASTIC_PG9"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_PLASTIC_PG9&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_8PINS"/>
</gates>
<devices>
<device name="" package="643220100608">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643220100608?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643220100608"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="RATED-CURRENT" value="2A"/>
<attribute name="VALUE" value="643220100608"/>
<attribute name="WITHSTANDING-VOLTAGE" value="650V"/>
<attribute name="WORKING-VOLTAGE" value="30V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643260100605" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector Female Metal PG9&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Female
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722384v209%20family-wr-circ-m12-6432601006xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722384v209%20family-wr-circ-m12-6432601006xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_FEMALE_METAL_PG9"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_FEMALE_METAL_PG9&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-03-14&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_5PINS"/>
</gates>
<devices>
<device name="" package="643260100605">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643260100605?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643260100605"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643260100605"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1000V"/>
<attribute name="WORKING-VOLTAGE" value="60V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643250100304" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Panel Connector PCB Metal M12&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722357v209%20family-wr-circm12-6432501003xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722357v209%20family-wr-circm12-6432501003xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_M12"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_M12&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_4PINS"/>
</gates>
<devices>
<device name="" package="643250100304">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643250100304?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643250100304"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643250100304"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1400V"/>
<attribute name="WORKING-VOLTAGE" value="250V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643250100608" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Panel Connector PCB Metal M12&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722364v209%20family-wrcircm12-6432501006xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722364v209%20family-wrcircm12-6432501006xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_PG9"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_PG9&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_8PINS"/>
</gates>
<devices>
<device name="" package="643250100608">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643250100608?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643250100608"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="RATED-CURRENT" value="2A"/>
<attribute name="VALUE" value="643250100608"/>
<attribute name="WITHSTANDING-VOLTAGE" value="650V"/>
<attribute name="WORKING-VOLTAGE" value="30V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643220100408" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Female
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722375v209%20family-wr-circm12-6432201004xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722375v209%20family-wr-circm12-6432201004xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_PLASTIC_M16"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_PLASTIC_M16&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_8PINS"/>
</gates>
<devices>
<device name="" package="643220100408">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643220100408?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643220100408"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="RATED-CURRENT" value="2A"/>
<attribute name="VALUE" value="643220100408"/>
<attribute name="WITHSTANDING-VOLTAGE" value="650V"/>
<attribute name="WORKING-VOLTAGE" value="30V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643220100405" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Female
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722375v209%20family-wr-circm12-6432201004xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722375v209%20family-wr-circm12-6432201004xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_PLASTIC_M16"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_PLASTIC_M16&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_5PINS"/>
</gates>
<devices>
<device name="" package="643220100405">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643220100405?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643220100405"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643220100405"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1000V"/>
<attribute name="WORKING-VOLTAGE" value="60V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643220100605" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Female
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722376v209%20family-wr-circm12-6432201006xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722376v209%20family-wr-circm12-6432201006xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_PLASTIC_PG9"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_PLASTIC_PG9&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_5PINS"/>
</gates>
<devices>
<device name="" package="643220100605">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643220100605?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643220100605"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643220100605"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1000V"/>
<attribute name="WORKING-VOLTAGE" value="60V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643210100605" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722351v209%20family-wr-circm12-6432101006xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722351v209%20family-wr-circm12-6432101006xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_PLASTIC_PG9"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_PLASTIC_PG9&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_5PINS"/>
</gates>
<devices>
<device name="" package="643210100605">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643210100605?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643210100605"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643210100605"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1000V"/>
<attribute name="WORKING-VOLTAGE" value="60V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643280100304" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector Angled 90° Female Metal M12&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Female
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;nsulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722386v209%20family-wr-circ-m12a-6432801003xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722386v209%20family-wr-circ-m12a-6432801003xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_ANGLED_90_FEMALE_METAL_M12"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_ANGLED_90_FEMALE_METAL_M12&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_4PINS_SHIELD"/>
</gates>
<devices>
<device name="" package="643280100304">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643280100304?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643280100304"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643280100304"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1400V"/>
<attribute name="WORKING-VOLTAGE" value="250V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643240100405" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Female Angled 90° Plastic M16&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Female
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722380v209%20family-wr-circm12-6432401004xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722380v209%20family-wr-circm12-6432401004xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_ANGLED_90_PLASTIC_M16"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_ANGLED_90_PLASTIC_M16&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-03-14&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_5PINS"/>
</gates>
<devices>
<device name="" package="643240100405">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643240100405?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643240100405"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643240100405"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1000V"/>
<attribute name="WORKING-VOLTAGE" value="60V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643240100408" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Female Angled 90° Plastic M16&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Female
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722380v209%20family-wr-circm12-6432401004xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722380v209%20family-wr-circm12-6432401004xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_ANGLED_90_PLASTIC_M16"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_ANGLED_90_PLASTIC_M16&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-03-14&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_8PINS"/>
</gates>
<devices>
<device name="" package="643240100408">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643240100408?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643240100408"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="RATED-CURRENT" value="2A"/>
<attribute name="VALUE" value="643240100408"/>
<attribute name="WITHSTANDING-VOLTAGE" value="650V"/>
<attribute name="WORKING-VOLTAGE" value="30V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643260100608" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector Female Metal PG9&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Female
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722384v209%20family-wr-circ-m12-6432601006xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722384v209%20family-wr-circ-m12-6432601006xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_FEMALE_METAL_PG9"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_FEMALE_METAL_PG9&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-03-14&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_8PINS"/>
</gates>
<devices>
<device name="" package="643260100608">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643260100608?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643260100608"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="RATED-CURRENT" value="2A"/>
<attribute name="VALUE" value="643260100608"/>
<attribute name="WITHSTANDING-VOLTAGE" value="650V"/>
<attribute name="WORKING-VOLTAGE" value="30V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643250100308" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Panel Connector PCB Metal M12&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722357v209%20family-wr-circm12-6432501003xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722357v209%20family-wr-circm12-6432501003xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_M12"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_M12&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_8PINS"/>
</gates>
<devices>
<device name="" package="643250100308">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643250100308?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643250100308"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="RATED-CURRENT" value="2A"/>
<attribute name="VALUE" value="643250100308"/>
<attribute name="WITHSTANDING-VOLTAGE" value="650V"/>
<attribute name="WORKING-VOLTAGE" value="30V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643210100405" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic M16&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 °C up to +90 °C
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722350v209%20family-wr-circm12-6432101004xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722350v209%20family-wr-circm12-6432101004xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_PLASTIC_M16"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_PLASTIC_M16&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_5PINS"/>
</gates>
<devices>
<device name="" package="643210100405">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643210100405?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643210100405"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643210100405"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1000V"/>
<attribute name="WORKING-VOLTAGE" value="60V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643210100404" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic M16&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 °C up to +90 °C
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722350v209%20family-wr-circm12-6432101004xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722350v209%20family-wr-circm12-6432101004xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_PLASTIC_M16"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_PLASTIC_M16&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_4PINS"/>
</gates>
<devices>
<device name="" package="643210100404">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643210100404?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643210100404"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643210100404"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1400V"/>
<attribute name="WORKING-VOLTAGE" value="250V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643210100608" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722351v209%20family-wr-circm12-6432101006xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722351v209%20family-wr-circm12-6432101006xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_PLASTIC_PG9"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_PLASTIC_PG9&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_8PINS"/>
</gates>
<devices>
<device name="" package="643210100608">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643210100608?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643210100608"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="RATED-CURRENT" value="2A"/>
<attribute name="VALUE" value="643210100608"/>
<attribute name="WITHSTANDING-VOLTAGE" value="650V"/>
<attribute name="WORKING-VOLTAGE" value="30V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643210100408" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic M16&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 °C up to +90 °C
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722350v209%20family-wr-circm12-6432101004xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722350v209%20family-wr-circm12-6432101004xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_PLASTIC_M16"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_PLASTIC_M16&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_8PINS"/>
</gates>
<devices>
<device name="" package="643210100408">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643210100408?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643210100408"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="RATED-CURRENT" value="2A"/>
<attribute name="VALUE" value="643210100408"/>
<attribute name="WITHSTANDING-VOLTAGE" value="650V"/>
<attribute name="WORKING-VOLTAGE" value="30V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643280100308" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector Angled 90° Female Metal M12&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Female
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;nsulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722386v209%20family-wr-circ-m12a-6432801003xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722386v209%20family-wr-circ-m12a-6432801003xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_ANGLED_90_FEMALE_METAL_M12"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_ANGLED_90_FEMALE_METAL_M12&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_8PINS_SHIELD"/>
</gates>
<devices>
<device name="" package="643280100308">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643280100308?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643280100308"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="RATED-CURRENT" value="2A"/>
<attribute name="VALUE" value="643280100308"/>
<attribute name="WITHSTANDING-VOLTAGE" value="650V"/>
<attribute name="WORKING-VOLTAGE" value="30V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643220100604" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Female
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722376v209%20family-wr-circm12-6432201006xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722376v209%20family-wr-circm12-6432201006xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_PLASTIC_PG9"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_PLASTIC_PG9&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_4PINS"/>
</gates>
<devices>
<device name="" package="643220100604">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643220100604?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643220100604"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643220100604"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1400V"/>
<attribute name="WORKING-VOLTAGE" value="250V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643230100404" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Angled 90° Plastic M16&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722353v209%20family-wr-circm12-6432301004xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722353v209%20family-wr-circm12-6432301004xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_ANGLED_PLASTICM16"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_ANGLED_PLASTICM16&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-03-14&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_4PINS"/>
</gates>
<devices>
<device name="" package="643230100404">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643230100404?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643230100404"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643230100404"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1400V"/>
<attribute name="WORKING-VOLTAGE" value="250V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643250100604" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Panel Connector PCB Metal M12&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722364v209%20family-wrcircm12-6432501006xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722364v209%20family-wrcircm12-6432501006xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_PG9"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_PG9&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_4PINS"/>
</gates>
<devices>
<device name="" package="643250100604">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643250100604?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643250100604"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643250100604"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1400V"/>
<attribute name="WORKING-VOLTAGE" value="250V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643270100304" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Angled 90° Metal M12&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722372v209%20family-wr-circm12-6432701003xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722372v209%20family-wr-circm12-6432701003xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_ANGLED_90_METAL_M12"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_ANGLED_90_METAL_M12&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_4PINS_SHIELD"/>
</gates>
<devices>
<device name="" package="643270100304">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643270100304?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643270100304"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643270100304"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1400V"/>
<attribute name="WORKING-VOLTAGE" value="250V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643270100308" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Angled 90° Metal M12&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722372v209%20family-wr-circm12-6432701003xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722372v209%20family-wr-circm12-6432701003xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_ANGLED_90_METAL_M12"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_ANGLED_90_METAL_M12&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_8PINS_SHIELD"/>
</gates>
<devices>
<device name="" package="643270100308">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643270100308?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643270100308"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="RATED-CURRENT" value="2A"/>
<attribute name="VALUE" value="643270100308"/>
<attribute name="WITHSTANDING-VOLTAGE" value="650V"/>
<attribute name="WORKING-VOLTAGE" value="30V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643260100604" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector Female Metal PG9&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Female
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722384v209%20family-wr-circ-m12-6432601006xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722384v209%20family-wr-circ-m12-6432601006xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_FEMALE_METAL_PG9"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_FEMALE_METAL_PG9&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-03-14&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_4PINS"/>
</gates>
<devices>
<device name="" package="643260100604">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643260100604?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643260100604"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643260100604"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1400V"/>
<attribute name="WORKING-VOLTAGE" value="250V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643260100405" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Female Metal M16&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Several panel cuts available
&lt;br&gt;IP68 rated connectors
&lt;br&gt;Can work in harsh environments

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Automation industry &amp; control systems
&lt;br&gt;Sensors' connectivity
&lt;br&gt;Building automation
&lt;br&gt;Renewable energies


&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Durability	100 Mating cycles
&lt;br&gt;Operating Temperature	-40 °C up to +90 °C
&lt;br&gt;Gender	Female

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	2 A; 5 A
&lt;br&gt;Working Voltage	30 V; 60 V; 250 V
&lt;br&gt;Withstanding Voltage	650 V; 1000 V; 1400 V
&lt;br&gt;RISO	100 MΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Gold

&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o850726v209%20Family-WR-CIRCM12-6432601004xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o850726v209%20Family-WR-CIRCM12-6432601004xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_METAL_M16/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_METAL_M16&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-06-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_5PINS"/>
</gates>
<devices>
<device name="" package="643260100405">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643260100405?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643260100405"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643260100405"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1000V"/>
<attribute name="WORKING-VOLTAGE" value="60V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643220110004" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 A Shieldingless socket Female THT&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Flexible solution
&lt;br&gt;Can adapt to customer own shell design
&lt;br&gt;UL pending

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Automation industry &amp; control systems
&lt;br&gt;Sensor’s connectivity
&lt;br&gt;Building automation
&lt;br&gt;Renewable energies


&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Durability	100 Mating cycles
&lt;br&gt;Operating Temperature	-40 °C up to +90 °C
&lt;br&gt;Gender	Female

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	4 A
&lt;br&gt;Working Voltage	60 V; 250 V
&lt;br&gt;Withstanding Voltage	1000 V (AC); 1400 V (AC)
&lt;br&gt;RISO	100 MΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA9T
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Gold

&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o822938v209%20Multi-WR-CIRCM12-643220110004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o822938v209%20Multi-WR-CIRCM12-643220110004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-CIRCM12_SHIELDINGSLESS_FEM_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-CIRCM12_SHIELDINGSLESS_FEM_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-06-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_4PINS"/>
</gates>
<devices>
<device name="" package="643220110004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643220110004?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643220110004"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="RATED-CURRENT" value="4A"/>
<attribute name="VALUE" value="643220110004"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1400V"/>
<attribute name="WORKING-VOLTAGE" value="250V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643240100404" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Female Angled 90° Plastic M16&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Female
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722380v209%20family-wr-circm12-6432401004xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722380v209%20family-wr-circm12-6432401004xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_ANGLED_90_PLASTIC_M16"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_ANGLED_90_PLASTIC_M16&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-03-14&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_4PINS"/>
</gates>
<devices>
<device name="" package="643240100404">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643240100404?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643240100404"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643240100404"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1400V"/>
<attribute name="WORKING-VOLTAGE" value="250V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643220110005" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 A Shieldingless socket Female THT&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Flexible solution
&lt;br&gt;Can adapt to customer own shell design
&lt;br&gt;UL pending

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Automation industry &amp; control systems
&lt;br&gt;Sensor’s connectivity
&lt;br&gt;Building automation
&lt;br&gt;Renewable energies


&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Durability	100 Mating cycles
&lt;br&gt;Operating Temperature	-40 °C up to +90 °C
&lt;br&gt;Gender	Female

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	4 A
&lt;br&gt;Working Voltage	60 V; 250 V
&lt;br&gt;Withstanding Voltage	1000 V (AC); 1400 V (AC)
&lt;br&gt;RISO	100 MΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA9T
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Gold

&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o822938v209%20Multi-WR-CIRCM12-643220110004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o822938v209%20Multi-WR-CIRCM12-643220110004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-CIRCM12_SHIELDINGSLESS_FEM_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-CIRCM12_SHIELDINGSLESS_FEM_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-06-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_5PINS"/>
</gates>
<devices>
<device name="" package="643220110005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643220110005?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643220110005"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="RATED-CURRENT" value="4A"/>
<attribute name="VALUE" value="643220110005"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1000V"/>
<attribute name="WORKING-VOLTAGE" value="60V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643260100408" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Female Metal M16&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Several panel cuts available
&lt;br&gt;IP68 rated connectors
&lt;br&gt;Can work in harsh environments

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Automation industry &amp; control systems
&lt;br&gt;Sensors' connectivity
&lt;br&gt;Building automation
&lt;br&gt;Renewable energies


&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Durability	100 Mating cycles
&lt;br&gt;Operating Temperature	-40 °C up to +90 °C
&lt;br&gt;Gender	Female

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	2 A; 5 A
&lt;br&gt;Working Voltage	30 V; 60 V; 250 V
&lt;br&gt;Withstanding Voltage	650 V; 1000 V; 1400 V
&lt;br&gt;RISO	100 MΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Gold

&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o850726v209%20Family-WR-CIRCM12-6432601004xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o850726v209%20Family-WR-CIRCM12-6432601004xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_METAL_M16/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_METAL_M16&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-06-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_8PINS"/>
</gates>
<devices>
<device name="" package="643260100408">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643260100408?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643260100408"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="RATED-CURRENT" value="2A"/>
<attribute name="VALUE" value="643260100408"/>
<attribute name="WITHSTANDING-VOLTAGE" value="650V"/>
<attribute name="WORKING-VOLTAGE" value="30V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643260100404" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Female Metal M16&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Several panel cuts available
&lt;br&gt;IP68 rated connectors
&lt;br&gt;Can work in harsh environments

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Automation industry &amp; control systems
&lt;br&gt;Sensors' connectivity
&lt;br&gt;Building automation
&lt;br&gt;Renewable energies


&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Durability	100 Mating cycles
&lt;br&gt;Operating Temperature	-40 °C up to +90 °C
&lt;br&gt;Gender	Female

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	2 A; 5 A
&lt;br&gt;Working Voltage	30 V; 60 V; 250 V
&lt;br&gt;Withstanding Voltage	650 V; 1000 V; 1400 V
&lt;br&gt;RISO	100 MΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Gold

&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o850726v209%20Family-WR-CIRCM12-6432601004xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o850726v209%20Family-WR-CIRCM12-6432601004xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_METAL_M16/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_METAL_M16&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-06-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_4PINS"/>
</gates>
<devices>
<device name="" package="643260100404">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643260100404?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643260100404"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643260100404"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1400V"/>
<attribute name="WORKING-VOLTAGE" value="250V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643270100305" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Angled 90° Metal M12&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722372v209%20family-wr-circm12-6432701003xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722372v209%20family-wr-circm12-6432701003xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_ANGLED_90_METAL_M12"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_ANGLED_90_METAL_M12&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_5PINS_SHIELD"/>
</gates>
<devices>
<device name="" package="643270100305">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="SHIELD" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643270100305?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643270100305"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643270100305"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1000V"/>
<attribute name="WORKING-VOLTAGE" value="60V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643250100605" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Panel Connector PCB Metal M12&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722364v209%20family-wrcircm12-6432501006xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722364v209%20family-wrcircm12-6432501006xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_PG9"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_PG9&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_5PINS"/>
</gates>
<devices>
<device name="" package="643250100605">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643250100605?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643250100605"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643250100605"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1000V"/>
<attribute name="WORKING-VOLTAGE" value="60V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643250100405" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Metal M16&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Several panel cuts available
&lt;br&gt;IP68 rated connectors
&lt;br&gt;Can work in harsh environments

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Automation industry &amp; control systems
&lt;br&gt;Sensors' connectivity
&lt;br&gt;Building automation
&lt;br&gt;Renewable energies


&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Durability	100 Mating cycles
&lt;br&gt;Operating Temperature	-40 °C up to +90 °C
&lt;br&gt;Gender	Male

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	2 A; 5 A
&lt;br&gt;Working Voltage	30 V; 60 V; 250 V
&lt;br&gt;Withstanding Voltage	650 V; 1000 V; 1400 V
&lt;br&gt;RISO	100 MΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Gold

&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o850116v209%20Multi-WR-CIRCM12-643250100404.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o850116v209%20Multi-WR-CIRCM12-643250100404.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_M16/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_M16&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-06-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_5PINS"/>
</gates>
<devices>
<device name="" package="643250100405">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643250100405?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643250100405"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643250100405"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1000V"/>
<attribute name="WORKING-VOLTAGE" value="60V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643230100408" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Angled 90° Plastic M16&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722353v209%20family-wr-circm12-6432301004xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722353v209%20family-wr-circm12-6432301004xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_ANGLED_PLASTICM16"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_ANGLED_PLASTICM16&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-03-14&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_8PINS"/>
</gates>
<devices>
<device name="" package="643230100408">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643230100408?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643230100408"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="RATED-CURRENT" value="2A"/>
<attribute name="VALUE" value="643230100408"/>
<attribute name="WITHSTANDING-VOLTAGE" value="650V"/>
<attribute name="WORKING-VOLTAGE" value="30V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643210100604" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Male
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722351v209%20family-wr-circm12-6432101006xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722351v209%20family-wr-circm12-6432101006xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_PLASTIC_PG9"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_MALE_PLASTIC_PG9&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_4PINS"/>
</gates>
<devices>
<device name="" package="643210100604">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643210100604?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643210100604"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643210100604"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1400V"/>
<attribute name="WORKING-VOLTAGE" value="250V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643250100404" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Metal M16&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Several panel cuts available
&lt;br&gt;IP68 rated connectors
&lt;br&gt;Can work in harsh environments

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Automation industry &amp; control systems
&lt;br&gt;Sensors' connectivity
&lt;br&gt;Building automation
&lt;br&gt;Renewable energies


&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Durability	100 Mating cycles
&lt;br&gt;Operating Temperature	-40 °C up to +90 °C
&lt;br&gt;Gender	Male

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	2 A; 5 A
&lt;br&gt;Working Voltage	30 V; 60 V; 250 V
&lt;br&gt;Withstanding Voltage	650 V; 1000 V; 1400 V
&lt;br&gt;RISO	100 MΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Gold

&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o850116v209%20Multi-WR-CIRCM12-643250100404.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o850116v209%20Multi-WR-CIRCM12-643250100404.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_M16/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_M16&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-06-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_4PINS"/>
</gates>
<devices>
<device name="" package="643250100404">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643250100404?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643250100404"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643250100404"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1400V"/>
<attribute name="WORKING-VOLTAGE" value="250V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643250100408" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Metal M16&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Several panel cuts available
&lt;br&gt;IP68 rated connectors
&lt;br&gt;Can work in harsh environments

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Automation industry &amp; control systems
&lt;br&gt;Sensors' connectivity
&lt;br&gt;Building automation
&lt;br&gt;Renewable energies


&lt;b&gt;&lt;br&gt;&lt;br&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Durability	100 Mating cycles
&lt;br&gt;Operating Temperature	-40 °C up to +90 °C
&lt;br&gt;Gender	Male

&lt;b&gt;&lt;br&gt;&lt;br&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	2 A; 5 A
&lt;br&gt;Working Voltage	30 V; 60 V; 250 V
&lt;br&gt;Withstanding Voltage	650 V; 1000 V; 1400 V
&lt;br&gt;RISO	100 MΩ

&lt;b&gt;&lt;br&gt;&lt;br&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Gold

&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o850116v209%20Multi-WR-CIRCM12-643250100404.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o850116v209%20Multi-WR-CIRCM12-643250100404.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_M16/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_METAL_M16&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-06-10 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MALE_8PINS"/>
</gates>
<devices>
<device name="" package="643250100408">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643250100408?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643250100408"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="RATED-CURRENT" value="2A"/>
<attribute name="VALUE" value="643250100408"/>
<attribute name="WITHSTANDING-VOLTAGE" value="650V"/>
<attribute name="WORKING-VOLTAGE" value="30V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="643220100404" prefix="J">
<description>&lt;b&gt;WR-CIRCM12 Screw Mating Panel Connector PCB Male Plastic PG9&lt;/b&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Gender	Female
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR	2 A; 5 A
&lt;BR&gt;Working Voltage	30 V; 60 V; 250 V
&lt;BR&gt;Withstanding Voltage	650 V (AC); 1000 V (AC); 1400 V (AC)
&lt;BR&gt;Contact Resistance Initial	10 mΩ
&lt;BR&gt;RISO	100 MΩ
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Durability	100 Mating cycles
&lt;BR&gt;Ingress Protection Code	IP68
&lt;BR&gt;Operating Temperature	-40 up to +90 °C
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Material Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA66
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	Black
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o722375v209%20family-wr-circm12-6432201004xx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o722375v209%20family-wr-circm12-6432201004xx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_PLASTIC_M16"&gt;www.we-online.com/en/components/products/WR-CIRCM12_PANEL_CONNECTOR_PCB_FEMALE_PLASTIC_M16&lt;/a&gt;&lt;p&gt;

Created by Ella 2023-11-30&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="FEMALE_4PINS"/>
</gates>
<devices>
<device name="" package="643220100404">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/643220100404?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="643220100404"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="RATED-CURRENT" value="5A"/>
<attribute name="VALUE" value="643220100404"/>
<attribute name="WITHSTANDING-VOLTAGE" value="1400V"/>
<attribute name="WORKING-VOLTAGE" value="250V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
