<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - DC Power Jacks - WR-DC &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2026a, 2026-01-02&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="694108402002">
<description>&lt;b&gt;WR-DC DC Power Jack Vertical THT Ø 6.4</description>
</package>
<package name="694105309102">
<description>&lt;b&gt;WR-DC Power Jack Right Angled Shielded THT Ø 4.93</description>
</package>
<package name="694106402002">
<description>&lt;b&gt;WR-DC DC Power Jack Vertical THT Ø 6.4</description>
</package>
<package name="694106105102">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled SMT Ø 6.4 with pegs</description>
</package>
<package name="694106106102">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled SMT Ø 6.4 with 4 soldering pads &amp; pegs</description>
</package>
<package name="694103107102">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled Low Profile SMT Ø 3.9 with 4 soldering pads &amp; pegs</description>
</package>
<package name="694106301002">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled (6.4)</description>
</package>
<package name="694108301002">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled (6.4)</description>
</package>
<package name="694108105102">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled SMT Ø 6.4 with pegs</description>
</package>
<package name="694102303002">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled (4.2)</description>
</package>
<package name="694108106102">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled SMT Ø 6.4 with 4 soldering pads &amp; pegs</description>
</package>
<package name="694103303002">
<description>&lt;b&gt;WR-DC DC Power Jack Right Angled (4.2)</description>
</package>
</packages>
<symbols>
<symbol name="WR-DC">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="694108402002" prefix="J">
<description>&lt;b&gt;WR-DC Power Jacks
&lt;br&gt;
&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
Properties
&lt;/b&gt;&lt;br&gt;Rated Current: 3 to 5.5 A
&lt;br&gt;Working Voltage: 20 to 30 V
&lt;br&gt;Operating Temperature: -40°C up to +85°C
&lt;br&gt;Ø Center pin : 1.0 to 2.5 mm
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Shunt terminal to plug In/plug Out detection
High Durability: 5000 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Consumer
&lt;br&gt;Electronic devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DC_POWER_JACKS_WR_DC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/DC_POWER_JACKS_WR_DC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-01-02&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694108402002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-PIN-DIAMETER" value="2.5mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/694108402002?ae"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="694108402002"/>
<attribute name="PLUG-OUTER-DIAMETER" value="mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="694108402002"/>
<attribute name="WORKING-VOLTAGE" value="30VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694105309102" prefix="J">
<description>&lt;b&gt;WR-DC Power Jacks
&lt;br&gt;
&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
Properties
&lt;/b&gt;&lt;br&gt;Rated Current: 3 to 5.5 A
&lt;br&gt;Working Voltage: 20 to 30 V
&lt;br&gt;Operating Temperature: -40°C up to +85°C
&lt;br&gt;Ø Center pin : 1.0 to 2.5 mm
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Shunt terminal to plug In/plug Out detection
High Durability: 5000 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Consumer
&lt;br&gt;Electronic devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DC_POWER_JACKS_WR_DC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/DC_POWER_JACKS_WR_DC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-01-02&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694105309102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-PIN-DIAMETER" value="1.65mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/694105309102?ae"/>
<attribute name="IR" value="5.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="694105309102"/>
<attribute name="PLUG-OUTER-DIAMETER" value="4.75mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="694105309102"/>
<attribute name="WORKING-VOLTAGE" value="20VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694106402002" prefix="J">
<description>&lt;b&gt;WR-DC Power Jacks
&lt;br&gt;
&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
Properties
&lt;/b&gt;&lt;br&gt;Rated Current: 3 to 5.5 A
&lt;br&gt;Working Voltage: 20 to 30 V
&lt;br&gt;Operating Temperature: -40°C up to +85°C
&lt;br&gt;Ø Center pin : 1.0 to 2.5 mm
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Shunt terminal to plug In/plug Out detection
High Durability: 5000 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Consumer
&lt;br&gt;Electronic devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DC_POWER_JACKS_WR_DC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/DC_POWER_JACKS_WR_DC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-01-02&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694106402002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-PIN-DIAMETER" value="2mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/694106402002?ae"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="694106402002"/>
<attribute name="PLUG-OUTER-DIAMETER" value="mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="694106402002"/>
<attribute name="WORKING-VOLTAGE" value="30VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694106106102" prefix="J">
<description>&lt;b&gt;WR-DC Power Jacks
&lt;br&gt;
&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
Properties
&lt;/b&gt;&lt;br&gt;Rated Current: 3 to 5.5 A
&lt;br&gt;Working Voltage: 20 to 30 V
&lt;br&gt;Operating Temperature: -40°C up to +85°C
&lt;br&gt;Ø Center pin : 1.0 to 2.5 mm
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Shunt terminal to plug In/plug Out detection
High Durability: 5000 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Consumer
&lt;br&gt;Electronic devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DC_POWER_JACKS_WR_DC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/DC_POWER_JACKS_WR_DC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-01-02&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694106106102">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-PIN-DIAMETER" value="2mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/694106106102?ae"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="694106106102"/>
<attribute name="PLUG-OUTER-DIAMETER" value="5.5mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="694106106102"/>
<attribute name="VARIANT" value="with Pegs"/>
<attribute name="WORKING-VOLTAGE" value="24VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694106105102" prefix="J">
<description>&lt;b&gt;WR-DC Power Jacks
&lt;br&gt;
&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
Properties
&lt;/b&gt;&lt;br&gt;Rated Current: 3 to 5.5 A
&lt;br&gt;Working Voltage: 20 to 30 V
&lt;br&gt;Operating Temperature: -40°C up to +85°C
&lt;br&gt;Ø Center pin : 1.0 to 2.5 mm
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Shunt terminal to plug In/plug Out detection
High Durability: 5000 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Consumer
&lt;br&gt;Electronic devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DC_POWER_JACKS_WR_DC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/DC_POWER_JACKS_WR_DC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-01-02&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694106105102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-PIN-DIAMETER" value="2mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/694106105102?ae"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="694106105102"/>
<attribute name="PLUG-OUTER-DIAMETER" value="5.5mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="694106105102"/>
<attribute name="VARIANT" value="with Pegs"/>
<attribute name="WORKING-VOLTAGE" value="24VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694103107102" prefix="J">
<description>&lt;b&gt;WR-DC Power Jacks
&lt;br&gt;
&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
Properties
&lt;/b&gt;&lt;br&gt;Rated Current: 3 to 5.5 A
&lt;br&gt;Working Voltage: 20 to 30 V
&lt;br&gt;Operating Temperature: -40°C up to +85°C
&lt;br&gt;Ø Center pin : 1.0 to 2.5 mm
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Shunt terminal to plug In/plug Out detection
High Durability: 5000 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Consumer
&lt;br&gt;Electronic devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DC_POWER_JACKS_WR_DC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/DC_POWER_JACKS_WR_DC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-01-02&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694103107102">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-PIN-DIAMETER" value="1.3mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/694103107102?ae"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="694103107102"/>
<attribute name="PLUG-OUTER-DIAMETER" value="3.5mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="694103107102"/>
<attribute name="VARIANT" value="Low Profile with Peg"/>
<attribute name="WORKING-VOLTAGE" value="24VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694108301002" prefix="J">
<description>&lt;b&gt;WR-DC Power Jacks
&lt;br&gt;
&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
Properties
&lt;/b&gt;&lt;br&gt;Rated Current: 3 to 5.5 A
&lt;br&gt;Working Voltage: 20 to 30 V
&lt;br&gt;Operating Temperature: -40°C up to +85°C
&lt;br&gt;Ø Center pin : 1.0 to 2.5 mm
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Shunt terminal to plug In/plug Out detection
High Durability: 5000 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Consumer
&lt;br&gt;Electronic devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DC_POWER_JACKS_WR_DC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/DC_POWER_JACKS_WR_DC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-01-02&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694108301002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-PIN-DIAMETER" value="2.5mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/694108301002?ae"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="694108301002"/>
<attribute name="PLUG-OUTER-DIAMETER" value="5.5mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="694108301002"/>
<attribute name="WORKING-VOLTAGE" value="30VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694106301002" prefix="J">
<description>&lt;b&gt;WR-DC Power Jacks
&lt;br&gt;
&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
Properties
&lt;/b&gt;&lt;br&gt;Rated Current: 3 to 5.5 A
&lt;br&gt;Working Voltage: 20 to 30 V
&lt;br&gt;Operating Temperature: -40°C up to +85°C
&lt;br&gt;Ø Center pin : 1.0 to 2.5 mm
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Shunt terminal to plug In/plug Out detection
High Durability: 5000 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Consumer
&lt;br&gt;Electronic devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DC_POWER_JACKS_WR_DC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/DC_POWER_JACKS_WR_DC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-01-02&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694106301002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-PIN-DIAMETER" value="2mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/694106301002?ae"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="694106301002"/>
<attribute name="PLUG-OUTER-DIAMETER" value="5.5mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="694106301002"/>
<attribute name="WORKING-VOLTAGE" value="30VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694108105102" prefix="J">
<description>&lt;b&gt;WR-DC Power Jacks
&lt;br&gt;
&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
Properties
&lt;/b&gt;&lt;br&gt;Rated Current: 3 to 5.5 A
&lt;br&gt;Working Voltage: 20 to 30 V
&lt;br&gt;Operating Temperature: -40°C up to +85°C
&lt;br&gt;Ø Center pin : 1.0 to 2.5 mm
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Shunt terminal to plug In/plug Out detection
High Durability: 5000 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Consumer
&lt;br&gt;Electronic devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DC_POWER_JACKS_WR_DC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/DC_POWER_JACKS_WR_DC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-01-02&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694108105102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-PIN-DIAMETER" value="2.5mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/694108105102?ae"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="694108105102"/>
<attribute name="PLUG-OUTER-DIAMETER" value="5.5mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="694108105102"/>
<attribute name="VARIANT" value="with Pegs"/>
<attribute name="WORKING-VOLTAGE" value="24VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694102303002" prefix="J">
<description>&lt;b&gt;WR-DC Power Jacks
&lt;br&gt;
&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
Properties
&lt;/b&gt;&lt;br&gt;Rated Current: 3 to 5.5 A
&lt;br&gt;Working Voltage: 20 to 30 V
&lt;br&gt;Operating Temperature: -40°C up to +85°C
&lt;br&gt;Ø Center pin : 1.0 to 2.5 mm
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Shunt terminal to plug In/plug Out detection
High Durability: 5000 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Consumer
&lt;br&gt;Electronic devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DC_POWER_JACKS_WR_DC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/DC_POWER_JACKS_WR_DC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-01-02&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694102303002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-PIN-DIAMETER" value="1mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/694102303002?ae"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="694102303002"/>
<attribute name="PLUG-OUTER-DIAMETER" value="3.5mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="694102303002"/>
<attribute name="WORKING-VOLTAGE" value="24VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694108106102" prefix="J">
<description>&lt;b&gt;WR-DC Power Jacks
&lt;br&gt;
&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
Properties
&lt;/b&gt;&lt;br&gt;Rated Current: 3 to 5.5 A
&lt;br&gt;Working Voltage: 20 to 30 V
&lt;br&gt;Operating Temperature: -40°C up to +85°C
&lt;br&gt;Ø Center pin : 1.0 to 2.5 mm
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Shunt terminal to plug In/plug Out detection
High Durability: 5000 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Consumer
&lt;br&gt;Electronic devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DC_POWER_JACKS_WR_DC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/DC_POWER_JACKS_WR_DC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-01-02&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694108106102">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-PIN-DIAMETER" value="2.5mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/694108106102?ae"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="694108106102"/>
<attribute name="PLUG-OUTER-DIAMETER" value="5.5mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="694108106102"/>
<attribute name="VARIANT" value="with Pegs"/>
<attribute name="WORKING-VOLTAGE" value="24VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="694103303002" prefix="J">
<description>&lt;b&gt;WR-DC Power Jacks
&lt;br&gt;
&lt;br&gt;
Characteristics
&lt;br&gt;&lt;br&gt;
Properties
&lt;/b&gt;&lt;br&gt;Rated Current: 3 to 5.5 A
&lt;br&gt;Working Voltage: 20 to 30 V
&lt;br&gt;Operating Temperature: -40°C up to +85°C
&lt;br&gt;Ø Center pin : 1.0 to 2.5 mm
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Shunt terminal to plug In/plug Out detection
High Durability: 5000 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Consumer
&lt;br&gt;Electronic devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o828637v209%20Jacks_Gruppenbild.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DC_POWER_JACKS_WR_DC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/DC_POWER_JACKS_WR_DC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-01-02&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-DC"/>
</gates>
<devices>
<device name="" package="694103303002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-PIN-DIAMETER" value="1.3mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/694103303002?ae"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="694103303002"/>
<attribute name="PLUG-OUTER-DIAMETER" value="3.5mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="694103303002"/>
<attribute name="WORKING-VOLTAGE" value="24VDC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
