<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Input/Output connectors - WR-DSUB &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-07-25&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="618009231421">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt; &lt;br&gt;10.3mm Male Angled PCB Connector with Hex Screw, 9 Pins</description>
</package>
<package name="618044325323">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; Male High Density Angled PCB Connector without Hex Screw,  44 Pins</description>
</package>
<package name="618062331023">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; Male High Density Angled PCB Connector with Hex Screw, 62 Pins</description>
</package>
<package name="61800929221">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; Male PCB Connector with Hex Screw, 9 Pins</description>
</package>
<package name="618015231321">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt;10.30 mm Female Angled PCB Connector w. Hex Screw,  15 Pins</description>
</package>
<package name="618025231321">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt;10.30 mm Female Angled PCB Connector w. Hex Screw, 25 Pins</description>
</package>
<package name="618015211721">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; 8.08mm Male Angled PCB Connector without Hex Screw, 15 pins</description>
</package>
<package name="618062325223">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt;Female High Density Angled PCB Connector w/o Hex Screw , 62 Pins</description>
</package>
<package name="618037233821">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt;10.3mm Female Angled PCB Connector without Hex Screw, 37 Pins</description>
</package>
<package name="61800925023">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt;Male PCB Connector, 9 Pins</description>
</package>
<package name="618009211721">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; 8.08mm Male Angled PCB Connector without Hex Screw, 9 pins</description>
</package>
<package name="618015233821">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt;10.30 mm Female Angled PCB Connector w/o Hex Screw, 15 Pins</description>
</package>
<package name="61801529221">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt; &lt;br&gt;Male PCB Connector with Hex Screw, 15 Pins</description>
</package>
<package name="618009231321">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt;10.30 mm Female Angled PCB Connector w. Hex Screw, 9 Pins</description>
</package>
<package name="618037231121">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; 8.08 mm Female Angled PCB Connector w. Hex Screw, 37 Pins</description>
</package>
<package name="618015211821">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; 8.08 mm Female Angled PCB Connector w/o Hex Screw,15 Pins</description>
</package>
<package name="618009233721">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt;  10.3mm Male Angled PCB Connector without Hex Screw, 9 pins</description>
</package>
<package name="618025211721">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; 8.08mm Male Angled PCB Connector without Hex Screw, 25 pins</description>
</package>
<package name="618037233721">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt;10.3mm Male Angled PCB Connector without Hex Screw, 37 pins</description>
</package>
<package name="618062325323">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt;Male High Density Angled PCB Connector without Hex Screw, 62 Pins</description>
</package>
<package name="618015233721">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; 10.3mm Male Angled PCB Connector without Hex Screw, 15 pins</description>
</package>
<package name="618026325223">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt;Female High Density Angled PCB Connector w/o Hex Screw , 26 Pins</description>
</package>
<package name="61801525123">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; Female PCB Connector, 15 Pins</description>
</package>
<package name="618009211821">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; 8.08 mm Female Angled PCB Connector w/o Hex Screw, 9 Pins</description>
</package>
<package name="61801529321">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; Female PCB Connector w. Hex Screw , 15 Pins</description>
</package>
<package name="618037231421">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt; &lt;br&gt;10.3mm Male Angled PCB Connector with Hex Screw, 37 Pins</description>
</package>
<package name="618044325223">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt;Female High Density Angled PCB Connector w/o Hex Screw ,44 Pins</description>
</package>
<package name="618044331023">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; Male High Density Angled PCB Connector with Hex Screw, 44 Pins</description>
</package>
<package name="618015325223">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; Male High Density Angled PCB Connector without Hex Screw, 15 Pins</description>
</package>
<package name="618015325323">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt;Male High Density Angled PCB Connector without Hex Screw, 15 Pins</description>
</package>
<package name="618037231321">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt;10.30 mm Female Angled PCB Connector w. Hex Screw, 37Pins</description>
</package>
<package name="61802529321">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; Female PCB Connector w. Hex Screw, 25 Pins</description>
</package>
<package name="618037211721">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; 8.08mm Male Angled PCB Connector without Hex Screw, 37 pins</description>
</package>
<package name="618015331023">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; Male High Density Angled PCB Connector with Hex Screw, 15 Pins</description>
</package>
<package name="618015231221">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; 8.08mm Male Angled PCB Connector with Hex Screw, 15 Pins</description>
</package>
<package name="618026330923">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; Female High Density Angled PCB Connector with Hex Screw,  26 Pins</description>
</package>
<package name="618025211821">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; 8.08 mm Female Angled PCB Connector w/o Hex Screw,25 Pins</description>
</package>
<package name="61800925123">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; Female PCB Connector, 9 Pins</description>
</package>
<package name="618015330923">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; Female High Density Angled PCB Connector with Hex Screw, 15 Pins</description>
</package>
<package name="618037231221">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; 8.08mm Male Angled PCB Connector with Hex Screw, 37 Pins</description>
</package>
<package name="61800929321">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; Female PCB Connector w. Hex Screw, 9 Pins</description>
</package>
<package name="61802525123">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt; &lt;br&gt;Female PCB Connector, 25 Pins</description>
</package>
<package name="618009231121">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; 8.08 mm Female Angled PCB Connector w. Hex Screw, 9 Pins</description>
</package>
<package name="61801525023">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; Male PCB Connector, 15 Pins</description>
</package>
<package name="618026325323">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; Male High Density Angled PCB Connector without Hex Screw, 26 Pins</description>
</package>
<package name="618025231221">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; 8.08mm Male Angled PCB Connector with Hex Screw, 25 Pins</description>
</package>
<package name="618025231121">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; 8.08 mm Female Angled PCB Connector w. Hex Screw,25 Pins</description>
</package>
<package name="618025233821">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt;10.3mm Female Angled PCB Connector without Hex Screw, 25 Pins</description>
</package>
<package name="61803729221">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; Male PCB Connector with Hex Screw, 37 Pins</description>
</package>
<package name="618009231221">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; 8.08mm Male Angled PCB Connector with Hex Screw, 9 Pins</description>
</package>
<package name="618025233721">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; 10.3mm Male Angled PCB Connector without Hex Screw, 25 pins</description>
</package>
<package name="618015231121">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; 8.08 mm Female Angled PCB Connector w. Hex Screw,15 Pins</description>
</package>
<package name="61803729321">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; Female PCB Connector w. Hex Screw, 37 Pins</description>
</package>
<package name="618037211821">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; 8.08 mm Female Angled PCB Connector w/o Hex Screw,37 Pins</description>
</package>
<package name="61802529221">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt;Male PCB Connector with Hex Screw, 25 Pins</description>
</package>
<package name="61803725023">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; Male PCB Connector, 37 Pins</description>
</package>
<package name="618009233821">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt;10.30 mm Female Angled PCB Connector w/o Hex Screw, 9 Pins</description>
</package>
<package name="618015231421">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt; &lt;br&gt;10.3mm Male Angled PCB Connector with Hex Screw, 15 Pins</description>
</package>
<package name="61802525023">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; Male PCB Connector, 25 Pins</description>
</package>
<package name="618026331023">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt;Male High Density Angled PCB Connector with Hex Screw, 26 Pins</description>
</package>
<package name="618025231421">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt; &lt;br&gt;10.3mm Male Angled PCB Connector with Hex Screw, 25 Pins</description>
</package>
<package name="618044330923">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; Female High Density Angled PCB Connector with Hex Screw,  44 Pins</description>
</package>
<package name="618062330923">
<description>&lt;B&gt;WR-DSUB&lt;/B&gt;&lt;BR&gt; Female High Density Angled PCB Connector with Hex Screw, 62 Pins</description>
</package>
<package name="61803725123">
<description>&lt;b&gt;WR-DSUB&lt;/b&gt;&lt;br&gt; Female PCB Connector, 37 Pins</description>
</package>
</packages>
<symbols>
<symbol name="R15-1">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
</symbol>
<symbol name="R37-1">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
</symbol>
<symbol name="R25-1">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
</symbol>
<symbol name="25FT_S">
<description>25Pins, Female,THT</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="44MT_S">
<description>44Pins, Male,THT</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38"/>
<pin name="39"/>
<pin name="40"/>
<pin name="41"/>
<pin name="42"/>
<pin name="43"/>
<pin name="44"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="R9-1">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
</symbol>
<symbol name="15FT_S">
<description>15Pins, Female,THT</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="62MT_S">
<description>62 Pins, Male ,THT</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38"/>
<pin name="39"/>
<pin name="40"/>
<pin name="41"/>
<pin name="42"/>
<pin name="43"/>
<pin name="44"/>
<pin name="45"/>
<pin name="46"/>
<pin name="47"/>
<pin name="48"/>
<pin name="49"/>
<pin name="50"/>
<pin name="51"/>
<pin name="52"/>
<pin name="53"/>
<pin name="54"/>
<pin name="55"/>
<pin name="56"/>
<pin name="57"/>
<pin name="58"/>
<pin name="59"/>
<pin name="60"/>
<pin name="61"/>
<pin name="62"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="9MT_S">
<description>9 Pins Male THT</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="37FT_S">
<description>37 Pins,Female, THT</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="9FT_S">
<description>9 Pins,Female ,THT</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="62FT_S">
<description>62Pins,Female,THT</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38"/>
<pin name="39"/>
<pin name="40"/>
<pin name="41"/>
<pin name="42"/>
<pin name="43"/>
<pin name="44"/>
<pin name="45"/>
<pin name="46"/>
<pin name="47"/>
<pin name="48"/>
<pin name="49"/>
<pin name="50"/>
<pin name="51"/>
<pin name="52"/>
<pin name="53"/>
<pin name="54"/>
<pin name="55"/>
<pin name="56"/>
<pin name="57"/>
<pin name="58"/>
<pin name="59"/>
<pin name="60"/>
<pin name="61"/>
<pin name="62"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="25MT_S">
<description>25 Pins,Male,THT</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="15MT_S">
<description>15 Pins.Male, THT</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="37MT_S">
<description>37 Pins,Male,THT</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="26FT_S">
<description>26 Pins, Female, THT</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="44FT_S">
<description>44 Pins,Female ,THT</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38"/>
<pin name="39"/>
<pin name="40"/>
<pin name="41"/>
<pin name="42"/>
<pin name="43"/>
<pin name="44"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="15FT_S_1">
<description>15Pins, Female,THT</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="SHIELD"/>
<pin name="9"/>
<pin name="10"/>
</symbol>
<symbol name="15MT_S_1">
<description>15 Pins, Male ,THT</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="SHIELD"/>
<pin name="9"/>
<pin name="10"/>
</symbol>
<symbol name="26MT_S">
<description>26Pins, Male,THT</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="SHIELD"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="6180XX231421_618009231421" prefix="J">
<description>&lt;b&gt;WR-DSUB 10.30 mm Male Angled PCB Connector w. Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60849v209%20Family_I-O_DSUB_PCB_Male_w-screw_6180xx231421_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60849v209%20Family_I-O_DSUB_PCB_Male_w-screw_6180xx231421_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_10_30MM_6180XX231421"&gt;https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_10_30MM_6180XX231421&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MT_S"/>
</gates>
<devices>
<device name="" package="618009231421">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618009231421?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618009231421"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618009231421"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX325323_618044325323" prefix="J">
<description>&lt;b&gt;WR-DSUB Male High Density Angled PCB Connector w/o Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:60 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33092v209%20Family_WR-DSUB_6180xx325323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33092v209%20Family_WR-DSUB_6180xx325323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_MALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_6180XX325323/"&gt;https://www.we-online.com/catalog/en/DSUB_MALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_6180XX325323/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-09&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="44MT_S"/>
</gates>
<devices>
<device name="" package="618044325323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618044325323?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618044325323"/>
<attribute name="PINS" value=" 44 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618044325323"/>
<attribute name="WORKING-VOLTAGE" value="60VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX331023_618062331023" prefix="J">
<description>&lt;b&gt;WR-DSUB Male High Density Angled PCB Connector w. Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:60 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33094v209%20Family_WR-DSUB_6180xx331023.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33094v209%20Family_WR-DSUB_6180xx331023.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_MALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_6180XX331023/"&gt;https://www.we-online.com/catalog/en/DSUB_MALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_6180XX331023/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-09&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="62MT_S"/>
</gates>
<devices>
<device name="" package="618062331023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618062331023?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618062331023"/>
<attribute name="PINS" value=" 62 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618062331023"/>
<attribute name="WORKING-VOLTAGE" value="60VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX29221_61800929221" prefix="J">
<description>&lt;b&gt;WR-DSUB Male PCB Connector with Hex Screw

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-55 °C up to +105 °C
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Straight
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;Shielding Material	Steel
&lt;BR&gt;Shielding Plating	Tin

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33089v209%20Family_WR-DSUB_6180xx29221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33089v209%20Family_WR-DSUB_6180xx29221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DSUB_MALE_PCB_CONNECTOR_W_HEX_SCREW_6180XX29221/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/DSUB_MALE_PCB_CONNECTOR_W_HEX_SCREW_6180XX29221&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MT_S"/>
</gates>
<devices>
<device name="" package="61800929221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61800929221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="61800929221"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61800929221"/>
<attribute name="WORKING-VOLTAGE" value="250VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX231321_618015231321" prefix="J">
<description>&lt;b&gt;WR-DSUB 10.30 mm Female Angled PCB Connector w. Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60808v209%20Family_I-O_DSUB_PCB_Female_w-screw_6180xx231321_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60808v209%20Family_I-O_DSUB_PCB_Female_w-screw_6180xx231321_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_10_30MM_6180XX231321/"&gt;https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_10_30MM_6180XX231321/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-14&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15FT_S"/>
</gates>
<devices>
<device name="" package="618015231321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618015231321?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618015231321"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618015231321"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX231321_618025231321" prefix="J">
<description>&lt;b&gt;WR-DSUB 10.30 mm Female Angled PCB Connector w. Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60808v209%20Family_I-O_DSUB_PCB_Female_w-screw_6180xx231321_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60808v209%20Family_I-O_DSUB_PCB_Female_w-screw_6180xx231321_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_10_30MM_6180XX231321/"&gt;https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_10_30MM_6180XX231321/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-14&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25FT_S"/>
</gates>
<devices>
<device name="" package="618025231321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618025231321?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618025231321"/>
<attribute name="PINS" value=" 25 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618025231321"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX211721_618015211721" prefix="J">
<description>&lt;b&gt;WR-DSUB 8.08 mm Male Angled PCB Connector w/o Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33075v209%20Family_WR-DSUB_6180xx211721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33075v209%20Family_WR-DSUB_6180xx211721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_8_08MM_6180XX211721"&gt;https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_8_08MM_6180XX211721&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15MT_S"/>
</gates>
<devices>
<device name="" package="618015211721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618015211721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618015211721"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618015211721"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX325223_618062325223" prefix="J">
<description>&lt;b&gt;WR-DSUB Female High Density Angled PCB Connector w/o Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;:Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Working Voltage:60V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33091v209%20Family_WR-DSUB_6180xx325223.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33091v209%20Family_WR-DSUB_6180xx325223.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_FEMALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_6180XX325223"&gt;www.we-online.com/en/components/products/DSUB_FEMALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_6180XX325223&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="62FT_S"/>
</gates>
<devices>
<device name="" package="618062325223">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618062325223?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618062325223"/>
<attribute name="PINS" value=" 62 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618062325223"/>
<attribute name="WORKING-VOLTAGE" value="60VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX233821_618037233821" prefix="J">
<description>&lt;b&gt;WR-DSUB 10.30 mm Female Angled PCB Connector w/o Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60818v209%20Family_I-O_DSUB_PCB_Female_wo-screw_6180xx211821_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60818v209%20Family_I-O_DSUB_PCB_Female_wo-screw_6180xx211821_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_10_30MM_6180XX233821/"&gt;https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_10_30MM_6180XX233821/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-14&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="37FT_S"/>
</gates>
<devices>
<device name="" package="618037233821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618037233821?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618037233821"/>
<attribute name="PINS" value=" 37 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618037233821"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX25023_61800925023" prefix="J">
<description>&lt;b&gt;WR-DSUB Male PCB Connector

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;QOperating Temperature	-55 °C up to +105 °C
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Straight
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;Shielding Material	Steel
&lt;BR&gt;Shielding Plating	Tin

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33086v209%20Family_I-O_DSUB_PCB_Male_6180xx25023_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33086v209%20Family_I-O_DSUB_PCB_Male_6180xx25023_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DSUB_MALE_PCB_CONNECTOR_6180XX25023/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/DSUB_MALE_PCB_CONNECTOR_6180XX25023&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MT_S"/>
</gates>
<devices>
<device name="" package="61800925023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61800925023?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="61800925023"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61800925023"/>
<attribute name="WORKING-VOLTAGE" value="250VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX233821_618015233821" prefix="J">
<description>&lt;b&gt;WR-DSUB 10.30 mm Female Angled PCB Connector w/o Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60818v209%20Family_I-O_DSUB_PCB_Female_wo-screw_6180xx211821_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60818v209%20Family_I-O_DSUB_PCB_Female_wo-screw_6180xx211821_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_10_30MM_6180XX233821/"&gt;https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_10_30MM_6180XX233821/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-14&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15FT_S"/>
</gates>
<devices>
<device name="" package="618015233821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618015233821?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618015233821"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618015233821"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX29221_61801529221" prefix="J">
<description>&lt;b&gt;WR-DSUB Male PCB Connector with Hex Screw

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-55 °C up to +105 °C
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Straight
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;Shielding Material	Steel
&lt;BR&gt;Shielding Plating	Tin

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33089v209%20Family_WR-DSUB_6180xx29221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33089v209%20Family_WR-DSUB_6180xx29221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DSUB_MALE_PCB_CONNECTOR_W_HEX_SCREW_6180XX29221/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/DSUB_MALE_PCB_CONNECTOR_W_HEX_SCREW_6180XX29221&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15MT_S"/>
</gates>
<devices>
<device name="" package="61801529221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61801529221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="61801529221"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61801529221"/>
<attribute name="WORKING-VOLTAGE" value="250VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX231321_618009231321" prefix="J">
<description>&lt;b&gt;WR-DSUB 10.30 mm Female Angled PCB Connector w. Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60808v209%20Family_I-O_DSUB_PCB_Female_w-screw_6180xx231321_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60808v209%20Family_I-O_DSUB_PCB_Female_w-screw_6180xx231321_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_10_30MM_6180XX231321/"&gt;https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_10_30MM_6180XX231321/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-14&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9FT_S"/>
</gates>
<devices>
<device name="" package="618009231321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618009231321?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618009231321"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618009231321"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX231121_618037231121" prefix="J">
<description>&lt;b&gt;WR-DSUB 8.08 mm Female Angled PCB Connector w. Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class：3 as per IEC 60 603-13
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance：RoHS
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR 1：3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33082v209%20Family_WR-DSUB_6180xx231121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33082v209%20Family_WR-DSUB_6180xx231121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_8_08MM_6180XX231121"&gt;https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_8_08MM_6180XX231121/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-13&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="37FT_S"/>
</gates>
<devices>
<device name="" package="618037231121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618037231121?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618037231121"/>
<attribute name="PINS" value=" 37 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618037231121"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX211721_618009211721" prefix="J">
<description>&lt;b&gt;WR-DSUB 8.08 mm Male Angled PCB Connector w/o Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33075v209%20Family_WR-DSUB_6180xx211721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33075v209%20Family_WR-DSUB_6180xx211721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_8_08MM_6180XX211721"&gt;https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_8_08MM_6180XX211721&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MT_S"/>
</gates>
<devices>
<device name="" package="618009211721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618009211721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618009211721"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618009211721"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX211821_618015211821" prefix="J">
<description>&lt;b&gt;WR-DSUB 8.08 mm Female Angled PCB Connector w/o Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33076v209%20Family_WR-DSUB_6180xx211821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33076v209%20Family_WR-DSUB_6180xx211821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_8_08MM_6180XX211821"&gt;https://www.we-online.com/en/components/products/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_8_08MM_6180XX211821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15FT_S"/>
</gates>
<devices>
<device name="" package="618015211821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618015211821?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618015211821"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618015211821"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX233721_618009233721" prefix="J">
<description>&lt;b&gt;WR-DSUB 10.30 mm Male Angled PCB Connector w/o Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60857v209%20Family_I-O_DSUB_PCB_Male_wo-screw_6180xx233721_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60857v209%20Family_I-O_DSUB_PCB_Male_wo-screw_6180xx233721_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_10_30MM_6180XX233721/"&gt;https://www.we-online.com/catalog/en/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_10_30MM_6180XX233721/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-09&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MT_S"/>
</gates>
<devices>
<device name="" package="618009233721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618009233721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618009233721"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618009233721"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX211721_618025211721" prefix="J">
<description>&lt;b&gt;WR-DSUB 8.08 mm Male Angled PCB Connector w/o Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33075v209%20Family_WR-DSUB_6180xx211721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33075v209%20Family_WR-DSUB_6180xx211721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_8_08MM_6180XX211721"&gt;https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_8_08MM_6180XX211721&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25MT_S"/>
</gates>
<devices>
<device name="" package="618025211721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618025211721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618025211721"/>
<attribute name="PINS" value=" 25 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618025211721"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX233721_618037233721" prefix="J">
<description>&lt;b&gt;WR-DSUB 10.30 mm Male Angled PCB Connector w/o Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60857v209%20Family_I-O_DSUB_PCB_Male_wo-screw_6180xx233721_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60857v209%20Family_I-O_DSUB_PCB_Male_wo-screw_6180xx233721_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_10_30MM_6180XX233721/"&gt;https://www.we-online.com/catalog/en/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_10_30MM_6180XX233721/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-09&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="37MT_S"/>
</gates>
<devices>
<device name="" package="618037233721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618037233721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618037233721"/>
<attribute name="PINS" value=" 37 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618037233721"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX325323_618062325323" prefix="J">
<description>&lt;b&gt;WR-DSUB Male High Density Angled PCB Connector w/o Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:60 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33092v209%20Family_WR-DSUB_6180xx325323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33092v209%20Family_WR-DSUB_6180xx325323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_MALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_6180XX325323/"&gt;https://www.we-online.com/catalog/en/DSUB_MALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_6180XX325323/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-09&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="62MT_S"/>
</gates>
<devices>
<device name="" package="618062325323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618062325323?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618062325323"/>
<attribute name="PINS" value=" 62 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618062325323"/>
<attribute name="WORKING-VOLTAGE" value="60VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX233721_618015233721" prefix="J">
<description>&lt;b&gt;WR-DSUB 10.30 mm Male Angled PCB Connector w/o Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60857v209%20Family_I-O_DSUB_PCB_Male_wo-screw_6180xx233721_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60857v209%20Family_I-O_DSUB_PCB_Male_wo-screw_6180xx233721_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_10_30MM_6180XX233721/"&gt;https://www.we-online.com/catalog/en/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_10_30MM_6180XX233721/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-09&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15MT_S"/>
</gates>
<devices>
<device name="" package="618015233721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618015233721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618015233721"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618015233721"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX325223_618026325223" prefix="J">
<description>&lt;b&gt;WR-DSUB Female High Density Angled PCB Connector w/o Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;:Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Working Voltage:60V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33091v209%20Family_WR-DSUB_6180xx325223.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33091v209%20Family_WR-DSUB_6180xx325223.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_FEMALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_6180XX325223"&gt;www.we-online.com/en/components/products/DSUB_FEMALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_6180XX325223&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="26FT_S"/>
</gates>
<devices>
<device name="" package="618026325223">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618026325223?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618026325223"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618026325223"/>
<attribute name="WORKING-VOLTAGE" value="60VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX25123_61801525123" prefix="J">
<description>&lt;b&gt;WR-DSUB Female PCB Connector

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-55 °C up to +105 °C
&lt;BR&gt;Gender	Female
&lt;BR&gt;Type	Straight
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;Shielding Material	Steel
&lt;BR&gt;Shielding Plating	Tin

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o60801v209%20Family_I-O_DSUB_PCB_Female_wo-screw_6180xx25123_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o60801v209%20Family_I-O_DSUB_PCB_Female_wo-screw_6180xx25123_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DSUB_FEMALE_PCB_CONNECTOR_6180XX25123/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/DSUB_FEMALE_PCB_CONNECTOR_6180XX25123&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15FT_S"/>
</gates>
<devices>
<device name="" package="61801525123">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61801525123?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="61801525123"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61801525123"/>
<attribute name="WORKING-VOLTAGE" value="250VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX211821_618009211821" prefix="J">
<description>&lt;b&gt;WR-DSUB 8.08 mm Female Angled PCB Connector w/o Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33076v209%20Family_WR-DSUB_6180xx211821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33076v209%20Family_WR-DSUB_6180xx211821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_8_08MM_6180XX211821"&gt;https://www.we-online.com/en/components/products/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_8_08MM_6180XX211821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9FT_S"/>
</gates>
<devices>
<device name="" package="618009211821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618009211821?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618009211821"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618009211821"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX29321_61801529321" prefix="J">
<description>&lt;b&gt;WR-DSUB Female PCB Connector w. Hex Screw

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-55 °C up to +105 °C
&lt;BR&gt;Gender	Female
&lt;BR&gt;Type	Straight
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;Shielding Material	Steel
&lt;BR&gt;Shielding Plating	Tin

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33090v209%20Family_WR-DSUB_6180xx29321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33090v209%20Family_WR-DSUB_6180xx29321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DSUB_FEMALE_PCB_CONNECTOR_W_HEX_SCREW_6180XX29321/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/DSUB_FEMALE_PCB_CONNECTOR_W_HEX_SCREW_6180XX29321&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15FT_S"/>
</gates>
<devices>
<device name="" package="61801529321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61801529321?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="61801529321"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61801529321"/>
<attribute name="WORKING-VOLTAGE" value="250VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX231421_618037231421" prefix="J">
<description>&lt;b&gt;WR-DSUB 10.30 mm Male Angled PCB Connector w. Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60849v209%20Family_I-O_DSUB_PCB_Male_w-screw_6180xx231421_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60849v209%20Family_I-O_DSUB_PCB_Male_w-screw_6180xx231421_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_10_30MM_6180XX231421"&gt;https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_10_30MM_6180XX231421&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="37MT_S"/>
</gates>
<devices>
<device name="" package="618037231421">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618037231421?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618037231421"/>
<attribute name="PINS" value=" 37 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618037231421"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX325223_618044325223" prefix="J">
<description>&lt;b&gt;WR-DSUB Female High Density Angled PCB Connector w/o Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;:Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Working Voltage:60V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33091v209%20Family_WR-DSUB_6180xx325223.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33091v209%20Family_WR-DSUB_6180xx325223.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_FEMALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_6180XX325223"&gt;www.we-online.com/en/components/products/DSUB_FEMALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_6180XX325223&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="44FT_S"/>
</gates>
<devices>
<device name="" package="618044325223">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618044325223?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618044325223"/>
<attribute name="PINS" value=" 44 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618044325223"/>
<attribute name="WORKING-VOLTAGE" value="60VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX331023_618044331023" prefix="J">
<description>&lt;b&gt;WR-DSUB Male High Density Angled PCB Connector w. Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:60 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33094v209%20Family_WR-DSUB_6180xx331023.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33094v209%20Family_WR-DSUB_6180xx331023.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_MALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_6180XX331023/"&gt;https://www.we-online.com/catalog/en/DSUB_MALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_6180XX331023/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-09&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="44MT_S"/>
</gates>
<devices>
<device name="" package="618044331023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618044331023?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618044331023"/>
<attribute name="PINS" value=" 44 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618044331023"/>
<attribute name="WORKING-VOLTAGE" value="60VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX325223_618015325223" prefix="J">
<description>&lt;b&gt;WR-DSUB Female High Density Angled PCB Connector w/o Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;:Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Working Voltage:60V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33091v209%20Family_WR-DSUB_6180xx325223.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33091v209%20Family_WR-DSUB_6180xx325223.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_FEMALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_6180XX325223"&gt;www.we-online.com/en/components/products/DSUB_FEMALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_6180XX325223&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15FT_S_1"/>
</gates>
<devices>
<device name="" package="618015325223">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618015325223?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618015325223"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618015325223"/>
<attribute name="WORKING-VOLTAGE" value="60VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX231321_618037231321" prefix="J">
<description>&lt;b&gt;WR-DSUB 10.30 mm Female Angled PCB Connector w. Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60808v209%20Family_I-O_DSUB_PCB_Female_w-screw_6180xx231321_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60808v209%20Family_I-O_DSUB_PCB_Female_w-screw_6180xx231321_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_10_30MM_6180XX231321/"&gt;https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_10_30MM_6180XX231321/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-14&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="37FT_S"/>
</gates>
<devices>
<device name="" package="618037231321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618037231321?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618037231321"/>
<attribute name="PINS" value=" 37 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618037231321"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX325323_618015325323" prefix="J">
<description>&lt;b&gt;WR-DSUB Male High Density Angled PCB Connector w/o Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:60 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33092v209%20Family_WR-DSUB_6180xx325323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33092v209%20Family_WR-DSUB_6180xx325323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_MALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_6180XX325323/"&gt;https://www.we-online.com/catalog/en/DSUB_MALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_6180XX325323/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-09&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15MT_S_1"/>
</gates>
<devices>
<device name="" package="618015325323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618015325323?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618015325323"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618015325323"/>
<attribute name="WORKING-VOLTAGE" value="60VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX29321_61802529321" prefix="J">
<description>&lt;b&gt;WR-DSUB Female PCB Connector w. Hex Screw

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-55 °C up to +105 °C
&lt;BR&gt;Gender	Female
&lt;BR&gt;Type	Straight
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;Shielding Material	Steel
&lt;BR&gt;Shielding Plating	Tin

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33090v209%20Family_WR-DSUB_6180xx29321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33090v209%20Family_WR-DSUB_6180xx29321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DSUB_FEMALE_PCB_CONNECTOR_W_HEX_SCREW_6180XX29321/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/DSUB_FEMALE_PCB_CONNECTOR_W_HEX_SCREW_6180XX29321&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25FT_S"/>
</gates>
<devices>
<device name="" package="61802529321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61802529321?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="61802529321"/>
<attribute name="PINS" value=" 25 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61802529321"/>
<attribute name="WORKING-VOLTAGE" value="250VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX211721_618037211721" prefix="J">
<description>&lt;b&gt;WR-DSUB 8.08 mm Male Angled PCB Connector w/o Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33075v209%20Family_WR-DSUB_6180xx211721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33075v209%20Family_WR-DSUB_6180xx211721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_8_08MM_6180XX211721"&gt;https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_8_08MM_6180XX211721&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="37MT_S"/>
</gates>
<devices>
<device name="" package="618037211721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618037211721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618037211721"/>
<attribute name="PINS" value=" 37 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618037211721"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX331023_618015331023" prefix="J">
<description>&lt;b&gt;WR-DSUB Male High Density Angled PCB Connector w. Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:60 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33094v209%20Family_WR-DSUB_6180xx331023.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33094v209%20Family_WR-DSUB_6180xx331023.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_MALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_6180XX331023/"&gt;https://www.we-online.com/catalog/en/DSUB_MALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_6180XX331023/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-09&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15MT_S_1"/>
</gates>
<devices>
<device name="" package="618015331023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618015331023?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618015331023"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618015331023"/>
<attribute name="WORKING-VOLTAGE" value="60VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX231221_618015231221" prefix="J">
<description>&lt;b&gt;WR-DSUB 8.08 mm Male Angled PCB Connector w. Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Quality Class:3 as per IEC 60 603-13
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:100 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33083v209%20Family_WR-DSUB_6180xx231221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33083v209%20Family_WR-DSUB_6180xx231221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_8_08MM_6180XX231221"&gt;www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_8_08MM_6180XX231221&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15MT_S"/>
</gates>
<devices>
<device name="" package="618015231221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618015231221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618015231221"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618015231221"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX330923_618026330923" prefix="J">
<description>&lt;b&gt;WR-DSUB Female High Density Angled PCB Connector w. Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;Working Voltage:60V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33093v209%20Family_WR-DSUB_6180xx330923.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33093v209%20Family_WR-DSUB_6180xx330923.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_FEMALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_6180XX330923/"&gt;https://www.we-online.com/catalog/en/DSUB_FEMALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_6180XX330923/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-14&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="26FT_S"/>
</gates>
<devices>
<device name="" package="618026330923">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618026330923?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618026330923"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618026330923"/>
<attribute name="WORKING-VOLTAGE" value="60VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX211821_618025211821" prefix="J">
<description>&lt;b&gt;WR-DSUB 8.08 mm Female Angled PCB Connector w/o Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33076v209%20Family_WR-DSUB_6180xx211821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33076v209%20Family_WR-DSUB_6180xx211821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_8_08MM_6180XX211821"&gt;https://www.we-online.com/en/components/products/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_8_08MM_6180XX211821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25FT_S"/>
</gates>
<devices>
<device name="" package="618025211821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618025211821?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618025211821"/>
<attribute name="PINS" value=" 25 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618025211821"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX25123_61800925123" prefix="J">
<description>&lt;b&gt;WR-DSUB Female PCB Connector

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-55 °C up to +105 °C
&lt;BR&gt;Gender	Female
&lt;BR&gt;Type	Straight
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;Shielding Material	Steel
&lt;BR&gt;Shielding Plating	Tin

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o60801v209%20Family_I-O_DSUB_PCB_Female_wo-screw_6180xx25123_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o60801v209%20Family_I-O_DSUB_PCB_Female_wo-screw_6180xx25123_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DSUB_FEMALE_PCB_CONNECTOR_6180XX25123/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/DSUB_FEMALE_PCB_CONNECTOR_6180XX25123&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9FT_S"/>
</gates>
<devices>
<device name="" package="61800925123">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61800925123?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="61800925123"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61800925123"/>
<attribute name="WORKING-VOLTAGE" value="250VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX330923_618015330923" prefix="J">
<description>&lt;b&gt;WR-DSUB Female High Density Angled PCB Connector w. Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;Working Voltage:60V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33093v209%20Family_WR-DSUB_6180xx330923.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33093v209%20Family_WR-DSUB_6180xx330923.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_FEMALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_6180XX330923/"&gt;https://www.we-online.com/catalog/en/DSUB_FEMALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_6180XX330923/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-14&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15FT_S_1"/>
</gates>
<devices>
<device name="" package="618015330923">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618015330923?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618015330923"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618015330923"/>
<attribute name="WORKING-VOLTAGE" value="60VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX231221_618037231221" prefix="J">
<description>&lt;b&gt;WR-DSUB 8.08 mm Male Angled PCB Connector w. Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Quality Class:3 as per IEC 60 603-13
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:100 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33083v209%20Family_WR-DSUB_6180xx231221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33083v209%20Family_WR-DSUB_6180xx231221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_8_08MM_6180XX231221"&gt;www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_8_08MM_6180XX231221&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="37MT_S"/>
</gates>
<devices>
<device name="" package="618037231221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618037231221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618037231221"/>
<attribute name="PINS" value=" 37 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618037231221"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX29321_61800929321" prefix="J">
<description>&lt;b&gt;WR-DSUB Female PCB Connector w. Hex Screw

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-55 °C up to +105 °C
&lt;BR&gt;Gender	Female
&lt;BR&gt;Type	Straight
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;Shielding Material	Steel
&lt;BR&gt;Shielding Plating	Tin

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33090v209%20Family_WR-DSUB_6180xx29321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33090v209%20Family_WR-DSUB_6180xx29321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DSUB_FEMALE_PCB_CONNECTOR_W_HEX_SCREW_6180XX29321/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/DSUB_FEMALE_PCB_CONNECTOR_W_HEX_SCREW_6180XX29321&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9FT_S"/>
</gates>
<devices>
<device name="" package="61800929321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61800929321?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="61800929321"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61800929321"/>
<attribute name="WORKING-VOLTAGE" value="250VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX25123_61802525123" prefix="J">
<description>&lt;b&gt;WR-DSUB Female PCB Connector

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-55 °C up to +105 °C
&lt;BR&gt;Gender	Female
&lt;BR&gt;Type	Straight
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;Shielding Material	Steel
&lt;BR&gt;Shielding Plating	Tin

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o60801v209%20Family_I-O_DSUB_PCB_Female_wo-screw_6180xx25123_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o60801v209%20Family_I-O_DSUB_PCB_Female_wo-screw_6180xx25123_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DSUB_FEMALE_PCB_CONNECTOR_6180XX25123/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/DSUB_FEMALE_PCB_CONNECTOR_6180XX25123&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25FT_S"/>
</gates>
<devices>
<device name="" package="61802525123">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61802525123?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="61802525123"/>
<attribute name="PINS" value=" 25 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61802525123"/>
<attribute name="WORKING-VOLTAGE" value="250VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX231121_618009231121" prefix="J">
<description>&lt;b&gt;WR-DSUB 8.08 mm Female Angled PCB Connector w. Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class：3 as per IEC 60 603-13
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance：RoHS
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR 1：3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33082v209%20Family_WR-DSUB_6180xx231121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33082v209%20Family_WR-DSUB_6180xx231121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_8_08MM_6180XX231121"&gt;https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_8_08MM_6180XX231121/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-13&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9FT_S"/>
</gates>
<devices>
<device name="" package="618009231121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618009231121?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618009231121"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618009231121"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX25023_61801525023" prefix="J">
<description>&lt;b&gt;WR-DSUB Male PCB Connector

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;QOperating Temperature	-55 °C up to +105 °C
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Straight
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;Shielding Material	Steel
&lt;BR&gt;Shielding Plating	Tin

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33086v209%20Family_I-O_DSUB_PCB_Male_6180xx25023_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33086v209%20Family_I-O_DSUB_PCB_Male_6180xx25023_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DSUB_MALE_PCB_CONNECTOR_6180XX25023/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/DSUB_MALE_PCB_CONNECTOR_6180XX25023&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15MT_S"/>
</gates>
<devices>
<device name="" package="61801525023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61801525023?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="61801525023"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61801525023"/>
<attribute name="WORKING-VOLTAGE" value="250VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX325323_618026325323" prefix="J">
<description>&lt;b&gt;WR-DSUB Male High Density Angled PCB Connector w/o Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:60 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33092v209%20Family_WR-DSUB_6180xx325323.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33092v209%20Family_WR-DSUB_6180xx325323.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_MALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_6180XX325323/"&gt;https://www.we-online.com/catalog/en/DSUB_MALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_6180XX325323/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-09&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="26MT_S"/>
</gates>
<devices>
<device name="" package="618026325323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618026325323?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618026325323"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618026325323"/>
<attribute name="WORKING-VOLTAGE" value="60VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX231221_618025231221" prefix="J">
<description>&lt;b&gt;WR-DSUB 8.08 mm Male Angled PCB Connector w. Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Quality Class:3 as per IEC 60 603-13
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:100 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33083v209%20Family_WR-DSUB_6180xx231221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33083v209%20Family_WR-DSUB_6180xx231221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_8_08MM_6180XX231221"&gt;www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_8_08MM_6180XX231221&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25MT_S"/>
</gates>
<devices>
<device name="" package="618025231221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618025231221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618025231221"/>
<attribute name="PINS" value=" 25 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618025231221"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX231121_618025231121" prefix="J">
<description>&lt;b&gt;WR-DSUB 8.08 mm Female Angled PCB Connector w. Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class：3 as per IEC 60 603-13
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance：RoHS
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR 1：3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33082v209%20Family_WR-DSUB_6180xx231121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33082v209%20Family_WR-DSUB_6180xx231121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_8_08MM_6180XX231121"&gt;https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_8_08MM_6180XX231121/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-13&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25FT_S"/>
</gates>
<devices>
<device name="" package="618025231121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618025231121?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618025231121"/>
<attribute name="PINS" value=" 25 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618025231121"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX233821_618025233821" prefix="J">
<description>&lt;b&gt;WR-DSUB 10.30 mm Female Angled PCB Connector w/o Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60818v209%20Family_I-O_DSUB_PCB_Female_wo-screw_6180xx211821_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60818v209%20Family_I-O_DSUB_PCB_Female_wo-screw_6180xx211821_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_10_30MM_6180XX233821/"&gt;https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_10_30MM_6180XX233821/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-14&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25FT_S"/>
</gates>
<devices>
<device name="" package="618025233821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618025233821?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618025233821"/>
<attribute name="PINS" value=" 25 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618025233821"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX29221_61803729221" prefix="J">
<description>&lt;b&gt;WR-DSUB Male PCB Connector with Hex Screw

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-55 °C up to +105 °C
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Straight
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;Shielding Material	Steel
&lt;BR&gt;Shielding Plating	Tin

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33089v209%20Family_WR-DSUB_6180xx29221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33089v209%20Family_WR-DSUB_6180xx29221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DSUB_MALE_PCB_CONNECTOR_W_HEX_SCREW_6180XX29221/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/DSUB_MALE_PCB_CONNECTOR_W_HEX_SCREW_6180XX29221&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="37MT_S"/>
</gates>
<devices>
<device name="" package="61803729221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61803729221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="61803729221"/>
<attribute name="PINS" value=" 37 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61803729221"/>
<attribute name="WORKING-VOLTAGE" value="250VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX231221_618009231221" prefix="J">
<description>&lt;b&gt;WR-DSUB 8.08 mm Male Angled PCB Connector w. Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Quality Class:3 as per IEC 60 603-13
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:100 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33083v209%20Family_WR-DSUB_6180xx231221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33083v209%20Family_WR-DSUB_6180xx231221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_8_08MM_6180XX231221"&gt;www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_8_08MM_6180XX231221&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MT_S"/>
</gates>
<devices>
<device name="" package="618009231221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618009231221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618009231221"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618009231221"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX233721_618025233721" prefix="J">
<description>&lt;b&gt;WR-DSUB 10.30 mm Male Angled PCB Connector w/o Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60857v209%20Family_I-O_DSUB_PCB_Male_wo-screw_6180xx233721_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60857v209%20Family_I-O_DSUB_PCB_Male_wo-screw_6180xx233721_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_10_30MM_6180XX233721/"&gt;https://www.we-online.com/catalog/en/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_10_30MM_6180XX233721/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-09&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25MT_S"/>
</gates>
<devices>
<device name="" package="618025233721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="SHELL SHELL1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618025233721?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618025233721"/>
<attribute name="PINS" value=" 25 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618025233721"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX231121_618015231121" prefix="J">
<description>&lt;b&gt;WR-DSUB 8.08 mm Female Angled PCB Connector w. Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class：3 as per IEC 60 603-13
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance：RoHS
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR 1：3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33082v209%20Family_WR-DSUB_6180xx231121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33082v209%20Family_WR-DSUB_6180xx231121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_8_08MM_6180XX231121"&gt;https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_8_08MM_6180XX231121/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-13&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15FT_S"/>
</gates>
<devices>
<device name="" package="618015231121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618015231121?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618015231121"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618015231121"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX29321_61803729321" prefix="J">
<description>&lt;b&gt;WR-DSUB Female PCB Connector w. Hex Screw

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-55 °C up to +105 °C
&lt;BR&gt;Gender	Female
&lt;BR&gt;Type	Straight
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;Shielding Material	Steel
&lt;BR&gt;Shielding Plating	Tin

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33090v209%20Family_WR-DSUB_6180xx29321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33090v209%20Family_WR-DSUB_6180xx29321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DSUB_FEMALE_PCB_CONNECTOR_W_HEX_SCREW_6180XX29321/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/DSUB_FEMALE_PCB_CONNECTOR_W_HEX_SCREW_6180XX29321&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="37FT_S"/>
</gates>
<devices>
<device name="" package="61803729321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61803729321?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="61803729321"/>
<attribute name="PINS" value=" 37 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61803729321"/>
<attribute name="WORKING-VOLTAGE" value="250VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX211821_618037211821" prefix="J">
<description>&lt;b&gt;WR-DSUB 8.08 mm Female Angled PCB Connector w/o Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33076v209%20Family_WR-DSUB_6180xx211821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33076v209%20Family_WR-DSUB_6180xx211821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_8_08MM_6180XX211821"&gt;https://www.we-online.com/en/components/products/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_8_08MM_6180XX211821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="37FT_S"/>
</gates>
<devices>
<device name="" package="618037211821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618037211821?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618037211821"/>
<attribute name="PINS" value=" 37 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618037211821"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX29221_61802529221" prefix="J">
<description>&lt;b&gt;WR-DSUB Male PCB Connector with Hex Screw

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-55 °C up to +105 °C
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Straight
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;Shielding Material	Steel
&lt;BR&gt;Shielding Plating	Tin

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33089v209%20Family_WR-DSUB_6180xx29221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33089v209%20Family_WR-DSUB_6180xx29221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DSUB_MALE_PCB_CONNECTOR_W_HEX_SCREW_6180XX29221/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/DSUB_MALE_PCB_CONNECTOR_W_HEX_SCREW_6180XX29221&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25MT_S"/>
</gates>
<devices>
<device name="" package="61802529221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61802529221?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="61802529221"/>
<attribute name="PINS" value=" 25 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61802529221"/>
<attribute name="WORKING-VOLTAGE" value="250VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX25023_61803725023" prefix="J">
<description>&lt;b&gt;WR-DSUB Male PCB Connector

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;QOperating Temperature	-55 °C up to +105 °C
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Straight
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;Shielding Material	Steel
&lt;BR&gt;Shielding Plating	Tin

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33086v209%20Family_I-O_DSUB_PCB_Male_6180xx25023_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33086v209%20Family_I-O_DSUB_PCB_Male_6180xx25023_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DSUB_MALE_PCB_CONNECTOR_6180XX25023/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/DSUB_MALE_PCB_CONNECTOR_6180XX25023&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="37MT_S"/>
</gates>
<devices>
<device name="" package="61803725023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61803725023?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="61803725023"/>
<attribute name="PINS" value=" 37 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61803725023"/>
<attribute name="WORKING-VOLTAGE" value="250VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX233821_618009233821" prefix="J">
<description>&lt;b&gt;WR-DSUB 10.30 mm Female Angled PCB Connector w/o Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60818v209%20Family_I-O_DSUB_PCB_Female_wo-screw_6180xx211821_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60818v209%20Family_I-O_DSUB_PCB_Female_wo-screw_6180xx211821_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_10_30MM_6180XX233821/"&gt;https://www.we-online.com/catalog/en/DSUB_FEMALE_ANGLED_PCB_CONNECTOR_W_O_HEX_SCREW_10_30MM_6180XX233821/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-14&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9FT_S"/>
</gates>
<devices>
<device name="" package="618009233821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618009233821?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618009233821"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618009233821"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX25023_61802525023" prefix="J">
<description>&lt;b&gt;WR-DSUB Male PCB Connector

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;QOperating Temperature	-55 °C up to +105 °C
&lt;BR&gt;Gender	Male
&lt;BR&gt;Type	Straight
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;Shielding Material	Steel
&lt;BR&gt;Shielding Plating	Tin

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33086v209%20Family_I-O_DSUB_PCB_Male_6180xx25023_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33086v209%20Family_I-O_DSUB_PCB_Male_6180xx25023_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DSUB_MALE_PCB_CONNECTOR_6180XX25023/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/DSUB_MALE_PCB_CONNECTOR_6180XX25023&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25MT_S"/>
</gates>
<devices>
<device name="" package="61802525023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61802525023?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="61802525023"/>
<attribute name="PINS" value=" 25 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61802525023"/>
<attribute name="WORKING-VOLTAGE" value="250VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX231421_618015231421" prefix="J">
<description>&lt;b&gt;WR-DSUB 10.30 mm Male Angled PCB Connector w. Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60849v209%20Family_I-O_DSUB_PCB_Male_w-screw_6180xx231421_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60849v209%20Family_I-O_DSUB_PCB_Male_w-screw_6180xx231421_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_10_30MM_6180XX231421"&gt;https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_10_30MM_6180XX231421&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15MT_S"/>
</gates>
<devices>
<device name="" package="618015231421">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618015231421?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618015231421"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618015231421"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX331023_618026331023" prefix="J">
<description>&lt;b&gt;WR-DSUB Male High Density Angled PCB Connector w. Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:60 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33094v209%20Family_WR-DSUB_6180xx331023.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33094v209%20Family_WR-DSUB_6180xx331023.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_MALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_6180XX331023/"&gt;https://www.we-online.com/catalog/en/DSUB_MALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_6180XX331023/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-09&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="26MT_S"/>
</gates>
<devices>
<device name="" package="618026331023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618026331023?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618026331023"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618026331023"/>
<attribute name="WORKING-VOLTAGE" value="60VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX330923_618044330923" prefix="J">
<description>&lt;b&gt;WR-DSUB Female High Density Angled PCB Connector w. Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;Working Voltage:60V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33093v209%20Family_WR-DSUB_6180xx330923.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33093v209%20Family_WR-DSUB_6180xx330923.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_FEMALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_6180XX330923/"&gt;https://www.we-online.com/catalog/en/DSUB_FEMALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_6180XX330923/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-14&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="44FT_S"/>
</gates>
<devices>
<device name="" package="618044330923">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618044330923?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618044330923"/>
<attribute name="PINS" value=" 44 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618044330923"/>
<attribute name="WORKING-VOLTAGE" value="60VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX231421_618025231421" prefix="J">
<description>&lt;b&gt;WR-DSUB 10.30 mm Male Angled PCB Connector w. Hex Screw 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Gender:Male
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;BR&gt;Compliance:RoHS&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Electrical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;IR1:3 A
&lt;BR&gt;Working Voltage:125 V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60849v209%20Family_I-O_DSUB_PCB_Male_w-screw_6180xx231421_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60849v209%20Family_I-O_DSUB_PCB_Male_w-screw_6180xx231421_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_10_30MM_6180XX231421"&gt;https://www.we-online.com/en/components/products/DSUB_MALE_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_10_30MM_6180XX231421&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-03-21&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25MT_S"/>
</gates>
<devices>
<device name="" package="618025231421">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618025231421?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618025231421"/>
<attribute name="PINS" value=" 25 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618025231421"/>
<attribute name="WORKING-VOLTAGE" value="125VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX330923_618062330923" prefix="J">
<description>&lt;b&gt;WR-DSUB Female High Density Angled PCB Connector w. Hex Screw
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Kind Properties&lt;/b&gt;
&lt;BR&gt;Gender:Female
&lt;BR&gt;Type:Angled
&lt;BR&gt;Insulator Material:PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Selective Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;Shielding Material:Steel
&lt;BR&gt;Shielding Plating:Nickel
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;Operating Temperature:-55 up to +105 °C
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;Working Voltage:60V (AC)
&lt;BR&gt;Withstanding Voltage:1000 V (AC)
&lt;BR&gt;Contact Resistance:30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33093v209%20Family_WR-DSUB_6180xx330923.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33093v209%20Family_WR-DSUB_6180xx330923.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DSUB_FEMALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_6180XX330923/"&gt;https://www.we-online.com/catalog/en/DSUB_FEMALE_HIGH_DENSITY_ANGLED_PCB_CONNECTOR_W_HEX_SCREW_6180XX330923/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-14&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="62FT_S"/>
</gates>
<devices>
<device name="" package="618062330923">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/618062330923?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="618062330923"/>
<attribute name="PINS" value=" 62 "/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="618062330923"/>
<attribute name="WORKING-VOLTAGE" value="60VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6180XX25123_61803725123" prefix="J">
<description>&lt;b&gt;WR-DSUB Female PCB Connector

&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-55 °C up to +105 °C
&lt;BR&gt;Gender	Female
&lt;BR&gt;Type	Straight
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Insulator Color	White
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;Shielding Material	Steel
&lt;BR&gt;Shielding Plating	Tin

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Working Voltage	250 V (AC)
&lt;BR&gt;Withstanding Voltage	1000 V (AC)
&lt;BR&gt;Contact Resistance	30 mΩ
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o60801v209%20Family_I-O_DSUB_PCB_Female_wo-screw_6180xx25123_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o60801v209%20Family_I-O_DSUB_PCB_Female_wo-screw_6180xx25123_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/DSUB_FEMALE_PCB_CONNECTOR_6180XX25123/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/DSUB_FEMALE_PCB_CONNECTOR_6180XX25123&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-25 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="37FT_S"/>
</gates>
<devices>
<device name="" package="61803725123">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61803725123?ae"/>
<attribute name="GENDER" value="Female"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="61803725123"/>
<attribute name="PINS" value=" 37 "/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61803725123"/>
<attribute name="WORKING-VOLTAGE" value="250VAC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
