<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Wire-to-Board Connectors - WR-FAST &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-08-11&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="638207122003">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 2863
&lt;br&gt;&lt;/b&gt;3pins</description>
</package>
<package name="638307222005">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 2863
&lt;br&gt;&lt;/b&gt;5pins</description>
</package>
<package name="638207222002">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 2863
&lt;br&gt;&lt;/b&gt;2pins</description>
</package>
<package name="638207222008">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 2863
&lt;br&gt;&lt;/b&gt;8pins</description>
</package>
<package name="638307122003">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 2863
&lt;br&gt;&lt;/b&gt;3pins</description>
</package>
<package name="638307122008">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 2863
&lt;br&gt;&lt;/b&gt;8pins</description>
</package>
<package name="638263122008">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 6.3
&lt;br&gt;&lt;/b&gt;8pins</description>
</package>
<package name="638363222008">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;&lt;/b&gt;8pins</description>
</package>
<package name="638307222008">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 2863
&lt;br&gt;&lt;/b&gt;8pins</description>
</package>
<package name="638263222004">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;&lt;/b&gt;4pins</description>
</package>
<package name="638307222007">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 2863
&lt;br&gt;&lt;/b&gt;7pins</description>
</package>
<package name="638263222003">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;&lt;/b&gt;3pins</description>
</package>
<package name="638263222005">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;&lt;/b&gt;5pins</description>
</package>
<package name="638363222003">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;&lt;/b&gt;3pins</description>
</package>
<package name="638263122004">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 6.3
&lt;br&gt;&lt;/b&gt;4pins</description>
</package>
<package name="638207122008">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 2863
&lt;br&gt;&lt;/b&gt;8pins</description>
</package>
<package name="638363222004">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;&lt;/b&gt;4pins</description>
</package>
<package name="638363122004">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 6.3
&lt;br&gt;&lt;/b&gt;4pins</description>
</package>
<package name="638207222005">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 2863
&lt;br&gt;&lt;/b&gt;5pins</description>
</package>
<package name="638307222002">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 2863
&lt;br&gt;&lt;/b&gt;2pins</description>
</package>
<package name="638363222007">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;&lt;/b&gt;7pins</description>
</package>
<package name="638263122002">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 6.3
&lt;br&gt;&lt;/b&gt;2pins</description>
</package>
<package name="638363122008">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 6.3
&lt;br&gt;&lt;/b&gt;8pins</description>
</package>
<package name="638363222005">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;&lt;/b&gt;5pins</description>
</package>
<package name="638207222006">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 2863
&lt;br&gt;&lt;/b&gt;6pins</description>
</package>
<package name="638207122006">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 2863
&lt;br&gt;&lt;/b&gt;6pins</description>
</package>
<package name="638263222007">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;&lt;/b&gt;7pins</description>
</package>
<package name="638207122004">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 2863
&lt;br&gt;&lt;/b&gt;4pins</description>
</package>
<package name="638307122005">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 2863
&lt;br&gt;&lt;/b&gt;5pins</description>
</package>
<package name="638363222002">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;&lt;/b&gt;2pins</description>
</package>
<package name="638307122007">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 2863
&lt;br&gt;&lt;/b&gt;7pins</description>
</package>
<package name="638263122007">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 6.3
&lt;br&gt;&lt;/b&gt;7pins</description>
</package>
<package name="638363122006">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 6.3
&lt;br&gt;&lt;/b&gt;6pins</description>
</package>
<package name="638307222006">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 2863
&lt;br&gt;&lt;/b&gt;6pins</description>
</package>
<package name="638363122003">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 6.3
&lt;br&gt;&lt;/b&gt;3pins</description>
</package>
<package name="638363122005">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 6.3
&lt;br&gt;&lt;/b&gt;5pins</description>
</package>
<package name="638363222006">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;&lt;/b&gt;6pins</description>
</package>
<package name="638263222008">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;&lt;/b&gt;8pins</description>
</package>
<package name="638363122002">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 6.3
&lt;br&gt;&lt;/b&gt;2pins</description>
</package>
<package name="638263222006">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;&lt;/b&gt;6pins</description>
</package>
<package name="638263122003">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 6.3
&lt;br&gt;&lt;/b&gt;3pins</description>
</package>
<package name="638207222003">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 2863
&lt;br&gt;&lt;/b&gt;3pins</description>
</package>
<package name="638207122005">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 2863
&lt;br&gt;&lt;/b&gt;5pins</description>
</package>
<package name="638207222004">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 2863
&lt;br&gt;&lt;/b&gt;4pins</description>
</package>
<package name="638363122007">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 6.3
&lt;br&gt;&lt;/b&gt;7pins</description>
</package>
<package name="638207122002">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 2863
&lt;br&gt;&lt;/b&gt;2pins</description>
</package>
<package name="638307122006">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 2863
&lt;br&gt;&lt;/b&gt;6pins</description>
</package>
<package name="638263122005">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 6.3
&lt;br&gt;&lt;/b&gt;5pins</description>
</package>
<package name="638307122004">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 2863
&lt;br&gt;&lt;/b&gt;4pins</description>
</package>
<package name="638307222004">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 2863
&lt;br&gt;&lt;/b&gt;4pins</description>
</package>
<package name="638307222003">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 2863
&lt;br&gt;&lt;/b&gt;3pins</description>
</package>
<package name="638207122007">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 2863
&lt;br&gt;&lt;/b&gt;7pins</description>
</package>
<package name="638307122002">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 2863
&lt;br&gt;&lt;/b&gt;2pins</description>
</package>
<package name="638263122006">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 6.3
&lt;br&gt;&lt;/b&gt;6pins</description>
</package>
<package name="638207222007">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 2863
&lt;br&gt;&lt;/b&gt;7pins</description>
</package>
<package name="638263222002">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;&lt;/b&gt;2pins</description>
</package>
</packages>
<symbols>
<symbol name="5PT_M">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="3PT_M">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="2PT_M">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="8PT_M">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="4PT_M">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="6PT_M">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="7PT_M">
<description>Gender : Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="638207122003" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o166976v209%20Family_WR-FAST_638207122003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o166976v209%20Family_WR-FAST_638207122003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382071220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382071220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT_M"/>
</gates>
<devices>
<device name="" package="638207122003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638207122003.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638207122003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638207122003 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638307222005" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161722v209%20Family_WR-FAST_638307222005.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161722v209%20Family_WR-FAST_638307222005.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383072220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383072220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT_M"/>
</gates>
<devices>
<device name="" package="638307222005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638307222005.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638307222005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638307222005 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638207222002" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o165124v209%20Family_ConFAST_638207222004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o165124v209%20Family_ConFAST_638207222004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382072220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382072220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT_M"/>
</gates>
<devices>
<device name="" package="638207222002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638207222002.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638207222002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638207222002 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638307122003" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161726v209%20Family_WR-FAST_638307122004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161726v209%20Family_WR-FAST_638307122004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383071220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383071220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT_M"/>
</gates>
<devices>
<device name="" package="638307122003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638307122003.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638307122003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638307122003 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638207222008" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o165124v209%20Family_ConFAST_638207222004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o165124v209%20Family_ConFAST_638207222004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382072220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382072220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT_M"/>
</gates>
<devices>
<device name="" package="638207222008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638207222008.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638207222008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638207222008 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638263122008" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o165125v209%20Family_WR-FAST_638263122004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o165125v209%20Family_WR-FAST_638263122004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382631220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382631220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT_M"/>
</gates>
<devices>
<device name="" package="638263122008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638263122008.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638263122008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638263122008 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638363222008" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161724v209%20Family_WR-FAST_638363222003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161724v209%20Family_WR-FAST_638363222003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383632220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383632220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT_M"/>
</gates>
<devices>
<device name="" package="638363222008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638363222008.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638363222008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638363222008 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638307222007" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161722v209%20Family_WR-FAST_638307222005.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161722v209%20Family_WR-FAST_638307222005.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383072220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383072220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT_M"/>
</gates>
<devices>
<device name="" package="638307222007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638307222007.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638307222007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638307222007 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638307222008" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161722v209%20Family_WR-FAST_638307222005.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161722v209%20Family_WR-FAST_638307222005.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383072220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383072220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT_M"/>
</gates>
<devices>
<device name="" package="638307222008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638307222008.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638307222008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638307222008 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638263222003" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o166977v209%20Family_WR-FAST_638263222003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o166977v209%20Family_WR-FAST_638263222003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382632220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382632220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT_M"/>
</gates>
<devices>
<device name="" package="638263222003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638263222003.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638263222003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638263222003 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638263222005" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o166977v209%20Family_WR-FAST_638263222003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o166977v209%20Family_WR-FAST_638263222003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382632220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382632220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT_M"/>
</gates>
<devices>
<device name="" package="638263222005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638263222005.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638263222005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638263222005 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638263222004" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o166977v209%20Family_WR-FAST_638263222003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o166977v209%20Family_WR-FAST_638263222003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382632220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382632220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT_M"/>
</gates>
<devices>
<device name="" package="638263222004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638263222004.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638263222004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638263222004 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638363222003" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161724v209%20Family_WR-FAST_638363222003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161724v209%20Family_WR-FAST_638363222003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383632220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383632220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT_M"/>
</gates>
<devices>
<device name="" package="638363222003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638363222003.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638363222003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638363222003 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638307122008" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161726v209%20Family_WR-FAST_638307122004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161726v209%20Family_WR-FAST_638307122004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383071220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383071220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT_M"/>
</gates>
<devices>
<device name="" package="638307122008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638307122008.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638307122008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638307122008 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638363222004" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161724v209%20Family_WR-FAST_638363222003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161724v209%20Family_WR-FAST_638363222003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383632220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383632220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT_M"/>
</gates>
<devices>
<device name="" package="638363222004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638363222004.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638363222004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638363222004 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638263122004" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o165125v209%20Family_WR-FAST_638263122004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o165125v209%20Family_WR-FAST_638263122004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382631220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382631220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT_M"/>
</gates>
<devices>
<device name="" package="638263122004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2" route="any"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638263122004.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638263122004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638263122004 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638207122008" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o166976v209%20Family_WR-FAST_638207122003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o166976v209%20Family_WR-FAST_638207122003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382071220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382071220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT_M"/>
</gates>
<devices>
<device name="" package="638207122008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638207122008.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638207122008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638207122008 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638207222005" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o165124v209%20Family_ConFAST_638207222004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o165124v209%20Family_ConFAST_638207222004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382072220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382072220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT_M"/>
</gates>
<devices>
<device name="" package="638207222005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638207222005.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638207222005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638207222005 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638363122004" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161720v209%20Family_WR-FAST_638363122003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161720v209%20Family_WR-FAST_638363122003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383631220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383631220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT_M"/>
</gates>
<devices>
<device name="" package="638363122004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638363122004.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638363122004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638363122004 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638307222002" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161722v209%20Family_WR-FAST_638307222005.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161722v209%20Family_WR-FAST_638307222005.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383072220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383072220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT_M"/>
</gates>
<devices>
<device name="" package="638307222002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638307222002.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638307222002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638307222002 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638263122002" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o165125v209%20Family_WR-FAST_638263122004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o165125v209%20Family_WR-FAST_638263122004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382631220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382631220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT_M"/>
</gates>
<devices>
<device name="" package="638263122002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638263122002.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638263122002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638263122002 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638363122008" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161720v209%20Family_WR-FAST_638363122003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161720v209%20Family_WR-FAST_638363122003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383631220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383631220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT_M"/>
</gates>
<devices>
<device name="" package="638363122008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7" route="any"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638363122008.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638363122008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638363122008 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638363222007" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161724v209%20Family_WR-FAST_638363222003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161724v209%20Family_WR-FAST_638363222003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383632220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383632220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT_M"/>
</gates>
<devices>
<device name="" package="638363222007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638363222007.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638363222007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638363222007 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638363222005" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161724v209%20Family_WR-FAST_638363222003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161724v209%20Family_WR-FAST_638363222003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383632220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383632220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT_M"/>
</gates>
<devices>
<device name="" package="638363222005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638363222005.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638363222005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638363222005 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638207222006" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o165124v209%20Family_ConFAST_638207222004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o165124v209%20Family_ConFAST_638207222004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382072220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382072220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT_M"/>
</gates>
<devices>
<device name="" package="638207222006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638207222006.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638207222006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638207222006 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638207122006" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o166976v209%20Family_WR-FAST_638207122003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o166976v209%20Family_WR-FAST_638207122003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382071220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382071220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT_M"/>
</gates>
<devices>
<device name="" package="638207122006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638207122006.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638207122006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638207122006 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638263222007" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o166977v209%20Family_WR-FAST_638263222003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o166977v209%20Family_WR-FAST_638263222003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382632220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382632220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT_M"/>
</gates>
<devices>
<device name="" package="638263222007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638263222007.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638263222007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638263222007 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638207122004" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o166976v209%20Family_WR-FAST_638207122003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o166976v209%20Family_WR-FAST_638207122003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382071220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382071220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT_M"/>
</gates>
<devices>
<device name="" package="638207122004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638207122004.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638207122004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638207122004 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638307122005" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161726v209%20Family_WR-FAST_638307122004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161726v209%20Family_WR-FAST_638307122004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383071220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383071220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT_M"/>
</gates>
<devices>
<device name="" package="638307122005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638307122005.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638307122005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638307122005 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638363222002" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161724v209%20Family_WR-FAST_638363222003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161724v209%20Family_WR-FAST_638363222003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383632220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383632220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT_M"/>
</gates>
<devices>
<device name="" package="638363222002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638363222002.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638363222002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638363222002 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638307122007" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161726v209%20Family_WR-FAST_638307122004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161726v209%20Family_WR-FAST_638307122004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383071220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383071220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT_M"/>
</gates>
<devices>
<device name="" package="638307122007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638307122007.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638307122007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638307122007 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638263122007" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o165125v209%20Family_WR-FAST_638263122004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o165125v209%20Family_WR-FAST_638263122004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382631220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382631220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT_M"/>
</gates>
<devices>
<device name="" package="638263122007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638263122007.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638263122007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638263122007 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638363122006" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161720v209%20Family_WR-FAST_638363122003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161720v209%20Family_WR-FAST_638363122003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383631220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383631220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT_M"/>
</gates>
<devices>
<device name="" package="638363122006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638363122006.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638363122006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638363122006 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638307222006" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161722v209%20Family_WR-FAST_638307222005.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161722v209%20Family_WR-FAST_638307222005.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383072220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383072220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT_M"/>
</gates>
<devices>
<device name="" package="638307222006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638307222006.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638307222006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638307222006 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638363122005" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161720v209%20Family_WR-FAST_638363122003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161720v209%20Family_WR-FAST_638363122003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383631220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383631220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT_M"/>
</gates>
<devices>
<device name="" package="638363122005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638363122005.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638363122005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638363122005 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638363122003" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161720v209%20Family_WR-FAST_638363122003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161720v209%20Family_WR-FAST_638363122003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383631220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383631220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT_M"/>
</gates>
<devices>
<device name="" package="638363122003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638363122003.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638363122003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638363122003 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638363222006" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161724v209%20Family_WR-FAST_638363222003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161724v209%20Family_WR-FAST_638363222003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383632220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383632220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT_M"/>
</gates>
<devices>
<device name="" package="638363222006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638363222006.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638363222006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638363222006 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638263222008" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o166977v209%20Family_WR-FAST_638263222003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o166977v209%20Family_WR-FAST_638263222003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382632220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382632220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT_M"/>
</gates>
<devices>
<device name="" package="638263222008">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638263222008.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638263222008 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638263222008 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638363122002" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161720v209%20Family_WR-FAST_638363122003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161720v209%20Family_WR-FAST_638363122003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383631220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383631220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT_M"/>
</gates>
<devices>
<device name="" package="638363122002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638363122002.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638363122002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638363122002 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638207222003" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o165124v209%20Family_ConFAST_638207222004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o165124v209%20Family_ConFAST_638207222004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382072220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382072220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT_M"/>
</gates>
<devices>
<device name="" package="638207222003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638207222003.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638207222003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638207222003 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638263222006" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o166977v209%20Family_WR-FAST_638263222003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o166977v209%20Family_WR-FAST_638263222003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382632220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382632220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT_M"/>
</gates>
<devices>
<device name="" package="638263222006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1" route="any"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638263222006.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638263222006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638263222006 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638207122005" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o166976v209%20Family_WR-FAST_638207122003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o166976v209%20Family_WR-FAST_638207122003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382071220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382071220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT_M"/>
</gates>
<devices>
<device name="" package="638207122005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2" route="any"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638207122005.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638207122005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638207122005 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638263122003" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o165125v209%20Family_WR-FAST_638263122004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o165125v209%20Family_WR-FAST_638263122004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382631220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382631220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT_M"/>
</gates>
<devices>
<device name="" package="638263122003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638263122003.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638263122003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638263122003 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638363122007" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161720v209%20Family_WR-FAST_638363122003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161720v209%20Family_WR-FAST_638363122003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383631220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383631220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT_M"/>
</gates>
<devices>
<device name="" package="638363122007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638363122007.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638363122007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638363122007 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638207222004" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o165124v209%20Family_ConFAST_638207222004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o165124v209%20Family_ConFAST_638207222004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382072220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382072220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT_M"/>
</gates>
<devices>
<device name="" package="638207222004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638207222004.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638207222004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638207222004 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638207122002" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o166976v209%20Family_WR-FAST_638207122003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o166976v209%20Family_WR-FAST_638207122003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382071220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382071220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT_M"/>
</gates>
<devices>
<device name="" package="638207122002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638207122002.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638207122002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638207122002 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638263122005" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o165125v209%20Family_WR-FAST_638263122004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o165125v209%20Family_WR-FAST_638263122004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382631220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382631220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT_M"/>
</gates>
<devices>
<device name="" package="638263122005">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638263122005.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638263122005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638263122005 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638307122006" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161726v209%20Family_WR-FAST_638307122004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161726v209%20Family_WR-FAST_638307122004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383071220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383071220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT_M"/>
</gates>
<devices>
<device name="" package="638307122006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638307122006.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638307122006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638307122006 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638307122004" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161726v209%20Family_WR-FAST_638307122004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161726v209%20Family_WR-FAST_638307122004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383071220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383071220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT_M"/>
</gates>
<devices>
<device name="" package="638307122004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638307122004.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638307122004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638307122004 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638307222004" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161722v209%20Family_WR-FAST_638307222005.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161722v209%20Family_WR-FAST_638307222005.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383072220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383072220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT_M"/>
</gates>
<devices>
<device name="" package="638307222004">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638307222004.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638307222004 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638307222004 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638307222003" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Vertical Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161722v209%20Family_WR-FAST_638307222005.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161722v209%20Family_WR-FAST_638307222005.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383072220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_VERTICAL_6383072220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT_M"/>
</gates>
<devices>
<device name="" package="638307222003">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638307222003.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638307222003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638307222003 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638307122002" prefix="J">
<description>&lt;b&gt;WR-FAST 7.62 mm THT Male Header Angled Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 7.62 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o161726v209%20Family_WR-FAST_638307122004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o161726v209%20Family_WR-FAST_638307122004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383071220XX/"&gt;https://www.we-online.com/catalog/en/FAST_7_6_2_THT_MALE_ANGLED_6383071220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT_M"/>
</gates>
<devices>
<device name="" package="638307122002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638307122002.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638307122002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="7.62mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638307122002 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638207122007" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o166976v209%20Family_WR-FAST_638207122003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o166976v209%20Family_WR-FAST_638207122003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382071220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382071220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT_M"/>
</gates>
<devices>
<device name="" package="638207122007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638207122007.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638207122007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638207122007 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638263122006" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Angled Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o165125v209%20Family_WR-FAST_638263122004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o165125v209%20Family_WR-FAST_638263122004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382631220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_ANGLED_6382631220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Udpated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT_M"/>
</gates>
<devices>
<device name="" package="638263122006">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638263122006.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638263122006 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 638263122006 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638207222007" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 2863
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o165124v209%20Family_ConFAST_638207222004.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o165124v209%20Family_ConFAST_638207222004.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382072220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382072220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT_M"/>
</gates>
<devices>
<device name="" package="638207222007">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638207222007.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638207222007 "/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638207222007 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="638263222002" prefix="J">
<description>&lt;b&gt;WR-FAST 5.08 mm THT Male Header Vertical Blade 6.3
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 5.08 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PC 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Steel 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 1600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 5 MΩ 
&lt;br&gt;IR 16 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E150931 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o166977v209%20Family_WR-FAST_638263222003.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o166977v209%20Family_WR-FAST_638263222003.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382632220XX/"&gt;https://www.we-online.com/catalog/en/FAST_5_08_THT_MALE_VERTICAL_6382632220XX/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-08-11&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT_M"/>
</gates>
<devices>
<device name="" package="638263222002">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/638263222002.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 638263222002 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 638263222002 "/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
