<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Fuseholder - WR-FSH &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-09-08&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="696315001002">
<description>&lt;b&gt;WR-FSH Shocksafe Fuseholder - Panel - Turn and Lock Cover - THT</description>
</package>
<package name="696213001002">
<description>&lt;b&gt;WR-FSH Shocksafe Fuseholder - Panel - Screw and Lock Cover - THT</description>
</package>
<package name="696314001002">
<description>&lt;b&gt;WR-FSH Shocksafe Fuseholder - Panel - Turn and Lock Cover - THT</description>
</package>
<package name="696103201002">
<description>&lt;b&gt;WR-FSH Fuseholder THR Blocks PCB Clip Cover</description>
</package>
<package name="696212001002">
<description>&lt;b&gt;WR-FSH Shocksafe Fuseholder - Panel - Screw and Lock Cover - THT</description>
</package>
<package name="696310001002">
<description>&lt;b&gt;WR-FSH Shocksafe Fuseholder - PCB - Turn and Lock Cover - THT</description>
</package>
<package name="696108003002">
<description>&lt;b&gt;WR-FSH Fuseholder THT Blocks PCB Clip Cover
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Mates with 696122003001</description>
</package>
<package name="696211001102">
<description>&lt;b&gt;WR-FSH Shocksafe Fuseholder - Panel - Screw and Lock Cover - THT - Glow wire Plastic</description>
</package>
<package name="696101000002">
<description>&lt;b&gt;WR-FSH Fuseholder THT Blocks PCB Clip Cover
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Mates with 696120004001</description>
</package>
<package name="696107003002">
<description>&lt;b&gt;WR-FSH Fuseholder THT Blocks PCB Clip Cover
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Mates with 696122003001</description>
</package>
<package name="696105003002">
<description>&lt;b&gt;WR-FSH Fuseholder THT Blocks PCB Clip Cover
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Mates with 696122003001</description>
</package>
<package name="696106003002">
<description>&lt;b&gt;WR-FSH Fuseholder THT Blocks PCB Clip Cover
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Mates with 696122003001</description>
</package>
<package name="696103101002">
<description>&lt;b&gt;WR-FSH Fuseholder SMT Blocks PCB Clip Cover</description>
</package>
<package name="696309001002">
<description>&lt;b&gt;WR-FSH Shocksafe Fuseholder - PCB - Turn and Lock Cover - THT</description>
</package>
</packages>
<symbols>
<symbol name="WR-FSH">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="696213001002" prefix="J">
<description>&lt;b&gt;WR-FSH Shocksafe Fuseholder - Panel - Screw and Lock Cover - THT
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Spring Material INOX Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION  
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 20 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;Contact Resistance [VDE] 10 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Protection Class I &amp; II 
&lt;br&gt;Fuse Size 5x20 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E157417 
&lt;br&gt;VDE Approval 133367 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;p&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o150743v209%20Family_WR-FUSE_696213001002.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o150743v209%20Family_WR-FUSE_696213001002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/SHOCKSAFE_FUSEHOLDER_696213001002"&gt;https://katalog.we-online.com/en/em/SHOCKSAFE_FUSEHOLDER_696213001002&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-10-25&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-FSH"/>
</gates>
<devices>
<device name="" package="696213001002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/696213001002.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 696213001002 "/>
<attribute name="VALUE" value=" 696213001002 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="696315001002" prefix="J">
<description>&lt;b&gt;WR-FSH Shocksafe Fuseholder - Panel - Turn and Lock Cover - THT
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Spring Material INOX Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION  
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 20 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;Contact Resistance [VDE] 10 mΩ 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Protection Class I &amp; II 
&lt;br&gt;Fuse Size 5x20 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E157417 
&lt;br&gt;VDE Approval 120170 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;p&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33111v209%20Family_WR-FSH_696315001002.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33111v209%20Family_WR-FSH_696315001002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/FSH_THT_PANEL_TURN_AND_LOCK_COVER_69631X001002"&gt;https://katalog.we-online.com/en/em/FSH_THT_PANEL_TURN_AND_LOCK_COVER_69631X001002&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-10-25&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-FSH"/>
</gates>
<devices>
<device name="" package="696314001002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/696315001002.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 696315001002 "/>
<attribute name="VALUE" value=" 696315001002 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="696314001002" prefix="J">
<description>&lt;b&gt;WR-FSH Shocksafe Fuseholder - Panel - Turn and Lock Cover - THT
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Spring Material INOX Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION  
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 20 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;Contact Resistance [VDE] 10 mΩ 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Protection Class I &amp; II 
&lt;br&gt;Fuse Size 5x20 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E157417 
&lt;br&gt;VDE Approval 120170 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;p&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33111v209%20Family_WR-FSH_696315001002.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33111v209%20Family_WR-FSH_696315001002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/FSH_THT_PANEL_TURN_AND_LOCK_COVER_69631X001002"&gt;https://katalog.we-online.com/en/em/FSH_THT_PANEL_TURN_AND_LOCK_COVER_69631X001002&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-10-25&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-FSH"/>
</gates>
<devices>
<device name="" package="696314001002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/696314001002.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 696314001002 "/>
<attribute name="VALUE" value=" 696314001002 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="696310001002" prefix="J">
<description>&lt;b&gt;WR-FSH Shocksafe Fuseholder - PCB - Turn and Lock Cover - THT
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Spring Material INOX Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION  
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 20 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;Contact Resistance [VDE] 10 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Protection Class II 
&lt;br&gt;Fuse Size 5x20 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E157417 
&lt;br&gt;VDE Approval 120170 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 

&lt;p&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o150670v209%20Family_WR-FSH_696309001002.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o150670v209%20Family_WR-FSH_696309001002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/FSH_THT_PCB_TURN_AND_LOCK_COVER_6963XX001002_2"&gt;https://katalog.we-online.com/en/em/FSH_THT_PCB_TURN_AND_LOCK_COVER_6963XX001002_2&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2020-07-21&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-FSH"/>
</gates>
<devices>
<device name="" package="696310001002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/696310001002.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value="696310001002"/>
<attribute name="VALUE" value="696310001002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="696103201002" prefix="J">
<description>&lt;b&gt;WR-FSH Fuseholder THR Blocks PCB Clip Cover
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PETG35 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION  
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 20 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;Contact Resistance [VDE] 10 mΩ 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Protection Class I &amp; II 
&lt;br&gt;Fuse Size 5x20 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E157417 
&lt;br&gt;VDE Approval 120170 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 

&lt;p&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58927v209%20Family_p748_WR-FUSE_6961032010xx_4C.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58927v209%20Family_p748_WR-FUSE_6961032010xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/FSH_THR_PCB_CLIP_COVER_696103201002"&gt;https://katalog.we-online.com/en/em/FSH_THR_PCB_CLIP_COVER_696103201002&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-10-25&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-FSH"/>
</gates>
<devices>
<device name="" package="696103201002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/696103201002.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value="696103201002"/>
<attribute name="VALUE" value="696103201002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="696212001002" prefix="J">
<description>&lt;b&gt;WR-FSH Shocksafe Fuseholder - Panel - Screw and Lock Cover - THT
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Spring Material INOX Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION  
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 20 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;Contact Resistance [VDE] 10 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Protection Class I &amp; II 
&lt;br&gt;Fuse Size 5x20 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E157417 
&lt;br&gt;VDE Approval 133367 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 

&lt;p&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58923v209%20Family_FSH_Shocksafe_696212001002_pf2.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58923v209%20Family_FSH_Shocksafe_696212001002_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/FSH_THT_PANEL_SCREW_AND_LOCK_COVER_69621X001002"&gt;https://katalog.we-online.com/en/em/FSH_THT_PANEL_SCREW_AND_LOCK_COVER_69621X001002&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-10-25&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-FSH"/>
</gates>
<devices>
<device name="" package="696212001002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/696212001002.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 696212001002 "/>
<attribute name="VALUE" value=" 696212001002 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="696108003002" prefix="J">
<description>&lt;b&gt;WR-FSH Fuseholder THT Blocks PCB Clip Cover
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION  
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 20 A 
&lt;br&gt;IR VDE 6.3 A 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;Contact Resistance [VDE] 10 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Protection Class I &amp; II 
&lt;br&gt;Fuse Size 5x20 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E157417 
&lt;br&gt;VDE Approval 129302 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;

&lt;p&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33102v209%20Family_WR-FSH_69610X003002.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33102v209%20Family_WR-FSH_69610X003002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/FSH_THT_PCB_CLIP_COVER_69610X003002"&gt;https://katalog.we-online.com/en/em/FSH_THT_PCB_CLIP_COVER_69610X003002&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-10-25&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-FSH"/>
</gates>
<devices>
<device name="" package="696108003002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/696108003002.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="6.3A"/>
<attribute name="MATES" value="696122003001 "/>
<attribute name="PART-NUMBER" value="696108003002"/>
<attribute name="VALUE" value="696108003002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="696211001102" prefix="J">
<description>&lt;b&gt;WR-FSH Shocksafe Fuseholder - Panel - Screw and Lock Cover - THT - Glow wire Plastic
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Spring Material INOX Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION  
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 20 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 3 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;Contact Resistance [VDE] 10 mΩ 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Protection Class I &amp; II 
&lt;br&gt;Fuse Size 5x20 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E157417 
&lt;br&gt;VDE Approval 133366 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;
&lt;p&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33107v209%20Family_WR-FSH_696211001102.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33107v209%20Family_WR-FSH_696211001102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/FSH_THT_PANEL_SCREW_AND_LOCK_COVER_696211001102"&gt;https://katalog.we-online.com/en/em/FSH_THT_PANEL_SCREW_AND_LOCK_COVER_696211001102&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-10-25&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-FSH"/>
</gates>
<devices>
<device name="" package="696211001102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/696211001102.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value=" 696211001102 "/>
<attribute name="VALUE" value=" 696211001102 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="696101000002" prefix="J">
<description>&lt;b&gt;WR-FSH Fuseholder THT Blocks PCB Clip Cover
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PPO (PPE+PS) 
&lt;br&gt;Insulator Flammability Rating UL94 V-1 
&lt;br&gt;Insulator Color Beige 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION  
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 18 A 
&lt;br&gt;IR VDE 6.3 A 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Protection Class I &amp; II 
&lt;br&gt;Fuse Size 5x20 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E157417 
&lt;br&gt;VDE Approval 129300 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 

&lt;p&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33101v209%20Family_WR-FSH_696101000002.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33101v209%20Family_WR-FSH_696101000002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/FSH_THT_PCB_CLIP_COVER_696101000002"&gt;https://katalog.we-online.com/en/em/FSH_THT_PCB_CLIP_COVER_696101000002&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-10-25&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-FSH"/>
</gates>
<devices>
<device name="" package="696101000002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/696101000002.pdf"/>
<attribute name="IR-UL" value="18A"/>
<attribute name="IR-VDE" value="6.3A"/>
<attribute name="MATES" value="696120004001"/>
<attribute name="PART-NUMBER" value="696101000002"/>
<attribute name="VALUE" value="696101000002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="696107003002" prefix="J">
<description>&lt;b&gt;WR-FSH Fuseholder THT Blocks PCB Clip Cover
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION  
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 20 A 
&lt;br&gt;IR VDE 6.3 A 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;Contact Resistance [VDE] 10 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Protection Class I &amp; II 
&lt;br&gt;Fuse Size 5x20 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E157417 
&lt;br&gt;VDE Approval 129302 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;

&lt;p&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33102v209%20Family_WR-FSH_69610X003002.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33102v209%20Family_WR-FSH_69610X003002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/FSH_THT_PCB_CLIP_COVER_69610X003002"&gt;https://katalog.we-online.com/en/em/FSH_THT_PCB_CLIP_COVER_69610X003002&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-10-25&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-FSH"/>
</gates>
<devices>
<device name="" package="696107003002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/696107003002.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="6.3A"/>
<attribute name="MATES" value="696122003001 "/>
<attribute name="PART-NUMBER" value="696107003002"/>
<attribute name="VALUE" value="696107003002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="696105003002" prefix="J">
<description>&lt;b&gt;WR-FSH Fuseholder THT Blocks PCB Clip Cover
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION  
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 20 A 
&lt;br&gt;IR VDE 6.3 A 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;Contact Resistance [VDE] 10 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Protection Class I &amp; II 
&lt;br&gt;Fuse Size 5x20 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E157417 
&lt;br&gt;VDE Approval 129302 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;

&lt;p&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33102v209%20Family_WR-FSH_69610X003002.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33102v209%20Family_WR-FSH_69610X003002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/FSH_THT_PCB_CLIP_COVER_69610X003002"&gt;https://katalog.we-online.com/en/em/FSH_THT_PCB_CLIP_COVER_69610X003002&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-10-25&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-FSH"/>
</gates>
<devices>
<device name="" package="696105003002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/696105003002.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="6.3A"/>
<attribute name="MATES" value="696122003001 "/>
<attribute name="PART-NUMBER" value="696105003002"/>
<attribute name="VALUE" value="696105003002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="696106003002" prefix="J">
<description>&lt;b&gt;WR-FSH Fuseholder THT Blocks PCB Clip Cover
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Green 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION  
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 20 A 
&lt;br&gt;IR VDE 6.3 A 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [cULus] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;Contact Resistance [VDE] 10 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Protection Class I &amp; II 
&lt;br&gt;Fuse Size 5x20 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E157417 
&lt;br&gt;VDE Approval 129302 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 
&lt;br&gt;

&lt;p&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33102v209%20Family_WR-FSH_69610X003002.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33102v209%20Family_WR-FSH_69610X003002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/FSH_THT_PCB_CLIP_COVER_69610X003002"&gt;https://katalog.we-online.com/en/em/FSH_THT_PCB_CLIP_COVER_69610X003002&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-10-25&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-FSH"/>
</gates>
<devices>
<device name="" package="696106003002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/696106003002.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="6.3A"/>
<attribute name="MATES" value="696122003001 "/>
<attribute name="PART-NUMBER" value="696106003002"/>
<attribute name="VALUE" value="696106003002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="696309001002" prefix="J">
<description>&lt;b&gt;WR-FSH Shocksafe Fuseholder - PCB - Turn and Lock Cover - THT
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA66 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Spring Material INOX Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION  
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 20 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 3000 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;Contact Resistance [VDE] 10 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Protection Class II 
&lt;br&gt;Fuse Size 5x20 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E157417 
&lt;br&gt;VDE Approval 120170 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 

&lt;p&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o150670v209%20Family_WR-FSH_696309001002.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o150670v209%20Family_WR-FSH_696309001002.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/FSH_THT_PCB_TURN_AND_LOCK_COVER_6963XX001002_2"&gt;https://katalog.we-online.com/en/em/FSH_THT_PCB_TURN_AND_LOCK_COVER_6963XX001002_2&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2020-07-21&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-FSH"/>
</gates>
<devices>
<device name="" package="696309001002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/696309001002.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value="696309001002"/>
<attribute name="VALUE" value="696309001002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="696103101002" prefix="J">
<description>&lt;b&gt;WR-FSH Fuseholder THT Blocks PCB Clip Cover
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PETG35 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION  
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -30 up to +120 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 20 A 
&lt;br&gt;IR VDE 10 A 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Working Voltage [VDE] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Withstanding Voltage [VDE] 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;Contact Resistance [VDE] 10 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Protection Class I &amp; II 
&lt;br&gt;Fuse Size 5x20 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E157417 
&lt;br&gt;VDE Approval 40038367 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Box 

&lt;p&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o72897v209%20Family_WR-FUSE_696103101002_4C.jpg"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o72897v209%20Family_WR-FUSE_696103101002_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/FSH_SMT_PCB_CLIP_COVER_696103101002"&gt;https://katalog.we-online.com/en/em/FSH_SMT_PCB_CLIP_COVER_696103101002&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-10-25&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-FSH"/>
</gates>
<devices>
<device name="" package="696103101002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/696103101002.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="10A"/>
<attribute name="PART-NUMBER" value="696103101002"/>
<attribute name="VALUE" value="696103101002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
