<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - LED Connectors - WR-LECO&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-06-06&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="695402151122">
<description>&lt;B&gt;WR-LECO 1.50 mm SMT Angled Receptacle Connector</description>
</package>
<package name="695402300222">
</package>
<package name="695401310222">
</package>
<package name="695401400222">
<description>&lt;B&gt;WR-LECO 4.00 mm SMT Horizontal Connector</description>
</package>
<package name="695401300222">
</package>
<package name="695404151122">
<description>&lt;B&gt;WR-LECO 1.50 mm SMT Angled Receptacle Connector</description>
</package>
<package name="695401000222">
<description>&lt;B&gt;WR-LECO Single Contact - Poke In Connector - Vertical Cable Entry - SMT 
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;SMT, 2pins</description>
</package>
<package name="695405151122">
<description>&lt;B&gt;WR-LECO 1.50 mm SMT Angled Receptacle Connector</description>
</package>
<package name="695403400222">
<description>&lt;B&gt;WR-LECO 4.00 mm SMT Horizontal Connector</description>
</package>
<package name="695402400222">
<description>&lt;B&gt;WR-LECO 4.00 mm SMT Horizontal Connector</description>
</package>
<package name="695403150122">
<description>&lt;B&gt;WR-LECO 1.50 mm SMT Angled Plug Connector</description>
</package>
<package name="695402150122">
<description>&lt;B&gt;WR-LECO 1.50 mm SMT Angled Plug Connector</description>
</package>
<package name="695405150122">
<description>&lt;B&gt;WR-LECO 1.50 mm SMT Angled Plug Connector</description>
</package>
<package name="695404150122">
<description>&lt;B&gt;WR-LECO 1.50 mm SMT Angled Plug Connector</description>
</package>
<package name="695403151122">
<description>&lt;B&gt;WR-LECO 1.50 mm SMT Angled Receptacle Connector</description>
</package>
<package name="695402250128">
<description>&lt;B&gt;WR-LECO 2.54 mm SMT Angled Hermaphroditic</description>
</package>
<package name="695402310222">
</package>
</packages>
<symbols>
<symbol name="1FS">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="1FS-2">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="2FS-1">
<description>Socket Header THT,3Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="2FS">
<description>Socket Header THT,3Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="1FS-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="4FS">
<description>Socket Header THT,3Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="3FS">
<description>Socket Header THT,3Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="5FS">
<description>Socket Header THT,3Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="5MS">
<description>2X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="2MS">
<description>2X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3MS">
<description>2X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="4MS">
<description>2X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="2FS-2">
<description>Socket Header THT,3Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="2MFS">
<description>2X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="695402151122" prefix="J">
<description>&lt;b&gt;WR-LECO 1.50 mm SMT Angled Receptacle Connector
&lt;br&gt;
&lt;br&gt;
Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 1.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 150 V (AC) 
&lt;br&gt;Withstanding Voltage 1300 V (AC) 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA6T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Solder Tabs Brass 
&lt;br&gt;Solder Tabs Thickness 3.05µm Mat Tin over 1.27µm Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58306v209%20Family_Receptacle_Connector_p81_WR-LECO_6954xx151122_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58306v209%20Family_Receptacle_Connector_p81_WR-LECO_6954xx151122_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/LECO_1_50_SMT_ANGLED_RECEPTACLE_6954XX151122/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/LECO_1_50_SMT_ANGLED_RECEPTACLE_6954XX151122&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-06-14&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2FS"/>
</gates>
<devices>
<device name="" package="695402151122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695402151122?ae"/>
<attribute name="GENDER" value="Receptacle"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="695402151122"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="695402151122"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="695402300222" prefix="J">
<description>&lt;b&gt;WR-LECO Series 300/310 - Slider 4.00 mm - Horizontal Cable Entry - SMT
&lt;br&gt;
&lt;br&gt;
Kind Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Pitch	4 mm
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 6 A; 9 A
&lt;br&gt;Working Voltage 250 V (AC); 600 V (AC)
&lt;br&gt;Withstanding Voltage 2000 V (AC)
&lt;br&gt;Contact Resistance 10 mΩ
&lt;br&gt;&lt;br&gt;
&lt;b&gt; Wire Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Solid Wire Section (AWG)	20 to 18 (AWG); 24 to 22 (AWG)
&lt;br&gt;Solid Wire Section (Metric)	0.2 to 0.34 (mm²); 0.5 to 0.75 (mm²)
&lt;br&gt;Wire Strip Length	6.8 (mm); 8.5 (mm)
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -60 up to +105 °C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material	LCP
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Ivory
&lt;br&gt;Pin Material	Copper Alloy
&lt;br&gt;Pin Plating	Matte Tin over Nickel


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o742300v209%20Multi-WR-LECO-695402300222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o742300v209%20Multi-WR-LECO-695402300222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_LECO_SERIES_300_310/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR_LECO_SERIES_300_310&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2023-06-06&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2FS-1"/>
</gates>
<devices>
<device name="" package="695402300222">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695402300222?ae"/>
<attribute name="GENDER" value="Cable Entry"/>
<attribute name="IR" value="9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 695402300222 "/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="4mm"/>
<attribute name="SOLID-WIRE-SECTION" value="20 to 18 (AWG)"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 695402300222 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="695401310222" prefix="J">
<description>&lt;b&gt;WR-LECO Series 300/310 - Slider 4.00 mm - Horizontal Cable Entry - SMT
&lt;br&gt;
&lt;br&gt;
Kind Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Pitch	4 mm
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 6 A; 9 A
&lt;br&gt;Working Voltage 250 V (AC); 600 V (AC)
&lt;br&gt;Withstanding Voltage 2000 V (AC)
&lt;br&gt;Contact Resistance 10 mΩ
&lt;br&gt;&lt;br&gt;
&lt;b&gt; Wire Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Solid Wire Section (AWG)	20 to 18 (AWG); 24 to 22 (AWG)
&lt;br&gt;Solid Wire Section (Metric)	0.2 to 0.34 (mm²); 0.5 to 0.75 (mm²)
&lt;br&gt;Wire Strip Length	6.8 (mm); 8.5 (mm)
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -60 up to +105 °C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material	LCP
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Ivory
&lt;br&gt;Pin Material	Copper Alloy
&lt;br&gt;Pin Plating	Matte Tin over Nickel


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o742300v209%20Multi-WR-LECO-695402300222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o742300v209%20Multi-WR-LECO-695402300222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_LECO_SERIES_300_310/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR_LECO_SERIES_300_310&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2023-06-06&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1FS-2"/>
</gates>
<devices>
<device name="" package="695401310222">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695401310222?ae"/>
<attribute name="GENDER" value="Cable Entry"/>
<attribute name="IR" value="6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 695401310222 "/>
<attribute name="PINS" value="1"/>
<attribute name="PITCH" value="4mm"/>
<attribute name="SOLID-WIRE-SECTION" value="24 to 22 (AWG)"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 695401310222 "/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="695401400222" prefix="J">
<description>&lt;b&gt;WR-LECO 4.00 mm SMT Horizontal Connector
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 4 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 9 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PPA-GF 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIREPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Solid Wire Section (AWG) 18 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.823 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 18 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.823 to 0.205 (mm²) 
&lt;br&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79410v209%20WR-LECO_6954xx400222_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79410v209%20WR-LECO_6954xx400222_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/LECO_4_00_SMT_WTB_CONNECTOR_HORIZONTAL_6954XX400222"&gt;https://www.we-online.com/catalog/en/LECO_4_00_SMT_WTB_CONNECTOR_HORIZONTAL_6954XX400222&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-10-30&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1FS"/>
</gates>
<devices>
<device name="" package="695401400222">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695401400222?ae"/>
<attribute name="GENDER" value="Wire to Board"/>
<attribute name="IR" value="9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="695401400222"/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="4mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="695401400222"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="695401300222" prefix="J">
<description>&lt;b&gt;WR-LECO Series 300/310 - Slider 4.00 mm - Horizontal Cable Entry - SMT
&lt;br&gt;
&lt;br&gt;
Kind Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Pitch	4 mm
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 6 A; 9 A
&lt;br&gt;Working Voltage 250 V (AC); 600 V (AC)
&lt;br&gt;Withstanding Voltage 2000 V (AC)
&lt;br&gt;Contact Resistance 10 mΩ
&lt;br&gt;&lt;br&gt;
&lt;b&gt; Wire Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Solid Wire Section (AWG)	20 to 18 (AWG); 24 to 22 (AWG)
&lt;br&gt;Solid Wire Section (Metric)	0.2 to 0.34 (mm²); 0.5 to 0.75 (mm²)
&lt;br&gt;Wire Strip Length	6.8 (mm); 8.5 (mm)
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -60 up to +105 °C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material	LCP
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Ivory
&lt;br&gt;Pin Material	Copper Alloy
&lt;br&gt;Pin Plating	Matte Tin over Nickel


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o742300v209%20Multi-WR-LECO-695402300222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o742300v209%20Multi-WR-LECO-695402300222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_LECO_SERIES_300_310/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR_LECO_SERIES_300_310&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2023-06-06&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1FS-1"/>
</gates>
<devices>
<device name="" package="695401300222">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695401300222?ae"/>
<attribute name="GENDER" value="Cable Entry"/>
<attribute name="IR" value="9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 695401300222 "/>
<attribute name="PINS" value="1"/>
<attribute name="PITCH" value="4mm"/>
<attribute name="SOLID-WIRE-SECTION" value="20 to 18 (AWG)"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 695401300222 "/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="695404151122" prefix="J">
<description>&lt;b&gt;WR-LECO 1.50 mm SMT Angled Receptacle Connector
&lt;br&gt;
&lt;br&gt;
Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 1.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 150 V (AC) 
&lt;br&gt;Withstanding Voltage 1300 V (AC) 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA6T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Solder Tabs Brass 
&lt;br&gt;Solder Tabs Thickness 3.05µm Mat Tin over 1.27µm Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58306v209%20Family_Receptacle_Connector_p81_WR-LECO_6954xx151122_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58306v209%20Family_Receptacle_Connector_p81_WR-LECO_6954xx151122_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/LECO_1_50_SMT_ANGLED_RECEPTACLE_6954XX151122/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/LECO_1_50_SMT_ANGLED_RECEPTACLE_6954XX151122&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-06-14&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4FS"/>
</gates>
<devices>
<device name="" package="695404151122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695404151122?ae"/>
<attribute name="GENDER" value="Receptacle"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="695404151122"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="695404151122"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="695401000222" prefix="J">
<description>&lt;b&gt;WR-LECO Single Contact - Poke In Connector - Vertical Cable Entry - SMT
&lt;br&gt;
&lt;br&gt;
ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 600 V (AC) 
&lt;br&gt;Withstanding Voltage 2200 V (AC) 
&lt;br&gt;IR 7 A 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +130 °C  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA 9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;&lt;br&gt;
&lt;b&gt; Wire Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Solid Wire Section (AWG) 18 to 20 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.823 to 0.518 (mm²) 
&lt;br&gt;Wire Strip Length 6 up to 7 (mm) 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o321293v209%20Family_WR-LECO_695401000222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o321293v209%20Family_WR-LECO_695401000222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/LECO_SINGLE_CONTACT_POKE_IN_CONNECTOR_VERTICAL"&gt;https://www.we-online.com/catalog/en/LECO_SINGLE_CONTACT_POKE_IN_CONNECTOR_VERTICAL&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2021-11-05&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="1FS"/>
</gates>
<devices>
<device name="" package="695401000222">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695401000222?ae"/>
<attribute name="GENDER" value="Cable Entry"/>
<attribute name="IR" value="7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="695401000222"/>
<attribute name="PINS" value="1"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="695401000222"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="695403400222" prefix="J">
<description>&lt;b&gt;WR-LECO 4.00 mm SMT Horizontal Connector
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 4 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 9 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PPA-GF 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIREPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Solid Wire Section (AWG) 18 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.823 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 18 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.823 to 0.205 (mm²) 
&lt;br&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79410v209%20WR-LECO_6954xx400222_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79410v209%20WR-LECO_6954xx400222_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/LECO_4_00_SMT_WTB_CONNECTOR_HORIZONTAL_6954XX400222"&gt;https://www.we-online.com/catalog/en/LECO_4_00_SMT_WTB_CONNECTOR_HORIZONTAL_6954XX400222&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-10-30&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3FS"/>
</gates>
<devices>
<device name="" package="695403400222">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695403400222?ae"/>
<attribute name="GENDER" value="Wire to Board"/>
<attribute name="IR" value="9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="695403400222"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="4mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="695403400222"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="695405151122" prefix="J">
<description>&lt;b&gt;WR-LECO 1.50 mm SMT Angled Receptacle Connector
&lt;br&gt;
&lt;br&gt;
Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 1.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 150 V (AC) 
&lt;br&gt;Withstanding Voltage 1300 V (AC) 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA6T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Solder Tabs Brass 
&lt;br&gt;Solder Tabs Thickness 3.05µm Mat Tin over 1.27µm Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58306v209%20Family_Receptacle_Connector_p81_WR-LECO_6954xx151122_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58306v209%20Family_Receptacle_Connector_p81_WR-LECO_6954xx151122_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/LECO_1_50_SMT_ANGLED_RECEPTACLE_6954XX151122/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/LECO_1_50_SMT_ANGLED_RECEPTACLE_6954XX151122&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-06-14&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5FS"/>
</gates>
<devices>
<device name="" package="695405151122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695405151122?ae"/>
<attribute name="GENDER" value="Receptacle"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="695405151122"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="695405151122"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="695402400222" prefix="J">
<description>&lt;b&gt;WR-LECO 4.00 mm SMT Horizontal Connector
&lt;br&gt;
&lt;br&gt;
KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 4 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR UL 9 A 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Working Voltage [UL] 250 V (AC) 
&lt;br&gt;Withstanding Voltage [UL] 1500 V (AC) 
&lt;br&gt;Contact Resistance [UL] 20 mΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PPA-GF 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Grey 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIREPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Solid Wire Section (AWG) 18 to 24 (AWG) 
&lt;br&gt;Solid Wire Section (Metric) 0.823 to 0.205 (mm²) 
&lt;br&gt;Stranded Wire Section (AWG) 18 to 24 (AWG) 
&lt;br&gt;Stranded Wire Section (Metric) 0.823 to 0.205 (mm²) 
&lt;br&gt;Wire Strip Length 8 up to 9 (mm) 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79410v209%20WR-LECO_6954xx400222_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79410v209%20WR-LECO_6954xx400222_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/LECO_4_00_SMT_WTB_CONNECTOR_HORIZONTAL_6954XX400222"&gt;https://www.we-online.com/catalog/en/LECO_4_00_SMT_WTB_CONNECTOR_HORIZONTAL_6954XX400222&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-10-30&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2FS"/>
</gates>
<devices>
<device name="" package="695402400222">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695402400222?ae"/>
<attribute name="GENDER" value="Wire to Board"/>
<attribute name="IR" value="9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="695402400222"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="4mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="695402400222"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="695403150122" prefix="J">
<description>&lt;b&gt;WR-LECO 1.50 mm SMT Angled Plug Connector
&lt;br&gt;
&lt;br&gt;
Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 1.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 150 V (AC) 
&lt;br&gt;Withstanding Voltage 1300 V (AC) 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA6T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Solder Tabs Brass 
&lt;br&gt;Solder Tabs Thickness 3.05µm Mat Tin over 1.27µm Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58302v209%20Family_Plug_Connector_p80_WR-LECO_6954xx150122_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58302v209%20Family_Plug_Connector_p80_WR-LECO_6954xx150122_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/LECO_1_50_SMT_ANGLED_PLUG_6954XX150122"&gt;https://www.we-online.com/catalog/en/LECO_1_50_SMT_ANGLED_PLUG_6954XX150122&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-10-30&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MS"/>
</gates>
<devices>
<device name="" package="695403150122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695403150122?ae"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="695403150122"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="695403150122"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="695404150122" prefix="J">
<description>&lt;b&gt;WR-LECO 1.50 mm SMT Angled Plug Connector
&lt;br&gt;
&lt;br&gt;
Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 1.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 150 V (AC) 
&lt;br&gt;Withstanding Voltage 1300 V (AC) 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA6T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Solder Tabs Brass 
&lt;br&gt;Solder Tabs Thickness 3.05µm Mat Tin over 1.27µm Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58302v209%20Family_Plug_Connector_p80_WR-LECO_6954xx150122_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58302v209%20Family_Plug_Connector_p80_WR-LECO_6954xx150122_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/LECO_1_50_SMT_ANGLED_PLUG_6954XX150122"&gt;https://www.we-online.com/catalog/en/LECO_1_50_SMT_ANGLED_PLUG_6954XX150122&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-10-30&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS"/>
</gates>
<devices>
<device name="" package="695404150122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695404150122?ae"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="695404150122"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="695404150122"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="695405150122" prefix="J">
<description>&lt;b&gt;WR-LECO 1.50 mm SMT Angled Plug Connector
&lt;br&gt;
&lt;br&gt;
Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 1.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 150 V (AC) 
&lt;br&gt;Withstanding Voltage 1300 V (AC) 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA6T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Solder Tabs Brass 
&lt;br&gt;Solder Tabs Thickness 3.05µm Mat Tin over 1.27µm Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58302v209%20Family_Plug_Connector_p80_WR-LECO_6954xx150122_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58302v209%20Family_Plug_Connector_p80_WR-LECO_6954xx150122_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/LECO_1_50_SMT_ANGLED_PLUG_6954XX150122"&gt;https://www.we-online.com/catalog/en/LECO_1_50_SMT_ANGLED_PLUG_6954XX150122&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-10-30&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MS"/>
</gates>
<devices>
<device name="" package="695405150122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695405150122?ae"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="695405150122"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="695405150122"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="695402250128" prefix="J">
<description>&lt;b&gt;WR-LECO 2.54 mm SMT Angled Hermaphroditic
&lt;br&gt;
&lt;br&gt;
Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 2.54 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 300 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;cULus Approval E478560 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Ivory 
&lt;br&gt;Contact Material Beryllium Copper 
&lt;br&gt;Contact Plating Gold Flash over Ni 
&lt;br&gt;Contact Type Stamped 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o79407v209%20WR-LECO_695402250128_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o79407v209%20WR-LECO_695402250128_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/LECO_2_54_SMT_ANGLED_HERMAPHRODITIC_695402250128"&gt;https://www.we-online.com/catalog/en/LECO_2_54_SMT_ANGLED_HERMAPHRODITIC_695402250128&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-10-30&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MFS"/>
</gates>
<devices>
<device name="" package="695402250128">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695402250128?ae"/>
<attribute name="GENDER" value="Hermaphroditic"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="695402250128"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="695402250128"/>
<attribute name="WORKING-VOLTAGE" value="300V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="695402150122" prefix="J">
<description>&lt;b&gt;WR-LECO 1.50 mm SMT Angled Plug Connector
&lt;br&gt;
&lt;br&gt;
Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 1.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 150 V (AC) 
&lt;br&gt;Withstanding Voltage 1300 V (AC) 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA6T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Solder Tabs Brass 
&lt;br&gt;Solder Tabs Thickness 3.05µm Mat Tin over 1.27µm Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58302v209%20Family_Plug_Connector_p80_WR-LECO_6954xx150122_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58302v209%20Family_Plug_Connector_p80_WR-LECO_6954xx150122_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/LECO_1_50_SMT_ANGLED_PLUG_6954XX150122"&gt;https://www.we-online.com/catalog/en/LECO_1_50_SMT_ANGLED_PLUG_6954XX150122&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-10-30&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS"/>
</gates>
<devices>
<device name="" package="695402150122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695402150122?ae"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="695402150122"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="695402150122"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="695402310222" prefix="J">
<description>&lt;b&gt;WR-LECO Series 300/310 - Slider 4.00 mm - Horizontal Cable Entry - SMT
&lt;br&gt;
&lt;br&gt;
Kind Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Pitch	4 mm
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 6 A; 9 A
&lt;br&gt;Working Voltage 250 V (AC); 600 V (AC)
&lt;br&gt;Withstanding Voltage 2000 V (AC)
&lt;br&gt;Contact Resistance 10 mΩ
&lt;br&gt;&lt;br&gt;
&lt;b&gt; Wire Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Solid Wire Section (AWG)	20 to 18 (AWG); 24 to 22 (AWG)
&lt;br&gt;Solid Wire Section (Metric)	0.2 to 0.34 (mm²); 0.5 to 0.75 (mm²)
&lt;br&gt;Wire Strip Length	6.8 (mm); 8.5 (mm)
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -60 up to +105 °C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material	LCP
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Ivory
&lt;br&gt;Pin Material	Copper Alloy
&lt;br&gt;Pin Plating	Matte Tin over Nickel


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o742300v209%20Multi-WR-LECO-695402300222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o742300v209%20Multi-WR-LECO-695402300222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_LECO_SERIES_300_310/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WR_LECO_SERIES_300_310&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2023-06-06&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2FS-2"/>
</gates>
<devices>
<device name="" package="695402310222">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695402310222?ae"/>
<attribute name="GENDER" value="Cable Entry"/>
<attribute name="IR" value="6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 695402310222 "/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="4mm"/>
<attribute name="SOLID-WIRE-SECTION" value="24 to 22 (AWG)"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 695402310222 "/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="695403151122" prefix="J">
<description>&lt;b&gt;WR-LECO 1.50 mm SMT Angled Receptacle Connector
&lt;br&gt;
&lt;br&gt;
Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 1.5 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 150 V (AC) 
&lt;br&gt;Withstanding Voltage 1300 V (AC) 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA6T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Contact Material Phosphor Bronze 
&lt;br&gt;Contact Plating Matte Tin over Nickel 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Solder Tabs Brass 
&lt;br&gt;Solder Tabs Thickness 3.05µm Mat Tin over 1.27µm Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o58306v209%20Family_Receptacle_Connector_p81_WR-LECO_6954xx151122_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o58306v209%20Family_Receptacle_Connector_p81_WR-LECO_6954xx151122_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/LECO_1_50_SMT_ANGLED_RECEPTACLE_6954XX151122/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/en/components/products/LECO_1_50_SMT_ANGLED_RECEPTACLE_6954XX151122&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-06-14&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3FS"/>
</gates>
<devices>
<device name="" package="695403151122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/695403151122?ae"/>
<attribute name="GENDER" value="Receptacle"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="695403151122"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="1.5mm"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="695403151122"/>
<attribute name="WORKING-VOLTAGE" value="150V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
