<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Coaxial Connectors - WR-MCX &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-09-10&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="60611102111303">
<description>&lt;b&gt;WR-MCX Right Angle</description>
</package>
<package name="60612202111307">
<description>&lt;B&gt;WR-MCX SMT Edge Card for PCB 1.6mm Max.</description>
</package>
<package name="60612002111504">
<description>&lt;b&gt;Straight Solder Leg 3.94mm MCX PCB THT Jack</description>
</package>
<package name="60612202111510">
<description>&lt;b&gt;WR-MCX Pin Edge for PCB 1.1mm</description>
</package>
<package name="60612102111406">
<description>&lt;b&gt;WR-MCX Straight</description>
</package>
<package name="60612202111511">
<description>&lt;b&gt;WR-MCX Pin Edge for PCB 1.6mm</description>
</package>
<package name="60612202111309">
<description>&lt;B&gt;WR-MCX Reversible SMT Edge Card for PCB 1.6mm max</description>
</package>
<package name="60612002111505">
<description>&lt;b&gt;WR-MCX Straight Solder Leg 1.73mm</description>
</package>
<package name="60614003121504">
<description>&lt;b&gt;WR-MCX Straight Solder Leg 3.94mm</description>
</package>
<package name="60613003121501">
<description>&lt;b&gt;Right Angle Solder Leg 3.94mm MCX PCB THT Plug</description>
</package>
<package name="60612202111308">
<description>&lt;b&gt;WR-MCX SMT Edge Card Extented solder leg for PCB 1.6mm max</description>
</package>
<package name="60611002111502">
<description>&lt;b&gt;WR-MCX Right Angle Solder Leg 1.73mm</description>
</package>
<package name="60611002111501">
<description>&lt;b&gt;WR-MCX Right Angle Solder Leg 3.94mm</description>
</package>
</packages>
<symbols>
<symbol name="JACK">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="PLUG">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="60611102111303" prefix="J">
<description>&lt;b&gt;WR-MCX Right Angle
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface IEC 61169-36 
&lt;br&gt;Connector Type MCX 
&lt;br&gt;Gender Jack  
&lt;br&gt;Orientation Type Right Angle 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;

&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;PACKAGINGPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Qty. 950 
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o150547v209%20Family_WR-MCX_60611102111303.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o150547v209%20Family_WR-MCX_60611102111303.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/em/WR-MCX_60611102111303"&gt;https://www.we-online.com/katalog/en/em/WR-MCX_60611102111303&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2019-11-04&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60611102111303">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/60611102111303.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="60611102111303"/>
<attribute name="VALUE" value="60611102111303"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60612202111307" prefix="J">
<description>&lt;b&gt;WR-MCX SMT Edge Card for PCB 1.6mm Max.
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface  IEC 61169-36
&lt;br&gt;Connector Type  MCX 
&lt;br&gt;Gender  Jack 
&lt;br&gt;Orientation Type  Straight 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;PACKAGINGPROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Qty. 1000 
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o150550v209%20Family_WR-MCX_60612202111307.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o150550v209%20Family_WR-MCX_60612202111307.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/em/WR-MCX_60612202111307"&gt;https://www.we-online.com/katalog/en/em/WR-MCX_60612202111307&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2019-11-04&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60612202111307">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/60612202111307.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="PART-NUMBER" value="60612202111307"/>
<attribute name="VALUE" value="60612202111307"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60612002111504" prefix="J">
<description>&lt;b&gt;Straight Solder Leg 3.94mm MCX PCB THT Jack
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface IEC 61169-36 
&lt;br&gt;Connector Type MCX 
&lt;br&gt;Gender Jack  
&lt;br&gt;Orientation Type  Straight 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;PACKAGINGPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Qty. 180 
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o150614v209%20Family-WR-MCX_60612002111504.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o150614v209%20Family-WR-MCX_60612002111504.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/em/WR-MCX_60612002111504"&gt;https://www.we-online.com/katalog/en/em/WR-MCX_60612002111504&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2019-11-04&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60612002111504">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/60612002111504.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="60612002111504"/>
<attribute name="VALUE" value="60612002111504"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60612202111510" prefix="J">
<description>&lt;b&gt;WR-MCX Pin Edge for PCB 1.1mm
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface IEC 61169-36 
&lt;br&gt;Connector Type MCX 
&lt;br&gt;Gender Jack  
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;PACKAGINGPROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Qty. 180 
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o150553v209%20Family_WR-MCX_60612202111510.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o150553v209%20Family_WR-MCX_60612202111510.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/em/WR-MCX_60612202111510"&gt;https://www.we-online.com/katalog/en/em/WR-MCX_60612202111510&lt;/a&gt;&lt;p&gt;

Udpated by Ella Wu  2019-11-04&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60612202111510">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/60612202111510.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="PART-NUMBER" value="60612202111510"/>
<attribute name="VALUE" value="60612202111510"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60612202111511" prefix="J">
<description>&lt;b&gt;WR-MCX Pin Edge for PCB 1.6mm
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface IEC 61169-36 
&lt;br&gt;Connector Type MCX 
&lt;br&gt;Gender Jack  
&lt;br&gt;Orientation Type Straight
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;PACKAGINGPROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Qty. 180  
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o150554v209%20Family_WR-MCX_60612202111511.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o150554v209%20Family_WR-MCX_60612202111511.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/em/WR-MCX_60612202111511"&gt;https://www.we-online.com/katalog/en/em/WR-MCX_60612202111511&lt;/a&gt;&lt;p&gt;

Updated  by Ella Wu  2019-11-04&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60612202111511">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/60612202111511.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="PART-NUMBER" value="60612202111511"/>
<attribute name="VALUE" value="60612202111511"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60612102111406" prefix="J">
<description>&lt;b&gt;WR-MCX Straight
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface IEC 61169-36 
&lt;br&gt;Connector Type MCX 
&lt;br&gt;Gender Jack  
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Center Contact Retention (Axial) 26.7 N 
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;PACKAGINGPROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Qty. 850 
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o150549v209%20Family_WR-MCX_60612102111406.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o150549v209%20Family_WR-MCX_60612102111406.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/em/WR-MCX_60612102111406"&gt;https://www.we-online.com/katalog/en/em/WR-MCX_60612102111406&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2019-11-04&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60612102111406">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/60612102111406.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="60612102111406"/>
<attribute name="VALUE" value="60612102111406"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60612202111309" prefix="J">
<description>&lt;b&gt;WR-MCX Reversible SMT Edge Card for PCB 1.6mm max.
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface  IEC 61169-36
&lt;br&gt;Connector Type  MCX 
&lt;br&gt;Gender  Jack 
&lt;br&gt;Orientation Type  Straight 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;PACKAGINGPROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Qty. 1000 
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o150552v209%20Family_WR-MCX_60612202111309.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o150552v209%20Family_WR-MCX_60612202111309.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/em/WR-MCX_60612202111309"&gt;https://www.we-online.com/katalog/en/em/WR-MCX_60612202111309&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2019-11-04&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60612202111309">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/60612202111309.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="PART-NUMBER" value="60612202111309"/>
<attribute name="VALUE" value="60612202111309"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60614003121504" prefix="J">
<description>&lt;b&gt;WR-MCX Straight Solder Leg 3.94mm
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface IEC 61169-36 
&lt;br&gt;Connector Type MCX 
&lt;br&gt;Gender Plug
&lt;br&gt;Orientation Type  Straight 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;PACKAGINGPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Qty. 180 
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o150557v209%20Family_WR-MCX_60614003121504.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o150557v209%20Family_WR-MCX_60614003121504.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/em/WR-MCX_60614003121504"&gt;https://www.we-online.com/katalog/en/em/WR-MCX_60614003121504&lt;/a&gt;&lt;p&gt;

Udpated by Ella Wu  2019-11-04&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60614003121504">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/60614003121504.pdf"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="60614003121504"/>
<attribute name="VALUE" value="60614003121504"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60612002111505" prefix="J">
<description>&lt;b&gt;WR-MCX Straight Solder Leg 1.73mm
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface IEC 61169-36 
&lt;br&gt;Connector Type MCX 
&lt;br&gt;Gender Jack  
&lt;br&gt;Orientation Type Straight
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;PACKAGINGPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Qty. 180 
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o150548v209%20Family_WR-MCX_60612002111505.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o150548v209%20Family_WR-MCX_60612002111505.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/em/WR-MCX_60612002111505"&gt;https://www.we-online.com/katalog/en/em/WR-MCX_60612002111505&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2019-11-04&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60612002111505">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/60612002111505.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="60612002111505"/>
<attribute name="VALUE" value="60612002111505"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60612202111308" prefix="J">
<description>&lt;b&gt;WR-MCX SMT Edge Card Extented solder leg for PCB 1.6mm max.
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface  IEC 61169-36
&lt;br&gt;Connector Type  MCX 
&lt;br&gt;Gender  Jack 
&lt;br&gt;Orientation Type  Straight 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;PACKAGINGPROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Qty. 1000 
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o150551v209%20Family_WR-MCX_60612202111308.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o150551v209%20Family_WR-MCX_60612202111308.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/em/WR-MCX_60612202111308"&gt;https://www.we-online.com/katalog/en/em/WR-MCX_60612202111308&lt;/a&gt;&lt;p&gt;

Updated  by Ella Wu  2019-11-04&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60612202111308">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/60612202111308.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="PART-NUMBER" value="60612202111308"/>
<attribute name="VALUE" value="60612202111308"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60613003121501" prefix="J">
<description>&lt;b&gt;Right Angle Solder Leg 3.94mm MCX PCB THT Plug
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface IEC 61169-36 
&lt;br&gt;Connector Type MCX 
&lt;br&gt;Gender Plug
&lt;br&gt;Orientation Type Right Angle 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;PACKAGINGPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Qty. 180 
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o150556v209%20Family_WR-MCX_60613003121501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o150556v209%20Family_WR-MCX_60613003121501.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/em/WR-MCX_60613003121501"&gt;https://www.we-online.com/katalog/en/em/WR-MCX_60613003121501&lt;/a&gt;&lt;p&gt;

Updated  by Ella Wu  2019-11-04&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60613003121501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/60613003121501.pdf"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="60613003121501"/>
<attribute name="VALUE" value="60613003121501"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60611002111502" prefix="J">
<description>&lt;b&gt;WR-MCX Right Angle Solder Leg 1.73mm
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface IEC 61169-36 
&lt;br&gt;Connector Type MCX 
&lt;br&gt;Gender Jack  
&lt;br&gt;Orientation Type Right Angle 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;PACKAGINGPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Qty. 180 
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o150546v209%20Family_WR-MCX_60611002111502.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o150546v209%20Family_WR-MCX_60611002111502.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/em/WR-MCX_60611002111502"&gt;https://www.we-online.com/katalog/en/em/WR-MCX_60611002111502&lt;/a&gt;&lt;p&gt;

Updated  by Ella Wu  2019-11-04&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60611002111502">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/60611002111502.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="60611002111502"/>
<attribute name="VALUE" value="60611002111502"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60611002111501" prefix="J">
<description>&lt;b&gt;WR-MCX Right Angle Solder Leg 3.94mm
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface IEC 61169-36 
&lt;br&gt;Connector Type MCX 
&lt;br&gt;Gender Jack  
&lt;br&gt;Orientation Type Right Angle 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;
PACKAGINGPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Qty. 180 
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o150545v209%20Family_WR-MCX_60611002111501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o150545v209%20Family_WR-MCX_60611002111501.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/em/WR-MCX_60611002111501"&gt;https://www.we-online.com/katalog/en/em/WR-MCX_60611002111501&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2019-11-04&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60611002111501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/60611002111501.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="60611002111501"/>
<attribute name="VALUE" value="60611002111501"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
