<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Coaxial Connectors - WR-MMCX &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-05-29&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="66011102111302">
<description>&lt;b&gt;WR-MMCX Right Angle Jack</description>
</package>
<package name="66013002121501">
<description>&lt;B&gt;WR-MMCX Right Angle
&lt;br&gt;&lt;/b&gt;Gender : Plug</description>
</package>
<package name="66012202111305">
<description>&lt;b&gt;WR-MMCX SMT Edge Card
&lt;br&gt;&lt;/b&gt;Gender : Jack</description>
</package>
<package name="66014002121503">
<description>&lt;B&gt;WR-MMCX Straight
&lt;br&gt;&lt;/b&gt;Gender : Plug</description>
</package>
<package name="66011002111501">
<description>&lt;b&gt;WR-MMCX Right Angle
&lt;br&gt;&lt;/b&gt;Gender : Jack</description>
</package>
<package name="66012102111404">
<description>&lt;B&gt;WR-MMCX Straight
&lt;br&gt;&lt;/b&gt;Gender : Jack</description>
</package>
<package name="66012002111503">
<description>&lt;b&gt;WR-MMCX Straight
&lt;br&gt;&lt;/b&gt;Gender : Jack</description>
</package>
</packages>
<symbols>
<symbol name="WR-MMCX_JACK">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WR-MMCX_PLUG">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="66011102111302" prefix="J">
<description>&lt;b&gt;WR-MMCX Right Angle Jack
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 

&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface IEC 61169-52 
&lt;br&gt;Connector Type MMCX 
&lt;br&gt;Gender Jack 
&lt;br&gt;Orientation Type Right Angle 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGINGPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Qty. 1500
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o176661v209%20Family_WR-MMCX_66011102111302.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o176661v209%20Family_WR-MMCX_66011102111302.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MMCX_SMT_JACK_RIGHT_ANGLE_JACK/"&gt;https://www.we-online.com/catalog/en/MMCX_SMT_JACK_RIGHT_ANGLE_JACK/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2020-05-29&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-MMCX_JACK"/>
</gates>
<devices>
<device name="" package="66011102111302">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/66011102111302.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="IEC 61169-52"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="ORIENTATION-TYPE" value="Right Angle"/>
<attribute name="PART-NUMBER" value=" 66011102111302 "/>
<attribute name="VALUE" value="66011102111302"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66014002121503" prefix="J">
<description>&lt;b&gt;WR-MMCX Straight
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface  IEC 61169-52 
&lt;br&gt;Connector Type  MMCX 
&lt;br&gt;Gender   Plug  
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;
PACKAGINGPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Qty. 198 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o150577v209%20Family_WR-MMCX_66014002121503.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o150577v209%20Family_WR-MMCX_66014002121503.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/WR-MMCX_66014002121503"&gt;https://katalog.we-online.com/en/em/WR-MMCX_66014002121503&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2019-11-01&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-MMCX_PLUG"/>
</gates>
<devices>
<device name="" package="66014002121503">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/66014002121503.pdf"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="INTERFACE" value="IEC 61169-52"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="66014002121503"/>
<attribute name="VALUE" value="66014002121503"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66012202111305" prefix="J">
<description>&lt;b&gt;WR-MMCX SMT Edge Card
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface  IEC 61169-52 
&lt;br&gt;Connector Type  MMCX 
&lt;br&gt;Gender  Jack 
&lt;br&gt;Orientation Type  Straight 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;
PACKAGINGPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Qty. 2000
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o150575v209%20Family_WR-MMCX_66012202111305.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o150575v209%20Family_WR-MMCX_66012202111305.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/WR-MMCX_66012202111305"&gt;https://katalog.we-online.com/en/em/WR-MMCX_66012202111305&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2019-11-01&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-MMCX_JACK"/>
</gates>
<devices>
<device name="" package="66012202111305">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/66012202111305.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="IEC 61169-52"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="66012202111305"/>
<attribute name="VALUE" value="66012202111305"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66013002121501" prefix="J">
<description>&lt;b&gt;WR-MMCX Right Angle
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface  IEC 61169-52 
&lt;br&gt;Connector Type  MMCX 
&lt;br&gt;Gender   Plug 
&lt;br&gt;Orientation Type Right Angle 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;
PACKAGINGPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Qty. 198 
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o150576v209%20Family_WR-MMCX_66013002121501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o150576v209%20Family_WR-MMCX_66013002121501.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/WR-MMCX_66013002121501"&gt;https://katalog.we-online.com/en/em/WR-MMCX_66013002121501&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2019-11-01&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-MMCX_PLUG"/>
</gates>
<devices>
<device name="" package="66013002121501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/66013002121501.pdf"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="INTERFACE" value="IEC 61169-52"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="ORIENTATION-TYPE" value="Right Angle"/>
<attribute name="PART-NUMBER" value="66013002121501"/>
<attribute name="VALUE" value="66013002121501"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66011002111501" prefix="J">
<description>&lt;b&gt;WR-MMCX Right Angle
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface  IEC 61169-52 
&lt;br&gt;Connector Type  MMCX 
&lt;br&gt;Gender  Jack 
&lt;br&gt;Orientation Type Right Angle 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGINGPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Qty. 198 
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o150572v209%20Family_WR-MMCX_66011002111501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o150572v209%20Family_WR-MMCX_66011002111501.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/WR-MMCX_66011002111501"&gt;https://katalog.we-online.com/en/em/WR-MMCX_66011002111501&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2019-11-01&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-MMCX_JACK"/>
</gates>
<devices>
<device name="" package="66011002111501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/66011002111501.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="IEC 61169-52"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="ORIENTATION-TYPE" value="Right Angle"/>
<attribute name="PART-NUMBER" value="66011002111501"/>
<attribute name="VALUE" value="66011002111501"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66012102111404" prefix="J">
<description>&lt;b&gt;WR-MMCX Straight
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface  IEC 61169-52 
&lt;br&gt;Connector Type  MMCX 
&lt;br&gt;Gender  Jack 
&lt;br&gt;Orientation Type  Straight 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;
PACKAGINGPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Qty. 1000
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o150574v209%20Family_WR-MMCX_66012102111404.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o150574v209%20Family_WR-MMCX_66012102111404.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/WR-MMCX_66012102111404"&gt;https://katalog.we-online.com/en/em/WR-MMCX_66012102111404&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2019-11-01&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-MMCX_JACK"/>
</gates>
<devices>
<device name="" package="66012102111404">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/66012102111404.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="IEC 61169-52"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="66012102111404"/>
<attribute name="VALUE" value="66012102111404"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="66012002111503" prefix="J">
<description>&lt;b&gt;WR-MMCX Straight
&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Beryllium Copper 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass  
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;KIND PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Interface  IEC 61169-52 
&lt;br&gt;Connector Type  MMCX 
&lt;br&gt;Gender  Jack 
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;GENERAL INFORMATION&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -55 up to +155 °C 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;ELECTRICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Impedance 50 Ω 
&lt;br&gt;Frequency Range  DC~6 GHz 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;MECHANICAL PROPERTIES&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;
PACKAGINGPROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Qty. 198 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o150573v209%20Family_WR-MMCX_66012002111503.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o150573v209%20Family_WR-MMCX_66012002111503.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/WR-MMCX_66012002111503"&gt;https://katalog.we-online.com/en/em/WR-MMCX_66012002111503&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2019-11-01&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WR-MMCX_JACK"/>
</gates>
<devices>
<device name="" package="66012002111503">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/66012002111503.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="IEC 61169-52"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="66012002111503"/>
<attribute name="VALUE" value="66012002111503"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
