<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Wire-to-Board Connectors - WR-MPC3 &lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-10-13&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="662114230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel),14Pins</description>
</package>
<package name="662106231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 6Pins</description>
</package>
<package name="662024236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs,24 Pins</description>
</package>
<package name="662014236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs, 14 Pins</description>
</package>
<package name="662010235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip,10 Pins</description>
</package>
<package name="662022236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs,22 Pins</description>
</package>
<package name="662014235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip,14 Pins</description>
</package>
<package name="662024235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip,24 Pins</description>
</package>
<package name="662314235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel),14Pins</description>
</package>
<package name="662306235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel),6Pins</description>
</package>
<package name="662104231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 4Pins</description>
</package>
<package name="662314231822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel),14Pins</description>
</package>
<package name="662304235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel),4Pins</description>
</package>
<package name="662006231822">
<description>&lt;B&gt;WR-MPC3&lt;/B&gt;&lt;BR&gt;SMT Male Dual Row Vertical Header with SMT Solder Tab,6 Pins</description>
</package>
<package name="662016231822">
<description>&lt;B&gt;WR-MPC3&lt;/B&gt;&lt;BR&gt;SMT Male Dual Row Vertical Header with SMT Solder Tab,16 Pins</description>
</package>
<package name="662022235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip,22 Pins</description>
</package>
<package name="662012235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip, 12 Pins</description>
</package>
<package name="662108231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 8Pins</description>
</package>
<package name="662010231822">
<description>&lt;B&gt;WR-MPC3&lt;/B&gt;&lt;BR&gt;SMT Male Dual Row Vertical Header with SMT Solder Tab, 10 Pins</description>
</package>
<package name="662102231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 2Pins</description>
</package>
<package name="662004235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip, 4 Pins</description>
</package>
<package name="66200421122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Vertical Header,4 pins</description>
</package>
<package name="662316235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel),16Pins</description>
</package>
<package name="66200821122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Vertical Header,8 pins</description>
</package>
<package name="662018231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab,18 Pins</description>
</package>
<package name="662302235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel),2 Pins</description>
</package>
<package name="662006235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip,6 Pins</description>
</package>
<package name="662014231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab,14 Pins</description>
</package>
<package name="662016235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip,16 Pins</description>
</package>
<package name="662308235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel),8Pins</description>
</package>
<package name="662310235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel),10Pins</description>
</package>
<package name="66200621122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Vertical Header,6 pins</description>
</package>
<package name="662022231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab,22 Pins</description>
</package>
<package name="66201621122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Vertical Header,16 pins</description>
</package>
<package name="662120231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 20 Pins</description>
</package>
<package name="662110231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 10Pins</description>
</package>
<package name="662024231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 24 Pins</description>
</package>
<package name="662116231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 16Pins</description>
</package>
<package name="662002231822">
<description>&lt;B&gt;WR-MPC3&lt;/B&gt;&lt;BR&gt;SMT Male Dual Row Vertical Header with SMT Solder Tab,2 Pins</description>
</package>
<package name="66201821122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Vertical Header,18 pins</description>
</package>
<package name="66201221122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Vertical Header,12 pins</description>
</package>
<package name="662118231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 18 Pins</description>
</package>
<package name="66201021122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Vertical Header,10 pins</description>
</package>
<package name="662124231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 24 Pins</description>
</package>
<package name="662122231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 22Pins</description>
</package>
<package name="662112231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 12Pins</description>
</package>
<package name="662303131822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Single Vertical Header with SMT Solder Tab,3Pins</description>
</package>
<package name="66202421122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Vertical Header,24 pins</description>
</package>
<package name="662305131822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Single Vertical Header with SMT Solder Tab,5Pins</description>
</package>
<package name="662014231822">
<description>&lt;B&gt;WR-MPC3&lt;/B&gt;&lt;BR&gt;SMT Male Dual Row Vertical Header with SMT Solder Tab, 14 Pins</description>
</package>
<package name="662302135922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Single Row Vertical Header with THT Retention Clip, 2Pins</description>
</package>
<package name="662020235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip, 20 Pins</description>
</package>
<package name="66202021122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Vertical Header,20 pins</description>
</package>
<package name="662008235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip, 8 Pins</description>
</package>
<package name="662004231822">
<description>&lt;B&gt;WR-MPC3&lt;/B&gt;&lt;BR&gt;SMT Male Dual Row Vertical Header with SMT Solder Tab,4 Pins</description>
</package>
<package name="66200221122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Vertical Header,2 pins</description>
</package>
<package name="662312235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel),12Pins</description>
</package>
<package name="66201421122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Vertical Header,14 pins</description>
</package>
<package name="662303135922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Single Row Vertical Header with THT Retention Clip,3Pins</description>
</package>
<package name="662302131822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Single Vertical Header with SMT Solder Tab,2Pins</description>
</package>
<package name="66202221122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Vertical Header,22 pins</description>
</package>
<package name="662018231822">
<description>&lt;B&gt;WR-MPC3&lt;/B&gt;&lt;BR&gt;SMT Male Dual Row Vertical Header with SMT Solder Tab,18 Pins</description>
</package>
<package name="66201221022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Angled Header w. Plastic Pegs,12 Pins</description>
</package>
<package name="662114231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 14Pins</description>
</package>
<package name="662306231822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel),6Pins</description>
</package>
<package name="66200221022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Angled Header w. Plastic Pegs,2 Pins</description>
</package>
<package name="66201621022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Angled Header w. Plastic Pegs, 16 Pins</description>
</package>
<package name="662304231822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel),4Pins</description>
</package>
<package name="66200621022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Angled Header w. Plastic Pegs, 6 Pins</description>
</package>
<package name="662324231822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel),24Pins</description>
</package>
<package name="66201821022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Angled Header w. Plastic Pegs, 18 Pins</description>
</package>
<package name="66202421022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Angled Header w. Plastic Pegs,24 Pins</description>
</package>
<package name="662308231822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel),8Pins</description>
</package>
<package name="662002236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs,2 Pins</description>
</package>
<package name="662008236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs, 8 Pins</description>
</package>
<package name="662310231822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel),10Pins</description>
</package>
<package name="662018236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs,18 Pins</description>
</package>
<package name="662004236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs,4 Pins</description>
</package>
<package name="662006236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs, 6 Pins</description>
</package>
<package name="662012231822">
<description>&lt;B&gt;WR-MPC3&lt;/B&gt;&lt;BR&gt;SMT Male Dual Row Vertical Header with SMT Solder Tab, 12 Pins</description>
</package>
<package name="66200421022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Angled Header w. Plastic Pegs,4 Pins</description>
</package>
<package name="662024231822">
<description>&lt;B&gt;WR-MPC3&lt;/B&gt;&lt;BR&gt;SMT Male Dual Row Vertical Header with SMT Solder Tab,24 Pins</description>
</package>
<package name="66201421022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Angled Header w. Plastic Pegs,14 Pins</description>
</package>
<package name="662302231822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel),2Pins</description>
</package>
<package name="66201021022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Angled Header w. Plastic Pegs,10 Pins</description>
</package>
<package name="662012236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs,12 Pins</description>
</package>
<package name="662008231822">
<description>&lt;B&gt;WR-MPC3&lt;/B&gt;&lt;BR&gt;SMT Male Dual Row Vertical Header with SMT Solder Tab,8 Pins</description>
</package>
<package name="662312231822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel),12Pins</description>
</package>
<package name="66200821022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Angled Header w. Plastic Pegs,8 Pins</description>
</package>
<package name="66200211022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Single Row Angled Header w. Plastic Pegs, 2 Pins</description>
</package>
<package name="66202021022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Angled Header w. Plastic Pegs,20 Pins</description>
</package>
<package name="662306131822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Single Vertical Header with SMT Solder Tab,6Pins</description>
</package>
<package name="66202221022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Dual Row Angled Header w. Plastic Pegs,22 Pins</description>
</package>
<package name="66200311122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00mm Male Single Row Vertical Header,  3 Pins</description>
</package>
<package name="662318231822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel),18Pins</description>
</package>
<package name="662018235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip,18 Pins</description>
</package>
<package name="66200611122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00mm Male Single Row Vertical Header,  6 Pins</description>
</package>
<package name="66200211122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00mm Male Single Row Vertical Header, 2 Pins</description>
</package>
<package name="662106236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs (Reel),6Pins</description>
</package>
<package name="66200311022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Single Row Angled Header w. Plastic Pegs,3 Pins</description>
</package>
<package name="662322231822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel),22Pins</description>
</package>
<package name="66200411022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Single Row Angled Header w. Plastic Pegs,4 Pins</description>
</package>
<package name="66200411122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00mm Male Single Row Vertical Header, 4 Pins</description>
</package>
<package name="662320231822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel),20Pins</description>
</package>
<package name="66200511022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Single Row Angled Header w. Plastic Pegs, 5 Pins</description>
</package>
<package name="662116236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs (Reel),16Pins</description>
</package>
<package name="66200511122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00mm Male Single Row Vertical Header, 5 Pins</description>
</package>
<package name="662108236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs (Reel),8Pins</description>
</package>
<package name="662316231822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel),16Pins</description>
</package>
<package name="66200611022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Single Row Angled Header w. Plastic Pegs,6 Pins</description>
</package>
<package name="662110236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs (Reel),10Pins</description>
</package>
<package name="662012230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip, 12 Pins</description>
</package>
<package name="662306135922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Single Row Vertical Header with THT Retention Clip,6Pins</description>
</package>
<package name="662305135922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Single Row Vertical Header with THT Retention Clip,5Pins</description>
</package>
<package name="662304135922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Single Row Vertical Header with THT Retention Clip,4Pins</description>
</package>
<package name="662008230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip, 8 Pins</description>
</package>
<package name="662114236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs (Reel),14Pins</description>
</package>
<package name="662104236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs (Reel),4Pins</description>
</package>
<package name="662020231822">
<description>&lt;B&gt;WR-MPC3&lt;/B&gt;&lt;BR&gt;SMT Male Dual Row Vertical Header with SMT Solder Tab,20 Pins</description>
</package>
<package name="66200711022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Single Row Angled Header w. Plastic Pegs, 7 Pins</description>
</package>
<package name="66200811022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Single Row Angled Header w. Plastic Pegs, 8 Pins</description>
</package>
<package name="66200711122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00mm Male Single Row Vertical Header, 7 Pins</description>
</package>
<package name="66201111122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00mm Male Single Row Vertical Header, 11 Pins</description>
</package>
<package name="66200811122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00mm Male Single Row Vertical Header, 8 Pins</description>
</package>
<package name="662024230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip,  24 Pins</description>
</package>
<package name="662304131822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Single Vertical Header with SMT Solder Tab,4Pins</description>
</package>
<package name="662002235922">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip,2 Pins</description>
</package>
<package name="66201011122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00mm Male Single Row Vertical Header, 10 Pins</description>
</package>
<package name="662006230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip, 6 Pins</description>
</package>
<package name="66200911122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00mm Male Single Row Vertical Header,  9 Pins</description>
</package>
<package name="66200911022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Single Row Angled Header w. Plastic Pegs,9 Pins</description>
</package>
<package name="662102136022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Right Angled Header with Snap-In Plastic Pegs,2Pins</description>
</package>
<package name="662103130822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Right Angled Header with Snap-In Plastic Pegs,3Pins</description>
</package>
<package name="662104145021">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs, 4 Pins</description>
</package>
<package name="66201111022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Single Row Angled Header w. Plastic Pegs, 11 Pins</description>
</package>
<package name="662102145021">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs, 2 Pins</description>
</package>
<package name="66201211122">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00mm Male Single Row Vertical Header, 12 Pins</description>
</package>
<package name="662105130822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Right Angled Header with Snap-In Plastic Pegs,5Pins</description>
</package>
<package name="662105136022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Right Angled Header with Snap-In Plastic Pegs,5Pins</description>
</package>
<package name="662103145021">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs, 3 Pins</description>
</package>
<package name="662102130822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Right Angled Header with Snap-In Plastic Pegs,2Pins</description>
</package>
<package name="662108145021">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs, 8 Pins</description>
</package>
<package name="662106136022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Right Angled Header with Snap-In Plastic Pegs,6Pins</description>
</package>
<package name="662106130822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Right Angled Header with Snap-In Plastic Pegs,6Pins</description>
</package>
<package name="662106145021">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs,  6 Pins</description>
</package>
<package name="662109145021">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs, 9 Pins</description>
</package>
<package name="662105145021">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs,  5 Pins</description>
</package>
<package name="662103136022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Right Angled Header with Snap-In Plastic Pegs,3Pins</description>
</package>
<package name="662107145021">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs, 7 Pins</description>
</package>
<package name="662111145021">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs, 11 Pins</description>
</package>
<package name="662004230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip, 4 Pins</description>
</package>
<package name="66201011022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Single Row Angled Header w. Plastic Pegs,10 Pins</description>
</package>
<package name="662104136022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Right Angled Header with Snap-In Plastic Pegs,4Pins</description>
</package>
<package name="66201211022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm Male Single Row Angled Header w. Plastic Pegs, 12 Pins</description>
</package>
<package name="662104130822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Right Angled Header with Snap-In Plastic Pegs,4Pins</description>
</package>
<package name="662112230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel),12 Pins</description>
</package>
<package name="662010230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip,  10 Pins</description>
</package>
<package name="662018230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip,  18 Pins</description>
</package>
<package name="662112145021">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs, 12 Pins</description>
</package>
<package name="662102230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel),2 Pins</description>
</package>
<package name="662016236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs,16 Pins</description>
</package>
<package name="662112236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs (Reel),12Pins</description>
</package>
<package name="662002230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip, 2 Pins</description>
</package>
<package name="662016230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip,  16 Pins</description>
</package>
<package name="662110145021">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt; 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs,  10 Pins</description>
</package>
<package name="662006231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 6 Pins</description>
</package>
<package name="662016231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 16 Pins</description>
</package>
<package name="662116230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel),16 Pins</description>
</package>
<package name="662022230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip, 22 Pins</description>
</package>
<package name="662010231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 10 Pins</description>
</package>
<package name="662104230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel),4 Pins</description>
</package>
<package name="662002231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab,2 Pins</description>
</package>
<package name="662014230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip, 14 Pins</description>
</package>
<package name="662106230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel),6Pins</description>
</package>
<package name="662012231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab,12 Pins</description>
</package>
<package name="66200411024">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Single Row Right Angled with Plastic Pegs - THT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt; 4 Pins</description>
</package>
<package name="662110230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel),10 Pins</description>
</package>
<package name="66200211024">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Single Row Right Angled with Plastic Pegs - THT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt; 2 Pins</description>
</package>
<package name="66200611024">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Single Row Right Angled with Plastic Pegs - THT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt; 6 Pins</description>
</package>
<package name="662022231822">
<description>&lt;B&gt;WR-MPC3&lt;/B&gt;&lt;BR&gt;SMT Male Dual Row Vertical Header with SMT Solder Tab,22 Pins</description>
</package>
<package name="662004231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 4 Pins</description>
</package>
<package name="66201011024">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Single Row Right Angled with Plastic Pegs - THT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt; 10 Pins</description>
</package>
<package name="66200611124">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical - THT - Selective Gold 
&lt;br&gt;&lt;br&gt;&lt;/b&gt; 6 Pins</description>
</package>
<package name="662102236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs (Reel),2Pins</description>
</package>
<package name="66200211124">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical - THT - Selective Gold 
&lt;br&gt;&lt;br&gt;&lt;/b&gt; 2 Pins</description>
</package>
<package name="662108230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel),8 Pins</description>
</package>
<package name="662010236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs,10 Pins</description>
</package>
<package name="662020230822">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip, 20 Pins</description>
</package>
<package name="66200811024">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Single Row Right Angled with Plastic Pegs - THT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt; 8 Pins</description>
</package>
<package name="662008231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab,8 Pins</description>
</package>
<package name="662020231722">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab, 20 Pins</description>
</package>
<package name="66200411124">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical - THT - Selective Gold 
&lt;br&gt;&lt;br&gt;&lt;/b&gt; 4 Pins</description>
</package>
<package name="66201011124">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical - THT - Selective Gold 
&lt;br&gt;&lt;br&gt;&lt;/b&gt; 10 Pins</description>
</package>
<package name="66200221024">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with Plastic Pegs - THT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;2 Pins</description>
</package>
<package name="662020236022">
<description>&lt;b&gt;WR-MPC3&lt;br&gt;&lt;/b&gt;3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs,20 Pins</description>
</package>
<package name="66200821024">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with Plastic Pegs - THT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;8 Pins</description>
</package>
<package name="66200811124">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical - THT - Selective Gold 
&lt;br&gt;&lt;br&gt;&lt;/b&gt; 8 Pins</description>
</package>
<package name="66200421024">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with Plastic Pegs - THT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;4 Pins</description>
</package>
<package name="66200621124">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Vertical - THT - Selective Gold 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;6 pins</description>
</package>
<package name="66200821124">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Vertical - THT - Selective Gold 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;8 pins</description>
</package>
<package name="66200221124">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Vertical - THT - Selective Gold 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;2 pins</description>
</package>
<package name="66201021024">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with Plastic Pegs - THT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;10 Pins</description>
</package>
<package name="66200621024">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with Plastic Pegs - THT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;6 Pins</description>
</package>
<package name="66200421124">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Vertical - THT - Selective Gold 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;4 pins</description>
</package>
<package name="662002231724">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;2 Pins</description>
</package>
<package name="662002231824">
<description>&lt;B&gt;WR-MPC3 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Selective Gold
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;2 Pins</description>
</package>
<package name="662008231724">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;8 Pins</description>
</package>
<package name="662004231724">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;4 Pins</description>
</package>
<package name="662006231724">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;6 Pins</description>
</package>
<package name="662010231724">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;10 Pins</description>
</package>
<package name="662004231824">
<description>&lt;B&gt;WR-MPC3 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Selective Gold
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;4 Pins</description>
</package>
<package name="66201021124">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Vertical - THT - Selective Gold 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;10 pins</description>
</package>
<package name="662006231824">
<description>&lt;B&gt;WR-MPC3 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Selective Gold
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;6 Pins</description>
</package>
<package name="662104145024">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Single Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;br&gt;&lt;/b&gt;&lt;br&gt; 4 Pins</description>
</package>
<package name="662008231824">
<description>&lt;B&gt;WR-MPC3 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Selective Gold
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;8 Pins</description>
</package>
<package name="662010231824">
<description>&lt;B&gt;WR-MPC3 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Selective Gold
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;10 Pins</description>
</package>
<package name="662110145024">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Single Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;br&gt;&lt;/b&gt;&lt;br&gt; 10 Pins</description>
</package>
<package name="662106145024">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Single Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;br&gt;&lt;/b&gt;&lt;br&gt; 6 Pins</description>
</package>
<package name="662104231724">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt; 4Pins</description>
</package>
<package name="662102145024">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Single Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;br&gt;&lt;/b&gt;&lt;br&gt; 2 Pins</description>
</package>
<package name="662108231724">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt; 8Pins</description>
</package>
<package name="662102231724">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt; 2Pins</description>
</package>
<package name="662108145024">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Single Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;br&gt;&lt;/b&gt;&lt;br&gt; 8 Pins</description>
</package>
<package name="662110231724">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt; 10Pins</description>
</package>
<package name="662106231724">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt; 6Pins</description>
</package>
<package name="662304131824">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical with SMT Solder Tabs - SMT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;4Pins</description>
</package>
<package name="662302131824">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical with SMT Solder Tabs - SMT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;2Pins</description>
</package>
<package name="662306131824">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical with SMT Solder Tabs - SMT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;6Pins</description>
</package>
<package name="662308131824">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical with SMT Solder Tabs - SMT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;8Pins</description>
</package>
<package name="662302231824">
<description>&lt;b&gt;WR-MPC3 WR-MPC3 - 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
2Pins</description>
</package>
<package name="662310131824">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical with SMT Solder Tabs - SMT - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;10Pins</description>
</package>
<package name="662310231824">
<description>&lt;b&gt;WR-MPC3 WR-MPC3 - 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
10Pins</description>
</package>
<package name="662308231824">
<description>&lt;b&gt;WR-MPC3 WR-MPC3 - 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
8Pins</description>
</package>
<package name="662304231824">
<description>&lt;b&gt;WR-MPC3 WR-MPC3 - 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
4Pins</description>
</package>
<package name="662306231824">
<description>&lt;b&gt;WR-MPC3 WR-MPC3 - 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
6Pins</description>
</package>
</packages>
<symbols>
<symbol name="11X2MS_2">
<description>11x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="12X2MS_2">
<description>12x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="5X2MS_2">
<description>5x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="2X2MS_2">
<description>2x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="6X2MS_2">
<description>6x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="8X2MS_2">
<description>8x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="7X2MS_2">
<description>7x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="9X2MS_2">
<description>9x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="8X2MT_2">
<description>8x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="4X2MS_2">
<description>4x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="2X2MT_2">
<description>2x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="1X2MS_2">
<description>1x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3X2MS_2">
<description>3x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="4X2MT_2">
<description>4x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="3X2MT_2">
<description>3x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="10X2MS_2">
<description>10x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="9X2MT_2">
<description>9x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="3MS_1">
<description>3 Pins MALE SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="6X2MT_2">
<description>6x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="5X2MT_2">
<description>5x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="5MS_1">
<description>5 Pins MALE SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="2MS_1">
<description>2Pins MALE SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="1X2MT_2">
<description>1x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="7X2MT_2">
<description>7x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="12X2MT_2">
<description>12x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="10X2MT_2">
<description>10x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="11X2MT_2">
<description>11x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="2MT_1">
<description>2Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3MT">
<description>3Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="6MS_1">
<description>6 Pins MALE SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="2MT">
<description>2Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3MT_1">
<description>3Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="6MT">
<description>6Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="4MT">
<description>4Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="4MT_1">
<description>4Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="5MT">
<description>5Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="5MT_1">
<description>5Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="6MT_1">
<description>6Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="7MT">
<description>7Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="4MS_1">
<description>4 Pins MALE SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="8MT">
<description>8Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="8MT_1">
<description>8Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="7MT_1">
<description>7Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="11MT">
<description>11Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="10MT">
<description>10Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="9MT_1">
<description>9Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="9MT">
<description>9Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="12MT">
<description>12Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="11MT_1">
<description>11Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="8MS_1">
<description>8Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="9MS_1">
<description>9Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="7MS_1">
<description>7Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="10MT_1">
<description>10Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="11MS_1">
<description>11Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="12MT_1">
<description>12Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="12MS_1">
<description>12Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="10MS_1">
<description>10Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="2MT_1-1">
<description>2Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="6MT_1-1">
<description>6Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="4MT_1-1">
<description>4Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="10MT_1-1">
<description>10Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="2MT-1">
<description>2Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="8MT_1-1">
<description>8Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="6MT-1">
<description>6Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="4MT-1">
<description>4Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="10MT-1">
<description>10Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="1X2MT_2-1">
<description>1x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="4X2MT_2-1">
<description>4x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="8MT-1">
<description>8Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="2X2MT_2-1">
<description>2x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="3X2MT_2-1">
<description>3x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="1X2MT_2-2">
<description>1x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="5X2MT_2-1">
<description>5x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="2X2MT_2-2">
<description>2x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="4X2MT_2-2">
<description>4x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="3X2MT_2-2">
<description>3x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="5X2MS_2-1">
<description>5x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="4X2MS_2-1">
<description>4x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="1X2MS_2-1">
<description>1x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="1X2MS_2-2">
<description>1x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="5X2MT_2-2">
<description>5x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="2X2MS_2-1">
<description>2x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="3X2MS_2-1">
<description>3x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="2X2MS_2-2">
<description>2x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="3X2MS_2-2">
<description>3x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="5X2MS_2-2">
<description>5x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="4X2MS_2-2">
<description>4x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="6MS_1-1">
<description>6 Pins MALE SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="10MS_1-1">
<description>10Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="1X2MS_2-3">
<description>1x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="4MS_1-1">
<description>4 Pins MALE SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="2MS_1-1">
<description>2Pins MALE SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="2X2MS_2-3">
<description>2x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="8MS_1-1">
<description>8Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="5X2MS_2-3">
<description>5x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="4X2MS_2-3">
<description>4x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="4MS_1-1-1">
<description>4 Pins MALE SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="6MS_1-1-1">
<description>6 Pins MALE SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="2MS_1-1-1">
<description>2Pins MALE SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3X2MS_2-3">
<description>3x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="10MS_1-2">
<description>10Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="8MS_1-2">
<description>8Pins Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="1X2MS_2-4">
<description>1x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="2X2MS_2-4">
<description>2x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="3X2MS_2-4">
<description>3x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="4X2MS_2-4">
<description>4x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="5X2MS_2-4">
<description>5x2Rows Male SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="6620XX236022_662024236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MS_2"/>
</gates>
<devices>
<device name="" package="662024236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662024236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662024236022"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662024236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX236022_662014236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MS_2"/>
</gates>
<devices>
<device name="" package="662014236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662014236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662014236022"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662014236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX235922_662010235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS_2"/>
</gates>
<devices>
<device name="" package="662010235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662010235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662010235922"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662010235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX236022_662022236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2MS_2"/>
</gates>
<devices>
<device name="" package="662022236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662022236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662022236022"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662022236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX235922_662014235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MS_2"/>
</gates>
<devices>
<device name="" package="662014235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662014235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662014235922"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662014235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX235922_662024235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MS_2"/>
</gates>
<devices>
<device name="" package="662024235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662024235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662024235922"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662024235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX235922_662314235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_REEL_6623XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_REEL_6623XX235922&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MS_2"/>
</gates>
<devices>
<device name="" package="662314235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662314235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662314235922"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662314235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX235922_662306235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_REEL_6623XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_REEL_6623XX235922&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MS_2"/>
</gates>
<devices>
<device name="" package="662306235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662306235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662306235922"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662306235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231722_662104231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MS_2"/>
</gates>
<devices>
<device name="" package="662104231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662104231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662104231722"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662104231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX235922_662304235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_REEL_6623XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_REEL_6623XX235922&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MS_2"/>
</gates>
<devices>
<device name="" package="662304235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662304235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662304235922"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662304235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231822_662006231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)
&lt;br&gt; 2 Pins&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging :Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MS_2"/>
</gates>
<devices>
<device name="" package="662006231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662006231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662006231822"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662006231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231822_662314231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MS_2"/>
</gates>
<devices>
<device name="" package="662314231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662314231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662314231822"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662314231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX235922_662022235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2MS_2"/>
</gates>
<devices>
<device name="" package="662022235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662022235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662022235922"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662022235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231822_662016231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)
&lt;br&gt; 2 Pins&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging :Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MS_2"/>
</gates>
<devices>
<device name="" package="662016231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662016231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662016231822"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662016231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX235922_662012235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MS_2"/>
</gates>
<devices>
<device name="" package="662012235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662012235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662012235922"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662012235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231722_662108231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MS_2"/>
</gates>
<devices>
<device name="" package="662108231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662108231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662108231722"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662108231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231722_662102231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MS_2"/>
</gates>
<devices>
<device name="" package="662102231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662102231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662102231722"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662102231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231822_662010231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)
&lt;br&gt; 2 Pins&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging :Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS_2"/>
</gates>
<devices>
<device name="" package="662010231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662010231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662010231822"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662010231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX235922_662316235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_REEL_6623XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_REEL_6623XX235922&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MS_2"/>
</gates>
<devices>
<device name="" package="662316235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662316235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662316235922"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662316235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX235922_662004235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MS_2"/>
</gates>
<devices>
<device name="" package="662004235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662004235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662004235922"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662004235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21122_66200421122" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_2"/>
</gates>
<devices>
<device name="" package="66200421122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200421122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200421122"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200421122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21122_66200821122" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_2"/>
</gates>
<devices>
<device name="" package="66200821122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200821122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200821122"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200821122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231722_662018231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MS_2"/>
</gates>
<devices>
<device name="" package="662018231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662018231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662018231722"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662018231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX235922_662006235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MS_2"/>
</gates>
<devices>
<device name="" package="662006235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662006235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662006235922"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662006235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX235922_662302235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_REEL_6623XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_REEL_6623XX235922&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MS_2"/>
</gates>
<devices>
<device name="" package="662302235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662302235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662302235922"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662302235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX235922_662016235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MS_2"/>
</gates>
<devices>
<device name="" package="662016235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662016235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662016235922"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662016235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX235922_662308235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_REEL_6623XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_REEL_6623XX235922&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MS_2"/>
</gates>
<devices>
<device name="" package="662308235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662308235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662308235922"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662308235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231722_662014231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MS_2"/>
</gates>
<devices>
<device name="" package="662014231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662014231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662014231722"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662014231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX235922_662310235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_REEL_6623XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_REEL_6623XX235922&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS_2"/>
</gates>
<devices>
<device name="" package="662310235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662310235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662310235922"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662310235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21122_66200621122" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_2"/>
</gates>
<devices>
<device name="" package="66200621122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200621122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200621122"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200621122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231722_662022231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2MS_2"/>
</gates>
<devices>
<device name="" package="662022231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662022231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662022231722"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662022231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21122_66201621122" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_2"/>
</gates>
<devices>
<device name="" package="66201621122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201621122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201621122"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66201621122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231722_662120231722">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MS_2"/>
</gates>
<devices>
<device name="" package="662120231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662120231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662120231722"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662120231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231722_662110231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS_2"/>
</gates>
<devices>
<device name="" package="662110231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662110231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662110231722"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662110231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231822_662002231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)
&lt;br&gt; 2 Pins&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging :Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MS_2"/>
</gates>
<devices>
<device name="" package="662002231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662002231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662002231822"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662002231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21122_66201821122" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MT_2"/>
</gates>
<devices>
<device name="" package="66201821122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201821122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201821122"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66201821122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231722_662116231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MS_2"/>
</gates>
<devices>
<device name="" package="662116231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662116231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662116231722"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662116231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231722_662024231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MS_2"/>
</gates>
<devices>
<device name="" package="662024231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662024231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662024231722"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662024231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21122_66201221122" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_2"/>
</gates>
<devices>
<device name="" package="66201221122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201221122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201221122"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66201221122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231722_662122231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2MS_2"/>
</gates>
<devices>
<device name="" package="662122231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662122231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662122231722"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662122231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21122_66201021122" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_2"/>
</gates>
<devices>
<device name="" package="66201021122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201021122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201021122"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66201021122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231722_662118231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MS_2"/>
</gates>
<devices>
<device name="" package="662118231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662118231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662118231722"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662118231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231722_662112231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MS_2"/>
</gates>
<devices>
<device name="" package="662112231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662112231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662112231722"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662112231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX131822_662305131822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Vertical Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o150745v209%20Family_WR-MPC3_6623xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o150745v209%20Family_WR-MPC3_6623xx131822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_SMT_SOLDER_TAB_6623XX131822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_SMT_SOLDER_TAB_6623XX131822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MS_1"/>
</gates>
<devices>
<device name="" package="662305131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662305131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662305131822"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662305131822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX135922_662302135922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Vertical Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58966v209%20Family_WR-MPC3-6623xx135922_SW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58966v209%20Family_WR-MPC3-6623xx135922_SW.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_THT_RETENTION_CLIP_6623XX135922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_THT_RETENTION_CLIP_6623XX135922&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS_1"/>
</gates>
<devices>
<device name="" package="662302135922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662302135922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662302135922"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662302135922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231722_662124231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MS_2"/>
</gates>
<devices>
<device name="" package="662124231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662124231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662124231722"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662124231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231822_662014231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)
&lt;br&gt; 2 Pins&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging :Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MS_2"/>
</gates>
<devices>
<device name="" package="662014231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662014231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662014231822"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662014231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX131822_662303131822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Vertical Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o150745v209%20Family_WR-MPC3_6623xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o150745v209%20Family_WR-MPC3_6623xx131822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_SMT_SOLDER_TAB_6623XX131822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_SMT_SOLDER_TAB_6623XX131822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MS_1"/>
</gates>
<devices>
<device name="" package="662303131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662303131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662303131822"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662303131822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21122_66202421122" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT_2"/>
</gates>
<devices>
<device name="" package="66202421122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66202421122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66202421122"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66202421122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX235922_662020235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MS_2"/>
</gates>
<devices>
<device name="" package="662020235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662020235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662020235922"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662020235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21122_66202021122" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT_2"/>
</gates>
<devices>
<device name="" package="66202021122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66202021122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66202021122"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66202021122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX235922_662008235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MS_2"/>
</gates>
<devices>
<device name="" package="662008235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662008235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662008235922"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662008235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231822_662004231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)
&lt;br&gt; 2 Pins&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging :Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MS_2"/>
</gates>
<devices>
<device name="" package="662004231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662004231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662004231822"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662004231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21122_66201421122" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_2"/>
</gates>
<devices>
<device name="" package="66201421122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201421122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201421122"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66201421122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX135922_662303135922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Vertical Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58966v209%20Family_WR-MPC3-6623xx135922_SW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58966v209%20Family_WR-MPC3-6623xx135922_SW.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_THT_RETENTION_CLIP_6623XX135922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_THT_RETENTION_CLIP_6623XX135922&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MS_1"/>
</gates>
<devices>
<device name="" package="662303135922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662303135922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662303135922"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662303135922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21122_66200221122" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MT_2"/>
</gates>
<devices>
<device name="" package="66200221122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200221122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200221122"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200221122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX235922_662312235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_REEL_6623XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_REEL_6623XX235922&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MS_2"/>
</gates>
<devices>
<device name="" package="662312235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662312235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662312235922"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662312235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21122_66202221122" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33170v209%20Family_WR-MPC3_6620xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_VERTICAL_HEADER_6620XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2MT_2"/>
</gates>
<devices>
<device name="" package="66202221122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66202221122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66202221122"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66202221122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX131822_662302131822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Vertical Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o150745v209%20Family_WR-MPC3_6623xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o150745v209%20Family_WR-MPC3_6623xx131822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_SMT_SOLDER_TAB_6623XX131822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_SMT_SOLDER_TAB_6623XX131822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS_1"/>
</gates>
<devices>
<device name="" package="662302131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662302131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662302131822"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662302131822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231822_662018231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)
&lt;br&gt; 2 Pins&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging :Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MS_2"/>
</gates>
<devices>
<device name="" package="662018231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662018231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662018231822"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662018231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21022_66201221022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating： Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging ：Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_2"/>
</gates>
<devices>
<device name="" package="66201221022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201221022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201221022"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66201221022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231722_662114231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MS_2"/>
</gates>
<devices>
<device name="" package="662114231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662114231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662114231722"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662114231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231822_662306231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MS_2"/>
</gates>
<devices>
<device name="" package="662306231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662306231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662306231822"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662306231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21022_66200221022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating： Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging ：Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MT_2"/>
</gates>
<devices>
<device name="" package="66200221022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200221022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200221022"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200221022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21022_66200621022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating： Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging ：Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_2"/>
</gates>
<devices>
<device name="" package="66200621022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200621022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200621022"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200621022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21022_66201621022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating： Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging ：Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_2"/>
</gates>
<devices>
<device name="" package="66201621022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201621022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201621022"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66201621022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231822_662304231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MS_2"/>
</gates>
<devices>
<device name="" package="662304231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662304231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662304231822"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662304231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21022_66201821022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating： Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging ：Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MT_2"/>
</gates>
<devices>
<device name="" package="66201821022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201821022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201821022"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66201821022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231822_662324231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MS_2"/>
</gates>
<devices>
<device name="" package="662324231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662324231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662324231822"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662324231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21022_66202421022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating： Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging ：Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT_2"/>
</gates>
<devices>
<device name="" package="66202421022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66202421022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66202421022"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66202421022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231822_662308231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MS_2"/>
</gates>
<devices>
<device name="" package="662308231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662308231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662308231822"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662308231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX236022_662002236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MS_2"/>
</gates>
<devices>
<device name="" package="662002236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662002236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662002236022"/>
<attribute name="PINS" value="2"/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662002236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231822_662310231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS_2"/>
</gates>
<devices>
<device name="" package="662310231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662310231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662310231822"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662310231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX236022_662008236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MS_2"/>
</gates>
<devices>
<device name="" package="662008236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662008236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662008236022"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662008236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX236022_662018236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MS_2"/>
</gates>
<devices>
<device name="" package="662018236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662018236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662018236022"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662018236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231822_662012231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)
&lt;br&gt; 2 Pins&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging :Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MS_2"/>
</gates>
<devices>
<device name="" package="662012231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662012231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662012231822"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662012231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX236022_662004236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MS_2"/>
</gates>
<devices>
<device name="" package="662004236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662004236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662004236022"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662004236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX236022_662006236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MS_2"/>
</gates>
<devices>
<device name="" package="662006236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662006236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662006236022"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662006236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231822_662024231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)
&lt;br&gt; 2 Pins&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging :Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MS_2"/>
</gates>
<devices>
<device name="" package="662024231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662024231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662024231822"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662024231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21022_66201421022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating： Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging ：Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_2"/>
</gates>
<devices>
<device name="" package="66201421022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201421022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201421022"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66201421022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21022_66200421022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating： Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging ：Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_2"/>
</gates>
<devices>
<device name="" package="66200421022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200421022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200421022"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200421022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231822_662302231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MS_2"/>
</gates>
<devices>
<device name="" package="662302231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662302231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662302231822"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662302231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231822_662008231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)
&lt;br&gt; 2 Pins&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging :Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MS_2"/>
</gates>
<devices>
<device name="" package="662008231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662008231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662008231822"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662008231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21022_66201021022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating： Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging ：Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_2"/>
</gates>
<devices>
<device name="" package="66201021022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201021022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201021022"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66201021022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX236022_662012236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MS_2"/>
</gates>
<devices>
<device name="" package="662012236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662012236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662012236022"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662012236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11022_66200211022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Single Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging:Tube 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT_1"/>
</gates>
<devices>
<device name="" package="66200211022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200211022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="66200211022"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200211022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231822_662312231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MS_2"/>
</gates>
<devices>
<device name="" package="662312231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662312231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662312231822"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662312231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21022_66200821022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating： Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging ：Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_2"/>
</gates>
<devices>
<device name="" package="66200821022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200821022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200821022"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200821022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX131822_662306131822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Vertical Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o150745v209%20Family_WR-MPC3_6623xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o150745v209%20Family_WR-MPC3_6623xx131822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_SMT_SOLDER_TAB_6623XX131822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_SMT_SOLDER_TAB_6623XX131822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS_1"/>
</gates>
<devices>
<device name="" package="662306131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662306131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662306131822"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662306131822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21022_66202021022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating： Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging ：Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT_2"/>
</gates>
<devices>
<device name="" package="66202021022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66202021022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66202021022"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66202021022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21022_66202221022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating： Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging ：Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33169v209%20Family_WR-MPC3_6620xx21022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX21022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2MT_2"/>
</gates>
<devices>
<device name="" package="66202221022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66202221022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66202221022"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66202221022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11122_66200311122" prefix="J">
<description>&lt;b&gt;WR-MPC3 Single Row Male Vertical Header&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="66200311122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200311122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200311122"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200311122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231822_662318231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MS_2"/>
</gates>
<devices>
<device name="" package="662318231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662318231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662318231822"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662318231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX235922_662018235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MS_2"/>
</gates>
<devices>
<device name="" package="662018235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662018235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662018235922"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662018235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11022_66200311022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Single Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging:Tube 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT_1"/>
</gates>
<devices>
<device name="" package="66200311022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200311022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="66200311022"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200311022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11122_66200611122" prefix="J">
<description>&lt;b&gt;WR-MPC3 Single Row Male Vertical Header&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT"/>
</gates>
<devices>
<device name="" package="66200611122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200611122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200611122"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200611122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11122_66200211122" prefix="J">
<description>&lt;b&gt;WR-MPC3 Single Row Male Vertical Header&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="66200211122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200211122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200211122"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200211122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX236022_662106236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_REEL_6621XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_REEL_6621XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MS_2"/>
</gates>
<devices>
<device name="" package="662106236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662106236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662106236022"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662106236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231822_662322231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2MS_2"/>
</gates>
<devices>
<device name="" package="662322231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662322231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662322231822"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662322231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11122_66200411122" prefix="J">
<description>&lt;b&gt;WR-MPC3 Single Row Male Vertical Header&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="66200411122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200411122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200411122"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200411122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231822_662320231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MS_2"/>
</gates>
<devices>
<device name="" package="662320231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662320231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662320231822"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662320231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11022_66200411022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Single Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging:Tube 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT_1"/>
</gates>
<devices>
<device name="" package="66200411022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200411022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="66200411022"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200411022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11022_66200511022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Single Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging:Tube 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT_1"/>
</gates>
<devices>
<device name="" package="66200511022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200511022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="66200511022"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200511022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11122_66200511122" prefix="J">
<description>&lt;b&gt;WR-MPC3 Single Row Male Vertical Header&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="66200511122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200511122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200511122"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200511122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX236022_662116236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_REEL_6621XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_REEL_6621XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MS_2"/>
</gates>
<devices>
<device name="" package="662116236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662116236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662116236022"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662116236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX236022_662108236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_REEL_6621XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_REEL_6621XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MS_2"/>
</gates>
<devices>
<device name="" package="662108236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662108236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662108236022"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662108236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231822_662316231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_REEL_6623XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MS_2"/>
</gates>
<devices>
<device name="" package="662316231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662316231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662316231822"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662316231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX230822_662012230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822"&gt;hhttps://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MS_2"/>
</gates>
<devices>
<device name="" package="662012230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662012230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662012230822"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662012230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX236022_662110236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_REEL_6621XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_REEL_6621XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS_2"/>
</gates>
<devices>
<device name="" package="662110236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662110236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662110236022"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662110236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX135922_662304135922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Vertical Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58966v209%20Family_WR-MPC3-6623xx135922_SW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58966v209%20Family_WR-MPC3-6623xx135922_SW.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_THT_RETENTION_CLIP_6623XX135922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_THT_RETENTION_CLIP_6623XX135922&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS_1"/>
</gates>
<devices>
<device name="" package="662304135922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662304135922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662304135922"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662304135922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX135922_662306135922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Vertical Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58966v209%20Family_WR-MPC3-6623xx135922_SW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58966v209%20Family_WR-MPC3-6623xx135922_SW.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_THT_RETENTION_CLIP_6623XX135922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_THT_RETENTION_CLIP_6623XX135922&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS_1"/>
</gates>
<devices>
<device name="" package="662306135922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662306135922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662306135922"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662306135922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11022_66200611022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Single Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging:Tube 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT_1"/>
</gates>
<devices>
<device name="" package="66200611022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200611022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="66200611022"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200611022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX230822_662008230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822"&gt;hhttps://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MS_2"/>
</gates>
<devices>
<device name="" package="662008230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662008230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662008230822"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662008230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX236022_662114236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_REEL_6621XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_REEL_6621XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MS_2"/>
</gates>
<devices>
<device name="" package="662114236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662114236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662114236022"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662114236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX230822_662114230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_REEL_6621XX230822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_REEL_6621XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MS_2"/>
</gates>
<devices>
<device name="" package="662114236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662114230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662114230822"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662114230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX135922_662305135922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Vertical Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o58966v209%20Family_WR-MPC3-6623xx135922_SW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o58966v209%20Family_WR-MPC3-6623xx135922_SW.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_THT_RETENTION_CLIP_6623XX135922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_THT_RETENTION_CLIP_6623XX135922&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MS_1"/>
</gates>
<devices>
<device name="" package="662305135922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662305135922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662305135922"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662305135922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX236022_662104236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_REEL_6621XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_REEL_6621XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MS_2"/>
</gates>
<devices>
<device name="" package="662104236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662104236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662104236022"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662104236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11022_66200711022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Single Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging:Tube 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT_1"/>
</gates>
<devices>
<device name="" package="66200711022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200711022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="66200711022"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200711022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231822_662020231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)
&lt;br&gt; 2 Pins&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging :Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MS_2"/>
</gates>
<devices>
<device name="" package="662020231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662020231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662020231822"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662020231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11122_66201111122" prefix="J">
<description>&lt;b&gt;WR-MPC3 Single Row Male Vertical Header&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11MT"/>
</gates>
<devices>
<device name="" package="66201111122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201111122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201111122"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66201111122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11122_66200811122" prefix="J">
<description>&lt;b&gt;WR-MPC3 Single Row Male Vertical Header&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT"/>
</gates>
<devices>
<device name="" package="66200811122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200811122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200811122"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200811122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11122_66200711122" prefix="J">
<description>&lt;b&gt;WR-MPC3 Single Row Male Vertical Header&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT"/>
</gates>
<devices>
<device name="" package="66200711122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200711122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200711122"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200711122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11022_66200811022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Single Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging:Tube 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT_1"/>
</gates>
<devices>
<device name="" package="66200811022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200811022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="66200811022"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200811022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX230822_662024230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822"&gt;hhttps://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MS_2"/>
</gates>
<devices>
<device name="" package="662024230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662024230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662024230822"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662024230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX131822_662304131822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Vertical Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o150745v209%20Family_WR-MPC3_6623xx131822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o150745v209%20Family_WR-MPC3_6623xx131822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_SMT_SOLDER_TAB_6623XX131822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_VERTICAL_W_SMT_SOLDER_TAB_6623XX131822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS_1"/>
</gates>
<devices>
<device name="" package="662304131822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662304131822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662304131822"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662304131822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX230822_662006230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822"&gt;hhttps://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MS_2"/>
</gates>
<devices>
<device name="" package="662006230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662006230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662006230822"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662006230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX235922_662002235922" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:3 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material:LCP
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:Black
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;Working Voltage:250V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33178v209%20Family_WR-MPC3_662xxx235922.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_THT_RETENTION_CLIP_6620XX235922&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-13
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MS_2"/>
</gates>
<devices>
<device name="" package="662002235922">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662002235922?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662002235922"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662002235922"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11122_66201011122" prefix="J">
<description>&lt;b&gt;WR-MPC3 Single Row Male Vertical Header&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT"/>
</gates>
<devices>
<device name="" package="66201011122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201011122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201011122"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66201011122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11022_66200911022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Single Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging:Tube 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MT_1"/>
</gates>
<devices>
<device name="" package="66200911022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200911022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="66200911022"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200911022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11122_66200911122" prefix="J">
<description>&lt;b&gt;WR-MPC3 Single Row Male Vertical Header&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MT"/>
</gates>
<devices>
<device name="" package="66200911122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200911122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200911122"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200911122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX130822_662103130822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o58957v209%20Family_WRMPC3-6621xx130822_SW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o58957v209%20Family_WRMPC3-6621xx130822_SW.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6621XX130822"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6621XX130822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MS_1"/>
</gates>
<devices>
<device name="" package="662103130822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662103130822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662103130822"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662103130822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX136022_662102136022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Right Angled Header with Snap-In Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o58962v209%20Family_WR-MPC3-6621xx136022_SW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o58962v209%20Family_WR-MPC3-6621xx136022_SW.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_RIGHT_ANGLED_W_PLASTIC_PEGS_6621XX136022"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_RIGHT_ANGLED_W_PLASTIC_PEGS_6621XX136022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS_1"/>
</gates>
<devices>
<device name="" package="662102136022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662102136022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662102136022"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662102136022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX145021_662104145021" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS_1"/>
</gates>
<devices>
<device name="" package="662104145021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662104145021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662104145021"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662104145021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11022_66201111022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Single Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging:Tube 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11MT_1"/>
</gates>
<devices>
<device name="" package="66201111022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201111022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="66201111022"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66201111022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX145021_662102145021" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS_1"/>
</gates>
<devices>
<device name="" package="662102145021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662102145021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662102145021"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662102145021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11122_66201211122" prefix="J">
<description>&lt;b&gt;WR-MPC3 Single Row Male Vertical Header&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33166v209%20Family_WR-MPC3_6620xx11122.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_VERTICAL_HEADER_6620XX11122&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12MT"/>
</gates>
<devices>
<device name="" package="66201211122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201211122?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201211122"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66201211122"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX130822_662105130822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o58957v209%20Family_WRMPC3-6621xx130822_SW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o58957v209%20Family_WRMPC3-6621xx130822_SW.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6621XX130822"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6621XX130822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MS_1"/>
</gates>
<devices>
<device name="" package="662105130822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662105130822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662105130822"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662105130822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX136022_662105136022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Right Angled Header with Snap-In Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o58962v209%20Family_WR-MPC3-6621xx136022_SW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o58962v209%20Family_WR-MPC3-6621xx136022_SW.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_RIGHT_ANGLED_W_PLASTIC_PEGS_6621XX136022"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_RIGHT_ANGLED_W_PLASTIC_PEGS_6621XX136022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MS_1"/>
</gates>
<devices>
<device name="" package="662105136022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662105136022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662105136022"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662105136022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX130822_662102130822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o58957v209%20Family_WRMPC3-6621xx130822_SW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o58957v209%20Family_WRMPC3-6621xx130822_SW.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6621XX130822"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6621XX130822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS_1"/>
</gates>
<devices>
<device name="" package="662102130822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662102130822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662102130822"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662102130822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX145021_662103145021" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MS_1"/>
</gates>
<devices>
<device name="" package="662103145021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662103145021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662103145021"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662103145021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX145021_662108145021" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MS_1"/>
</gates>
<devices>
<device name="" package="662108145021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662108145021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662108145021"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662108145021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX136022_662106136022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Right Angled Header with Snap-In Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o58962v209%20Family_WR-MPC3-6621xx136022_SW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o58962v209%20Family_WR-MPC3-6621xx136022_SW.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_RIGHT_ANGLED_W_PLASTIC_PEGS_6621XX136022"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_RIGHT_ANGLED_W_PLASTIC_PEGS_6621XX136022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS_1"/>
</gates>
<devices>
<device name="" package="662106136022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662106136022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662106136022"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662106136022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX145021_662106145021" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS_1"/>
</gates>
<devices>
<device name="" package="662106145021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662106145021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662106145021"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662106145021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX130822_662106130822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o58957v209%20Family_WRMPC3-6621xx130822_SW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o58957v209%20Family_WRMPC3-6621xx130822_SW.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6621XX130822"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6621XX130822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS_1"/>
</gates>
<devices>
<device name="" package="662106130822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662106130822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662106130822"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662106130822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX145021_662105145021" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MS_1"/>
</gates>
<devices>
<device name="" package="662105145021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662105145021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662105145021"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662105145021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX136022_662103136022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Right Angled Header with Snap-In Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o58962v209%20Family_WR-MPC3-6621xx136022_SW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o58962v209%20Family_WR-MPC3-6621xx136022_SW.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_RIGHT_ANGLED_W_PLASTIC_PEGS_6621XX136022"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_RIGHT_ANGLED_W_PLASTIC_PEGS_6621XX136022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MS_1"/>
</gates>
<devices>
<device name="" package="662103136022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662103136022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662103136022"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662103136022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX145021_662109145021" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9MS_1"/>
</gates>
<devices>
<device name="" package="662109145021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662109145021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662109145021"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662109145021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX145021_662107145021" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MS_1"/>
</gates>
<devices>
<device name="" package="662107145021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662107145021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662107145021"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662107145021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11022_66201011022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Single Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging:Tube 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT_1"/>
</gates>
<devices>
<device name="" package="66201011022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201011022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="66201011022"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66201011022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX145021_662111145021" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11MS_1"/>
</gates>
<devices>
<device name="" package="662111145021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662111145021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662111145021"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662111145021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX230822_662004230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822"&gt;hhttps://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MS_2"/>
</gates>
<devices>
<device name="" package="662004230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662004230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662004230822"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662004230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11022_66201211022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Single Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging:Tube 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33165v209%20Family_WR-MPC3_6620xx11022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX11022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12MT_1"/>
</gates>
<devices>
<device name="" package="66201211022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201211022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="66201211022"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66201211022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX130822_662104130822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o58957v209%20Family_WRMPC3-6621xx130822_SW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o58957v209%20Family_WRMPC3-6621xx130822_SW.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6621XX130822"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_SINGLE_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6621XX130822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS_1"/>
</gates>
<devices>
<device name="" package="662104130822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662104130822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662104130822"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662104130822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX136022_662104136022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Right Angled Header with Snap-In Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o58962v209%20Family_WR-MPC3-6621xx136022_SW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o58962v209%20Family_WR-MPC3-6621xx136022_SW.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_RIGHT_ANGLED_W_PLASTIC_PEGS_6621XX136022"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_SMT_MALE_RIGHT_ANGLED_W_PLASTIC_PEGS_6621XX136022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS_1"/>
</gates>
<devices>
<device name="" package="662104136022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662104136022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662104136022"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662104136022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX230822_662112230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_REEL_6621XX230822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_REEL_6621XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MS_2"/>
</gates>
<devices>
<device name="" package="662112230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662112230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662112230822"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662112230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX230822_662010230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822"&gt;hhttps://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS_2"/>
</gates>
<devices>
<device name="" package="662010230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662010230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662010230822"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662010230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX230822_662018230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822"&gt;hhttps://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MS_2"/>
</gates>
<devices>
<device name="" package="662018230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662018230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662018230822"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662018230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX145021_662112145021" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12MS_1"/>
</gates>
<devices>
<device name="" package="662112145021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662112145021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662112145021"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662112145021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX236022_662016236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MS_2"/>
</gates>
<devices>
<device name="" package="662016236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662016236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662016236022"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662016236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX230822_662102230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_REEL_6621XX230822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_REEL_6621XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MS_2"/>
</gates>
<devices>
<device name="" package="662102230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662102230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662102230822"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662102230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX230822_662002230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822"&gt;hhttps://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MS_2"/>
</gates>
<devices>
<device name="" package="662002230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662002230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662002230822"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662002230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX230822_662016230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822"&gt;hhttps://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MS_2"/>
</gates>
<devices>
<device name="" package="662016230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662016230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662016230822"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662016230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX236022_662112236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_REEL_6621XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_REEL_6621XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MS_2"/>
</gates>
<devices>
<device name="" package="662112236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662112236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662112236022"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662112236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX145021_662110145021" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Single Row Angled Header with SMT Solder Tabs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o33172v209%20Family_WR-MPC3_6621xx145021.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021"&gt;https://katalog.we-online.de/en/em/MPC3_3_00_MALE_SINGLE_ROW_ANGLED_HEADER_6621XX145021&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-15&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MS_1"/>
</gates>
<devices>
<device name="" package="662110145021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662110145021?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662110145021"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662110145021"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231722_662106231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_REEL_6621XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MS_2"/>
</gates>
<devices>
<device name="" package="662006231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662106231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662106231722"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662106231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231722_662006231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MS_2"/>
</gates>
<devices>
<device name="" package="662006231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662006231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662006231722"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662006231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231722_662016231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MS_2"/>
</gates>
<devices>
<device name="" package="662016231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662016231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662016231722"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662016231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX230822_662116230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_REEL_6621XX230822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_REEL_6621XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MS_2"/>
</gates>
<devices>
<device name="" package="662116230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662116230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662116230822"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662116230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX230822_662022230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822"&gt;hhttps://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2MS_2"/>
</gates>
<devices>
<device name="" package="662022230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662022230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662022230822"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662022230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX230822_662104230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_REEL_6621XX230822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_REEL_6621XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MS_2"/>
</gates>
<devices>
<device name="" package="662104230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662104230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662104230822"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662104230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231722_662002231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MS_2"/>
</gates>
<devices>
<device name="" package="662002231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662002231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662002231722"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662002231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231722_662010231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS_2"/>
</gates>
<devices>
<device name="" package="662010231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662010231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662010231722"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662010231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX230822_662014230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822"&gt;hhttps://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MS_2"/>
</gates>
<devices>
<device name="" package="662014230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662014230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662014230822"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662014230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX230822_662106230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_REEL_6621XX230822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_REEL_6621XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MS_2"/>
</gates>
<devices>
<device name="" package="662106230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662106230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662106230822"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662106230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231722_662012231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MS_2"/>
</gates>
<devices>
<device name="" package="662012231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662012231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662012231722"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662012231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX230822_662110230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_REEL_6621XX230822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_REEL_6621XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS_2"/>
</gates>
<devices>
<device name="" package="662110230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662110230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662110230822"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662110230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11024_66200411024" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical - THT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT_1-1"/>
</gates>
<devices>
<device name="" package="66200411024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200411024?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200411024"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200411024"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11024_66200211024" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical - THT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT_1-1"/>
</gates>
<devices>
<device name="" package="66200211024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200211024?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200211024"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200211024"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11024_66200611024" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical - THT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT_1-1"/>
</gates>
<devices>
<device name="" package="66200611024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200611024?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200611024"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200611024"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231822_662022231822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Vertical Header with THT Retention Clip (Reel)
&lt;br&gt; 2 Pins&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging :Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33177v209%20Family_WR-MPC3_662xxx231822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_VERTICAL_HEADER_W_SMT_SOLDER_TAB_6620XX231822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2MS_2"/>
</gates>
<devices>
<device name="" package="662022231822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662022231822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662022231822"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662022231822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231722_662004231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MS_2"/>
</gates>
<devices>
<device name="" package="662004231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662004231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662004231722"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662004231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11024_66201011024" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical - THT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT_1-1"/>
</gates>
<devices>
<device name="" package="66201011024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201011024?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201011024"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66201011024"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11124_66200611124" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical - THT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT-1"/>
</gates>
<devices>
<device name="" package="66200611124">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200611124?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200611124"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200611124"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX230822_662108230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_REEL_6621XX230822"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_REEL_6621XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MS_2"/>
</gates>
<devices>
<device name="" package="662108230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662108230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662108230822"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662108230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11124_66200211124" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical - THT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT-1"/>
</gates>
<devices>
<device name="" package="66200211124">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200211124?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200211124"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200211124"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX236022_662010236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS_2"/>
</gates>
<devices>
<device name="" package="662010236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662010236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662010236022"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662010236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX236022_662102236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs (Reel)&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_REEL_6621XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_REEL_6621XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MS_2"/>
</gates>
<devices>
<device name="" package="662102236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662102236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662102236022"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662102236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX230822_662020230822" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with THT Retention Clip&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33175v209%20Family_WR-MPC3_662xxx230822.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822"&gt;hhttps://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_THT_RETENTION_CLIP_6620XX230822&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MS_2"/>
</gates>
<devices>
<device name="" package="662020230822">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662020230822?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662020230822"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662020230822"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11024_66200811024" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical - THT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT_1-1"/>
</gates>
<devices>
<device name="" package="66200811024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200811024?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200811024"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200811024"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231722_662008231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MS_2"/>
</gates>
<devices>
<device name="" package="662008231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662008231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662008231722"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662008231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11124_66200411124" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical - THT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT-1"/>
</gates>
<devices>
<device name="" package="66200411124">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200411124?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200411124"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200411124"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11124_66201011124" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical - THT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MT-1"/>
</gates>
<devices>
<device name="" package="66201011124">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201011124?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201011124"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66201011124"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231722_662020231722" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header with SMT Solder Tab&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;b&gt;Compliance:RoHS
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33176v209%20Family_WR-MPC3_662xxx231722.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_SMT_SOLDER_TAB_6620XX231722&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-14&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MS_2"/>
</gates>
<devices>
<device name="" package="662020231722">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662020231722?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662020231722"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662020231722"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX236022_662020236022" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm SMT Male Dual Row Angled Header w. Plastic Pegs&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Gender Male 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Tin 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;CERTIFICATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;WIRE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33179v209%20Family_WR-MPC3_662xxx236022.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022"&gt;https://katalog.we-online.com/en/em/MPC3_3_00_SMT_MALE_DUAL_ROW_ANGLED_HEADER_W_PLASTIC_PEGS_6620XX236022&lt;/a&gt;&lt;p&gt;
Created by Yingchun,Shan  2019-11-13&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MS_2"/>
</gates>
<devices>
<device name="" package="662020236022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662020236022?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662020236022"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662020236022"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX11124_66200811124" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical - THT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727040v209%206620xx11122_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_VERTICAL_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT-1"/>
</gates>
<devices>
<device name="" package="66200811124">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200811124?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200811124"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200811124"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21024_66200221024" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with Plastic Pegs - THT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727037v209%206620xx21022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727037v209%206620xx21022_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_PLASTIC_PEGS_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_PLASTIC_PEGS_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MT_2-1"/>
</gates>
<devices>
<device name="" package="66200221024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200221024?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200221024"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200221024"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21024_66200821024" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with Plastic Pegs - THT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727037v209%206620xx21022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727037v209%206620xx21022_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_PLASTIC_PEGS_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_PLASTIC_PEGS_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_2-1"/>
</gates>
<devices>
<device name="" package="66200821024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200821024?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200821024"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200821024"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21024_66200421024" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with Plastic Pegs - THT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727037v209%206620xx21022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727037v209%206620xx21022_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_PLASTIC_PEGS_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_PLASTIC_PEGS_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_2-1"/>
</gates>
<devices>
<device name="" package="66200421024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200421024?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200421024"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200421024"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21124_66200621124" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727035v209%206620xx21122_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727035v209%206620xx21122_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_2-2"/>
</gates>
<devices>
<device name="" package="66200621124">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200621124?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200621124"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200621124"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21124_66200221124" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727035v209%206620xx21122_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727035v209%206620xx21122_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MT_2-2"/>
</gates>
<devices>
<device name="" package="66200221124">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200221124?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200221124"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200221124"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21024_66201021024" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with Plastic Pegs - THT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727037v209%206620xx21022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727037v209%206620xx21022_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_PLASTIC_PEGS_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_PLASTIC_PEGS_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_2-1"/>
</gates>
<devices>
<device name="" package="66201021024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201021024?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201021024"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66201021024"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21024_66200621024" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with Plastic Pegs - THT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727037v209%206620xx21022_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727037v209%206620xx21022_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_PLASTIC_PEGS_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_PLASTIC_PEGS_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_2-1"/>
</gates>
<devices>
<device name="" package="66200621024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200621024?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200621024"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="66200621024"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21124_66200821124" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727035v209%206620xx21122_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727035v209%206620xx21122_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_2-2"/>
</gates>
<devices>
<device name="" package="66200821124">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200821124?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200821124"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200821124"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21124_66200421124" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727035v209%206620xx21122_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727035v209%206620xx21122_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_2-2"/>
</gates>
<devices>
<device name="" package="66200421124">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66200421124?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66200421124"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66200421124"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231724_662002231724" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727029v209%206620xx231722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727029v209%206620xx231722_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MS_2-1"/>
</gates>
<devices>
<device name="" package="662002231724">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662002231724?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662002231724"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662002231724"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231824_662002231824" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Selective Gold 
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726920v209%206620xx231822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726920v209%206620xx231822_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MS_2-2"/>
</gates>
<devices>
<device name="" package="662002231824">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662002231824?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662002231824"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662002231824"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231724_662008231724" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727029v209%206620xx231722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727029v209%206620xx231722_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MS_2-1"/>
</gates>
<devices>
<device name="" package="662008231724">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662008231724?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662008231724"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662008231724"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231724_662004231724" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727029v209%206620xx231722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727029v209%206620xx231722_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MS_2-1"/>
</gates>
<devices>
<device name="" package="662004231724">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662004231724?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662004231724"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662004231724"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231724_662010231724" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727029v209%206620xx231722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727029v209%206620xx231722_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS_2-1"/>
</gates>
<devices>
<device name="" package="662010231724">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662010231724?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662010231724"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662010231724"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231724_662006231724" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727029v209%206620xx231722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727029v209%206620xx231722_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MS_2-1"/>
</gates>
<devices>
<device name="" package="662006231724">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662006231724?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662006231724"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662006231724"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231824_662004231824" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Selective Gold 
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726920v209%206620xx231822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726920v209%206620xx231822_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MS_2-2"/>
</gates>
<devices>
<device name="" package="662004231824">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662004231824?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662004231824"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662004231824"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231824_662006231824" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Selective Gold 
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726920v209%206620xx231822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726920v209%206620xx231822_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MS_2-2"/>
</gates>
<devices>
<device name="" package="662006231824">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662006231824?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662006231824"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662006231824"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX145024_662104145024" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726918v209%206621xx145021_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726918v209%206621xx145021_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS_1-1"/>
</gates>
<devices>
<device name="" package="662104145024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662104145024?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662104145024"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662104145024"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX21124_66201021124" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o727035v209%206620xx21122_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o727035v209%206620xx21122_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_THT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_THT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_2-2"/>
</gates>
<devices>
<device name="" package="66201021124">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/66201021124?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="66201021124"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="66201021124"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX145024_662110145024" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726918v209%206621xx145021_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726918v209%206621xx145021_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MS_1-1"/>
</gates>
<devices>
<device name="" package="662110145024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662110145024?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662110145024"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662110145024"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231824_662008231824" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Selective Gold 
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726920v209%206620xx231822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726920v209%206620xx231822_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MS_2-2"/>
</gates>
<devices>
<device name="" package="662008231824">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662008231824?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662008231824"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662008231824"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6620XX231824_662010231824" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Selective Gold 
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726920v209%206620xx231822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726920v209%206620xx231822_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS_2-2"/>
</gates>
<devices>
<device name="" package="662010231824">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662010231824?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662010231824"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662010231824"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX145024_662106145024" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726918v209%206621xx145021_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726918v209%206621xx145021_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS_1-1"/>
</gates>
<devices>
<device name="" package="662106145024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662106145024?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662106145024"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662106145024"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX145024_662102145024" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726918v209%206621xx145021_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726918v209%206621xx145021_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS_1-1"/>
</gates>
<devices>
<device name="" package="662102145024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662102145024?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662102145024"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662102145024"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231724_662104231724" prefix="J">
<description>&lt;b&gt;WR-MPC3 WR-MPC3 - 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726917v209%206620xx231722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726917v209%206620xx231722_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MS_2-3"/>
</gates>
<devices>
<device name="" package="662104231724">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662104231724?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662104231724"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662104231724"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231724_662108231724" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726917v209%206620xx231722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726917v209%206620xx231722_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MS_2-3"/>
</gates>
<devices>
<device name="" package="662108231724">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662108231724?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662108231724"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662108231724"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX145024_662108145024" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726918v209%206621xx145021_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726918v209%206621xx145021_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MS_1-1"/>
</gates>
<devices>
<device name="" package="662108145024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662108145024?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662108145024"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662108145024"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231724_662102231724" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726917v209%206620xx231722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726917v209%206620xx231722_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MS_2-3"/>
</gates>
<devices>
<device name="" package="662102231724">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662102231724?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662102231724"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662102231724"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231724_662110231724" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726917v209%206620xx231722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726917v209%206620xx231722_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS_2-3"/>
</gates>
<devices>
<device name="" package="662110231724">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662110231724?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662110231724"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662110231724"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6621XX231724_662106231724" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00 mm Male Header Dual Row Right Angled with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Right Angled 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726917v209%206620xx231722_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726917v209%206620xx231722_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MS_2-3"/>
</gates>
<devices>
<device name="" package="662106231724">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662106231724?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662106231724"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="662106231724"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX131824_662302131824" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical with SMT Solder Tabs - SMT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 


&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726810v209%206623xx131822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726810v209%206623xx131822_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MS_1-1-1"/>
</gates>
<devices>
<device name="" package="662302131824">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662302131824?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662302131824"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662302131824"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX131824_662304131824" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical with SMT Solder Tabs - SMT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 


&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726810v209%206623xx131822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726810v209%206623xx131822_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MS_1-1-1"/>
</gates>
<devices>
<device name="" package="662304131824">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662304131824?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662304131824"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662304131824"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX131824_662306131824" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical with SMT Solder Tabs - SMT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 


&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726810v209%206623xx131822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726810v209%206623xx131822_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MS_1-1-1"/>
</gates>
<devices>
<device name="" package="662306131824">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662306131824?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662306131824"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662306131824"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX131824_662308131824" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical with SMT Solder Tabs - SMT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 


&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726810v209%206623xx131822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726810v209%206623xx131822_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MS_1-2"/>
</gates>
<devices>
<device name="" package="662308131824">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662308131824?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662308131824"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662308131824"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231824_662302231824" prefix="J">
<description>&lt;b&gt;WR-MPC3 WR-MPC3 - 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726730v209%206620xx231822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726730v209%206620xx231822_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MS_2-4"/>
</gates>
<devices>
<device name="" package="662302231824">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662302231824?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662302231824"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662302231824"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX131824_662310131824" prefix="J">
<description>&lt;b&gt;WR-MPC3 3.00mm Male Header Single Row Vertical with SMT Solder Tabs - SMT - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Single 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 


&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel with Cap 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726810v209%206623xx131822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726810v209%206623xx131822_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10MS_1-2"/>
</gates>
<devices>
<device name="" package="662310131824">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662310131824?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662310131824"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662310131824"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231824_662308231824" prefix="J">
<description>&lt;b&gt;WR-MPC3 WR-MPC3 - 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726730v209%206620xx231822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726730v209%206620xx231822_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MS_2-4"/>
</gates>
<devices>
<device name="" package="662308231824">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662308231824?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662308231824"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662308231824"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231824_662306231824" prefix="J">
<description>&lt;b&gt;WR-MPC3 WR-MPC3 - 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726730v209%206620xx231822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726730v209%206620xx231822_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MS_2-4"/>
</gates>
<devices>
<device name="" package="662306231824">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662306231824?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662306231824"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662306231824"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231824_662310231824" prefix="J">
<description>&lt;b&gt;WR-MPC3 WR-MPC3 - 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726730v209%206620xx231822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726730v209%206620xx231822_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MS_2-4"/>
</gates>
<devices>
<device name="" package="662310231824">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662310231824?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662310231824"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662310231824"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6623XX231824_662304231824" prefix="J">
<description>&lt;b&gt;WR-MPC3 WR-MPC3 - 3.00 mm Male Header Dual Row Vertical with SMT Solder Tabs - SMT - Reel - Selective Gold
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Pitch 3 mm 
&lt;br&gt;Rows Dual 
&lt;br&gt;Type Vertical 
&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Durability 75 Mating cycles 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Pin Material Copper Alloy 
&lt;br&gt;Pin Plating Selective Gold 
 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 5 A 
&lt;br&gt;Working Voltage 250 V (AC) 
&lt;br&gt;Withstanding Voltage 1500 V (AC) 
&lt;br&gt;Contact Resistance 10 mΩ 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Packaging Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tape and Reel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Certification
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;UL Approval E323964 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o726730v209%206620xx231822_Multi-Parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o726730v209%206620xx231822_Multi-Parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC3_3_00MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SMT_SOLDER_TABS_SMT_REEL_SELECTIVE_GOLD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-10-12&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MS_2-4"/>
</gates>
<devices>
<device name="" package="662304231824">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10Ohm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/662304231824?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="662304231824"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="3mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="662304231824"/>
<attribute name="WORKING-VOLTAGE" value="250V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
