<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Wire-to-Board Connectors - WR-MPC4 &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019b, 2019-11-12&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="64901221122">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header,12 Pins</description>
</package>
<package name="649008227222">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Pegs,8 pins</description>
</package>
<package name="64900229522">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header,2 pins</description>
</package>
<package name="64902221122">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header,22 Pins</description>
</package>
<package name="64901821122">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header,18 Pins</description>
</package>
<package name="64900629522">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header,6 pins</description>
</package>
<package name="649008221732">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header w. Mounting Pegs, 8 Pins</description>
</package>
<package name="64902021122">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header, 20 Pins</description>
</package>
<package name="64900221122">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header, 2 Pins</description>
</package>
<package name="649022221732">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header w. Mounting Pegs,22 Pins</description>
</package>
<package name="649004221732">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header w. Mounting Pegs,4 Pins</description>
</package>
<package name="64901421122">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header,14 Pins</description>
</package>
<package name="649020221732">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header w. Mounting Pegs, 20 Pins</description>
</package>
<package name="649006221732">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header w. Mounting Pegs, 6 Pins</description>
</package>
<package name="64900821122">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header, 8 Pins</description>
</package>
<package name="64901621122">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header,16 Pins</description>
</package>
<package name="649018221732">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header w. Mounting Pegs,18 Pins</description>
</package>
<package name="649002221732">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header w. Mounting Pegs, 2 Pins</description>
</package>
<package name="649012221732">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header w. Mounting Pegs, 12 Pins</description>
</package>
<package name="649006227222">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Pegs,6 pins</description>
</package>
<package name="649016221732">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header w. Mounting Pegs,16 Pins</description>
</package>
<package name="649024221732">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header w. Mounting Pegs, 24 Pins</description>
</package>
<package name="64901021122">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header,  10 Pins</description>
</package>
<package name="649014221732">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header w. Mounting Pegs,14 Pins</description>
</package>
<package name="64900421122">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header,  4 Pins</description>
</package>
<package name="649010221732">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header w. Mounting Pegs,10 Pins</description>
</package>
<package name="649002227222">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Pegs,2 pins</description>
</package>
<package name="649004227222">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Pegs,4 pins</description>
</package>
<package name="649012227222">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Pegs,12 pins</description>
</package>
<package name="649010227222">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Pegs,10 pins</description>
</package>
<package name="64902421122">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header,24 Pins</description>
</package>
<package name="64900429522">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header,4 pins</description>
</package>
<package name="64901629522">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header,16 pins</description>
</package>
<package name="64900621122">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Vertical Header, 6 Pins</description>
</package>
<package name="649014227222">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Pegs,14 pins</description>
</package>
<package name="64900829522">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header,,8 pins</description>
</package>
<package name="64901229522">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header,12 pins</description>
</package>
<package name="64901029522">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header,10 pins</description>
</package>
<package name="649016227222">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Pegs,16 pins</description>
</package>
<package name="64901829522">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header,18 pins</description>
</package>
<package name="64901421022">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention,14 pins</description>
</package>
<package name="64901429522">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header,14 pins</description>
</package>
<package name="649020227222">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Pegs,20 pins</description>
</package>
<package name="64900821022">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention,8 pins</description>
</package>
<package name="649024227222">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Pegs,24 pins</description>
</package>
<package name="64902029522">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header,20 pins</description>
</package>
<package name="64900221022">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention,2 pins</description>
</package>
<package name="64902429522">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header,24 pins</description>
</package>
<package name="64900621022">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention,6 pins</description>
</package>
<package name="64901221022">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention,12 pins</description>
</package>
<package name="649022227222">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Pegs,22 pins</description>
</package>
<package name="64902221022">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention,22 pins</description>
</package>
<package name="64900419522">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Single Row Angled Header,  4 Pins</description>
</package>
<package name="649018227222">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Pegs,18 pins</description>
</package>
<package name="64900319522">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Single Row Angled Header, 3 Pins</description>
</package>
<package name="64901021022">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention,10 pins</description>
</package>
<package name="64900421022">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention,4 pins</description>
</package>
<package name="64901821022">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention,18 pins</description>
</package>
<package name="64902421022">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention,24 pins</description>
</package>
<package name="64900211122">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Single Row Vertical Header,2 Pins</description>
</package>
<package name="64902229522">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header,22 pins</description>
</package>
<package name="649005127222">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Single Row Angled Header w. Mounting Pegs, 5 Pins</description>
</package>
<package name="64900411022">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Single Row Angled Header w. Mounting Flanges for Screw-in Retention, 4 Pins</description>
</package>
<package name="64900211022">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Single Row Angled Header w. Mounting Flanges for Screw-in Retention, 2 Pins</description>
</package>
<package name="64900311022">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Single Row Angled Header w. Mounting Flanges for Screw-in Retention, 3 Pins</description>
</package>
<package name="649005121732">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt; 4.20 mm Male Single Row Vertical Header w. Mounting Pegs, 5 Pins</description>
</package>
<package name="64900511022">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Single Row Angled Header w. Mounting Flanges for Screw-in Retention, 5 Pins</description>
</package>
<package name="64900519522">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Single Row Angled Header, 5 Pins</description>
</package>
<package name="649004121732">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt; 4.20 mm Male Single Row Vertical Header w. Mounting Pegs,  4 Pins</description>
</package>
<package name="649003121732">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt; 4.20 mm Male Single Row Vertical Header w. Mounting Pegs,  3 Pins</description>
</package>
<package name="64901621022">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention,16 pins</description>
</package>
<package name="64900411122">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Single Row Vertical Header,4 Pins</description>
</package>
<package name="64900219522">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Single Row Angled Header,  2 Pins</description>
</package>
<package name="64902021022">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention,20 pins</description>
</package>
<package name="649004127222">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Single Row Angled Header w. Mounting Pegs, 4Pins</description>
</package>
<package name="649002127222">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Single Row Angled Header w. Mounting Pegs,2Pins</description>
</package>
<package name="64900311122">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Single Row Vertical Header,3 Pins</description>
</package>
<package name="649003127222">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Single Row Angled Header w. Mounting Pegs,3Pins</description>
</package>
<package name="64900511122">
<description>&lt;B&gt;WR-MPC4 &lt;/B&gt;&lt;BR&gt;4.20 mm Male Single Row Vertical Header,5 Pins</description>
</package>
</packages>
<symbols>
<symbol name="4X2MT_2">
<description>4X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="1X2MT_2">
<description>1X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="6X2MT_2">
<description>6X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="11X2MT_2">
<description>11X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="10X2MT_2">
<description>10X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="9X2MT_2">
<description>9X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="2X2MT_2">
<description>2X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="3X2MT_2">
<description>3X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="7X2MT_2">
<description>7X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="5X2MT_2">
<description>5X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="8X2MT_2">
<description>8X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="12X2MT_2">
<description>12X2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="4MT_1">
<description>4Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="3MT_1">
<description>3Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="2MT">
<description>2Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="5MT">
<description>5Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="2MT_1">
<description>2Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="5MT_1">
<description>5Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="4MT">
<description>4Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="3MT">
<description>3Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="6490XX21122_64901221122" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin over Nickel
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_2"/>
</gates>
<devices>
<device name="" package="64901221122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64901221122.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="26.4mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64901221122 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX227222_649008227222" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Tin over Nickel
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_2"/>
</gates>
<devices>
<device name="" package="649008227222">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649008227222.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="18mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649008227222"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX29522_64900229522" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MT_2"/>
</gates>
<devices>
<device name="" package="64900229522">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900229522.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="5.4mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900229522 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21122_64902221122" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin over Nickel
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2MT_2"/>
</gates>
<devices>
<device name="" package="64902221122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64902221122.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="47.4mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64902221122 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21122_64901821122" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin over Nickel
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MT_2"/>
</gates>
<devices>
<device name="" package="64901821122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64901821122.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="39mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64901821122 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX29522_64900629522" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_2"/>
</gates>
<devices>
<device name="" package="64900629522">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900629522.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="13.8mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900629522 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21122_64902021122" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin over Nickel
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT_2"/>
</gates>
<devices>
<device name="" package="64902021122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64902021122.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="43.2mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64902021122 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX221732_649008221732" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_2"/>
</gates>
<devices>
<device name="" package="649008221732">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649008221732.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="22mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649008221732"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21122_64900221122" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin over Nickel
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MT_2"/>
</gates>
<devices>
<device name="" package="64900221122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900221122.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="5.4mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="64900221122"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX221732_649004221732" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_2"/>
</gates>
<devices>
<device name="" package="649004221732">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649004221732.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="13.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649004221732"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21122_64901421122" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin over Nickel
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_2"/>
</gates>
<devices>
<device name="" package="64901421122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64901421122.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="30.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64901421122 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX221732_649020221732" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT_2"/>
</gates>
<devices>
<device name="" package="649020221732">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649020221732.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="47.2mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649020221732"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX221732_649006221732" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_2"/>
</gates>
<devices>
<device name="" package="649006221732">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649006221732.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="17.8mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649006221732"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21122_64901621122" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin over Nickel
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_2"/>
</gates>
<devices>
<device name="" package="64901621122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64901621122.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="34.8mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64901621122 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX221732_649018221732" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MT_2"/>
</gates>
<devices>
<device name="" package="649018221732">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649018221732.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="43mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649018221732"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21122_64900821122" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin over Nickel
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_2"/>
</gates>
<devices>
<device name="" package="64900821122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900821122.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="18mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900821122 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX221732_649022221732" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2MT_2"/>
</gates>
<devices>
<device name="" package="649022221732">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649022221732.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="51.4mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649022221732"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX221732_649002221732" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MT_2"/>
</gates>
<devices>
<device name="" package="649002221732">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649002221732.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="9.4mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649002221732"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX221732_649012221732" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_2"/>
</gates>
<devices>
<device name="" package="649012221732">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649012221732.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="30.4mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649012221732"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX227222_649006227222" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Tin over Nickel
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_2"/>
</gates>
<devices>
<device name="" package="649006227222">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649006227222.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="13.8mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649006227222"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX221732_649016221732" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_2"/>
</gates>
<devices>
<device name="" package="649016221732">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649016221732.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="38.8mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649016221732"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21122_64901021122" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin over Nickel
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_2"/>
</gates>
<devices>
<device name="" package="64901021122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64901021122.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="22.2mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64901021122 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX221732_649024221732" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT_2"/>
</gates>
<devices>
<device name="" package="649024221732">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649024221732.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="55.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649024221732"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX221732_649014221732" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_2"/>
</gates>
<devices>
<device name="" package="649014221732">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649014221732.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="34.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649014221732"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21122_64900421122" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin over Nickel
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_2"/>
</gates>
<devices>
<device name="" package="64900421122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900421122.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="9.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900421122 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX221732_649010221732" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33190v209%20Family_WR-MPC4_6490xx221732.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX221732&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_2"/>
</gates>
<devices>
<device name="" package="649010221732">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649010221732.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="26.2mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649010221732"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX227222_649002227222" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Tin over Nickel
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MT_2"/>
</gates>
<devices>
<device name="" package="649002227222">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649002227222.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="5.4mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649002227222"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX227222_649004227222" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Tin over Nickel
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_2"/>
</gates>
<devices>
<device name="" package="649004227222">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649004227222.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="9.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649004227222"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX227222_649012227222" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Tin over Nickel
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_2"/>
</gates>
<devices>
<device name="" package="649012227222">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649012227222.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="26.4mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649012227222"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX227222_649010227222" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Tin over Nickel
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_2"/>
</gates>
<devices>
<device name="" package="649010227222">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649010227222.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="22.2mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649010227222"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21122_64902421122" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin over Nickel
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT_2"/>
</gates>
<devices>
<device name="" package="64902421122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64902421122.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="51.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64902421122 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX29522_64900429522" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_2"/>
</gates>
<devices>
<device name="" package="64900429522">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900429522.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="9.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900429522 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX29522_64901629522" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_2"/>
</gates>
<devices>
<device name="" package="64901629522">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64901629522.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="34.8mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64901629522 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21122_64900621122" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Vertical Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin over Nickel
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33113v209%20Family_WR-MCP4_6490xx21122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_VERTICAL_HEADER_6490XX21122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_2"/>
</gates>
<devices>
<device name="" package="64900621122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900621122.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="13.8mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900621122 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX227222_649014227222" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Tin over Nickel
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_2"/>
</gates>
<devices>
<device name="" package="649014227222">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649014227222.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="30.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649014227222"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX29522_64901029522" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_2"/>
</gates>
<devices>
<device name="" package="64901029522">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64901029522.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="22.2mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64901029522 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX29522_64901229522" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_2"/>
</gates>
<devices>
<device name="" package="64901229522">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64901229522.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="26.4mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64901229522 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX29522_64900829522" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_2"/>
</gates>
<devices>
<device name="" package="64900829522">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900829522.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="18mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900829522 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX227222_649016227222" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Tin over Nickel
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_2"/>
</gates>
<devices>
<device name="" package="649016227222">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649016227222.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="34.8mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649016227222"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX29522_64901829522" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MT_2"/>
</gates>
<devices>
<device name="" package="64901829522">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64901829522.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="39mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64901829522 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21022_64901421022" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_2"/>
</gates>
<devices>
<device name="" package="64901421022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64901421022.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="40.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64901421022 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX29522_64901429522" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_2"/>
</gates>
<devices>
<device name="" package="64901429522">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64901429522.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="30.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64901429522 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX227222_649020227222" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Tin over Nickel
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT_2"/>
</gates>
<devices>
<device name="" package="649020227222">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649020227222.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="43.2mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649020227222"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21022_64900821022" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_2"/>
</gates>
<devices>
<device name="" package="64900821022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900821022.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="28mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900821022 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX227222_649024227222" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Tin over Nickel
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT_2"/>
</gates>
<devices>
<device name="" package="649024227222">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649024227222.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="51.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649024227222"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX29522_64902029522" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT_2"/>
</gates>
<devices>
<device name="" package="64902029522">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64902029522.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="43.2mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64902029522 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21022_64900221022" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MT_2"/>
</gates>
<devices>
<device name="" package="64900221022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900221022.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="15.4mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900221022 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21022_64900621022" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_2"/>
</gates>
<devices>
<device name="" package="64900621022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900621022.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="23.8mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900621022 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX29522_64902429522" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT_2"/>
</gates>
<devices>
<device name="" package="64902429522">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64902429522.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="51.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64902429522 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21022_64901221022" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_2"/>
</gates>
<devices>
<device name="" package="64901221022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64901221022.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="36.4mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64901221022 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX227222_649022227222" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Tin over Nickel
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2MT_2"/>
</gates>
<devices>
<device name="" package="649022227222">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649022227222.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="47.4mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649022227222"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21022_64902221022" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2MT_2"/>
</gates>
<devices>
<device name="" package="64902221022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64902221022.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="57.4mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64902221022 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX19522_64900419522" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Single Row Angled Header
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33184v209%20Family_WR-MPC4_64900x19522.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33184v209%20Family_WR-MPC4_64900x19522.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_6490XX19522"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_6490XX19522&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT_1"/>
</gates>
<devices>
<device name="" package="64900419522">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900419522.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="18mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900419522 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX227222_649018227222" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Tin over Nickel
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33191v209%20Family_WR-MPC4_6490xx227222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX227222&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MT_2"/>
</gates>
<devices>
<device name="" package="649018227222">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649018227222.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="39mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649018227222"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX19522_64900319522" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Single Row Angled Header
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33184v209%20Family_WR-MPC4_64900x19522.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33184v209%20Family_WR-MPC4_64900x19522.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_6490XX19522"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_6490XX19522&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT_1"/>
</gates>
<devices>
<device name="" package="64900319522">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900319522.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="13.8mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900319522 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21022_64901021022" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_2"/>
</gates>
<devices>
<device name="" package="64901021022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64901021022.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="32.2mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64901021022 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21022_64901821022" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2MT_2"/>
</gates>
<devices>
<device name="" package="64901821022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64901821022.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="49mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64901821022 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21022_64900421022" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_2"/>
</gates>
<devices>
<device name="" package="64900421022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900421022.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="19.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900421022 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21022_64902421022" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2MT_2"/>
</gates>
<devices>
<device name="" package="64902421022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64902421022.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="61.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64902421022 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX11122_64900211122" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR- MPC4 4.20 mm Male Single Row Vertical Header
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33185v209%20Family_WR-MPC4_6490xx11122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33185v209%20Family_WR-MPC4_6490xx11122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_VERTICAL_HEADER_6490XX11122"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_VERTICAL_HEADER_6490XX11122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="64900211122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900211122.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="9.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="64900211122"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX29522_64902229522" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33114v209%20Family_WR-MCP4_6490xx29522.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_6490XX29522&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2MT_2"/>
</gates>
<devices>
<device name="" package="64902229522">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64902229522.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="47.4mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64902229522 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX127222_649005127222" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Single Row Angled Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33183v209%20Family_WR-MPC4_64900x127222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33183v209%20Family_WR-MPC4_64900x127222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX127222"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX127222&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="649005127222">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649005127222.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="22.2mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649005127222"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX11022_64900311022" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Single Row Angled Header w. Mounting Flanges for Screw-in Retention&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33181v209%20Family_WR-MPC4_64900x11022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33181v209%20Family_WR-MPC4_64900x11022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX11022"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX11022&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT_1"/>
</gates>
<devices>
<device name="" package="64900311022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900311022.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="23.8mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900311022 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX11022_64900411022" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Single Row Angled Header w. Mounting Flanges for Screw-in Retention&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33181v209%20Family_WR-MPC4_64900x11022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33181v209%20Family_WR-MPC4_64900x11022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX11022"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX11022&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT_1"/>
</gates>
<devices>
<device name="" package="64900411022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900411022.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="28mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900411022 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX11022_64900211022" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Single Row Angled Header w. Mounting Flanges for Screw-in Retention&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33181v209%20Family_WR-MPC4_64900x11022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33181v209%20Family_WR-MPC4_64900x11022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX11022"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX11022&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT_1"/>
</gates>
<devices>
<device name="" package="64900211022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900211022.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="19.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="64900211022"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX121732_649005121732" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Single Row Vertical Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33186v209%20Family_WR-MPC4_6490xx121732.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33186v209%20Family_WR-MPC4_6490xx121732.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX121732"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX121732&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="649005121732">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649005121732.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="22.2mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649005121732"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX11022_64900511022" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Single Row Angled Header w. Mounting Flanges for Screw-in Retention&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33181v209%20Family_WR-MPC4_64900x11022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33181v209%20Family_WR-MPC4_64900x11022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX11022"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX11022&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT_1"/>
</gates>
<devices>
<device name="" package="64900511022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900511022.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="32.2mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900511022 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX121732_649004121732" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Single Row Vertical Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33186v209%20Family_WR-MPC4_6490xx121732.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33186v209%20Family_WR-MPC4_6490xx121732.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX121732"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX121732&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="649004121732">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649004121732.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="18mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649004121732"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21022_64901621022" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_2"/>
</gates>
<devices>
<device name="" package="64901621022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64901621022.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="44.8mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64901621022 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX19522_64900519522" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Single Row Angled Header
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33184v209%20Family_WR-MPC4_64900x19522.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33184v209%20Family_WR-MPC4_64900x19522.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_6490XX19522"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_6490XX19522&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT_1"/>
</gates>
<devices>
<device name="" package="64900519522">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900519522.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="22.2mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900519522 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX121732_649003121732" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Single Row Vertical Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33186v209%20Family_WR-MPC4_6490xx121732.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33186v209%20Family_WR-MPC4_6490xx121732.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX121732"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_VERTICAL_HEADER_W_MOUNTING_PEGS_6490XX121732&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="649003121732">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649003121732.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="13.8mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649003121732"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX11122_64900411122" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR- MPC4 4.20 mm Male Single Row Vertical Header
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33185v209%20Family_WR-MPC4_6490xx11122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33185v209%20Family_WR-MPC4_6490xx11122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_VERTICAL_HEADER_6490XX11122"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_VERTICAL_HEADER_6490XX11122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="64900411122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900411122.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="18mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900411122 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX19522_64900219522" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Single Row Angled Header
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33184v209%20Family_WR-MPC4_64900x19522.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33184v209%20Family_WR-MPC4_64900x19522.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_6490XX19522"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_6490XX19522&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT_1"/>
</gates>
<devices>
<device name="" package="64900219522">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900219522.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="9.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="64900219522"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX21022_64902021022" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Dual Row Angled Header w. Mounting Flanges for Screw-in Retention
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33189v209%20Family_WR-MPC4_6490xx21022.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_DUAL_ROW_ANGLED_HEADER_W_MOUNTING_FLANGES_6490XX21022&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2MT_2"/>
</gates>
<devices>
<device name="" package="64902021022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64902021022.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="53.2mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Dual Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64902021022 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX127222_649004127222" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Single Row Angled Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33183v209%20Family_WR-MPC4_64900x127222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33183v209%20Family_WR-MPC4_64900x127222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX127222"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX127222&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="649004127222">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649004127222.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="18mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649004127222"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX127222_649002127222" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Single Row Angled Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33183v209%20Family_WR-MPC4_64900x127222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33183v209%20Family_WR-MPC4_64900x127222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX127222"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX127222&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="649002127222">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649002127222.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="9.6mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649002127222"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX11122_64900311122" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR- MPC4 4.20 mm Male Single Row Vertical Header
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33185v209%20Family_WR-MPC4_6490xx11122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33185v209%20Family_WR-MPC4_6490xx11122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_VERTICAL_HEADER_6490XX11122"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_VERTICAL_HEADER_6490XX11122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="64900311122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900311122.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="13.8mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900311122 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX127222_649003127222" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-MPC4 4.20 mm Male Single Row Angled Header w. Mounting Pegs&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33183v209%20Family_WR-MPC4_64900x127222.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33183v209%20Family_WR-MPC4_64900x127222.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX127222"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_ANGLED_HEADER_W_MOUNTING_PEGS_6490XX127222&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="649003127222">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/649003127222.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="13.8mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="649003127222"/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6490XX11122_64900511122" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR- MPC4 4.20 mm Male Single Row Vertical Header
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch:4.2 mm
&lt;BR&gt;Gender:Male
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA66
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Insulator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Tin
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Working Voltage:600V (AC)
&lt;BR&gt;Withstanding Voltage:1500 V (AC)
&lt;BR&gt;Contact Resistance:10 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33185v209%20Family_WR-MPC4_6490xx11122.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33185v209%20Family_WR-MPC4_6490xx11122.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_VERTICAL_HEADER_6490XX11122"&gt;https://katalog.we-online.com/en/em/MPC4_4_20_MALE_SINGLE_ROW_VERTICAL_HEADER_6490XX11122&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-11-12
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="64900511122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/64900511122.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="L" value="22.2mm"/>
<attribute name="MATE-WITH" value="WR-MPC4 4.20 mm Female Single Row Plug"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 64900511122 "/>
<attribute name="PCB-CABLE-PANEL" value="PCB"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="4.2mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TOL-R" value="max."/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE" value="600V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
