<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Wire-to-Board Connectors - WR-MPC5&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-10-09&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="657005130101">
<description>&lt;B&gt;WR-MPC5 THT Single Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="657010230201">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Vertical
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 10pins</description>
</package>
<package name="657002230201">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Vertical
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 2pins</description>
</package>
<package name="657004130201">
<description>&lt;B&gt;WR-MPC5 Single Row Male Header Vertical
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="657003130101">
<description>&lt;B&gt;WR-MPC5 THT Single Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 3pins</description>
</package>
<package name="657007130101">
<description>&lt;B&gt;WR-MPC5 THT Single Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 7pins</description>
</package>
<package name="657002140201">
<description>&lt;B&gt;WR-MPC5 Single Row Male Header Vertical with Pegs
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 2pins</description>
</package>
<package name="657002130101">
<description>&lt;B&gt;WR-MPC5 THT Single Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 2pins</description>
</package>
<package name="657004130101">
<description>&lt;B&gt;WR-MPC5 THT Single Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="657007130201">
<description>&lt;B&gt;WR-MPC5 Single Row Male Header Vertical
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 7pins</description>
</package>
<package name="657006140101">
<description>&lt;B&gt;WR-MPC5 THT Single Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 6pins</description>
</package>
<package name="657010230101">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="657008130201">
<description>&lt;B&gt;WR-MPC5 Single Row Male Header Vertical
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="657006130201">
<description>&lt;B&gt;WR-MPC5 Single Row Male Header Vertical
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 6pins</description>
</package>
<package name="657006130101">
<description>&lt;B&gt;WR-MPC5 THT Single Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 6pins</description>
</package>
<package name="657012230201">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Vertical
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 12pins</description>
</package>
<package name="657006230101">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 6pins</description>
</package>
<package name="657003130201">
<description>&lt;B&gt;WR-MPC5 Single Row Male Header Vertical
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 3pins</description>
</package>
<package name="657008230201">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Vertical
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="657005130201">
<description>&lt;B&gt;WR-MPC5 Single Row Male Header Vertical
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="657005140201">
<description>&lt;B&gt;WR-MPC5 Single Row Male Header Vertical with Pegs
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="657004230101">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="657004140201">
<description>&lt;B&gt;WR-MPC5 Single Row Male Header Vertical with Pegs
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="657008130101">
<description>&lt;B&gt;WR-MPC5 THT Single Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="657007140201">
<description>&lt;B&gt;WR-MPC5 Single Row Male Header Vertical with Pegs
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 7pins</description>
</package>
<package name="657002140101">
<description>&lt;B&gt;WR-MPC5 THT Single Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 2pins</description>
</package>
<package name="657007140101">
<description>&lt;B&gt;WR-MPC5 THT Single Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 7pins</description>
</package>
<package name="657012230101">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 12pins</description>
</package>
<package name="657004230201">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Vertical
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="657004140101">
<description>&lt;B&gt;WR-MPC5 THT Single Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="657002230101">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 2pins</description>
</package>
<package name="657008240201">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Vertical with Pegs
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="657006240101">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 6pins</description>
</package>
<package name="657005140101">
<description>&lt;B&gt;WR-MPC5 THT Single Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 5pins</description>
</package>
<package name="657002130201">
<description>&lt;B&gt;WR-MPC5 Single Row Male Header Vertical
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 2pins</description>
</package>
<package name="657006140201">
<description>&lt;B&gt;WR-MPC5 Single Row Male Header Vertical with Pegs
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 6pins</description>
</package>
<package name="657006230201">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Vertical
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 6pins</description>
</package>
<package name="657004240101">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="657010240101">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="657003140201">
<description>&lt;B&gt;WR-MPC5 Single Row Male Header Vertical with Pegs
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 3pins</description>
</package>
<package name="657008140201">
<description>&lt;B&gt;WR-MPC5 Single Row Male Header Vertical with Pegs
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="657010240201">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Vertical with Pegs
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 10pins</description>
</package>
<package name="657004240201">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Vertical with Pegs
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="657003140101">
<description>&lt;B&gt;WR-MPC5 THT Single Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 3pins</description>
</package>
<package name="657012240101">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 12pins</description>
</package>
<package name="657008230101">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="657002240201">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Vertical with Pegs
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 2pins</description>
</package>
<package name="657008240101">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
<package name="657012240201">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Vertical with Pegs
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 12pins</description>
</package>
<package name="657006240201">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Vertical with Pegs
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 6pins</description>
</package>
<package name="657002240101">
<description>&lt;B&gt;WR-MPC5 THT Dual Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 2pins</description>
</package>
<package name="657008140101">
<description>&lt;B&gt;WR-MPC5 THT Single Row Male Header Right Angled
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 8pins</description>
</package>
</packages>
<symbols>
<symbol name="5X2MT">
<description>5x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="5MT">
<description>5Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="3MT">
<description>3Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="2MT">
<description>2Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="7MT">
<description>7Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="4MT">
<description>4Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="1X2MT">
<description>1x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="8MT">
<description>8Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="6MT">
<description>6Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="3X2MT">
<description>3x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="6X2MT">
<description>6x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="2X2MT">
<description>2x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="4X2MT">
<description>4x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="6570XX230201_657010230201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Vertical &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731514v209%20WR-MPC5_6570xx230201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731514v209%20WR-MPC5_6570xx230201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="657010230201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657010230201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657010230201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="10"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657010230201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX130101_657005130101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Right Angled &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731506v209%20WR-MPC5_6570xx130101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731506v209%20WR-MPC5_6570xx130101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="657005130101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657005130101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657005130101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="5"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657005130101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX130201_657004130201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Vertical &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731532v209%20WR-MPC5_6570xx130201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731532v209%20WR-MPC5_6570xx130201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="657004130201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657004130201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657004130201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="4"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657004130201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX230201_657002230201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Vertical &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731514v209%20WR-MPC5_6570xx230201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731514v209%20WR-MPC5_6570xx230201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MT"/>
</gates>
<devices>
<device name="" package="657002230201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657002230201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657002230201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="2"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657002230201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX130101_657003130101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Right Angled &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731506v209%20WR-MPC5_6570xx130101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731506v209%20WR-MPC5_6570xx130101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="657003130101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657003130101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657003130101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="3"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657003130101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX140201_657002140201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Vertical with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731519v209%20WR-MPC5_6570xx140201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731519v209%20WR-MPC5_6570xx140201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="657002140201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657002140201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657002140201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="2"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657002140201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX130101_657007130101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Right Angled &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731506v209%20WR-MPC5_6570xx130101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731506v209%20WR-MPC5_6570xx130101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT"/>
</gates>
<devices>
<device name="" package="657007130101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657007130101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657007130101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="7"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657007130101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX130101_657002130101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Right Angled &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731506v209%20WR-MPC5_6570xx130101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731506v209%20WR-MPC5_6570xx130101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="657002130101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657002130101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657002130101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="2"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657002130101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX130101_657004130101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Right Angled &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731506v209%20WR-MPC5_6570xx130101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731506v209%20WR-MPC5_6570xx130101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="657004130101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657004130101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657004130101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="4"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657004130101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX130201_657007130201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Vertical &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731532v209%20WR-MPC5_6570xx130201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731532v209%20WR-MPC5_6570xx130201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT"/>
</gates>
<devices>
<device name="" package="657007130201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657007130201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657007130201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="7"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657007130201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX140101_657006140101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Right Angled with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Right Angled
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731536v209%20WR-MPC5_6570xx140101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731536v209%20WR-MPC5_6570xx140101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT"/>
</gates>
<devices>
<device name="" package="657006140101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657006140101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657006140101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="6"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657006140101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX230101_657010230101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Right Angled &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731517v209%20WR-MPC5_6570xx230101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731517v209%20WR-MPC5_6570xx230101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="657010230101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657010230101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657010230101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="10"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657010230101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX130201_657008130201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Vertical &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731532v209%20WR-MPC5_6570xx130201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731532v209%20WR-MPC5_6570xx130201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT"/>
</gates>
<devices>
<device name="" package="657008130201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657008130201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657008130201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="8"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657008130201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX230201_657012230201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Vertical &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731514v209%20WR-MPC5_6570xx230201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731514v209%20WR-MPC5_6570xx230201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="657012230201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657012230201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657012230201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="12"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657012230201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX130101_657006130101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Right Angled &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731506v209%20WR-MPC5_6570xx130101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731506v209%20WR-MPC5_6570xx130101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT"/>
</gates>
<devices>
<device name="" package="657006130101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657006130101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657006130101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="6"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657006130101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX230101_657006230101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Right Angled &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731517v209%20WR-MPC5_6570xx230101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731517v209%20WR-MPC5_6570xx230101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="657006230101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657006230101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657006230101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="6"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657006230101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX130201_657006130201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Vertical &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731532v209%20WR-MPC5_6570xx130201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731532v209%20WR-MPC5_6570xx130201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT"/>
</gates>
<devices>
<device name="" package="657006130201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657006130201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657006130201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="6"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657006130201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX130201_657003130201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Vertical &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731532v209%20WR-MPC5_6570xx130201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731532v209%20WR-MPC5_6570xx130201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="657003130201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657003130201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657003130201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="3"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657003130201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX230201_657008230201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Vertical &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731514v209%20WR-MPC5_6570xx230201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731514v209%20WR-MPC5_6570xx230201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="657008230201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657008230201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657008230201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="8"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657008230201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX130201_657005130201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Vertical &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731532v209%20WR-MPC5_6570xx130201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731532v209%20WR-MPC5_6570xx130201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="657005130201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657005130201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657005130201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="5"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657005130201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX140201_657004140201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Vertical with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731519v209%20WR-MPC5_6570xx140201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731519v209%20WR-MPC5_6570xx140201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="657004140201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657004140201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657004140201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="4"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657004140201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX140201_657005140201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Vertical with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731519v209%20WR-MPC5_6570xx140201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731519v209%20WR-MPC5_6570xx140201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="657005140201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657005140201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657005140201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="5"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657005140201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX230101_657004230101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Right Angled &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731517v209%20WR-MPC5_6570xx230101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731517v209%20WR-MPC5_6570xx230101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT"/>
</gates>
<devices>
<device name="" package="657004230101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657004230101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657004230101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="4"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657004230101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX130101_657008130101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Right Angled &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731506v209%20WR-MPC5_6570xx130101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731506v209%20WR-MPC5_6570xx130101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR-MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR-MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT"/>
</gates>
<devices>
<device name="" package="657008130101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657008130101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657008130101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="8"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657008130101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX140201_657007140201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Vertical with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731519v209%20WR-MPC5_6570xx140201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731519v209%20WR-MPC5_6570xx140201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT"/>
</gates>
<devices>
<device name="" package="657007140201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657007140201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657007140201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="7"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657007140201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX140101_657002140101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Right Angled with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Right Angled
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731536v209%20WR-MPC5_6570xx140101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731536v209%20WR-MPC5_6570xx140101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="657002140101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657002140101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657002140101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="2"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657002140101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX140101_657007140101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Right Angled with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Right Angled
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731536v209%20WR-MPC5_6570xx140101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731536v209%20WR-MPC5_6570xx140101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT"/>
</gates>
<devices>
<device name="" package="657007140101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657007140101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657007140101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="7"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657007140101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX230201_657004230201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Vertical &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731514v209%20WR-MPC5_6570xx230201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731514v209%20WR-MPC5_6570xx230201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT"/>
</gates>
<devices>
<device name="" package="657004230201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657004230201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657004230201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="4"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657004230201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX230101_657002230101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Right Angled &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731517v209%20WR-MPC5_6570xx230101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731517v209%20WR-MPC5_6570xx230101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MT"/>
</gates>
<devices>
<device name="" package="657002230101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657002230101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657002230101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="2"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657002230101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX230101_657012230101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Right Angled &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731517v209%20WR-MPC5_6570xx230101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731517v209%20WR-MPC5_6570xx230101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="657012230101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657012230101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657012230101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="12"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657012230101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX240101_657006240101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Right Angled with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731507v209%20WR-MPC5_6570xx240101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731507v209%20WR-MPC5_6570xx240101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="657006240101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657006240101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657006240101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="6"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657006240101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX140101_657004140101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Right Angled with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Right Angled
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731536v209%20WR-MPC5_6570xx140101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731536v209%20WR-MPC5_6570xx140101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="657004140101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657004140101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657004140101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="4"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657004140101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX140101_657005140101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Right Angled with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Right Angled
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731536v209%20WR-MPC5_6570xx140101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731536v209%20WR-MPC5_6570xx140101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="657005140101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657005140101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657005140101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="5"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657005140101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX130201_657002130201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Vertical &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731532v209%20WR-MPC5_6570xx130201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731532v209%20WR-MPC5_6570xx130201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="657002130201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657002130201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657002130201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="2"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657002130201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX240201_657008240201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Vertical with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731511v209%20WR-MPC5_6570xx240201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731511v209%20WR-MPC5_6570xx240201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="657008240201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657008240201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657008240201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="8"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657008240201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX230201_657006230201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Vertical &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731514v209%20WR-MPC5_6570xx230201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731514v209%20WR-MPC5_6570xx230201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="657006230201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657006230201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657006230201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="6"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657006230201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX240101_657004240101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Right Angled with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731507v209%20WR-MPC5_6570xx240101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731507v209%20WR-MPC5_6570xx240101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT"/>
</gates>
<devices>
<device name="" package="657004240101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657004240101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657004240101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="4"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657004240101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX240101_657010240101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Right Angled with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731507v209%20WR-MPC5_6570xx240101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731507v209%20WR-MPC5_6570xx240101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="657010240101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657010240101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657010240101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="10"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657010240101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX140201_657003140201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Vertical with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731519v209%20WR-MPC5_6570xx140201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731519v209%20WR-MPC5_6570xx140201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="657003140201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657003140201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657003140201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="3"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657003140201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX240201_657010240201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Vertical with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731511v209%20WR-MPC5_6570xx240201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731511v209%20WR-MPC5_6570xx240201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT"/>
</gates>
<devices>
<device name="" package="657010240201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657010240201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657010240201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="10"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657010240201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX240101_657012240101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Right Angled with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731507v209%20WR-MPC5_6570xx240101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731507v209%20WR-MPC5_6570xx240101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="657012240101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657012240101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657012240101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="12"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657012240101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX140201_657008140201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Vertical with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731519v209%20WR-MPC5_6570xx140201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731519v209%20WR-MPC5_6570xx140201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT"/>
</gates>
<devices>
<device name="" package="657008140201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657008140201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657008140201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="8"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657008140201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX140101_657003140101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Right Angled with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Right Angled
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731536v209%20WR-MPC5_6570xx140101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731536v209%20WR-MPC5_6570xx140101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="657003140101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657003140101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657003140101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="3"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657003140101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX140201_657006140201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Vertical with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731519v209%20WR-MPC5_6570xx140201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731519v209%20WR-MPC5_6570xx140201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT"/>
</gates>
<devices>
<device name="" package="657006140201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657006140201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657006140201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="6"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657006140201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX240201_657004240201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Vertical with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731511v209%20WR-MPC5_6570xx240201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731511v209%20WR-MPC5_6570xx240201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT"/>
</gates>
<devices>
<device name="" package="657004240201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657004240201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657004240201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="4"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657004240201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX230101_657008230101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Right Angled &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731517v209%20WR-MPC5_6570xx230101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731517v209%20WR-MPC5_6570xx230101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="657008230101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657008230101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657008230101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="8"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657008230101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX240201_657002240201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Vertical with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731511v209%20WR-MPC5_6570xx240201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731511v209%20WR-MPC5_6570xx240201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MT"/>
</gates>
<devices>
<device name="" package="657002240201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657002240201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657002240201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="2"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657002240201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX240101_657008240101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Right Angled with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731507v209%20WR-MPC5_6570xx240101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731507v209%20WR-MPC5_6570xx240101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT"/>
</gates>
<devices>
<device name="" package="657008240101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657008240101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657008240101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="8"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657008240101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX240201_657012240201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Vertical with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731511v209%20WR-MPC5_6570xx240201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731511v209%20WR-MPC5_6570xx240201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT"/>
</gates>
<devices>
<device name="" package="657012240201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657012240201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657012240201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="12"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657012240201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX240201_657006240201" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Vertical with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Vertical 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731511v209%20WR-MPC5_6570xx240201_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731511v209%20WR-MPC5_6570xx240201_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_VERTICAL_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT"/>
</gates>
<devices>
<device name="" package="657006240201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657006240201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657006240201"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="6"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="657006240201"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX240101_657002240101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Dual Row Right Angled with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Dual 
&lt;BR&gt;Type Right Angled 
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;REACh Approval Conform or declared [(EC)1907/2006] 
&lt;BR&gt;RoHS Approval Compliant [2011/65/EU&amp;2015/863] 
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731507v209%20WR-MPC5_6570xx240101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731507v209%20WR-MPC5_6570xx240101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_DUAL_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1X2MT"/>
</gates>
<devices>
<device name="" package="657002240101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657002240101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657002240101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="2"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657002240101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6570XX140101_657008140101" prefix="J">
<description>&lt;b&gt;WR-MPC5 5.70 mm Male Header Single Row Right Angled with Snap-in Plastic Pegs &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Kind Properties
&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pitch 5.7 mm 
&lt;BR&gt;Rows Single 
&lt;BR&gt;Type Right Angled
&lt;BR&gt;Operating Temperature -40 up to +105 °C 
&lt;BR&gt;Durability 25 Mating cycles 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material LCP 
&lt;BR&gt;Insulator Color Black 
&lt;BR&gt;Insulator Flammability Rating UL94 V-0 
&lt;BR&gt;Pin Material Copper Alloy 
&lt;BR&gt;Pin Plating Tin over Nickel 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging Tray 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electric Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR 26 A 
&lt;BR&gt;Working Voltage 600 V (AC) 
&lt;BR&gt;Withstanding Voltage 2200 V (AC) 
&lt;BR&gt;Contact Resistance 2 mΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964 
 &lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o731536v209%20WR-MPC5_6570xx140101_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o731536v209%20WR-MPC5_6570xx140101_Multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_MPC5_5_70_MM_MALE_HEADER_SINGLE_ROW_RIGHT_ANGLED_WITH_SNAP_IN_PLASTIC_PEGS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-10-09&lt;BR&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT"/>
</gates>
<devices>
<device name="" package="657008140101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="2mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/657008140101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="26A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="657008140101"/>
<attribute name="PITCH" value="5.7mm"/>
<attribute name="POLARITY" value="8"/>
<attribute name="ROWS" value="single"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value="657008140101"/>
<attribute name="WORKING-VOLTAGE" value="600V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
