<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Wire-to-Board Connectors - WR-NPC2&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-11-06&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="626012210201">
<description>&lt;B&gt;WR-NPC2 THT Dual Row Male Header Angled with Snap-in Plastic Pegs
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 12pins</description>
</package>
<package name="626016220101">
<description>&lt;B&gt;WR-NPC2 THT Dual Row Male Header Vertical Classic with Poka-Yoke
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 16pins</description>
</package>
<package name="626008120101">
<description>&lt;B&gt;WR-NPC2 THT Single Row Male Header Vertical
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 8pins</description>
</package>
<package name="626016210201">
<description>&lt;B&gt;WR-NPC2 THT Dual Row Male Header Angled with Snap-in Plastic Pegs
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 16pins</description>
</package>
<package name="626004220101">
<description>&lt;B&gt;WR-NPC2 THT Dual Row Male Header Vertical Classic with Poka-Yoke
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 4pins</description>
</package>
<package name="626006220101">
<description>&lt;B&gt;WR-NPC2 THT Dual Row Male Header Vertical Classic with Poka-Yoke
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 6pins</description>
</package>
<package name="626010220101">
<description>&lt;B&gt;THT Dual Row Male Header Vertical Classic with Poka-Yoke
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 10pins</description>
</package>
<package name="626014220101">
<description>&lt;B&gt;WR-NPC2 THT Dual Row Male Header Vertical Classic with Poka-Yoke
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 14pins</description>
</package>
<package name="626008220101">
<description>&lt;B&gt;WR-NPC2 THT Dual Row Male Header Vertical Classic with Poka-Yoke
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 8pins</description>
</package>
<package name="626010210201">
<description>&lt;B&gt;WR-NPC2 THT Dual Row Male Header Angled with Snap-in Plastic Pegs
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 10pins</description>
</package>
<package name="626004210201">
<description>&lt;B&gt;WR-NPC2 THT Dual Row Male Header Angled with Snap-in Plastic Pegs
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 4pins</description>
</package>
<package name="626012220101">
<description>&lt;B&gt;WR-NPC2 THT Dual Row Male Header Vertical Classic with Poka-Yoke
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 12pins</description>
</package>
<package name="626008210201">
<description>&lt;B&gt;WR-NPC2 THT Dual Row Male Header Angled with Snap-in Plastic Pegs
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 8pins</description>
</package>
<package name="626014210201">
<description>&lt;B&gt;WR-NPC2 THT Dual Row Male Header Angled with Snap-in Plastic Pegs
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 14pins</description>
</package>
<package name="626002110201">
<description>&lt;B&gt;WR-NPC2 THT Single Row Male Header Right Angled without Plastic Pegs
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt; THT, 2pins</description>
</package>
<package name="626007110201">
<description>&lt;B&gt;WR-NPC2 THT Single Row Male Header Right Angled without Plastic Pegs
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt; THT, 7pins</description>
</package>
<package name="626003120101">
<description>&lt;B&gt;WR-NPC2 THT Single Row Male Header Vertical
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 3pins</description>
</package>
<package name="626006210201">
<description>&lt;B&gt;WR-NPC2 THT Dual Row Male Header Angled with Snap-in Plastic Pegs
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 6pins</description>
</package>
<package name="626004110201">
<description>&lt;B&gt;WR-NPC2 THT Single Row Male Header Right Angled without Plastic Pegs
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt; THT, 4pins</description>
</package>
<package name="626003110201">
<description>&lt;B&gt;WR-NPC2 THT Single Row Male Header Right Angled without Plastic Pegs
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt; THT, 3pins</description>
</package>
<package name="626006110201">
<description>&lt;B&gt;WR-NPC2 THT Single Row Male Header Right Angled without Plastic Pegs
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt; THT, 6pins</description>
</package>
<package name="626002120101">
<description>&lt;B&gt;WR-NPC2 THT Single Row Male Header Vertical
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 2pins</description>
</package>
<package name="626005110201">
<description>&lt;B&gt;WR-NPC2 THT Single Row Male Header Right Angled without Plastic Pegs
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt; THT, 5pins</description>
</package>
<package name="626006120101">
<description>&lt;B&gt;WR-NPC2 THT Single Row Male Header Vertical
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 6pins</description>
</package>
<package name="626004120101">
<description>&lt;B&gt;WR-NPC2 THT Single Row Male Header Vertical
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 4pins</description>
</package>
<package name="626007120101">
<description>&lt;B&gt;WR-NPC2 THT Single Row Male Header Vertical
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 7pins</description>
</package>
<package name="626005120101">
<description>&lt;B&gt;WR-NPC2 THT Single Row Male Header Vertical
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;THT, 5pins</description>
</package>
<package name="626008110201">
<description>&lt;B&gt;WR-NPC2 THT Single Row Male Header Right Angled without Plastic Pegs
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt; THT, 8pins</description>
</package>
</packages>
<symbols>
<symbol name="8X2MT_BOTTOM_LEFT">
<description>8x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="6X2MT_BOTTOM_LEFT">
<description>6x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="2X2MT_BOTTOM_LEFT">
<description>2x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="6X2MT_TOP_RIGHT">
<description>6x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="8MT_LEFT">
<description>8Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="3X2MT_BOTTOM_LEFT">
<description>3x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="8X2MT_TOP_RIGHT">
<description>8x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="7X2MT_BOTTOM_LEFT">
<description>7x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="2X2MT_TOP_RIGHT">
<description>2x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="3X2MT_TOP_RIGHT">
<description>3x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="5X2MT_TOP_RIGHT">
<description>5x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="4X2MT_TOP_RIGHT">
<description>4x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="4X2MT_BOTTOM_LEFT">
<description>4x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="7X2MT_TOP_RIGHT">
<description>7x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="7MT">
<description>7Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="5X2MT_BOTTOM_LEFT">
<description>5x2Rows Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="2MT">
<description>2Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3MT_LEFT">
<description>3Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="4MT">
<description>4Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="2MT_LEFT">
<description>2Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3MT">
<description>3Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="6MT">
<description>6Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="5MT">
<description>5Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="4MT_LEFT">
<description>4Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="6MT_LEFT">
<description>6Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="7MT_LEFT">
<description>7Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="5MT_LEFT">
<description>5Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="8MT">
<description>8Pins Male THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="6260XX210201_626012210201" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Dual Row - THT&lt;br&gt;
2.5mm pitch - Glow Wire

&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected Contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="626012210201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626012210201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626012210201 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 12 "/>
<attribute name="ROWS" value="Dual Row"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 626012210201 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX220101_626016220101" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Dual Row - THT&lt;br&gt;
2.5mm pitch - Glow Wire

&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected Contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="626016220101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626016220101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626016220101 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 16 "/>
<attribute name="ROWS" value="Dual Row"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 626016220101 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX120101_626008120101" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Single Row - THT&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating Temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT_LEFT"/>
</gates>
<devices>
<device name="" package="626008120101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626008120101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626008120101 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="ROWS" value="Single Row"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 626008120101 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX210201_626016210201" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Dual Row - THT&lt;br&gt;
2.5mm pitch - Glow Wire

&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected Contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2MT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="626016210201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626016210201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626016210201 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 16 "/>
<attribute name="ROWS" value="Dual Row"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 626016210201 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX220101_626004220101" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Dual Row - THT&lt;br&gt;
2.5mm pitch - Glow Wire

&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected Contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="626004220101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626004220101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626004220101 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="ROWS" value="Dual Row"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 626004220101 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX220101_626006220101" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Dual Row - THT&lt;br&gt;
2.5mm pitch - Glow Wire

&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected Contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="626006220101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626006220101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626006220101 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 6 "/>
<attribute name="ROWS" value="Dual Row"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 626006220101 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX220101_626010220101" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Dual Row - THT&lt;br&gt;
2.5mm pitch - Glow Wire

&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected Contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="626010220101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626010220101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626010220101 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 10 "/>
<attribute name="ROWS" value="Dual Row"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 626010220101 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX220101_626014220101" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Dual Row - THT&lt;br&gt;
2.5mm pitch - Glow Wire

&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected Contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="626014220101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626014220101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626014220101 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 14 "/>
<attribute name="ROWS" value="Dual Row"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 626014220101 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX220101_626008220101" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Dual Row - THT&lt;br&gt;
2.5mm pitch - Glow Wire

&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected Contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="626008220101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626008220101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626008220101 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="ROWS" value="Dual Row"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 626008220101 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX210201_626004210201" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Dual Row - THT&lt;br&gt;
2.5mm pitch - Glow Wire

&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected Contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2MT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="626004210201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626004210201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626004210201 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="ROWS" value="Dual Row"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 626004210201 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX220101_626012220101" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Dual Row - THT&lt;br&gt;
2.5mm pitch - Glow Wire

&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected Contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2MT_BOTTOM_LEFT"/>
</gates>
<devices>
<device name="" package="626012220101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626012220101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626012220101 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 12 "/>
<attribute name="ROWS" value="Dual Row"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 626012220101 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX210201_626010210201" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Dual Row - THT&lt;br&gt;
2.5mm pitch - Glow Wire

&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected Contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2MT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="626010210201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626010210201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626010210201 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 10 "/>
<attribute name="ROWS" value="Dual Row"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 626010210201 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX210201_626008210201" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Dual Row - THT&lt;br&gt;
2.5mm pitch - Glow Wire

&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected Contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2MT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="626008210201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626008210201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626008210201 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="ROWS" value="Dual Row"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 626008210201 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX210201_626014210201" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Dual Row - THT&lt;br&gt;
2.5mm pitch - Glow Wire

&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected Contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2MT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="626014210201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626014210201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626014210201 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 14 "/>
<attribute name="ROWS" value="Dual Row"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 626014210201 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX110201_626002110201" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Single Row - THT&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating Temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT"/>
</gates>
<devices>
<device name="" package="626002110201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626002110201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626002110201 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 2 "/>
<attribute name="ROWS" value="Single Row"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 626002110201 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX110201_626007110201" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Single Row - THT&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating Temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT"/>
</gates>
<devices>
<device name="" package="626007110201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626007110201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626007110201 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 7 "/>
<attribute name="ROWS" value="Single Row"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 626007110201 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX120101_626003120101" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Single Row - THT&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating Temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT_LEFT"/>
</gates>
<devices>
<device name="" package="626003120101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626003120101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626003120101 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 3 "/>
<attribute name="ROWS" value="Single Row"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 626003120101 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX210201_626006210201" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Dual Row - THT&lt;br&gt;
2.5mm pitch - Glow Wire

&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected Contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786372v209%20Family-WR-NPC2-6260xx220101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_DUAL_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_DUAL_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2MT_TOP_RIGHT"/>
</gates>
<devices>
<device name="" package="626006210201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626006210201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626006210201 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 6 "/>
<attribute name="ROWS" value="Dual Row"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 626006210201 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX110201_626004110201" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Single Row - THT&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating Temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT"/>
</gates>
<devices>
<device name="" package="626004110201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626004110201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626004110201 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="ROWS" value="Single Row"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 626004110201 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX110201_626003110201" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Single Row - THT&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating Temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3MT"/>
</gates>
<devices>
<device name="" package="626003110201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626003110201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626003110201 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 3 "/>
<attribute name="ROWS" value="Single Row"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 626003110201 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX110201_626006110201" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Single Row - THT&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating Temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT"/>
</gates>
<devices>
<device name="" package="626006110201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626006110201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626006110201 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 6 "/>
<attribute name="ROWS" value="Single Row"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 626006110201 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX120101_626002120101" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Single Row - THT&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating Temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2MT_LEFT"/>
</gates>
<devices>
<device name="" package="626002120101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626002120101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626002120101 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 2 "/>
<attribute name="ROWS" value="Single Row"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 626002120101 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX110201_626005110201" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Single Row - THT&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating Temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT"/>
</gates>
<devices>
<device name="" package="626005110201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626005110201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626005110201 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="ROWS" value="Single Row"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 626005110201 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX120101_626006120101" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Single Row - THT&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating Temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6MT_LEFT"/>
</gates>
<devices>
<device name="" package="626006120101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626006120101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626006120101 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 6 "/>
<attribute name="ROWS" value="Single Row"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 626006120101 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX120101_626004120101" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Single Row - THT&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating Temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4MT_LEFT"/>
</gates>
<devices>
<device name="" package="626004120101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626004120101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626004120101 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="ROWS" value="Single Row"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 626004120101 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX120101_626007120101" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Single Row - THT&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating Temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7MT_LEFT"/>
</gates>
<devices>
<device name="" package="626007120101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626007120101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626007120101 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 7 "/>
<attribute name="ROWS" value="Single Row"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 626007120101 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX120101_626005120101" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Single Row - THT&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating Temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5MT_LEFT"/>
</gates>
<devices>
<device name="" package="626005120101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626005120101?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626005120101 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="ROWS" value="Single Row"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value=" 626005120101 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6260XX110201_626008110201" prefix="J">
<description>&lt;b&gt;WR-NPC2 Male Header - Single Row - THT&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt; 
&lt;br&gt;Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage: 250 V
&lt;br&gt;Operating Temperature: -40°C up to +105°C
&lt;br&gt;Durability: 25 Mating cycles
&lt;br&gt;UL Approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Glow Wire Approval: IEC 60335-1
&lt;br&gt;Fully isolated &amp; Protected contacts

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Features
&lt;br&gt;&lt;/b&gt;
Coding against Mismating

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial
&lt;br&gt;Home Appliances
&lt;br&gt;Telecommunication
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o786322v209%20Multi-WR-NPC2-626007120101.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_NPC2_MALE_HEADER_SINGLE_ROW_THT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-11-06 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8MT"/>
</gates>
<devices>
<device name="" package="626008110201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/626008110201?ae"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 626008110201 "/>
<attribute name="PITCH" value="2.5mm"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="ROWS" value="Single Row"/>
<attribute name="TYPE" value="Right Angled"/>
<attribute name="VALUE" value=" 626008110201 "/>
<attribute name="WORKING-VOLTAGE" value="250V (AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
