<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Board-to-Board Connectors - WR-PHD &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-04-23&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="62131421921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMD Dual Pin Header (Reel), 14 Pins</description>
</package>
<package name="61000418221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Pin Headerr, 4 Pins</description>
</package>
<package name="61301211821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header, 12 Pins</description>
</package>
<package name="61003218321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54 mm SMT Pin Headerr, 32 Pins</description>
</package>
<package name="61031421121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header (Reel), 14Pins</description>
</package>
<package name="61304011121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 40 Pins</description>
</package>
<package name="61307221021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header, 72 Pins</description>
</package>
<package name="61303611821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header, 36 Pins</description>
</package>
<package name="61001018321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Pin Headerr, 10Pins</description>
</package>
<package name="61303611121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 36 Pins</description>
</package>
<package name="61300421021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header, 4 Pins</description>
</package>
<package name="61300411821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header, 4 Pins</description>
</package>
<package name="61303021121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual Pin Header, 30 Pins</description>
</package>
<package name="61301221021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header,  12 Pins</description>
</package>
<package name="613002143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header, 2 Pins</description>
</package>
<package name="61302011121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Pin Header, 20 Pins</description>
</package>
<package name="61003218221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54 mm SMT Pin Headerr, 32 Pins</description>
</package>
<package name="61003221121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header, 32 Pins</description>
</package>
<package name="61303421821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header,34 Pins</description>
</package>
<package name="61303211321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Board Stacker,32 Pins</description>
</package>
<package name="61302021821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Dual Socket Header,20 Pins</description>
</package>
<package name="61304021821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header,40 Pins</description>
</package>
<package name="61001221121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header, 12 Pins</description>
</package>
<package name="613006143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header, 6 Pins</description>
</package>
<package name="61031221121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header (Reel), 12Pins</description>
</package>
<package name="61302211121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 22 Pins</description>
</package>
<package name="61301611021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Angled Pin Header, 16 Pins</description>
</package>
<package name="61300911821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header, 9 Pins</description>
</package>
<package name="61300311821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Socket Header,  3 Pins</description>
</package>
<package name="61300821821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Dual Socket Header, 8 Pins</description>
</package>
<package name="613012243121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Angled Socket Header, 12 Pins</description>
</package>
<package name="61301821821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header,18 Pins</description>
</package>
<package name="61001621121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header, 16 Pins</description>
</package>
<package name="61307221821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Dual Socket Header, 72 Pins</description>
</package>
<package name="61302411821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Socket Header, 24 Pins</description>
</package>
<package name="61303021821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header, 30 Pins</description>
</package>
<package name="610106249121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;SMT Pin Header Double Row Right Angled,6 Pins</description>
</package>
<package name="61300421821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header,4 Pins</description>
</package>
<package name="61303211821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Socket Header, 32 Pins</description>
</package>
<package name="61302821821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Dual Socket Header,28 Pins</description>
</package>
<package name="61301621121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual Pin Header, 16 Pins</description>
</package>
<package name="61301211121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 12 Pins</description>
</package>
<package name="61303621821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Dual Socket Header,36 Pins</description>
</package>
<package name="61030821121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header (Reel), 8Pins</description>
</package>
<package name="61303621121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual Pin Header, 36 Pins</description>
</package>
<package name="61302011821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;WR-PHD 2.54 mm Socket Header,  20 Pins</description>
</package>
<package name="61300211021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Angled Pin Header, 2 Pins</description>
</package>
<package name="61300621021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header,  6 Pins</description>
</package>
<package name="61300611021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54mm Angled Pin Header, 6 Pins</description>
</package>
<package name="61300811821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header,  8 Pins</description>
</package>
<package name="61301211021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54mm Angled Pin Header, 12 Pins</description>
</package>
<package name="61000621121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header, 6 Pins</description>
</package>
<package name="61300511021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54mm Angled Pin Header, 5 Pins</description>
</package>
<package name="61302221021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header, ,22Pins</description>
</package>
<package name="61000618321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54 mm SMT Pin Headerr, 6 Pins</description>
</package>
<package name="61300621821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header, 6 Pins</description>
</package>
<package name="61001418221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54 mm SMT Pin Headerr, 14 Pins</description>
</package>
<package name="61003421121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header,  34 Pins</description>
</package>
<package name="610112249121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;SMT Pin Header Double Row Right Angled,12Pins</description>
</package>
<package name="613003143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header,  3 Pins</description>
</package>
<package name="613011143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header, 11 Pins</description>
</package>
<package name="61307221121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual Pin Header, 72 Pins</description>
</package>
<package name="61001618321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Pin Headerr, 16 Pins</description>
</package>
<package name="61306428521">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm THT Dual Board Stacker, 64 Pins</description>
</package>
<package name="613016143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Angled Socket Header, 16 Pins</description>
</package>
<package name="61002418221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Pin Headerr,  24 Pins</description>
</package>
<package name="613004243121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Angled Socket Header, 4 Pins</description>
</package>
<package name="61002621121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header, 26 Pins</description>
</package>
<package name="613008243121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Angled Socket Header, 8 Pins</description>
</package>
<package name="61301311121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 13 Pins</description>
</package>
<package name="613005143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header, 5 Pins</description>
</package>
<package name="61303221121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual Pin Header, 32 Pins</description>
</package>
<package name="61308021121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual Pin Header, 80 Pins</description>
</package>
<package name="61300811021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54mm Angled Pin Header, 8 Pins</description>
</package>
<package name="61302511121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 25 Pins</description>
</package>
<package name="61306421321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm THT Dual Board Stacker, 64 Pins</description>
</package>
<package name="61000418321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Pin Headerr,  4 Pins</description>
</package>
<package name="61300511121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 5 Pin</description>
</package>
<package name="61302211021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54mm Angled Pin Header, 22 Pins</description>
</package>
<package name="61306428421">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Dual Board Stacker, 64 Pins</description>
</package>
<package name="61300821121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual Pin Header; 8 Pins</description>
</package>
<package name="61302421821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header, 24 Pins</description>
</package>
<package name="61301021021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header, 10 Pins</description>
</package>
<package name="61000421121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header, 4 Pins</description>
</package>
<package name="61303218521">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Board Stacker,32 Pins</description>
</package>
<package name="61301021821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header,10 Pins</description>
</package>
<package name="61306421121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual Board Stacker, 64 Pins</description>
</package>
<package name="61001421121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header,  14 Pins</description>
</package>
<package name="61306421021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header, 64 Pins</description>
</package>
<package name="61301511121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Pin Header, 15 Pins</description>
</package>
<package name="61300821021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header, 8 Pins</description>
</package>
<package name="61301011121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 10 Pins</description>
</package>
<package name="61303221021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header, 32 Pins</description>
</package>
<package name="610110249121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;SMT Pin Header Double Row Right Angled,10 Pins</description>
</package>
<package name="613018143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header,  18 Pins</description>
</package>
<package name="61300815721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header Bottom Entry,  8 Pins</description>
</package>
<package name="613020143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header,  20 Pins</description>
</package>
<package name="61301811121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 18 Pins</description>
</package>
<package name="61302211821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Socket Header, 22 Pins</description>
</package>
<package name="61301111821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header, 11 Pins</description>
</package>
<package name="61301011021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54mm Angled Pin Header, 10 Pins</description>
</package>
<package name="61302621821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Dual Socket Header,26 Pins</description>
</package>
<package name="61304421121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual Pin Header, 40 Pins</description>
</package>
<package name="61302421121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual Pin Header, 24 Pins</description>
</package>
<package name="61301411121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 14 Pins</description>
</package>
<package name="61300311121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 3 Pin</description>
</package>
<package name="613012143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header, 12 Pins</description>
</package>
<package name="613013143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54 mm Angled Socket Header, 13 Pins</description>
</package>
<package name="61304421821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Dual Socket Header,44 Pins</description>
</package>
<package name="61302421021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header, 24 Pins</description>
</package>
<package name="613007143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header, 7 Pins</description>
</package>
<package name="61301821021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header,  18 Pins</description>
</package>
<package name="61302021021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header, 20 Pins</description>
</package>
<package name="61302411121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 24 Pins</description>
</package>
<package name="613008143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header, 8 Pins</description>
</package>
<package name="610126249121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;SMT Pin Header Double Row Right Angled,26Pins</description>
</package>
<package name="61002221121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header, 22 Pins</description>
</package>
<package name="613010243121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Angled Socket Header, 10 Pins</description>
</package>
<package name="61304011021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54mm Angled Pin Header, 40 Pins</description>
</package>
<package name="613036143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Angled Socket Header,  36 Pins</description>
</package>
<package name="613010143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header, 10 Pins</description>
</package>
<package name="61300211121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 2 Pin</description>
</package>
<package name="613014243121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Angled Socket Header, 14 Pins</description>
</package>
<package name="61303211221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Board Stacker, 32 Pins</description>
</package>
<package name="61300421121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual Pin Header, 4 Pins</description>
</package>
<package name="61300811121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 9 Pins</description>
</package>
<package name="61300411121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Pin Header, 4 Pin</description>
</package>
<package name="61303411021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54mm Angled Pin Header, 34 Pins</description>
</package>
<package name="613009143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header, 9 Pins</description>
</package>
<package name="610108249121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;SMT Pin Header Double Row Right Angled,8 Pins</description>
</package>
<package name="613040243121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header, 40 Pins</description>
</package>
<package name="61003418321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Pin Headerr,  34 Pins</description>
</package>
<package name="61301021121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual Pin Header, 10 Pins</description>
</package>
<package name="61302511821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header, 25 Pins</description>
</package>
<package name="61301411021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Angled Pin Header, 14 Pins</description>
</package>
<package name="61300611121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 6 Pin</description>
</package>
<package name="61303621021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header, 36 Pins</description>
</package>
<package name="61001021121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header, 10 Pins</description>
</package>
<package name="61303221821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header,32 Pins</description>
</package>
<package name="61304011821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Socket Header, 40 Pins</description>
</package>
<package name="61303421021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header, 34 Pins</description>
</package>
<package name="61300111121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Pin Header, 1 Pin</description>
</package>
<package name="613016243121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Angled Socket Header, 16 Pins</description>
</package>
<package name="61302821121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual Pin Header, 28 Pins</description>
</package>
<package name="61301011821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header,  10 Pins</description>
</package>
<package name="610122249121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;SMT Pin Header Double Row Right Angled,22Pins</description>
</package>
<package name="61306421821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header,64 Pins</description>
</package>
<package name="61002418321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Pin Headerr, 24 Pins</description>
</package>
<package name="61304021121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual Pin Header, 40 Pins</description>
</package>
<package name="61301421121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual Pin Header, 14 Pins</description>
</package>
<package name="610114249121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;SMT Pin Header Double Row Right Angled,14Pins</description>
</package>
<package name="61300311021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54mm Angled Pin Header, 3 Pins</description>
</package>
<package name="610124249121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;SMT Pin Header Double Row Right Angled,24Pins</description>
</package>
<package name="61300411021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54mm Angled Pin Header, 4 Pins</description>
</package>
<package name="61300711821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header, 7 Pins</description>
</package>
<package name="61300711121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 7 Pins</description>
</package>
<package name="61301221821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header, 12 Pins</description>
</package>
<package name="61300615721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header Bottom Entry,  6 Pins</description>
</package>
<package name="61000821121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header,  8 Pins</description>
</package>
<package name="61300211821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Socket Header,  2 Pins</description>
</package>
<package name="61303211121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 32 Pins</description>
</package>
<package name="61300711021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54mm Angled Pin Header, 7 Pins</description>
</package>
<package name="61301811021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Angled Pin Header, 18 Pins</description>
</package>
<package name="61301311821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header, 13  Pins</description>
</package>
<package name="61030621121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header (Reel), 6Pins</description>
</package>
<package name="61031021121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header (Reel), 10Pins</description>
</package>
<package name="613006243121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header,6 Pins</description>
</package>
<package name="61303611021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54mm Angled Pin Header, 36 Pins</description>
</package>
<package name="613024243121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Angled Socket Header, 24 Pins</description>
</package>
<package name="61302221121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual Pin Header, 22 Pins</description>
</package>
<package name="61003621121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header,  36 Pins</description>
</package>
<package name="61300911021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54mm Angled Pin Header, 9 Pins</description>
</package>
<package name="61301811821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Socket Header, 18 Pins</description>
</package>
<package name="61300415721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Socket Header Bottom Entry, 4 Pins</description>
</package>
<package name="61303218421">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Board Stacker, 32 Pins</description>
</package>
<package name="613034243121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header,  34 Pins</description>
</package>
<package name="610120249121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;SMT Pin Header Double Row Right Angled,20Pins</description>
</package>
<package name="61301821121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual Pin Header, 18 Pins</description>
</package>
<package name="613032143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Angled Socket Header, 32 Pins</description>
</package>
<package name="61032021121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header (Reel), 20Pins</description>
</package>
<package name="613032243121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Angled Socket Header,  32 Pins</description>
</package>
<package name="61301025721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Dual Socket Header Bottom Entry, 10 Pins</description>
</package>
<package name="61300825721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header Bottom Entry,8 Pins</description>
</package>
<package name="61302021121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual Pin Header, 20 Pins</description>
</package>
<package name="61300515721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header Bottom Entry, 5 Pins</description>
</package>
<package name="61304021021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header,  40 Pins</description>
</package>
<package name="61300911121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 9 Pins</description>
</package>
<package name="61301221121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual Pin Header, 12 Pins</description>
</package>
<package name="61301625721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Dual Socket Header Bottom Entry,16 Pins</description>
</package>
<package name="61301611821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Socket Header, 16 Pins</description>
</package>
<package name="61302221821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header,22 Pins</description>
</package>
<package name="61303211021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54mm Angled Pin Header, 32 Pins</description>
</package>
<package name="61301421821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header,14 Pins</description>
</package>
<package name="61000618221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54 mm SMT Pin Headerr,  6 Pins</description>
</package>
<package name="61302621021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header, 26Pins</description>
</package>
<package name="613004143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header, 4 Pins</description>
</package>
<package name="613072243121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header, 72 Pins</description>
</package>
<package name="61301611121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 16 Pins</description>
</package>
<package name="61301621821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header,16 Pins</description>
</package>
<package name="610116249121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;SMT Pin Header Double Row Right Angled,16Pins</description>
</package>
<package name="61300511821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Socket Header, 5 Pins</description>
</package>
<package name="61301421021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header, 14 Pins</description>
</package>
<package name="61303421121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual Pin Header, 34 Pins</description>
</package>
<package name="61002421121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header, 24 Pins</description>
</package>
<package name="61301411821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header, 14 Pins</description>
</package>
<package name="61002021121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header,  20 Pins</description>
</package>
<package name="61302621121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual Pin Header, 26 Pins</description>
</package>
<package name="61302025721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header Bottom Entry,20 Pins</description>
</package>
<package name="61030421121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header (Reel), 4Pins</description>
</package>
<package name="61031621121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Pin Header (Reel), 16Pins</description>
</package>
<package name="613022243121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Angled Socket Header, 22 Pins</description>
</package>
<package name="61300425721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header Bottom Entry, 4 Pins</description>
</package>
<package name="613020243121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header,  20 Pins</description>
</package>
<package name="61003618321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Pin Headerr, 36 Pins</description>
</package>
<package name="61300625721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header Bottom Entry,6 Pins</description>
</package>
<package name="61306421221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm THT Dual Board Stacker, 64 Pins</description>
</package>
<package name="61301015721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header Bottom Entry, 10 Pins</description>
</package>
<package name="61302425721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header Bottom Entry,24 Pins</description>
</package>
<package name="613010216921">
<description>&lt;b&gt;WR-PHD&lt;/b&gt; &lt;br&gt;2.54 mm Dual Socket Header Bottom Entry Large, 10 Pins</description>
</package>
<package name="61302625721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header Bottom Entry,26 Pins</description>
</package>
<package name="61001618221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Pin Headerr, 16 Pins</description>
</package>
<package name="61303225721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header Bottom Entry, 32 Pins</description>
</package>
<package name="613024143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header, 24 Pins</description>
</package>
<package name="61302015721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header Bottom Entry, 20 Pins</description>
</package>
<package name="613064243121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Angled Socket Header,  64 Pins</description>
</package>
<package name="613026243121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Angled Socket Header,  26 Pins</description>
</package>
<package name="613008216921">
<description>&lt;b&gt;WR-PHD&lt;/b&gt; &lt;br&gt;2.54 mm Dual Socket Header Bottom Entry Large,  8 Pins</description>
</package>
<package name="61303425721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm Dual Socket Header Bottom Entry,34 Pins</description>
</package>
<package name="613012216921">
<description>&lt;b&gt;WR-PHD&lt;/b&gt; &lt;br&gt;2.54 mm Dual Socket Header Bottom Entry Large, 12 Pins</description>
</package>
<package name="61301225721">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header Bottom Entry, 12 Pins</description>
</package>
<package name="613004216921">
<description>&lt;b&gt;WR-PHD&lt;/b&gt; &lt;br&gt;2.54 mm Dual Socket Header Bottom Entry Large, 4 Pins</description>
</package>
<package name="613006216921">
<description>&lt;b&gt;WR-PHD&lt;/b&gt; &lt;br&gt;2.54 mm Dual Socket Header Bottom Entry Large,  6 Pins</description>
</package>
<package name="61300621121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual Pin Header, 6 Pins</description>
</package>
<package name="613022216921">
<description>&lt;b&gt;WR-PHD&lt;/b&gt; &lt;br&gt;2.54 mm Dual Socket Header Bottom Entry Large, 22 Pins</description>
</package>
<package name="613020216921">
<description>&lt;b&gt;WR-PHD&lt;/b&gt; &lt;br&gt;2.54 mm Dual Socket Header Bottom Entry Large,  20 Pins</description>
</package>
<package name="610004243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry, 4 Pins</description>
</package>
<package name="613018216921">
<description>&lt;b&gt;WR-PHD&lt;/b&gt; &lt;br&gt;2.54 mm Dual Socket Header Bottom Entry Large, 18 Pins</description>
</package>
<package name="610008243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry, 8 Pins</description>
</package>
<package name="613026216921">
<description>&lt;b&gt;WR-PHD&lt;/b&gt; &lt;br&gt;2.54 mm Dual Socket Header Bottom Entry Large,  26 Pins</description>
</package>
<package name="610312243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry (Reel), 12 Pins</description>
</package>
<package name="610310243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry (Reel), 10Pins</description>
</package>
<package name="610018243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Dual Socket Header Bottom Entry,  18 Pins</description>
</package>
<package name="610316243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry (Reel), 16Pins</description>
</package>
<package name="610318243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry (Reel), 18Pins</description>
</package>
<package name="610020243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Dual Socket Header Bottom Entry,  20 Pins</description>
</package>
<package name="613016216921">
<description>&lt;b&gt;WR-PHD&lt;/b&gt; &lt;br&gt;2.54 mm Dual Socket Header Bottom Entry Large,  16 Pins</description>
</package>
<package name="610016243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry, 16 Pins</description>
</package>
<package name="610006243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry, 6 Pins</description>
</package>
<package name="61300611821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header,  6 Pins</description>
</package>
<package name="610034243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry, 34 Pins</description>
</package>
<package name="61001011921">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;2.54 mm SMT Socket Header, 10 Pins</description>
</package>
<package name="613034216921">
<description>&lt;b&gt;WR-PHD&lt;/b&gt; &lt;br&gt;2.54 mm Dual Socket Header Bottom Entry Large, 34 Pins</description>
</package>
<package name="61001018221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54 mm SMT Pin Headerr, 10 Pins</description>
</package>
<package name="610012243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry, 12Pins</description>
</package>
<package name="61001211921">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;2.54 mm SMT Socket Header, 12 Pins</description>
</package>
<package name="610022243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry, 22 Pins</description>
</package>
<package name="610306243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry (Reel), 6 Pins</description>
</package>
<package name="61000511921">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;2.54 mm SMT Socket Header,  5 Pins</description>
</package>
<package name="610024243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry,  24 Pins</description>
</package>
<package name="61000611921">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;2.54 mm SMT Socket Header,  6 Pins</description>
</package>
<package name="610320243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry (Reel), 20 Pins</description>
</package>
<package name="610304243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry (Reel), 4 Pins</description>
</package>
<package name="610026243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry,  26 Pins</description>
</package>
<package name="610308243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry (Reel), 8 Pins</description>
</package>
<package name="610010243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry, 10 Pins</description>
</package>
<package name="61002021821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual SMT Socket Header, 20 Pins</description>
</package>
<package name="61000811921">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;2.54 mm SMT Socket Header,  8 Pins</description>
</package>
<package name="61000613321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm SMT Socket Header, 6 Pins</description>
</package>
<package name="61002421821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual SMT Socket Header, 24 Pins</description>
</package>
<package name="613024216921">
<description>&lt;b&gt;WR-PHD&lt;/b&gt; &lt;br&gt;2.54 mm Dual Socket Header Bottom Entry Large,  24 Pins</description>
</package>
<package name="61000413321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm SMT Socket Header, 4 Pins</description>
</package>
<package name="613032216921">
<description>&lt;b&gt;WR-PHD&lt;/b&gt; &lt;br&gt;2.54 mm Dual Socket Header Bottom Entry Large,  32 Pins</description>
</package>
<package name="61000621821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual SMT Socket Header, 6 Pins</description>
</package>
<package name="61001611921">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;2.54 mm SMT Socket Header, 16 Pins</description>
</package>
<package name="610032243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry,  32 Pins</description>
</package>
<package name="61002221821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual SMT Socket Header, 22 Pins</description>
</package>
<package name="61000411921">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;2.54 mm SMT Socket Header, 4 Pins</description>
</package>
<package name="61002621821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual SMT Socket Header, 26 Pins</description>
</package>
<package name="61002013321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm SMT Socket Header, 20 Pins</description>
</package>
<package name="61002011921">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;2.54 mm SMT Socket Header, 20 Pins</description>
</package>
<package name="61001013321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm SMT Socket Header, 10 Pins</description>
</package>
<package name="61001021821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual SMT Socket Header, 10 Pins</description>
</package>
<package name="61003021821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual SMT Socket Header, 28 Pins</description>
</package>
<package name="61002821821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual SMT Socket Header, 28 Pins</description>
</package>
<package name="61001613321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm SMT Socket Header, 16 Pins</description>
</package>
<package name="61002413321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm SMT Socket Header, 24 Pins</description>
</package>
<package name="61000813321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm SMT Socket Header, 8 Pins</description>
</package>
<package name="61003621821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual SMT Socket Header, 36 Pins</description>
</package>
<package name="61000421821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual SMT Socket Header, 4 Pins</description>
</package>
<package name="61002411921">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;2.54 mm SMT Socket Header, 24 Pins</description>
</package>
<package name="61031421821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Dual Socket Header (Reel) , 14 Pins</description>
</package>
<package name="61001621821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual SMT Socket Header, 16 Pins</description>
</package>
<package name="61001221821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual SMT Socket Header, 12 Pins</description>
</package>
<package name="61001421821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual SMT Socket Header, 14 Pins</description>
</package>
<package name="61003221821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual SMT Socket Header, 32 Pins</description>
</package>
<package name="61001213321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm SMT Socket Header, 12 Pins</description>
</package>
<package name="61000513321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm SMT Socket Header, 5 Pins</description>
</package>
<package name="61004021821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual SMT Socket Header, 40 Pins</description>
</package>
<package name="61030821821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Dual Socket Header (Reel) , 8 Pins</description>
</package>
<package name="61032021821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Dual Socket Header (Reel) , 20 Pins</description>
</package>
<package name="610108249221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle,8 pins</description>
</package>
<package name="61001413321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm SMT Socket Header, 14 Pins</description>
</package>
<package name="61032621821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header (Reel) , 26 Pins</description>
</package>
<package name="610112249221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle, 12 pins</description>
</package>
<package name="61031621821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header (Reel) ,16 Pins</description>
</package>
<package name="61001821821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual SMT Socket Header, 18 Pins</description>
</package>
<package name="62133221921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMD Dual Pin Header (Reel), 32 Pins</description>
</package>
<package name="61000821821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm Dual SMT Socket Header, 8 Pins</description>
</package>
<package name="61030421821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Dual Socket Header (Reel) , 4 Pins</description>
</package>
<package name="610114249221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle, 14 pins</description>
</package>
<package name="62002021121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Dual Pin Header, 20 Pins</description>
</package>
<package name="62000211121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Pin Header,2 Pins</description>
</package>
<package name="61031821821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Dual Socket Header (Reel) , 18 Pins</description>
</package>
<package name="61003421821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual SMT Socket Header, 34 Pins</description>
</package>
<package name="61031021821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header (Reel) , 10 Pins</description>
</package>
<package name="62000611121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Pin Header, 6 Pins</description>
</package>
<package name="61032421821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Dual Socket Header (Reel) , 24 Pins</description>
</package>
<package name="61032221821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Dual Socket Header (Reel) , 22 Pins</description>
</package>
<package name="62000311121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Pin Header,3Pins</description>
</package>
<package name="62001021121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Dual Pin Header,10 Pins</description>
</package>
<package name="62000411121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Pin Header,4 Pins</description>
</package>
<package name="610106249221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle, 6 pins</description>
</package>
<package name="610120249221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle, 20pins</description>
</package>
<package name="610122249221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle, 22 pins</description>
</package>
<package name="610116249221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle, 16 pins</description>
</package>
<package name="62000811121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Pin Header, 8 Pins</description>
</package>
<package name="610110249221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle, 10 pins</description>
</package>
<package name="62001011121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Pin Header,10Pins</description>
</package>
<package name="61030621821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Dual Socket Header (Reel) , 6 Pins</description>
</package>
<package name="62100821921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header, 8 Pins</description>
</package>
<package name="610124249221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle, 24pins</description>
</package>
<package name="610126249221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle, 26 pins</description>
</package>
<package name="62004021121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Dual Pin Header, 40 Pins</description>
</package>
<package name="62101021921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header, 10 Pins</description>
</package>
<package name="62132421921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMD Dual Pin Header (Reel), 24 Pins</description>
</package>
<package name="62134421921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMD Dual Pin Header (Reel), 44 Pins</description>
</package>
<package name="62000821121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Dual Pin Header,8 Pins</description>
</package>
<package name="62003221121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Dual Pin Header,32 Pins</description>
</package>
<package name="61031221821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm SMT Dual Socket Header (Reel) , 12 Pins</description>
</package>
<package name="62103221921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header, 32 Pins</description>
</package>
<package name="62002011121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Pin Header,20 Pins</description>
</package>
<package name="62001621121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Dual Pin Header,16 Pins</description>
</package>
<package name="62101421921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header, 14 Pins</description>
</package>
<package name="62100621921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header, 6 Pins</description>
</package>
<package name="62130821921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMD Dual Pin Header (Reel), 8 Pins</description>
</package>
<package name="62130421921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMD Dual Pin Header (Reel), 4 Pins</description>
</package>
<package name="62101621921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header, 16 Pins</description>
</package>
<package name="62131021921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMD Dual Pin Header (Reel), 10Pins</description>
</package>
<package name="62100421921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header,  4 Pins</description>
</package>
<package name="62002821121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Dual Pin Header,28Pins</description>
</package>
<package name="62102021921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header, 20 Pins</description>
</package>
<package name="62000421121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Dual Pin Header,4 Pins</description>
</package>
<package name="62102421921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header,  24 Pins</description>
</package>
<package name="621016245821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header Low Profile,16Pins</description>
</package>
<package name="62003211121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Pin Header,32 Pins</description>
</package>
<package name="621020245821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header Low Profile,20Pins</description>
</package>
<package name="621006245821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header Low Profile,6Pins</description>
</package>
<package name="62104421921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header, 44 Pins</description>
</package>
<package name="621324245821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header Low Profile (Reel),24Pins</description>
</package>
<package name="62130621921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMD Dual Pin Header (Reel), 6 Pins</description>
</package>
<package name="621010245821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header Low Profile,10Pins</description>
</package>
<package name="621024245821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header Low Profile,24Pins</description>
</package>
<package name="621314245821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header Low Profile (Reel),14Pins</description>
</package>
<package name="621304245821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header Low Profile (Reel),4 Pins</description>
</package>
<package name="621008245821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header Low Profile,8Pins</description>
</package>
<package name="62004421121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Dual Pin Header, 44 Pins</description>
</package>
<package name="621004245821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header Low Profile,4Pins</description>
</package>
<package name="621310245821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header Low Profile (Reel),10Pins</description>
</package>
<package name="62131621921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMD Dual Pin Header (Reel), 16 Pins</description>
</package>
<package name="621304284521">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Angled Dual Pin Header,4 Pins</description>
</package>
<package name="621308284521">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Angled Dual Pin Header,8Pins</description>
</package>
<package name="62000821821">
<description>&lt;b&gt;WR-PHD&lt;/b&gt;&lt;br&gt; 2.00 mm Dual Socket Header THT, 8 Pins</description>
</package>
<package name="621014245821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header Low Profile,14Pins</description>
</package>
<package name="62000621121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Dual Pin Header, 6 Pins</description>
</package>
<package name="621306284521">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Angled Dual Pin Header,6 Pins</description>
</package>
<package name="62002421821">
<description>&lt;b&gt;WR-PHD&lt;/b&gt;&lt;br&gt; 2.00 mm Dual Socket Header THT,24 Pins</description>
</package>
<package name="62000411821">
<description>&lt;b&gt;WR-PHD 2.00mm Socket Header, 4 Pins</description>
</package>
<package name="62000421821">
<description>&lt;b&gt;WR-PHD&lt;/b&gt;&lt;br&gt; 2.00 mm Dual Socket Header THT,4 Pins</description>
</package>
<package name="621308245821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header Low Profile (Reel),8Pins</description>
</package>
<package name="621306245821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header Low Profile (Reel),6Pins</description>
</package>
<package name="621316245821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header Low Profile (Reel),16Pins</description>
</package>
<package name="62002421121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.00 mm THT Dual Pin Header, 24 Pins</description>
</package>
<package name="62132021921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMD Dual Pin Header (Reel), 20 Pins</description>
</package>
<package name="62001021821">
<description>&lt;b&gt;WR-PHD&lt;/b&gt;&lt;br&gt; 2.00 mm Dual Socket Header THT, 10 Pins</description>
</package>
<package name="621008242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header, 8 Pins</description>
</package>
<package name="62002021821">
<description>&lt;b&gt;WR-PHD&lt;/b&gt;&lt;br&gt; 2.00 mm Dual Socket Header THT, 20 Pins</description>
</package>
<package name="62003221821">
<description>&lt;b&gt;WR-PHD&lt;/b&gt;&lt;br&gt; 2.00 mm Dual Socket Header THT,32 Pins</description>
</package>
<package name="621004242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header,4 Pins</description>
</package>
<package name="621310284521">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Angled Dual Pin Header,10 Pins</description>
</package>
<package name="62001621821">
<description>&lt;b&gt;WR-PHD&lt;/b&gt;&lt;br&gt; 2.00 mm Dual Socket Header THT, 16 Pins</description>
</package>
<package name="62000611821">
<description>&lt;b&gt;WR-PHD 2.00mm Socket Header, 6 Pins</description>
</package>
<package name="621320245821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Dual Pin Header Low Profile (Reel),20Pins</description>
</package>
<package name="621032242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header,32 Pins</description>
</package>
<package name="62002011821">
<description>&lt;b&gt;WR-PHD 2.00mm Socket Header, 20 Pins</description>
</package>
<package name="621316284521">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Angled Dual Pin Header,16 Pins</description>
</package>
<package name="62002821821">
<description>&lt;b&gt;WR-PHD&lt;/b&gt;&lt;br&gt; 2.00 mm Dual Socket Header THT, 28 Pins</description>
</package>
<package name="62000621821">
<description>&lt;b&gt;WR-PHD&lt;/b&gt;&lt;br&gt; 2.00 mm Dual Socket Header THT, 6 Pins</description>
</package>
<package name="62000211821">
<description>&lt;b&gt;WR-PHD 2.00mm Socket Header, 2 Pins</description>
</package>
<package name="62001011821">
<description>&lt;b&gt;WR-PHD 2.00mm Socket Header, 10 Pins</description>
</package>
<package name="62001421821">
<description>&lt;b&gt;WR-PHD&lt;/b&gt;&lt;br&gt; 2.00 mm Dual Socket Header THT,14 Pins</description>
</package>
<package name="62004021821">
<description>&lt;b&gt;WR-PHD&lt;/b&gt;&lt;br&gt; 2.00 mm Dual Socket Header THT,40 Pins</description>
</package>
<package name="621312284521">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Angled Dual Pin Header,12 Pins</description>
</package>
<package name="621316242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header (Reel), 16Pins</description>
</package>
<package name="621016242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header,16 Pins</description>
</package>
<package name="621320284521">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Angled Dual Pin Header,20 Pins</description>
</package>
<package name="621304242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header (Reel), 4 Pins</description>
</package>
<package name="621006242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header,6 Pins</description>
</package>
<package name="62003211821">
<description>WR-PHD 2.00 mm Socket Header 32p, 1 row, straight, gold plating;</description>
</package>
<package name="621320242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header (Reel), 20 Pins</description>
</package>
<package name="621010242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header,10 Pins</description>
</package>
<package name="621314284521">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm SMT Angled Dual Pin Header,14Pins</description>
</package>
<package name="62000811821">
<description>&lt;b&gt;WR-PHD 2.00mm Socket Header, 8 Pins</description>
</package>
<package name="621020242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header,20 Pins</description>
</package>
<package name="62004421821">
<description>&lt;b&gt;WR-PHD&lt;/b&gt;&lt;br&gt; 2.00 mm Dual Socket Header THT, 44 Pins</description>
</package>
<package name="621324242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header (Reel), 24 Pins</description>
</package>
<package name="621014242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header,14 Pins</description>
</package>
<package name="621344242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header (Reel), 44 Pins</description>
</package>
<package name="621310242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header (Reel), 10 Pins</description>
</package>
<package name="62101421821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Low Profile,14 Pins</description>
</package>
<package name="62100621821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Low Profile,6 Pins</description>
</package>
<package name="621024242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header,24 Pins</description>
</package>
<package name="62101621821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Low Profile,16 Pins</description>
</package>
<package name="621308242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header (Reel), 8 Pins</description>
</package>
<package name="621044242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header,44 Pins</description>
</package>
<package name="62100421821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Low Profile,4 Pins</description>
</package>
<package name="62130421821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Low Profile (Reel),4 Pins</description>
</package>
<package name="621306242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header (Reel), 6 Pins</description>
</package>
<package name="62131021821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Low Profile (Reel),10 Pins</description>
</package>
<package name="62100821821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Low Profile,8 Pins</description>
</package>
<package name="621104284621">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Angled,4 Pins</description>
</package>
<package name="62130621821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Low Profile (Reel),6 Pins</description>
</package>
<package name="62102021821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Low Profile, 20 Pins</description>
</package>
<package name="621314242921">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header (Reel), 14 Pins</description>
</package>
<package name="62130821821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Low Profile (Reel),08 Pins</description>
</package>
<package name="621120284621">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Angled,20 Pins</description>
</package>
<package name="62200421121">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm THT Dual Pin Header, 4 Pins&lt;b&gt;</description>
</package>
<package name="62131621821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Low Profile (Reel),18 Pins</description>
</package>
<package name="62101021821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Low Profile,10 Pins</description>
</package>
<package name="621114284621">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Angled,14 Pins</description>
</package>
<package name="62201021121">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm THT Dual Pin Header,10 Pins&lt;b&gt;</description>
</package>
<package name="62102421821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Low Profile, 24 Pins</description>
</package>
<package name="62132021821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Low Profile (Reel),20Pins</description>
</package>
<package name="62101021021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm, 10Pins&lt;b&gt;</description>
</package>
<package name="621108284621">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Angled,8 Pins</description>
</package>
<package name="621116284621">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Angled,16 Pins</description>
</package>
<package name="621110284621">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Angled,10 Pins</description>
</package>
<package name="62102821021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm, 28 Pins</description>
</package>
<package name="621112284621">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Angled,12 Pins</description>
</package>
<package name="62130421021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm, 4Pins&lt;b&gt;</description>
</package>
<package name="62202021121">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm THT Dual Pin Header, 20 Pins&lt;b&gt;</description>
</package>
<package name="62200821121">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm THT Dual Pin Header, 8 Pins&lt;b&gt;</description>
</package>
<package name="62131421821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Low Profile (Reel),14 Pins</description>
</package>
<package name="62105021021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm, 50 Pins</description>
</package>
<package name="62100821021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm,  8 Pins&lt;b&gt;</description>
</package>
<package name="62132421821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Low Profile (Reel),24 Pins</description>
</package>
<package name="62102021021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm, 20 Pins</description>
</package>
<package name="62135021021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm, 50Pins&lt;b&gt;</description>
</package>
<package name="62134421021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm, 44Pins&lt;b&gt;</description>
</package>
<package name="62101421021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm,  14 Pins&lt;b&gt;</description>
</package>
<package name="62100421021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm, 4 Pins&lt;b&gt;</description>
</package>
<package name="62104421021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm,  44 Pins&lt;b&gt;</description>
</package>
<package name="62201421121">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm THT Dual Pin Header,14 Pins&lt;b&gt;</description>
</package>
<package name="62132021021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm, 20Pins&lt;b&gt;</description>
</package>
<package name="62101621021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm, 16 Pins</description>
</package>
<package name="62131021021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm, 10Pins&lt;b&gt;</description>
</package>
<package name="623350235521">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt; 1.27 mm SMT Dual Pin Header, H=1.80 mm,50 Pins&lt;b&gt;</description>
</package>
<package name="62132821021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm, 28Pins&lt;b&gt;</description>
</package>
<package name="62131421021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm,14Pins&lt;b&gt;</description>
</package>
<package name="623310235321">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt; 1.27 mm SMT Dual Socket Header Bottom Entry, H=2.20 mm (Reel), 10 Pins&lt;b&gt;</description>
</package>
<package name="623326235321">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt; 1.27 mm SMT Dual Socket Header Bottom Entry, H=2.20 mm (Reel), 26 Pins&lt;b&gt;</description>
</package>
<package name="62202821121">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm THT Dual Pin Header, 28 Pins&lt;b&gt;</description>
</package>
<package name="62131621021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm,16Pins&lt;b&gt;</description>
</package>
<package name="62130821021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm, 8Pins&lt;b&gt;</description>
</package>
<package name="62201021821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm Dual Socket Header, 10 Pins&lt;b&gt;</description>
</package>
<package name="623310235521">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt; 1.27 mm SMT Dual Pin Header, H=1.80 mm, 10 Pins</description>
</package>
<package name="62134021021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm, 40Pins&lt;b&gt;</description>
</package>
<package name="62201621821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm Dual Socket Header,  16 Pins&lt;b&gt;</description>
</package>
<package name="62104021021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm,  40 Pins&lt;b&gt;</description>
</package>
<package name="62130621021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm, 6Pins&lt;b&gt;</description>
</package>
<package name="62200821821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm Dual Socket Header, 8 Pins&lt;b&gt;</description>
</package>
<package name="62300421021">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;1.27 mm SMT Dual Socket Header, H=4.50 mm, 4 Pins&lt;b&gt;</description>
</package>
<package name="61001513321">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54mm SMT Socket Header, 16 Pins</description>
</package>
<package name="62201421821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm Dual Socket Header, 14 Pins&lt;b&gt;</description>
</package>
<package name="62200421821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm Dual Socket Header, 4 Pins&lt;b&gt;</description>
</package>
<package name="623350235321">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt; 1.27 mm SMT Dual Socket Header Bottom Entry, H=2.20 mm (Reel), 50 Pins&lt;b&gt;</description>
</package>
<package name="623326235521">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt; 1.27 mm SMT Dual Pin Header, H=1.80 mm,26 Pins&lt;b&gt;</description>
</package>
<package name="62331421021">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;1.27 mm SMT Dual Socket Header, H=4.50 mm (Reel), 14 Pins&lt;b&gt;</description>
</package>
<package name="62301021021">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;1.27 mm SMT Dual Socket Header, H=4.50 mm,  10 Pins&lt;b&gt;</description>
</package>
<package name="61301511821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Socket Header, 15 Pins</description>
</package>
<package name="62301621021">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;1.27 mm SMT Dual Socket Header, H=4.50 mm, 16 Pins&lt;b&gt;</description>
</package>
<package name="621106284621">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;2.00 mm Dual SMT Socket Header Angled,6 Pins</description>
</package>
<package name="613015143121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54 mm Angled Socket Header, 15 Pins</description>
</package>
<package name="62202021821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm Dual Socket Header, 20 Pins&lt;b&gt;</description>
</package>
<package name="610040243021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm SMT Dual Socket Header Bottom Entry, 40 Pins</description>
</package>
<package name="62330421021">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;1.27 mm SMT Dual Socket Header, H=4.50 mm (Reel), 4 Pins&lt;b&gt;</description>
</package>
<package name="62331021021">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;1.27 mm SMT Dual Socket Header, H=4.50 mm (Reel), 10 Pins&lt;b&gt;</description>
</package>
<package name="61301621021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54 mm THT Angled Dual Pin Header, 16 Pins</description>
</package>
<package name="61301511021">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Angled Pin Header, 15 Pins</description>
</package>
<package name="62302821021">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;1.27 mm SMT Dual Socket Header, H=4.50 mm, 28 Pins&lt;b&gt;</description>
</package>
<package name="61001518221">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;  2.54 mm SMT Pin Headerr, 15 Pins</description>
</package>
<package name="62301421021">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;1.27 mm SMT Dual Socket Header, H=4.50 mm,  14 Pins&lt;b&gt;</description>
</package>
<package name="62332021021">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;1.27 mm SMT Dual Socket Header, H=4.50 mm (Reel), 20 Pins&lt;b&gt;</description>
</package>
<package name="61001511921">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;2.54 mm SMT Socket Header, 15 Pins</description>
</package>
<package name="62330821021">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;1.27 mm SMT Dual Socket Header, H=4.50 mm (Reel), 8 Pins&lt;b&gt;</description>
</package>
<package name="62331621021">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;1.27 mm SMT Dual Socket Header, H=4.50 mm (Reel), 16 Pins&lt;b&gt;</description>
</package>
<package name="62300821021">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;1.27 mm SMT Dual Socket Header, H=4.50 mm,  8 Pins&lt;b&gt;</description>
</package>
<package name="62201621121">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm THT Dual Pin Header,16 Pins&lt;b&gt;</description>
</package>
<package name="613040216921">
<description>&lt;b&gt;WR-PHD&lt;/b&gt; &lt;br&gt;2.54 mm Dual Socket Header Bottom Entry Large, 40 Pins</description>
</package>
<package name="62332821021">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;1.27 mm SMT Dual Socket Header, H=4.50 mm (Reel), 28 Pins&lt;b&gt;</description>
</package>
<package name="62302021021">
<description>&lt;B&gt;WR-PHD&lt;/B&gt;&lt;BR&gt;1.27 mm SMT Dual Socket Header, H=4.50 mm, 20 Pins&lt;b&gt;</description>
</package>
<package name="62202821821">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm Dual Socket Header, 28 Pins&lt;b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="15PS">
<description>Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="15X2SS">
<description>15X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
</symbol>
<symbol name="14X2SS">
<description>14X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
</symbol>
<symbol name="4PS_1">
<description>Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="36X2PT_1">
<description>36X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
<pin name="51" direction="pas"/>
<pin name="52" direction="pas"/>
<pin name="53" direction="pas"/>
<pin name="54" direction="pas"/>
<pin name="55" direction="pas"/>
<pin name="56" direction="pas"/>
<pin name="57" direction="pas"/>
<pin name="58" direction="pas"/>
<pin name="59" direction="pas"/>
<pin name="60" direction="pas"/>
<pin name="61" direction="pas"/>
<pin name="62" direction="pas"/>
<pin name="63" direction="pas"/>
<pin name="64" direction="pas"/>
<pin name="65" direction="pas"/>
<pin name="66" direction="pas"/>
<pin name="67" direction="pas"/>
<pin name="68" direction="pas"/>
<pin name="69" direction="pas"/>
<pin name="70" direction="pas"/>
<pin name="71" direction="pas"/>
<pin name="72" direction="pas"/>
</symbol>
<symbol name="2X2PT_1">
<description>2X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="12ST">
<description>Socket Header THT,12Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="40PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="36ST">
<description>Socket Header THT,36Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
</symbol>
<symbol name="7X2PS">
<description>7X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="15X2PT">
<description>15X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
</symbol>
<symbol name="32PS">
<description>Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
</symbol>
<symbol name="3ST">
<description>Socket Header THT,3Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="20X2ST">
<description>20X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="16PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="4X2ST">
<description>4X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="22PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="6ST">
<description>Socket Header THT,6Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="9X2ST">
<description>9X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="18X2ST">
<description>18X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
</symbol>
<symbol name="3X2PT_1">
<description>3X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="2PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="18X2PT">
<description>18X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
</symbol>
<symbol name="20ST">
<description>Socket Header THT,20Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="12PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="6PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="3X2PS">
<description>3X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="8ST">
<description>Socket Header THT,8Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="8X2PS">
<description>8X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="15X2ST">
<description>15X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
</symbol>
<symbol name="10PS">
<description>Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="4ST">
<description>Socket Header THT,4Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="36PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
</symbol>
<symbol name="2ST">
<description>Socket Header THT,2Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="6X2PS">
<description>6X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="5PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="20PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="32PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
</symbol>
<symbol name="6X2PT_1">
<description>6X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="17X2ST">
<description>17X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="16X2PS">
<description>16X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
</symbol>
<symbol name="11X2PT_1">
<description>11X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="10X2ST">
<description>10X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="32PS_1">
<description>Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
</symbol>
<symbol name="14X2ST">
<description>14X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
</symbol>
<symbol name="9ST">
<description>Socket Header THT,9Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="36X2ST">
<description>36X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
<pin name="51" direction="pas"/>
<pin name="52" direction="pas"/>
<pin name="53" direction="pas"/>
<pin name="54" direction="pas"/>
<pin name="55" direction="pas"/>
<pin name="56" direction="pas"/>
<pin name="57" direction="pas"/>
<pin name="58" direction="pas"/>
<pin name="59" direction="pas"/>
<pin name="60" direction="pas"/>
<pin name="61" direction="pas"/>
<pin name="62" direction="pas"/>
<pin name="63" direction="pas"/>
<pin name="64" direction="pas"/>
<pin name="65" direction="pas"/>
<pin name="66" direction="pas"/>
<pin name="67" direction="pas"/>
<pin name="68" direction="pas"/>
<pin name="69" direction="pas"/>
<pin name="70" direction="pas"/>
<pin name="71" direction="pas"/>
<pin name="72" direction="pas"/>
</symbol>
<symbol name="6X2ST">
<description>6X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="32ST">
<description>Socket Header THT,32Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
</symbol>
<symbol name="8X2PT">
<description>8X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="4X2PS">
<description>4X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="3X2ST">
<description>3X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="24ST">
<description>Socket Header THT,24Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="2X2ST">
<description>2X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="3X2PS_1">
<description>3X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="6PS">
<description>Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="36X2PT">
<description>36X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
<pin name="51" direction="pas"/>
<pin name="52" direction="pas"/>
<pin name="53" direction="pas"/>
<pin name="54" direction="pas"/>
<pin name="55" direction="pas"/>
<pin name="56" direction="pas"/>
<pin name="57" direction="pas"/>
<pin name="58" direction="pas"/>
<pin name="59" direction="pas"/>
<pin name="60" direction="pas"/>
<pin name="61" direction="pas"/>
<pin name="62" direction="pas"/>
<pin name="63" direction="pas"/>
<pin name="64" direction="pas"/>
<pin name="65" direction="pas"/>
<pin name="66" direction="pas"/>
<pin name="67" direction="pas"/>
<pin name="68" direction="pas"/>
<pin name="69" direction="pas"/>
<pin name="70" direction="pas"/>
<pin name="71" direction="pas"/>
<pin name="72" direction="pas"/>
</symbol>
<symbol name="6X2PS_1">
<description>6X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="12PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="17X2PS">
<description>17X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="16PS">
<description>Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="14PS_1">
<description>Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="11ST">
<description>Socket Header THT,11Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="24PS_1">
<description>Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="32X2PT">
<description>32X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
<pin name="51" direction="pas"/>
<pin name="52" direction="pas"/>
<pin name="53" direction="pas"/>
<pin name="54" direction="pas"/>
<pin name="55" direction="pas"/>
<pin name="56" direction="pas"/>
<pin name="57" direction="pas"/>
<pin name="58" direction="pas"/>
<pin name="59" direction="pas"/>
<pin name="60" direction="pas"/>
<pin name="61" direction="pas"/>
<pin name="62" direction="pas"/>
<pin name="63" direction="pas"/>
<pin name="64" direction="pas"/>
</symbol>
<symbol name="16ST">
<description>Socket Header THT,16Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="13X2PS">
<description>13X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="40X2PT">
<description>40X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
<pin name="51" direction="pas"/>
<pin name="52" direction="pas"/>
<pin name="53" direction="pas"/>
<pin name="54" direction="pas"/>
<pin name="55" direction="pas"/>
<pin name="56" direction="pas"/>
<pin name="57" direction="pas"/>
<pin name="58" direction="pas"/>
<pin name="59" direction="pas"/>
<pin name="60" direction="pas"/>
<pin name="61" direction="pas"/>
<pin name="62" direction="pas"/>
<pin name="63" direction="pas"/>
<pin name="64" direction="pas"/>
<pin name="65" direction="pas"/>
<pin name="66" direction="pas"/>
<pin name="67" direction="pas"/>
<pin name="68" direction="pas"/>
<pin name="69" direction="pas"/>
<pin name="70" direction="pas"/>
<pin name="71" direction="pas"/>
<pin name="72" direction="pas"/>
<pin name="73" direction="pas"/>
<pin name="74" direction="pas"/>
<pin name="75" direction="pas"/>
<pin name="76" direction="pas"/>
<pin name="77" direction="pas"/>
<pin name="78" direction="pas"/>
<pin name="79" direction="pas"/>
<pin name="80" direction="pas"/>
</symbol>
<symbol name="13PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="16X2PT">
<description>16X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
</symbol>
<symbol name="5ST">
<description>Socket Header THT,5Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="25PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
</symbol>
<symbol name="5PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="8PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="4PS">
<description>Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="22PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="2X2PS">
<description>2X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="4X2PT">
<description>4X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="12X2ST">
<description>12X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="5X2ST">
<description>5X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="5X2PT_1">
<description>5X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="15PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
</symbol>
<symbol name="4X2PT_1">
<description>4X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="5X2PS_1">
<description>5X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="8ST_1">
<description>Socket Header THT,8Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="16X2PT_1">
<description>16X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
</symbol>
<symbol name="18ST">
<description>Socket Header THT,18Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="10PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="10PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="32X2PT_1">
<description>32X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
<pin name="51" direction="pas"/>
<pin name="52" direction="pas"/>
<pin name="53" direction="pas"/>
<pin name="54" direction="pas"/>
<pin name="55" direction="pas"/>
<pin name="56" direction="pas"/>
<pin name="57" direction="pas"/>
<pin name="58" direction="pas"/>
<pin name="59" direction="pas"/>
<pin name="60" direction="pas"/>
<pin name="61" direction="pas"/>
<pin name="62" direction="pas"/>
<pin name="63" direction="pas"/>
<pin name="64" direction="pas"/>
</symbol>
<symbol name="18PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="22ST">
<description>Socket Header THT,22Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="14PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="13X2ST">
<description>13X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="22X2PT">
<description>22X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
</symbol>
<symbol name="3PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="12X2PT">
<description>12X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="7ST">
<description>Socket Header THT,7Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="13ST">
<description>Socket Header THT,13Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="13X2PS_1">
<description>13X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="22X2ST">
<description>22X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
</symbol>
<symbol name="12X2PT_1">
<description>12X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="10X2PT_1">
<description>10X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="24PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="40PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="9X2PT_1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="11X2PS">
<description>11X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="7X2ST">
<description>7X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="10ST">
<description>Socket Header THT,10Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="2PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="4PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="34PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="8PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="2X2PT">
<description>2X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="4X2PS_1">
<description>4X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="34PS">
<description>Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="6PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="25ST">
<description>Socket Header THT,25Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
</symbol>
<symbol name="5X2PT">
<description>5X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="5X2PS">
<description>5X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="14PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="16X2ST">
<description>16X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
</symbol>
<symbol name="18X2PT_1">
<description>18X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
</symbol>
<symbol name="17X2PT_1">
<description>17X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="11X2PS_1">
<description>11X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="14X2PT">
<description>14X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
</symbol>
<symbol name="40ST">
<description>Socket Header THT,40Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="1PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="8X2ST">
<description>8X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="24PS">
<description>Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="7X2PT">
<description>7X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="20X2PT">
<description>20X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="7X2PS_1">
<description>7X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="12X2PS_1">
<description>12X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="3PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="32X2ST">
<description>32X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
<pin name="51" direction="pas"/>
<pin name="52" direction="pas"/>
<pin name="53" direction="pas"/>
<pin name="54" direction="pas"/>
<pin name="55" direction="pas"/>
<pin name="56" direction="pas"/>
<pin name="57" direction="pas"/>
<pin name="58" direction="pas"/>
<pin name="59" direction="pas"/>
<pin name="60" direction="pas"/>
<pin name="61" direction="pas"/>
<pin name="62" direction="pas"/>
<pin name="63" direction="pas"/>
<pin name="64" direction="pas"/>
</symbol>
<symbol name="4PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="7PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="7PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="6ST_1">
<description>Socket Header THT,6Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="18PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="36PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
</symbol>
<symbol name="18X2PS">
<description>18X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
</symbol>
<symbol name="11X2PT">
<description>11X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="9PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="4ST_1">
<description>Socket Header THT,4Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="9X2PT">
<description>9X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="10X2PS_1">
<description>10X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="10X2PS">
<description>10X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="20X2PT_1">
<description>20X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="10X2PT">
<description>10X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="9PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="5ST_1">
<description>Socket Header THT,5Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="6X2PT">
<description>6X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="32PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
</symbol>
<symbol name="11X2ST">
<description>11X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="6PS_1">
<description>Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="13X2PT_1">
<description>13X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="16PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="17X2PT">
<description>17X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="12X2PS">
<description>12X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="8X2PS_1">
<description>8X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="7X2PT_1">
<description>7X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="14ST">
<description>Socket Header THT,14Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="36PS">
<description>Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
</symbol>
<symbol name="13X2PT">
<description>13X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="10ST_1">
<description>Socket Header THT,10Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="16PS_1">
<description>8X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="20ST_1">
<description>Socket Header THT,20Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="3X2PT">
<description>3X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="2X2SS">
<description>2X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="4X2SS">
<description>4X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="6X2SS">
<description>6X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="9X2SS">
<description>9X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="5X2SS">
<description>5X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="8X2SS">
<description>8X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="3X2SS">
<description>3X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="17X2SS">
<description>17X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="10X2SS">
<description>10X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="10SS">
<description>Socket Header SMT,10Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="11X2SS">
<description>11X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="10PS_1">
<description>Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="12SS">
<description>Socket Header SMT,12Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="6SS">
<description>Socket Header SMT,6Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="5SS">
<description>Socket Header SMT,5Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="12X2SS">
<description>12X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="13X2SS">
<description>13X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="10X2SS_1">
<description>10X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="8SS">
<description>Socket Header SMT,8Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="4SS_1">
<description>Socket Header SMT,4Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="6SS_1">
<description>Socket Header SMT,6Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="12X2SS_1">
<description>12X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="3X2SS_1">
<description>3X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="16X2SS">
<description>16X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
</symbol>
<symbol name="16SS">
<description>Socket Header SMT,16Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="20SS_1">
<description>Socket Header SMT,20Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="20SS">
<description>Socket Header SMT,20Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="4SS">
<description>Socket Header SMT,4Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="10SS_1">
<description>Socket Header SMT,10Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="13X2SS_1">
<description>13X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
</symbol>
<symbol name="11X2SS_1">
<description>11X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
</symbol>
<symbol name="15X2SS_1">
<description>15X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
</symbol>
<symbol name="5X2SS_1">
<description>5X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="16SS_1">
<description>Socket Header SMT,16Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="24SS_1">
<description>Socket Header SMT,24Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="18X2SS_1">
<description>18X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
</symbol>
<symbol name="14X2SS_1">
<description>14X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
</symbol>
<symbol name="8SS_1">
<description>Socket Header SMT,8Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="2X2SS_1">
<description>2X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="7X2SS_1">
<description>7X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="24SS">
<description>Socket Header SMT,24Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="8X2SS_1">
<description>8X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="6X2SS_1">
<description>6X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="16X2SS_1">
<description>16X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
</symbol>
<symbol name="12SS_1">
<description>Socket Header SMT,12Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="14SS_1">
<description>Socket Header SMT,14Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="5SS_1">
<description>Socket Header SMT,5Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="20X2SS_1">
<description>20X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="4X2SS_1">
<description>4X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="9X2SS_1">
<description>9X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="7X2SS">
<description>7X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="17X2SS_1">
<description>17X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
</symbol>
<symbol name="22X2PS">
<description>22X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
</symbol>
<symbol name="2X2PS_1">
<description>2X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="22X2SS">
<description>22X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
</symbol>
<symbol name="2X2SS_RIGHTBOTTOM">
<description>2X2 Dual Socket Heade SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="10X2SS_RIGHTBOTTOM">
<description>10X2Row Dual Socket Heade SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="7X2SS_RIGHTBOTTOM">
<description>7X2Row Dual Socket Heade SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="4X2SS_RIGHTBOTTOM">
<description>4X2Row Dual Socket Heade SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="8X2SS_RIGHTBOTTOM">
<description>8X2Row Dual Socket Heade SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="14X2PS">
<description>14X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
</symbol>
<symbol name="5X2SS_RIGHTBOTTOM">
<description>5X2Row Dual Socket Heade SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="6X2SS_RIGHTBOTTOM">
<description>6X2Row Dual Socket Heade SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="25X2PS">
<description>25X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
</symbol>
<symbol name="20X2PS">
<description>20X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="5X2ST_RIGHTBOTTOM">
<description>5X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="7X2ST_RIGHTBOTTOM">
<description>7X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="8X2ST_RIGHTBOTTOM">
<description>8X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="15ST">
<description>Socket Header THT,14Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
</symbol>
<symbol name="4X2ST_RIGHTBOTTOM">
<description>4X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="15SS_1">
<description>Socket Header SMT,14Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
</symbol>
<symbol name="2X2ST_RIGHTBOTTOM">
<description>2X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="25X2SS">
<description>25X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
</symbol>
<symbol name="3X2SS_RIGHTBOTTOM">
<description>3X2 Dual Socket Heade SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="10X2ST_RIGHTBOTTOM">
<description>10X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="20X2SS">
<description>17X2Row Socket Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="15PT_1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
</symbol>
<symbol name="14X2SS_RIGHTBOTTOM">
<description>10X2Row Dual Socket Heade SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
</symbol>
<symbol name="8X2PT_1">
<description>8X2Row Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="15PS_1">
<description>8X2Row Pin Header SMT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
</symbol>
<symbol name="15SS">
<description>Socket Header SMT,15Pins</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
</symbol>
<symbol name="14X2ST_RIGHTBOTTOM">
<description>14X2Row Socket Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="6100XX18221_61000418221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 10 unitless; 14 unitless; 15 unitless; 16 unitless; 24 unitless; 32 unitless; 34 unitless; 36 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_PIN_HEADER_6100XX18X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_PIN_HEADER_6100XX18X21&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-18&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PS_1"/>
</gates>
<devices>
<device name="" package="61000418221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000418221?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000418221"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61000418221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61301211821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST"/>
</gates>
<devices>
<device name="" package="61301211821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301211821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61301211821"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301211821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX18321_61003218321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 10 unitless; 14 unitless; 15 unitless; 16 unitless; 24 unitless; 32 unitless; 34 unitless; 36 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_PIN_HEADER_6100XX18X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_PIN_HEADER_6100XX18X21&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-18&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32PS"/>
</gates>
<devices>
<device name="" package="61003218321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61003218321?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61003218321"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61003218321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21121_61031421121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:max.
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;Packaging:Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2021-11-04
&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PS"/>
</gates>
<devices>
<device name="" package="61031421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61031421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61031421121"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61031421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61304011121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="40PT"/>
</gates>
<devices>
<device name="" package="61304011121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61304011121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61304011121"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61304011121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61307221021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="36X2PT_1"/>
</gates>
<devices>
<device name="" package="61307221021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="65" pad="65"/>
<connect gate="G$1" pin="66" pad="66"/>
<connect gate="G$1" pin="67" pad="67"/>
<connect gate="G$1" pin="68" pad="68"/>
<connect gate="G$1" pin="69" pad="69"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="70" pad="70"/>
<connect gate="G$1" pin="71" pad="71"/>
<connect gate="G$1" pin="72" pad="72"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61307221021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61307221021"/>
<attribute name="PINS" value=" 72 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61307221021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61303611821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="36ST"/>
</gates>
<devices>
<device name="" package="61303611821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303611821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61303611821"/>
<attribute name="PINS" value=" 36 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61303611821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX18321_61001018321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 10 unitless; 14 unitless; 15 unitless; 16 unitless; 24 unitless; 32 unitless; 34 unitless; 36 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_PIN_HEADER_6100XX18X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_PIN_HEADER_6100XX18X21&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-18&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PS"/>
</gates>
<devices>
<device name="" package="61001018321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001018321?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001018321"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61001018321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61303611121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="36PT"/>
</gates>
<devices>
<device name="" package="61303611121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303611121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61303611121"/>
<attribute name="PINS" value=" 36 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61303611121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61300411821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="61300411821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300411821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61300411821"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300411821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61300421021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PT_1"/>
</gates>
<devices>
<device name="" package="61300421021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300421021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300421021"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61300421021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61303021121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15X2PT"/>
</gates>
<devices>
<device name="" package="61303021121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303021121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61303021121"/>
<attribute name="PINS" value=" 30 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61303021121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61301221021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2PT_1"/>
</gates>
<devices>
<device name="" package="61301221021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301221021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301221021"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61301221021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613002143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="613002143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613002143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613002143121"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613002143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX18221_61003218221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 10 unitless; 14 unitless; 15 unitless; 16 unitless; 24 unitless; 32 unitless; 34 unitless; 36 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_PIN_HEADER_6100XX18X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_PIN_HEADER_6100XX18X21&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-18&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32PS_1"/>
</gates>
<devices>
<device name="" package="61003218221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61003218221?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61003218221"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61003218221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61302011121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20PT"/>
</gates>
<devices>
<device name="" package="61302011121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302011121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61302011121"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302011121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21121_61003221121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16X2PS"/>
</gates>
<devices>
<device name="" package="61003221121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61003221121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61003221121"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61003221121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61303421821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2ST"/>
</gates>
<devices>
<device name="" package="61303421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61303421821"/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61303421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130321XX21_61303211321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:32
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33208v209%20Family_WR-PHD_6130321xx21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33208v209%20Family_WR-PHD_6130321xx21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_BOARD_STACKER_6130321XX21"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_BOARD_STACKER_6130321XX21&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32PT"/>
</gates>
<devices>
<device name="" package="61303211321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303211321?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61303211321"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Board Stacker"/>
<attribute name="VALUE" value="61303211321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61302021821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2ST"/>
</gates>
<devices>
<device name="" package="61302021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61302021821"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61304021821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2ST"/>
</gates>
<devices>
<device name="" package="61304021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61304021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61304021821"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61304021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21121_61001221121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2PS"/>
</gates>
<devices>
<device name="" package="61001221121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001221121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001221121"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61001221121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613006143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="613006143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613006143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613006143121"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613006143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21121_61031221121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:max.
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;Packaging:Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2021-11-04
&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2PS"/>
</gates>
<devices>
<device name="" package="61031221121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61031221121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61031221121"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61031221121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61302211121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22PT"/>
</gates>
<devices>
<device name="" package="61302211121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302211121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61302211121"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302211121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61300911821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9ST"/>
</gates>
<devices>
<device name="" package="61300911821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300911821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61300911821"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300911821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61300311821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="61300311821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300311821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61300311821"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300311821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61301611021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16PT_1"/>
</gates>
<devices>
<device name="" package="61301611021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301611021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301611021"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61301611021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61300821821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2ST"/>
</gates>
<devices>
<device name="" package="61300821821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300821821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61300821821"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300821821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX243121_613012243121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins	4; 6; 8; 10; 12; 14; 16; 20; 22; 24; 26; 32; 34; 40; 64; 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-13&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2ST"/>
</gates>
<devices>
<device name="" package="613012243121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613012243121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613012243121"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613012243121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61301821821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2ST"/>
</gates>
<devices>
<device name="" package="61301821821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301821821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61301821821"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301821821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21121_61001621121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PS"/>
</gates>
<devices>
<device name="" package="61001621121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001621121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001621121"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61001621121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61307221821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="36X2ST"/>
</gates>
<devices>
<device name="" package="61307221821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="65" pad="65"/>
<connect gate="G$1" pin="66" pad="66"/>
<connect gate="G$1" pin="67" pad="67"/>
<connect gate="G$1" pin="68" pad="68"/>
<connect gate="G$1" pin="69" pad="69"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="70" pad="70"/>
<connect gate="G$1" pin="71" pad="71"/>
<connect gate="G$1" pin="72" pad="72"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61307221821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61307221821"/>
<attribute name="PINS" value=" 72 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61307221821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61302411821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24ST"/>
</gates>
<devices>
<device name="" package="61302411821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302411821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61302411821"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302411821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61303021821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15X2ST"/>
</gates>
<devices>
<device name="" package="61303021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61303021821"/>
<attribute name="PINS" value=" 30 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61303021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249121_610106249121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header Double Row Right Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 600 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PS_1"/>
</gates>
<devices>
<device name="" package="610106249121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610106249121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610106249121"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610106249121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61300421821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2ST"/>
</gates>
<devices>
<device name="" package="61300421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61300421821"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61303211821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32ST"/>
</gates>
<devices>
<device name="" package="61303211821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303211821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61303211821"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61303211821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61302821821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14X2ST"/>
</gates>
<devices>
<device name="" package="61302821821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302821821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61302821821"/>
<attribute name="PINS" value=" 28 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302821821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61301621121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PT"/>
</gates>
<devices>
<device name="" package="61301621121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301621121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301621121"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301621121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61301211121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT"/>
</gates>
<devices>
<device name="" package="61301211121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301211121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301211121"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301211121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21121_61030821121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:max.
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;Packaging:Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2021-11-04
&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PS"/>
</gates>
<devices>
<device name="" package="61030821121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61030821121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61030821121"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61030821121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61303621121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18X2PT"/>
</gates>
<devices>
<device name="" package="61303621121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303621121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61303621121"/>
<attribute name="PINS" value=" 36 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61303621121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61302011821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20ST"/>
</gates>
<devices>
<device name="" package="61302011821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302011821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61302011821"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302011821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61300621021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PT_1"/>
</gates>
<devices>
<device name="" package="61300621021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300621021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300621021"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61300621021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61300211021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT_1"/>
</gates>
<devices>
<device name="" package="61300211021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300211021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300211021"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61300211021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61303621821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18X2ST"/>
</gates>
<devices>
<device name="" package="61303621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61303621821"/>
<attribute name="PINS" value=" 36 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61303621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61300611021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT_1"/>
</gates>
<devices>
<device name="" package="61300611021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300611021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300611021"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61300611021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61300811821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="61300811821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300811821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61300811821"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300811821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61301211021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12PT_1"/>
</gates>
<devices>
<device name="" package="61301211021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301211021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301211021"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61301211021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61300511021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT_1"/>
</gates>
<devices>
<device name="" package="61300511021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300511021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300511021"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61300511021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61302221021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2PT_1"/>
</gates>
<devices>
<device name="" package="61302221021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302221021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61302221021"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61302221021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21121_61000621121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PS"/>
</gates>
<devices>
<device name="" package="61000621121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000621121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000621121"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61000621121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX18321_61000618321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 10 unitless; 14 unitless; 15 unitless; 16 unitless; 24 unitless; 32 unitless; 34 unitless; 36 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_PIN_HEADER_6100XX18X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_PIN_HEADER_6100XX18X21&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-18&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PS"/>
</gates>
<devices>
<device name="" package="61000618321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000618321?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000618321"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61000618321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61300621821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2ST"/>
</gates>
<devices>
<device name="" package="61300621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61300621821"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX18221_61001418221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 10 unitless; 14 unitless; 15 unitless; 16 unitless; 24 unitless; 32 unitless; 34 unitless; 36 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_PIN_HEADER_6100XX18X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_PIN_HEADER_6100XX18X21&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-18&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14PS_1"/>
</gates>
<devices>
<device name="" package="61001418221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001418221?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001418221"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61001418221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249121_610112249121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header Double Row Right Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 600 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2PS_1"/>
</gates>
<devices>
<device name="" package="610112249121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610112249121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610112249121"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610112249121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613011143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11ST"/>
</gates>
<devices>
<device name="" package="613011143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613011143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613011143121"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613011143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613003143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3ST"/>
</gates>
<devices>
<device name="" package="613003143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613003143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613003143121"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613003143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61307221121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="36X2PT"/>
</gates>
<devices>
<device name="" package="61307221121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="65" pad="65"/>
<connect gate="G$1" pin="66" pad="66"/>
<connect gate="G$1" pin="67" pad="67"/>
<connect gate="G$1" pin="68" pad="68"/>
<connect gate="G$1" pin="69" pad="69"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="70" pad="70"/>
<connect gate="G$1" pin="71" pad="71"/>
<connect gate="G$1" pin="72" pad="72"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61307221121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61307221121"/>
<attribute name="PINS" value=" 72 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61307221121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21121_61003421121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2PS"/>
</gates>
<devices>
<device name="" package="61003421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61003421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61003421121"/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61003421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX18321_61001618321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 10 unitless; 14 unitless; 15 unitless; 16 unitless; 24 unitless; 32 unitless; 34 unitless; 36 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_PIN_HEADER_6100XX18X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_PIN_HEADER_6100XX18X21&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-18&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16PS"/>
</gates>
<devices>
<device name="" package="61001618321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001618321?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001618321"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61001618321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130642XX21_61306428521" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Board Stacker &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:64
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33209v209%20Family_WR-PHD_6130642xx21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33209v209%20Family_WR-PHD_6130642xx21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_BOARD_STACKER_6130642XX21"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_BOARD_STACKER_6130642XX21&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32X2PT"/>
</gates>
<devices>
<device name="" package="61306428521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61306428521?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61306428521"/>
<attribute name="PINS" value=" 64 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Board Stacker"/>
<attribute name="VALUE" value="61306428521"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX18221_61002418221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 10 unitless; 14 unitless; 15 unitless; 16 unitless; 24 unitless; 32 unitless; 34 unitless; 36 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_PIN_HEADER_6100XX18X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_PIN_HEADER_6100XX18X21&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-18&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24PS_1"/>
</gates>
<devices>
<device name="" package="61002418221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61002418221?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61002418221"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61002418221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613016143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16ST"/>
</gates>
<devices>
<device name="" package="613016143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613016143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613016143121"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613016143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX243121_613004243121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins	4; 6; 8; 10; 12; 14; 16; 20; 22; 24; 26; 32; 34; 40; 64; 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-13&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2ST"/>
</gates>
<devices>
<device name="" package="613004243121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613004243121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613004243121"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613004243121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21121_61002621121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2PS"/>
</gates>
<devices>
<device name="" package="61002621121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61002621121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61002621121"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61002621121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX243121_613008243121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins	4; 6; 8; 10; 12; 14; 16; 20; 22; 24; 26; 32; 34; 40; 64; 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-13&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2ST"/>
</gates>
<devices>
<device name="" package="613008243121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613008243121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613008243121"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613008243121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61301311121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13PT"/>
</gates>
<devices>
<device name="" package="61301311121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301311121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301311121"/>
<attribute name="PINS" value=" 13 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301311121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613005143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="613005143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613005143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613005143121"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613005143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61308021121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="40X2PT"/>
</gates>
<devices>
<device name="" package="61308021121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="65" pad="65"/>
<connect gate="G$1" pin="66" pad="66"/>
<connect gate="G$1" pin="67" pad="67"/>
<connect gate="G$1" pin="68" pad="68"/>
<connect gate="G$1" pin="69" pad="69"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="70" pad="70"/>
<connect gate="G$1" pin="71" pad="71"/>
<connect gate="G$1" pin="72" pad="72"/>
<connect gate="G$1" pin="73" pad="73"/>
<connect gate="G$1" pin="74" pad="74"/>
<connect gate="G$1" pin="75" pad="75"/>
<connect gate="G$1" pin="76" pad="76"/>
<connect gate="G$1" pin="77" pad="77"/>
<connect gate="G$1" pin="78" pad="78"/>
<connect gate="G$1" pin="79" pad="79"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="80" pad="80"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61308021121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61308021121"/>
<attribute name="PINS" value=" 80 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61308021121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61300811021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT_1"/>
</gates>
<devices>
<device name="" package="61300811021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300811021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300811021"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61300811021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61303221121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16X2PT"/>
</gates>
<devices>
<device name="" package="61303221121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303221121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61303221121"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61303221121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61302511121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25PT"/>
</gates>
<devices>
<device name="" package="61302511121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302511121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61302511121"/>
<attribute name="PINS" value=" 25 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302511121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX18321_61000418321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 10 unitless; 14 unitless; 15 unitless; 16 unitless; 24 unitless; 32 unitless; 34 unitless; 36 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_PIN_HEADER_6100XX18X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_PIN_HEADER_6100XX18X21&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-18&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PS"/>
</gates>
<devices>
<device name="" package="61000418321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000418321?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000418321"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61000418321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130642XX21_61306421321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Board Stacker &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:64
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33209v209%20Family_WR-PHD_6130642xx21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33209v209%20Family_WR-PHD_6130642xx21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_BOARD_STACKER_6130642XX21"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_BOARD_STACKER_6130642XX21&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32X2PT"/>
</gates>
<devices>
<device name="" package="61306421321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61306421321?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61306421321"/>
<attribute name="PINS" value=" 64 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Board Stacker"/>
<attribute name="VALUE" value="61306421321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61300511121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="61300511121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300511121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300511121"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300511121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130642XX21_61306428421" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Board Stacker &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:64
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33209v209%20Family_WR-PHD_6130642xx21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33209v209%20Family_WR-PHD_6130642xx21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_BOARD_STACKER_6130642XX21"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_BOARD_STACKER_6130642XX21&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32X2PT"/>
</gates>
<devices>
<device name="" package="61306428421">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61306428421?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61306428421"/>
<attribute name="PINS" value=" 64 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Board Stacker"/>
<attribute name="VALUE" value="61306428421"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61302211021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22PT_1"/>
</gates>
<devices>
<device name="" package="61302211021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302211021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61302211021"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61302211021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61300821121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PT"/>
</gates>
<devices>
<device name="" package="61300821121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300821121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300821121"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300821121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61302421821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2ST"/>
</gates>
<devices>
<device name="" package="61302421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61302421821"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21121_61000421121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PS"/>
</gates>
<devices>
<device name="" package="61000421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000421121"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61000421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130321XX21_61303218521" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:32
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33208v209%20Family_WR-PHD_6130321xx21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33208v209%20Family_WR-PHD_6130321xx21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_BOARD_STACKER_6130321XX21"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_BOARD_STACKER_6130321XX21&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32PT"/>
</gates>
<devices>
<device name="" package="61303218521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303218521?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61303218521"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Board Stacker"/>
<attribute name="VALUE" value="61303218521"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61301021821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2ST"/>
</gates>
<devices>
<device name="" package="61301021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61301021821"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61301021021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PT_1"/>
</gates>
<devices>
<device name="" package="61301021021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301021021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301021021"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61301021021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61306421121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32X2PT"/>
</gates>
<devices>
<device name="" package="61306421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61306421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61306421121"/>
<attribute name="PINS" value=" 64 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61306421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21121_61001421121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PS"/>
</gates>
<devices>
<device name="" package="61001421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001421121"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61001421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61306421021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32X2PT_1"/>
</gates>
<devices>
<device name="" package="61306421021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61306421021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61306421021"/>
<attribute name="PINS" value=" 64 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61306421021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61301511121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15PT"/>
</gates>
<devices>
<device name="" package="61301511121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301511121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301511121"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301511121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61300821021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PT_1"/>
</gates>
<devices>
<device name="" package="61300821021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300821021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300821021"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61300821021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61301011121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="61301011121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301011121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301011121"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301011121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613018143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18ST"/>
</gates>
<devices>
<device name="" package="613018143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613018143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613018143121"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613018143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61303221021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16X2PT_1"/>
</gates>
<devices>
<device name="" package="61303221021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303221021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61303221021"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61303221021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249121_610110249121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header Double Row Right Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 600 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PS_1"/>
</gates>
<devices>
<device name="" package="610110249121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610110249121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610110249121"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610110249121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX15721_61300815721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 5;​ 6;​ 8;​ 10;​ 20
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR1:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33213v209%20Family_WR-PHD_6130xx15721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33213v209%20Family_WR-PHD_6130xx15721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SOCKET_HEADER_BOTTOM_ENTRY_6130XX15721"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SOCKET_HEADER_BOTTOM_ENTRY_6130XX15721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2021-12-08
&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST_1"/>
</gates>
<devices>
<device name="" package="61300815721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300815721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61300815721"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61300815721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613020143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20ST"/>
</gates>
<devices>
<device name="" package="613020143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613020143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613020143121"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613020143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61301811121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18PT"/>
</gates>
<devices>
<device name="" package="61301811121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301811121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301811121"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301811121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61302211821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22ST"/>
</gates>
<devices>
<device name="" package="61302211821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302211821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61302211821"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302211821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61301111821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11ST"/>
</gates>
<devices>
<device name="" package="61301111821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301111821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61301111821"/>
<attribute name="PINS" value=" 11 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301111821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61302621821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2ST"/>
</gates>
<devices>
<device name="" package="61302621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61302621821"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61301011021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT_1"/>
</gates>
<devices>
<device name="" package="61301011021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301011021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301011021"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61301011021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61304421121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2PT"/>
</gates>
<devices>
<device name="" package="61304421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61304421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61304421121"/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61304421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61302421121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PT"/>
</gates>
<devices>
<device name="" package="61302421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61302421121"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61301411121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14PT"/>
</gates>
<devices>
<device name="" package="61301411121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301411121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301411121"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301411121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61300311121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="61300311121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300311121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300311121"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300311121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613012143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12ST"/>
</gates>
<devices>
<device name="" package="613012143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613012143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613012143121"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613012143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613013143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13ST"/>
</gates>
<devices>
<device name="" package="613013143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613013143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613013143121"/>
<attribute name="PINS" value=" 13 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613013143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61304421821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2ST"/>
</gates>
<devices>
<device name="" package="61304421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61304421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61304421821"/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61304421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61302421021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PT_1"/>
</gates>
<devices>
<device name="" package="61302421021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302421021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61302421021"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61302421021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613007143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST"/>
</gates>
<devices>
<device name="" package="613007143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613007143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613007143121"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613007143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61301821021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2PT_1"/>
</gates>
<devices>
<device name="" package="61301821021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301821021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301821021"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61301821021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61302411121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24PT"/>
</gates>
<devices>
<device name="" package="61302411121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302411121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61302411121"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302411121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61302021021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PT_1"/>
</gates>
<devices>
<device name="" package="61302021021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302021021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61302021021"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61302021021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613008143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="613008143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613008143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613008143121"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613008143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249121_610126249121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header Double Row Right Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 600 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2PS_1"/>
</gates>
<devices>
<device name="" package="610126249121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610126249121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610126249121"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610126249121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21121_61002221121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2PS"/>
</gates>
<devices>
<device name="" package="61002221121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61002221121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61002221121"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61002221121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX243121_613010243121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins	4; 6; 8; 10; 12; 14; 16; 20; 22; 24; 26; 32; 34; 40; 64; 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-13&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2ST"/>
</gates>
<devices>
<device name="" package="613010243121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613010243121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613010243121"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613010243121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613036143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="36ST"/>
</gates>
<devices>
<device name="" package="613036143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613036143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613036143121"/>
<attribute name="PINS" value=" 36 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613036143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX243121_613014243121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins	4; 6; 8; 10; 12; 14; 16; 20; 22; 24; 26; 32; 34; 40; 64; 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-13&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2ST"/>
</gates>
<devices>
<device name="" package="613014243121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613014243121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613014243121"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613014243121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613010143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10ST"/>
</gates>
<devices>
<device name="" package="613010143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613010143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613010143121"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613010143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61300211121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="61300211121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300211121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300211121"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300211121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61304011021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="40PT_1"/>
</gates>
<devices>
<device name="" package="61304011021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61304011021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61304011021"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61304011021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130321XX21_61303211221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:32
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33208v209%20Family_WR-PHD_6130321xx21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33208v209%20Family_WR-PHD_6130321xx21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_BOARD_STACKER_6130321XX21"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_BOARD_STACKER_6130321XX21&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32PT"/>
</gates>
<devices>
<device name="" package="61303211221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303211221?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61303211221"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Board Stacker"/>
<attribute name="VALUE" value="61303211221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61300421121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PT"/>
</gates>
<devices>
<device name="" package="61300421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300421121"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61300411121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="61300411121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300411121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300411121"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300411121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61300811121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="61300811121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300811121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300811121"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300811121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61303411021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="34PT_1"/>
</gates>
<devices>
<device name="" package="61303411021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303411021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61303411021"/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61303411021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249121_610108249121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header Double Row Right Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 600 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PS_1"/>
</gates>
<devices>
<device name="" package="610108249121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610108249121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610108249121"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610108249121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613009143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9ST"/>
</gates>
<devices>
<device name="" package="613009143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613009143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613009143121"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613009143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX243121_613040243121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins	4; 6; 8; 10; 12; 14; 16; 20; 22; 24; 26; 32; 34; 40; 64; 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-13&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2ST"/>
</gates>
<devices>
<device name="" package="613040243121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613040243121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613040243121"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613040243121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX18321_61003418321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 10 unitless; 14 unitless; 15 unitless; 16 unitless; 24 unitless; 32 unitless; 34 unitless; 36 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_PIN_HEADER_6100XX18X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_PIN_HEADER_6100XX18X21&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-18&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="34PS"/>
</gates>
<devices>
<device name="" package="61003418321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61003418321?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61003418321"/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61003418321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61301021121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PT"/>
</gates>
<devices>
<device name="" package="61301021121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301021121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301021121"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301021121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61302511821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25ST"/>
</gates>
<devices>
<device name="" package="61302511821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302511821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61302511821"/>
<attribute name="PINS" value=" 25 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302511821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61301411021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14PT_1"/>
</gates>
<devices>
<device name="" package="61301411021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301411021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301411021"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61301411021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61300611121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="61300611121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300611121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300611121"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300611121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21121_61001021121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PS"/>
</gates>
<devices>
<device name="" package="61001021121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001021121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001021121"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61001021121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61303221821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16X2ST"/>
</gates>
<devices>
<device name="" package="61303221821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303221821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61303221821"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61303221821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61304011821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="40ST"/>
</gates>
<devices>
<device name="" package="61304011821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61304011821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61304011821"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61304011821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61303621021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18X2PT_1"/>
</gates>
<devices>
<device name="" package="61303621021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303621021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61303621021"/>
<attribute name="PINS" value=" 36 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61303621021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61303421021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2PT_1"/>
</gates>
<devices>
<device name="" package="61303421021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303421021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61303421021"/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61303421021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61300111121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1PT"/>
</gates>
<devices>
<device name="" package="61300111121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300111121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300111121"/>
<attribute name="PINS" value=" 1 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300111121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX243121_613016243121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins	4; 6; 8; 10; 12; 14; 16; 20; 22; 24; 26; 32; 34; 40; 64; 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-13&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2ST"/>
</gates>
<devices>
<device name="" package="613016243121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613016243121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613016243121"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613016243121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61302821121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14X2PT"/>
</gates>
<devices>
<device name="" package="61302821121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302821121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61302821121"/>
<attribute name="PINS" value=" 28 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302821121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61301011821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10ST"/>
</gates>
<devices>
<device name="" package="61301011821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301011821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61301011821"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301011821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249121_610122249121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header Double Row Right Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 600 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2PS_1"/>
</gates>
<devices>
<device name="" package="610122249121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610122249121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610122249121"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610122249121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61306421821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32X2ST"/>
</gates>
<devices>
<device name="" package="61306421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61306421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61306421821"/>
<attribute name="PINS" value=" 64 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61306421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX18321_61002418321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 10 unitless; 14 unitless; 15 unitless; 16 unitless; 24 unitless; 32 unitless; 34 unitless; 36 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_PIN_HEADER_6100XX18X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_PIN_HEADER_6100XX18X21&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-18&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24PS"/>
</gates>
<devices>
<device name="" package="61002418321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61002418321?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61002418321"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61002418321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61301421121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PT"/>
</gates>
<devices>
<device name="" package="61301421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301421121"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61304021121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2PT"/>
</gates>
<devices>
<device name="" package="61304021121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61304021121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61304021121"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61304021121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249121_610114249121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header Double Row Right Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 600 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PS_1"/>
</gates>
<devices>
<device name="" package="610114249121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610114249121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610114249121"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610114249121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61300311021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT_1"/>
</gates>
<devices>
<device name="" package="61300311021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300311021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300311021"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61300311021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61300411021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT_1"/>
</gates>
<devices>
<device name="" package="61300411021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300411021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300411021"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61300411021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249121_610124249121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header Double Row Right Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 600 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PS_1"/>
</gates>
<devices>
<device name="" package="610124249121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610124249121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610124249121"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610124249121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61300711121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="61300711121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300711121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300711121"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300711121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61300711821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7ST"/>
</gates>
<devices>
<device name="" package="61300711821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300711821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61300711821"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300711821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61301221821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2ST"/>
</gates>
<devices>
<device name="" package="61301221821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301221821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61301221821"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301221821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX15721_61300615721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 5;​ 6;​ 8;​ 10;​ 20
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR1:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33213v209%20Family_WR-PHD_6130xx15721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33213v209%20Family_WR-PHD_6130xx15721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SOCKET_HEADER_BOTTOM_ENTRY_6130XX15721"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SOCKET_HEADER_BOTTOM_ENTRY_6130XX15721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2021-12-08
&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST_1"/>
</gates>
<devices>
<device name="" package="61300615721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300615721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61300615721"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61300615721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21121_61000821121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PS"/>
</gates>
<devices>
<device name="" package="61000821121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000821121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000821121"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61000821121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61300211821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="61300211821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300211821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61300211821"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300211821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61303211121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32PT"/>
</gates>
<devices>
<device name="" package="61303211121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303211121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61303211121"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61303211121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61301811021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18PT_1"/>
</gates>
<devices>
<device name="" package="61301811021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301811021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301811021"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61301811021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61300711021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT_1"/>
</gates>
<devices>
<device name="" package="61300711021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300711021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300711021"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61300711021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61301311821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13ST"/>
</gates>
<devices>
<device name="" package="61301311821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301311821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61301311821"/>
<attribute name="PINS" value=" 13 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301311821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21121_61031021121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:max.
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;Packaging:Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2021-11-04
&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PS"/>
</gates>
<devices>
<device name="" package="61031021121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61031021121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61031021121"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61031021121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21121_61030621121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:max.
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;Packaging:Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2021-11-04
&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PS"/>
</gates>
<devices>
<device name="" package="61030621121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61030621121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61030621121"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61030621121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX243121_613006243121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins	4; 6; 8; 10; 12; 14; 16; 20; 22; 24; 26; 32; 34; 40; 64; 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-13&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2ST"/>
</gates>
<devices>
<device name="" package="613006243121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613006243121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613006243121"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613006243121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61303611021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="36PT_1"/>
</gates>
<devices>
<device name="" package="61303611021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303611021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61303611021"/>
<attribute name="PINS" value=" 36 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61303611021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX243121_613024243121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins	4; 6; 8; 10; 12; 14; 16; 20; 22; 24; 26; 32; 34; 40; 64; 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-13&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2ST"/>
</gates>
<devices>
<device name="" package="613024243121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613024243121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613024243121"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613024243121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61302221121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2PT"/>
</gates>
<devices>
<device name="" package="61302221121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302221121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61302221121"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302221121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21121_61003621121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18X2PS"/>
</gates>
<devices>
<device name="" package="61003621121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61003621121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61003621121"/>
<attribute name="PINS" value=" 36 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61003621121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61301811821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18ST"/>
</gates>
<devices>
<device name="" package="61301811821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301811821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61301811821"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301811821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX15721_61300415721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 5;​ 6;​ 8;​ 10;​ 20
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR1:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33213v209%20Family_WR-PHD_6130xx15721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33213v209%20Family_WR-PHD_6130xx15721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SOCKET_HEADER_BOTTOM_ENTRY_6130XX15721"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SOCKET_HEADER_BOTTOM_ENTRY_6130XX15721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2021-12-08
&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST_1"/>
</gates>
<devices>
<device name="" package="61300415721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300415721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61300415721"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61300415721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61300911021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT_1"/>
</gates>
<devices>
<device name="" package="61300911021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300911021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300911021"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61300911021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130321XX21_61303218421" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:32
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33208v209%20Family_WR-PHD_6130321xx21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33208v209%20Family_WR-PHD_6130321xx21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_BOARD_STACKER_6130321XX21"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_BOARD_STACKER_6130321XX21&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32PT"/>
</gates>
<devices>
<device name="" package="61303218421">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303218421?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61303218421"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Board Stacker"/>
<attribute name="VALUE" value="61303218421"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249121_610120249121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header Double Row Right Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 600 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PS_1"/>
</gates>
<devices>
<device name="" package="610120249121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610120249121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610120249121"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610120249121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX243121_613034243121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins	4; 6; 8; 10; 12; 14; 16; 20; 22; 24; 26; 32; 34; 40; 64; 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-13&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2ST"/>
</gates>
<devices>
<device name="" package="613034243121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613034243121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613034243121"/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613034243121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613032143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32ST"/>
</gates>
<devices>
<device name="" package="613032143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613032143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613032143121"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613032143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21121_61032021121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:max.
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;Packaging:Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2021-11-04
&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PS"/>
</gates>
<devices>
<device name="" package="61032021121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61032021121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61032021121"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61032021121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX243121_613032243121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins	4; 6; 8; 10; 12; 14; 16; 20; 22; 24; 26; 32; 34; 40; 64; 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-13&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16X2ST"/>
</gates>
<devices>
<device name="" package="613032243121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613032243121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613032243121"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613032243121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX25721_61301025721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 20;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-22
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2ST"/>
</gates>
<devices>
<device name="" package="61301025721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301025721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61301025721"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61301025721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61301821121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2PT"/>
</gates>
<devices>
<device name="" package="61301821121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301821121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301821121"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301821121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX25721_61300825721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 20;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-22
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2ST"/>
</gates>
<devices>
<device name="" package="61300825721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300825721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61300825721"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61300825721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61302021121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PT"/>
</gates>
<devices>
<device name="" package="61302021121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302021121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61302021121"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302021121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX15721_61300515721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 5;​ 6;​ 8;​ 10;​ 20
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR1:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33213v209%20Family_WR-PHD_6130xx15721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33213v209%20Family_WR-PHD_6130xx15721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SOCKET_HEADER_BOTTOM_ENTRY_6130XX15721"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SOCKET_HEADER_BOTTOM_ENTRY_6130XX15721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2021-12-08
&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST_1"/>
</gates>
<devices>
<device name="" package="61300515721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300515721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61300515721"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61300515721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61304021021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2PT_1"/>
</gates>
<devices>
<device name="" package="61304021021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61304021021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61304021021"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61304021021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61300911121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT"/>
</gates>
<devices>
<device name="" package="61300911121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300911121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300911121"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300911121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61301221121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2PT"/>
</gates>
<devices>
<device name="" package="61301221121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301221121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301221121"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301221121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61301611821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16ST"/>
</gates>
<devices>
<device name="" package="61301611821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301611821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61301611821"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301611821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX25721_61301625721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 20;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-22
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2ST"/>
</gates>
<devices>
<device name="" package="61301625721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301625721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61301625721"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61301625721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61301421821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2ST"/>
</gates>
<devices>
<device name="" package="61301421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61301421821"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61303211021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32PT_1"/>
</gates>
<devices>
<device name="" package="61303211021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303211021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61303211021"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61303211021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX18221_61000618221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 10 unitless; 14 unitless; 15 unitless; 16 unitless; 24 unitless; 32 unitless; 34 unitless; 36 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_PIN_HEADER_6100XX18X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_PIN_HEADER_6100XX18X21&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-18&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PS_1"/>
</gates>
<devices>
<device name="" package="61000618221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000618221?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000618221"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61000618221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61302221821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2ST"/>
</gates>
<devices>
<device name="" package="61302221821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302221821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61302221821"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302221821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61302621021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2PT_1"/>
</gates>
<devices>
<device name="" package="61302621021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302621021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61302621021"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61302621021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613004143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="613004143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613004143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613004143121"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613004143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11121_61301611121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:1;​ 2;​ 3;​ 4;​ 5;​ 6;​ 7;​ 8;​ 9;​ 10;​ 12;​ 13;​ 14;​ 15;​ 16;​ 18;​ 20;​ 22;​ 24;​ 25;​ 32;​ 36;​ 40
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA6T; PBT 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 500 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33211v209%20Family_BTB_PHD_6130xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121"&gt;https://www.we-online.com/katalog/en/em/PHD_2_54_THT_PIN_HEADER_6130XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16PT"/>
</gates>
<devices>
<device name="" package="61301611121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301611121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301611121"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301611121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX243121_613072243121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins	4; 6; 8; 10; 12; 14; 16; 20; 22; 24; 26; 32; 34; 40; 64; 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-13&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="36X2ST"/>
</gates>
<devices>
<device name="" package="613072243121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="65" pad="65"/>
<connect gate="G$1" pin="66" pad="66"/>
<connect gate="G$1" pin="67" pad="67"/>
<connect gate="G$1" pin="68" pad="68"/>
<connect gate="G$1" pin="69" pad="69"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="70" pad="70"/>
<connect gate="G$1" pin="71" pad="71"/>
<connect gate="G$1" pin="72" pad="72"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613072243121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613072243121"/>
<attribute name="PINS" value=" 72 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613072243121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21821_61301621821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Straight
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PBT
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o57948v209%20Family_Dual_Socket_Header_WR-PHD_6130xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_6130XX21821&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-21
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2ST"/>
</gates>
<devices>
<device name="" package="61301621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61301621821"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249121_610116249121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header Double Row Right Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage 600 V (AC) 
&lt;BR&gt;Contact Resistance 20 mΩ 
&lt;BR&gt;RISO 1000 MΩ 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33203v209%20Family_WR-PHD_6101_xx249121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLED_PIN_HEADER_6101XX249121&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PS_1"/>
</gates>
<devices>
<device name="" package="610116249121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610116249121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610116249121"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610116249121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61300511821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5ST"/>
</gates>
<devices>
<device name="" package="61300511821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300511821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61300511821"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300511821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61301421021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PT_1"/>
</gates>
<devices>
<device name="" package="61301421021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301421021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301421021"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61301421021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61303421121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2PT"/>
</gates>
<devices>
<device name="" package="61303421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61303421121"/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61303421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21121_61002421121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PS"/>
</gates>
<devices>
<device name="" package="61002421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61002421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61002421121"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61002421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61301411821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14ST"/>
</gates>
<devices>
<device name="" package="61301411821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301411821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61301411821"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301411821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21121_61002021121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-18
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PS"/>
</gates>
<devices>
<device name="" package="61002021121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61002021121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61002021121"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61002021121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61302621121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2PT"/>
</gates>
<devices>
<device name="" package="61302621121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302621121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61302621121"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61302621121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX25721_61302025721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 20;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-22
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2ST"/>
</gates>
<devices>
<device name="" package="61302025721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302025721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61302025721"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61302025721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21121_61030421121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:max.
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;Packaging:Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2021-11-04
&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PS"/>
</gates>
<devices>
<device name="" package="61030421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61030421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61030421121"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61030421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21121_61031621121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Straight 
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:max.
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;Packaging:Tape and Reel with Cap
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33205v209%20Family_WR-PHD_610xxx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33205v209%20Family_WR-PHD_610xxx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_PIN_HEADER_6100XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2021-11-04
&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PS"/>
</gates>
<devices>
<device name="" package="61031621121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61031621121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61031621121"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61031621121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX243121_613022243121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins	4; 6; 8; 10; 12; 14; 16; 20; 22; 24; 26; 32; 34; 40; 64; 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-13&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2ST"/>
</gates>
<devices>
<device name="" package="613022243121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613022243121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613022243121"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613022243121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX25721_61300425721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 20;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-22
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2ST"/>
</gates>
<devices>
<device name="" package="61300425721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300425721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61300425721"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61300425721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX18321_61003618321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 10 unitless; 14 unitless; 15 unitless; 16 unitless; 24 unitless; 32 unitless; 34 unitless; 36 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_PIN_HEADER_6100XX18X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_PIN_HEADER_6100XX18X21&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-18&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="36PS"/>
</gates>
<devices>
<device name="" package="61003618321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61003618321?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61003618321"/>
<attribute name="PINS" value=" 36 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61003618321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX25721_61300625721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 20;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-22
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2ST"/>
</gates>
<devices>
<device name="" package="61300625721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300625721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61300625721"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61300625721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX243121_613020243121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins	4; 6; 8; 10; 12; 14; 16; 20; 22; 24; 26; 32; 34; 40; 64; 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-13&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2ST"/>
</gates>
<devices>
<device name="" package="613020243121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613020243121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613020243121"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613020243121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX15721_61301015721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 5;​ 6;​ 8;​ 10;​ 20
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR1:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33213v209%20Family_WR-PHD_6130xx15721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33213v209%20Family_WR-PHD_6130xx15721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SOCKET_HEADER_BOTTOM_ENTRY_6130XX15721"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SOCKET_HEADER_BOTTOM_ENTRY_6130XX15721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2021-12-08
&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10ST_1"/>
</gates>
<devices>
<device name="" package="61301015721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301015721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61301015721"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61301015721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130642XX21_61306421221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Board Stacker &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:64
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33209v209%20Family_WR-PHD_6130642xx21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33209v209%20Family_WR-PHD_6130642xx21.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_BOARD_STACKER_6130642XX21"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_BOARD_STACKER_6130642XX21&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32X2PT"/>
</gates>
<devices>
<device name="" package="61306421221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61306421221?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61306421221"/>
<attribute name="PINS" value=" 64 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Board Stacker"/>
<attribute name="VALUE" value="61306421221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX25721_61302425721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 20;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-22
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2ST"/>
</gates>
<devices>
<device name="" package="61302425721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302425721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61302425721"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61302425721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX216921_613010216921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry Large&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-23&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2ST"/>
</gates>
<devices>
<device name="" package="613010216921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613010216921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="613010216921"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Large"/>
<attribute name="VALUE" value="613010216921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX25721_61302625721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 20;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-22
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2ST"/>
</gates>
<devices>
<device name="" package="61302625721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302625721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61302625721"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61302625721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX18221_61001618221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 10 unitless; 14 unitless; 15 unitless; 16 unitless; 24 unitless; 32 unitless; 34 unitless; 36 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_PIN_HEADER_6100XX18X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_PIN_HEADER_6100XX18X21&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-18&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16PS_1"/>
</gates>
<devices>
<device name="" package="61001618221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001618221?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001618221"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61001618221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613024143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-22&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24ST"/>
</gates>
<devices>
<device name="" package="613024143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613024143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613024143121"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613024143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX25721_61303225721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 20;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-22
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16X2ST"/>
</gates>
<devices>
<device name="" package="61303225721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303225721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61303225721"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61303225721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX243121_613064243121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins	4; 6; 8; 10; 12; 14; 16; 20; 22; 24; 26; 32; 34; 40; 64; 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-13&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32X2ST"/>
</gates>
<devices>
<device name="" package="613064243121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613064243121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613064243121"/>
<attribute name="PINS" value=" 64 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613064243121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX15721_61302015721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 5;​ 6;​ 8;​ 10;​ 20
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Single
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR1:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33213v209%20Family_WR-PHD_6130xx15721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33213v209%20Family_WR-PHD_6130xx15721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SOCKET_HEADER_BOTTOM_ENTRY_6130XX15721"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SOCKET_HEADER_BOTTOM_ENTRY_6130XX15721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Ella Wu 2021-12-08
&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20ST_1"/>
</gates>
<devices>
<device name="" package="61302015721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61302015721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61302015721"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61302015721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX243121_613026243121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Dual Socket Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins	4; 6; 8; 10; 12; 14; 16; 20; 22; 24; 26; 32; 34; 40; 64; 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Packaging	Tray
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33216v209%20Family_WR-PHD_6130xx243121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_DUAL_SOCKET_HEADER_6130XX243121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-13&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2ST"/>
</gates>
<devices>
<device name="" package="613026243121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613026243121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613026243121"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613026243121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX216921_613008216921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry Large&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-23&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2ST"/>
</gates>
<devices>
<device name="" package="613008216921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613008216921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="613008216921"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Large"/>
<attribute name="VALUE" value="613008216921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX25721_61303425721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 20;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-22
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2ST"/>
</gates>
<devices>
<device name="" package="61303425721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61303425721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61303425721"/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61303425721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX216921_613012216921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry Large&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-23&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2ST"/>
</gates>
<devices>
<device name="" package="613012216921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613012216921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="613012216921"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Large"/>
<attribute name="VALUE" value="613012216921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX25721_61301225721" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 20;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA46
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR:3A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33217v209%20Family_WR-PHD_6130xx25721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721"&gt;https://katalog.we-online.com/en/em/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6130XX25721&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-22
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2ST"/>
</gates>
<devices>
<device name="" package="61301225721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301225721?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61301225721"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="61301225721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX216921_613004216921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry Large&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-23&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2ST"/>
</gates>
<devices>
<device name="" package="613004216921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613004216921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="613004216921"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Large"/>
<attribute name="VALUE" value="613004216921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX216921_613006216921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry Large&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-23&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2ST"/>
</gates>
<devices>
<device name="" package="613006216921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613006216921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="613006216921"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Large"/>
<attribute name="VALUE" value="613006216921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21121_61300621121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40;​ 44;​ 64;​ 72;​ 80
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33215v209%20Family_WR-PHD_6130xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_DUAL_PIN_HEADER_6130XX21121&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PT"/>
</gates>
<devices>
<device name="" package="61300621121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300621121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61300621121"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300621121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX216921_613022216921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry Large&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-23&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2ST"/>
</gates>
<devices>
<device name="" package="613022216921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613022216921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="613022216921"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Large"/>
<attribute name="VALUE" value="613022216921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX243021_610004243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy; Phosphor Bronze
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC); 600 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2SS"/>
</gates>
<devices>
<device name="" package="610004243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610004243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="610004243021"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610004243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX216921_613018216921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry Large&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-23&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2ST"/>
</gates>
<devices>
<device name="" package="613018216921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613018216921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="613018216921"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Large"/>
<attribute name="VALUE" value="613018216921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX243021_610008243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy; Phosphor Bronze
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC); 600 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2SS"/>
</gates>
<devices>
<device name="" package="610008243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610008243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="610008243021"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610008243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX243021_610312243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry Large
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2SS"/>
</gates>
<devices>
<device name="" package="610312243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610312243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="610312243021"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610312243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX216921_613026216921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry Large&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-23&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2ST"/>
</gates>
<devices>
<device name="" package="613026216921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613026216921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="613026216921"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Large"/>
<attribute name="VALUE" value="613026216921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX216921_613020216921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry Large&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-23&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2ST"/>
</gates>
<devices>
<device name="" package="613020216921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613020216921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="613020216921"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Large"/>
<attribute name="VALUE" value="613020216921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX243021_610310243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry Large
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-12-06&lt;BR&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2SS"/>
</gates>
<devices>
<device name="" package="610310243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610310243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="610310243021"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610310243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX243021_610316243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry Large
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2SS"/>
</gates>
<devices>
<device name="" package="610316243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610316243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="610316243021"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610316243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX243021_610018243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy; Phosphor Bronze
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC); 600 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2SS"/>
</gates>
<devices>
<device name="" package="610018243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610018243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="610018243021"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610018243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX243021_610318243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry Large
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2SS"/>
</gates>
<devices>
<device name="" package="610318243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610318243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="610318243021"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610318243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX243021_610020243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy; Phosphor Bronze
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC); 600 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2SS"/>
</gates>
<devices>
<device name="" package="610020243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610020243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="610020243021"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610020243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX216921_613016216921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry Large&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-23&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2ST"/>
</gates>
<devices>
<device name="" package="613016216921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613016216921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="613016216921"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Large"/>
<attribute name="VALUE" value="613016216921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX243021_610016243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy; Phosphor Bronze
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC); 600 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2SS"/>
</gates>
<devices>
<device name="" package="610016243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610016243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="610016243021"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610016243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61300611821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-11&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="61300611821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61300611821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61300611821"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61300611821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX243021_610034243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy; Phosphor Bronze
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC); 600 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2SS"/>
</gates>
<devices>
<device name="" package="610034243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610034243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="610034243021"/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610034243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX11921_61001011921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10SS"/>
</gates>
<devices>
<device name="" package="61001011921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001011921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001011921"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61001011921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX243021_610006243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy; Phosphor Bronze
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC); 600 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2SS"/>
</gates>
<devices>
<device name="" package="610006243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610006243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="610006243021"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610006243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX216921_613034216921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry Large&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-23&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2ST"/>
</gates>
<devices>
<device name="" package="613034216921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613034216921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="613034216921"/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Large"/>
<attribute name="VALUE" value="613034216921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX18221_61001018221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 10 unitless; 14 unitless; 15 unitless; 16 unitless; 24 unitless; 32 unitless; 34 unitless; 36 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_PIN_HEADER_6100XX18X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_PIN_HEADER_6100XX18X21&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-18&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PS_1"/>
</gates>
<devices>
<device name="" package="61001018221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001018221?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001018221"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61001018221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX11921_61001211921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12SS"/>
</gates>
<devices>
<device name="" package="61001211921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001211921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001211921"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61001211921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX243021_610012243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy; Phosphor Bronze
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC); 600 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2SS"/>
</gates>
<devices>
<device name="" package="610012243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610012243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="610012243021"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610012243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX243021_610022243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy; Phosphor Bronze
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC); 600 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2SS"/>
</gates>
<devices>
<device name="" package="610022243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610022243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="610022243021"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610022243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX243021_610306243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry Large
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2SS"/>
</gates>
<devices>
<device name="" package="610306243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610306243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="610306243021"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610306243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX11921_61000511921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5SS"/>
</gates>
<devices>
<device name="" package="61000511921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000511921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000511921"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61000511921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX243021_610024243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy; Phosphor Bronze
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC); 600 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2SS"/>
</gates>
<devices>
<device name="" package="610024243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610024243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="610024243021"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610024243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX243021_610320243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry Large
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2SS"/>
</gates>
<devices>
<device name="" package="610320243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610320243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="610320243021"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610320243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX11921_61000611921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6SS"/>
</gates>
<devices>
<device name="" package="61000611921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000611921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000611921"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61000611921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX243021_610304243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry Large
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-12-06&lt;BR&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2SS"/>
</gates>
<devices>
<device name="" package="610304243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610304243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="610304243021"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610304243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX243021_610026243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy; Phosphor Bronze
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC); 600 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2SS"/>
</gates>
<devices>
<device name="" package="610026243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610026243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="610026243021"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610026243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX243021_610010243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy; Phosphor Bronze
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC); 600 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2SS"/>
</gates>
<devices>
<device name="" package="610010243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610010243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="610010243021"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610010243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX243021_610308243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Bottom Entry Large
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material PA9T 
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +125 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging:Tube
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021"&gt;https://www.we-online.com/catalog/en/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2SS"/>
</gates>
<devices>
<device name="" package="610308243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610308243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="610308243021"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610308243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61002021821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2SS_1"/>
</gates>
<devices>
<device name="" package="61002021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61002021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61002021821"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61002021821"/>
<attribute name="WE-NUMBER" value="61002021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX11921_61000811921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8SS"/>
</gates>
<devices>
<device name="" package="61000811921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000811921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000811921"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61000811921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX13321_61000613321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6SS_1"/>
</gates>
<devices>
<device name="" package="61000613321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000613321?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000613321"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61000613321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61002421821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2SS_1"/>
</gates>
<devices>
<device name="" package="61002421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61002421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61002421821"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61002421821"/>
<attribute name="WE-NUMBER" value="61002421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX13321_61000413321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4SS_1"/>
</gates>
<devices>
<device name="" package="61000413321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000413321?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000413321"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61000413321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX216921_613032216921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry Large&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-23&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16X2ST"/>
</gates>
<devices>
<device name="" package="613032216921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613032216921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="613032216921"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Large"/>
<attribute name="VALUE" value="613032216921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61000621821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;�� 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2SS_1"/>
</gates>
<devices>
<device name="" package="61000621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000621821"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61000621821"/>
<attribute name="WE-NUMBER" value="61000621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX216921_613024216921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry Large&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-23&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2ST"/>
</gates>
<devices>
<device name="" package="613024216921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613024216921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="613024216921"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Large"/>
<attribute name="VALUE" value="613024216921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX11921_61001611921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16SS"/>
</gates>
<devices>
<device name="" package="61001611921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001611921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001611921"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61001611921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX243021_610032243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy; Phosphor Bronze
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC); 600 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;BR&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16X2SS"/>
</gates>
<devices>
<device name="" package="610032243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610032243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="610032243021"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610032243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX11921_61000411921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4SS"/>
</gates>
<devices>
<device name="" package="61000411921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000411921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000411921"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61000411921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61002221821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2SS_1"/>
</gates>
<devices>
<device name="" package="61002221821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61002221821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61002221821"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61002221821"/>
<attribute name="WE-NUMBER" value="61002221821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61002621821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2SS_1"/>
</gates>
<devices>
<device name="" package="61002621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61002621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61002621821"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61002621821"/>
<attribute name="WE-NUMBER" value="61002621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX13321_61002013321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20SS_1"/>
</gates>
<devices>
<device name="" package="61002013321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61002013321?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61002013321"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61002013321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX11921_61002011921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20SS"/>
</gates>
<devices>
<device name="" package="61002011921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61002011921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61002011921"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61002011921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX13321_61001013321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10SS_1"/>
</gates>
<devices>
<device name="" package="61001013321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001013321?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001013321"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61001013321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61003021821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15X2SS_1"/>
</gates>
<devices>
<device name="" package="61003021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61003021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61003021821"/>
<attribute name="PINS" value=" 30 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61003021821"/>
<attribute name="WE-NUMBER" value="61003021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61001021821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2SS_1"/>
</gates>
<devices>
<device name="" package="61001021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001021821"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61001021821"/>
<attribute name="WE-NUMBER" value="61001021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX13321_61002413321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24SS_1"/>
</gates>
<devices>
<device name="" package="61002413321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61002413321?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61002413321"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61002413321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61002821821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14X2SS_1"/>
</gates>
<devices>
<device name="" package="61002821821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61002821821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61002821821"/>
<attribute name="PINS" value=" 28 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61002821821"/>
<attribute name="WE-NUMBER" value="61002821821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX13321_61001613321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16SS_1"/>
</gates>
<devices>
<device name="" package="61001613321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001613321?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001613321"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61001613321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX13321_61000813321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8SS_1"/>
</gates>
<devices>
<device name="" package="61000813321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000813321?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000813321"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61000813321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61003621821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="18X2SS_1"/>
</gates>
<devices>
<device name="" package="61003621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61003621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61003621821"/>
<attribute name="PINS" value=" 36 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61003621821"/>
<attribute name="WE-NUMBER" value="61003621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61000421821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2SS_1"/>
</gates>
<devices>
<device name="" package="61000421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000421821"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61000421821"/>
<attribute name="WE-NUMBER" value="61000421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21821_61031421821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54 mm SMT Dual Socket Header (Reel)&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins ： 4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight Type 2 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA46 
Insulator Flammability Rating UL94 V-0 
Contact Material Copper Alloy 
Contact Plating Gold 
Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A 
&lt;br&gt;IR1 = 3A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;CERTIFICATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;UL Approval E323964 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tape and Reel with Cap  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2SS_1"/>
</gates>
<devices>
<device name="" package="61031421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61031421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61031421821"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61031421821"/>
<attribute name="WE-NUMBER" value="61031421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX11921_61002411921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="24SS"/>
</gates>
<devices>
<device name="" package="61002411921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61002411921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61002411921"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61002411921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61001621821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2SS_1"/>
</gates>
<devices>
<device name="" package="61001621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001621821"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61001621821"/>
<attribute name="WE-NUMBER" value="61001621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61001221821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2SS_1"/>
</gates>
<devices>
<device name="" package="61001221821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001221821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001221821"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61001221821"/>
<attribute name="WE-NUMBER" value="61001221821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61001421821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2SS_1"/>
</gates>
<devices>
<device name="" package="61001421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001421821"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61001421821"/>
<attribute name="WE-NUMBER" value="61001421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61003221821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16X2SS_1"/>
</gates>
<devices>
<device name="" package="61003221821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61003221821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61003221821"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61003221821"/>
<attribute name="WE-NUMBER" value="61003221821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX13321_61000513321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5SS_1"/>
</gates>
<devices>
<device name="" package="61000513321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000513321?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000513321"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61000513321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX13321_61001213321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12SS_1"/>
</gates>
<devices>
<device name="" package="61001213321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001213321?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001213321"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61001213321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61004021821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2SS_1"/>
</gates>
<devices>
<device name="" package="61004021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61004021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61004021821"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61004021821"/>
<attribute name="WE-NUMBER" value="61004021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249221_610108249221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:600 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-24
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2SS"/>
</gates>
<devices>
<device name="" package="610108249221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610108249221?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610108249221"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610108249221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX13321_61001413321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14SS_1"/>
</gates>
<devices>
<device name="" package="61001413321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001413321?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001413321"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61001413321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21821_61032021821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54 mm SMT Dual Socket Header (Reel)&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins ： 4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight Type 2 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA46 
Insulator Flammability Rating UL94 V-0 
Contact Material Copper Alloy 
Contact Plating Gold 
Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A 
&lt;br&gt;IR1 = 3A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;CERTIFICATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;UL Approval E323964 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tape and Reel with Cap  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2SS_1"/>
</gates>
<devices>
<device name="" package="61032021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61032021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61032021821"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61032021821"/>
<attribute name="WE-NUMBER" value="61032021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21821_61032621821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54 mm SMT Dual Socket Header (Reel)&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins ： 4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight Type 2 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA46 
Insulator Flammability Rating UL94 V-0 
Contact Material Copper Alloy 
Contact Plating Gold 
Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A 
&lt;br&gt;IR1 = 3A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;CERTIFICATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;UL Approval E323964 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tape and Reel with Cap  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2SS_1"/>
</gates>
<devices>
<device name="" package="61032621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61032621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61032621821"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61032621821"/>
<attribute name="WE-NUMBER" value="61032621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21821_61030821821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54 mm SMT Dual Socket Header (Reel)&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins ： 4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight Type 2 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA46 
Insulator Flammability Rating UL94 V-0 
Contact Material Copper Alloy 
Contact Plating Gold 
Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A 
&lt;br&gt;IR1 = 3A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;CERTIFICATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;UL Approval E323964 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tape and Reel with Cap  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2SS_1"/>
</gates>
<devices>
<device name="" package="61030821821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61030821821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61030821821"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61030821821"/>
<attribute name="WE-NUMBER" value="61030821821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249221_610112249221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:600 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-24
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2SS"/>
</gates>
<devices>
<device name="" package="610112249221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610112249221?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610112249221"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610112249221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21821_61031621821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54 mm SMT Dual Socket Header (Reel)&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins ： 4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight Type 2 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA46 
Insulator Flammability Rating UL94 V-0 
Contact Material Copper Alloy 
Contact Plating Gold 
Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A 
&lt;br&gt;IR1 = 3A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;CERTIFICATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;UL Approval E323964 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tape and Reel with Cap  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2SS_1"/>
</gates>
<devices>
<device name="" package="61031621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61031621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61031621821"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61031621821"/>
<attribute name="WE-NUMBER" value="61031621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61000821821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2SS_1"/>
</gates>
<devices>
<device name="" package="61000821821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61000821821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61000821821"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61000821821"/>
<attribute name="WE-NUMBER" value="61000821821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21821_61030421821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54 mm SMT Dual Socket Header (Reel)&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins ： 4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight Type 2 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA46 
Insulator Flammability Rating UL94 V-0 
Contact Material Copper Alloy 
Contact Plating Gold 
Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A 
&lt;br&gt;IR1 = 3A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;CERTIFICATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;UL Approval E323964 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tape and Reel with Cap  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2SS_1"/>
</gates>
<devices>
<device name="" package="61030421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61030421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61030421821"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61030421821"/>
<attribute name="WE-NUMBER" value="61030421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61001821821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2SS_1"/>
</gates>
<devices>
<device name="" package="61001821821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001821821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001821821"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61001821821"/>
<attribute name="WE-NUMBER" value="61001821821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21921_62133221921" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16X2PS"/>
</gates>
<devices>
<device name="" package="62133221921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/62133221921.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="MATES" value="WR-PHD 2.0mm Dual SMT Socket Header/ Socket Header(Reel)/ Socket Header Low Profile/Socket Header Low Profile(Reel)/Dual Socket Header"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 62133221921 "/>
<attribute name="PINS" value=""/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249221_610114249221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:600 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-24
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2SS"/>
</gates>
<devices>
<device name="" package="610114249221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610114249221?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610114249221"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610114249221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21121_62002021121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PT"/>
</gates>
<devices>
<device name="" package="62002021121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62002021121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62002021121"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62002021121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX11121_62000211121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  2 unitless; 3 unitless; 4 unitless; 6 unitless; 8 unitless; 10 unitless; 20 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33219v209%20Family_WR-PHD_6200xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33219v209%20Family_WR-PHD_6200xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_PIN_HEADER_6200XX11121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_PIN_HEADER_6200XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="62000211121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000211121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000211121"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62000211121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21821_61031821821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54 mm SMT Dual Socket Header (Reel)&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins ： 4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight Type 2 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA46 
Insulator Flammability Rating UL94 V-0 
Contact Material Copper Alloy 
Contact Plating Gold 
Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A 
&lt;br&gt;IR1 = 3A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;CERTIFICATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;UL Approval E323964 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tape and Reel with Cap  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9X2SS_1"/>
</gates>
<devices>
<device name="" package="61031821821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61031821821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61031821821"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61031821821"/>
<attribute name="WE-NUMBER" value="61031821821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21821_61031021821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54 mm SMT Dual Socket Header (Reel)&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins ： 4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight Type 2 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA46 
Insulator Flammability Rating UL94 V-0 
Contact Material Copper Alloy 
Contact Plating Gold 
Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A 
&lt;br&gt;IR1 = 3A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;CERTIFICATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;UL Approval E323964 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tape and Reel with Cap  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2SS_1"/>
</gates>
<devices>
<device name="" package="61031021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61031021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61031021821"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61031021821"/>
<attribute name="WE-NUMBER" value="61031021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX21821_61003421821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54mm SMT Socket Header&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins:  4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 28;​ 30;​ 32;​ 34;​ 36;​ 40 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 
&lt;br&gt;Compliance Lead free / RoHS 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A;​ max. 
&lt;br&gt;IR 1 3 A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tube 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821"&gt;http://katalog.we-online.de/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_6100XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="17X2SS_1"/>
</gates>
<devices>
<device name="" package="61003421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61003421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61003421821"/>
<attribute name="PINS" value=" 34 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61003421821"/>
<attribute name="WE-NUMBER" value="61003421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX11121_62000611121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  2 unitless; 3 unitless; 4 unitless; 6 unitless; 8 unitless; 10 unitless; 20 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33219v209%20Family_WR-PHD_6200xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33219v209%20Family_WR-PHD_6200xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_PIN_HEADER_6200XX11121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_PIN_HEADER_6200XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="62000611121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000611121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000611121"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62000611121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21821_61032421821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54 mm SMT Dual Socket Header (Reel)&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins ： 4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight Type 2 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA46 
Insulator Flammability Rating UL94 V-0 
Contact Material Copper Alloy 
Contact Plating Gold 
Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A 
&lt;br&gt;IR1 = 3A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;CERTIFICATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;UL Approval E323964 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tape and Reel with Cap  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2SS_1"/>
</gates>
<devices>
<device name="" package="61032421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61032421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61032421821"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61032421821"/>
<attribute name="WE-NUMBER" value="61032421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21821_61032221821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54 mm SMT Dual Socket Header (Reel)&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins ： 4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight Type 2 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA46 
Insulator Flammability Rating UL94 V-0 
Contact Material Copper Alloy 
Contact Plating Gold 
Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A 
&lt;br&gt;IR1 = 3A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;CERTIFICATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;UL Approval E323964 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tape and Reel with Cap  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2SS_1"/>
</gates>
<devices>
<device name="" package="61032221821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61032221821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61032221821"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61032221821"/>
<attribute name="WE-NUMBER" value="61032221821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX11121_62000311121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  2 unitless; 3 unitless; 4 unitless; 6 unitless; 8 unitless; 10 unitless; 20 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33219v209%20Family_WR-PHD_6200xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33219v209%20Family_WR-PHD_6200xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_PIN_HEADER_6200XX11121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_PIN_HEADER_6200XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="62000311121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000311121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000311121"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62000311121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX11121_62000411121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  2 unitless; 3 unitless; 4 unitless; 6 unitless; 8 unitless; 10 unitless; 20 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33219v209%20Family_WR-PHD_6200xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33219v209%20Family_WR-PHD_6200xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_PIN_HEADER_6200XX11121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_PIN_HEADER_6200XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="62000411121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000411121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000411121"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62000411121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249221_610106249221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:600 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-24
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2SS"/>
</gates>
<devices>
<device name="" package="610106249221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610106249221?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610106249221"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610106249221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249221_610120249221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:600 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-24
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2SS"/>
</gates>
<devices>
<device name="" package="610120249221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610120249221?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610120249221"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610120249221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21121_62001021121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PT"/>
</gates>
<devices>
<device name="" package="62001021121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62001021121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62001021121"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62001021121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249221_610122249221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:600 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-24
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="11X2SS"/>
</gates>
<devices>
<device name="" package="610122249221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610122249221?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610122249221"/>
<attribute name="PINS" value=" 22 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610122249221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249221_610116249221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:600 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-24
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2SS"/>
</gates>
<devices>
<device name="" package="610116249221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610116249221?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610116249221"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610116249221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX11121_62000811121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  2 unitless; 3 unitless; 4 unitless; 6 unitless; 8 unitless; 10 unitless; 20 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33219v209%20Family_WR-PHD_6200xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33219v209%20Family_WR-PHD_6200xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_PIN_HEADER_6200XX11121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_PIN_HEADER_6200XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="62000811121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000811121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000811121"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62000811121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249221_610110249221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:600 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-24
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2SS"/>
</gates>
<devices>
<device name="" package="610110249221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610110249221?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610110249221"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610110249221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX11121_62001011121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  2 unitless; 3 unitless; 4 unitless; 6 unitless; 8 unitless; 10 unitless; 20 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33219v209%20Family_WR-PHD_6200xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33219v209%20Family_WR-PHD_6200xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_PIN_HEADER_6200XX11121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_PIN_HEADER_6200XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="62001011121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62001011121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62001011121"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62001011121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21821_61030621821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54 mm SMT Dual Socket Header (Reel)&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins ： 4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight Type 2 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA46 
Insulator Flammability Rating UL94 V-0 
Contact Material Copper Alloy 
Contact Plating Gold 
Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A 
&lt;br&gt;IR1 = 3A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;CERTIFICATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;UL Approval E323964 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tape and Reel with Cap  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2SS_1"/>
</gates>
<devices>
<device name="" package="61030621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61030621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61030621821"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61030621821"/>
<attribute name="WE-NUMBER" value="61030621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21921_62100821921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PS"/>
</gates>
<devices>
<device name="" package="62100821921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62100821921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62100821921"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62100821921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249221_610124249221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:600 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-24
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2SS"/>
</gates>
<devices>
<device name="" package="610124249221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610124249221?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610124249221"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610124249221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6101XX249221_610126249221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm PCB Socket Header - SMT Type - Double Row - Right Angle&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 20;​ 22;​ 24;​ 26
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Socket Header
&lt;BR&gt;Type：Angled
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:Lead free / RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:600 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Tape and Reel
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33204v209%20Family_WR-PHD_6101_xx249221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DOUBLE_ROW_RIGHT_ANGLE_PCB_SOCKET_HEADER_6101XX249221&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-24
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2SS"/>
</gates>
<devices>
<device name="" package="610126249221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610126249221?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="610126249221"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="610126249221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21121_62004021121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2PT"/>
</gates>
<devices>
<device name="" package="62004021121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62004021121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62004021121"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62004021121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21921_62101021921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PS"/>
</gates>
<devices>
<device name="" package="62101021921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62101021921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62101021921"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62101021921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21921_62132421921" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PS"/>
</gates>
<devices>
<device name="" package="62132421921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/62132421921.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="MATES" value="WR-PHD 2.0mm Dual SMT Socket Header/ Socket Header(Reel)/ Socket Header Low Profile/Socket Header Low Profile(Reel)/Dual Socket Header"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 62132421921 "/>
<attribute name="PINS" value=""/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21921_62134421921" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2PS"/>
</gates>
<devices>
<device name="" package="62134421921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/62134421921.pdf"/>
<attribute name="GENDER" value="Male"/>
<attribute name="IR" value="2A"/>
<attribute name="MATES" value="WR-PHD 2.0mm Dual SMT Socket Header/ Socket Header(Reel)/ Socket Header Low Profile/Socket Header Low Profile(Reel)/Dual Socket Header"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value=" 62134421921 "/>
<attribute name="PINS" value=""/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21121_62000821121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PT"/>
</gates>
<devices>
<device name="" package="62000821121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000821121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000821121"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62000821121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21121_62003221121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16X2PT"/>
</gates>
<devices>
<device name="" package="62003221121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62003221121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62003221121"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62003221121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6103XX21821_61031221821" prefix="J">
<description>&lt;b&gt; WR-PHD 2.54 mm SMT Dual Socket Header (Reel)&lt;/b&gt;

&lt;b&gt;&lt;br&gt;&lt;br&gt;ARTICLE PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pins ： 4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26 

&lt;b&gt;&lt;br&gt;&lt;br&gt;KIND PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch 2.54 mm 
&lt;br&gt;Quality Class 3 as per CECC 75 301-802 
&lt;br&gt;Rows Dual 
&lt;br&gt;Gender Socket Header 
&lt;br&gt;Type Straight Type 2 

&lt;b&gt;&lt;br&gt;&lt;br&gt;MATERIAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material PA46 
Insulator Flammability Rating UL94 V-0 
Contact Material Copper Alloy 
Contact Plating Gold 
Contact Type Stamped 

&lt;b&gt;&lt;br&gt;&lt;br&gt;GENERAL INFORMATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Operating Temperature -40 up to +105 °C 

&lt;b&gt;&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Rated Current  3 A 
&lt;br&gt;IR1 = 3A 
&lt;br&gt;Withstanding Voltage 600 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 

&lt;b&gt;&lt;br&gt;&lt;br&gt;CERTIFICATION 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;UL Approval E323964 

&lt;b&gt;&lt;br&gt;&lt;br&gt;PACKAGING PROPERTIES 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging Tape and Reel with Cap  
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33206v209%20Family_WR-PHD_610xxx21821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821"&gt;https://katalog.we-online.com/en/em/PHD_2_54_SMT_DUAL_SOCKET_HEADER_REEL_6103XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-06-12&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2SS_1"/>
</gates>
<devices>
<device name="" package="61031221821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61031221821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="61031221821"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61031221821"/>
<attribute name="WE-NUMBER" value="61031221821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX11121_62002011121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  2 unitless; 3 unitless; 4 unitless; 6 unitless; 8 unitless; 10 unitless; 20 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33219v209%20Family_WR-PHD_6200xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33219v209%20Family_WR-PHD_6200xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_PIN_HEADER_6200XX11121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_PIN_HEADER_6200XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20PT"/>
</gates>
<devices>
<device name="" package="62002011121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62002011121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62002011121"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62002011121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21921_62103221921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16X2PS"/>
</gates>
<devices>
<device name="" package="62103221921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62103221921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62103221921"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62103221921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21121_62001621121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PT"/>
</gates>
<devices>
<device name="" package="62001621121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62001621121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62001621121"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62001621121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21921_62101421921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PS"/>
</gates>
<devices>
<device name="" package="62101421921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62101421921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62101421921"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62101421921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21921_62100621921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PS"/>
</gates>
<devices>
<device name="" package="62100621921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62100621921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62100621921"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62100621921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21921_62130821921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PS"/>
</gates>
<devices>
<device name="" package="62130821921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62130821921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62130821921"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62130821921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21921_62101621921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PS"/>
</gates>
<devices>
<device name="" package="62101621921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62101621921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62101621921"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62101621921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21921_62130421921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PS"/>
</gates>
<devices>
<device name="" package="62130421921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62130421921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62130421921"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62130421921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21921_62131421921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PS"/>
</gates>
<devices>
<device name="" package="62131021921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62131421921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62131421921"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62131421921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21921_62100421921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PS"/>
</gates>
<devices>
<device name="" package="62100421921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62100421921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62100421921"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62100421921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21921_62131021921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PS"/>
</gates>
<devices>
<device name="" package="62131021921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62131021921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62131021921"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62131021921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21121_62002821121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14X2PT"/>
</gates>
<devices>
<device name="" package="62002821121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62002821121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62002821121"/>
<attribute name="PINS" value=" 28 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62002821121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21921_62102021921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PS"/>
</gates>
<devices>
<device name="" package="62102021921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62102021921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62102021921"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62102021921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21121_62000421121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PT"/>
</gates>
<devices>
<device name="" package="62000421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000421121"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62000421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21921_62102421921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PS"/>
</gates>
<devices>
<device name="" package="62102421921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62102421921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62102421921"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62102421921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX245821_621016245821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header Low Profile&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Low Profile

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PS"/>
</gates>
<devices>
<device name="" package="621016245821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621016245821?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621016245821"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Low Profile"/>
<attribute name="VALUE" value="621016245821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX11121_62003211121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  2 unitless; 3 unitless; 4 unitless; 6 unitless; 8 unitless; 10 unitless; 20 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33219v209%20Family_WR-PHD_6200xx11121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33219v209%20Family_WR-PHD_6200xx11121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_PIN_HEADER_6200XX11121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_PIN_HEADER_6200XX11121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32PT"/>
</gates>
<devices>
<device name="" package="62003211121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62003211121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62003211121"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62003211121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX245821_621006245821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header Low Profile&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Low Profile

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PS"/>
</gates>
<devices>
<device name="" package="621006245821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621006245821?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621006245821"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Low Profile"/>
<attribute name="VALUE" value="621006245821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX245821_621020245821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header Low Profile&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Low Profile

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PS"/>
</gates>
<devices>
<device name="" package="621020245821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621020245821?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621020245821"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Low Profile"/>
<attribute name="VALUE" value="621020245821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX245821_621324245821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header Low Profile&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Low Profile

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PS"/>
</gates>
<devices>
<device name="" package="621324245821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621324245821?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621324245821"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Low Profile"/>
<attribute name="VALUE" value="621324245821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21921_62130621921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PS"/>
</gates>
<devices>
<device name="" package="62130621921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62130621921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62130621921"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62130621921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX245821_621010245821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header Low Profile&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Low Profile

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PS"/>
</gates>
<devices>
<device name="" package="621010245821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621010245821?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621010245821"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Low Profile"/>
<attribute name="VALUE" value="621010245821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX245821_621314245821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header Low Profile&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Low Profile

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PS"/>
</gates>
<devices>
<device name="" package="621314245821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621314245821?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621314245821"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Low Profile"/>
<attribute name="VALUE" value="621314245821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21921_62104421921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2PS"/>
</gates>
<devices>
<device name="" package="62104421921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62104421921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62104421921"/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62104421921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX245821_621008245821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header Low Profile&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Low Profile

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PS"/>
</gates>
<devices>
<device name="" package="621008245821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621008245821?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621008245821"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Low Profile"/>
<attribute name="VALUE" value="621008245821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX245821_621024245821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header Low Profile&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Low Profile

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PS"/>
</gates>
<devices>
<device name="" package="621024245821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621024245821?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621024245821"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Low Profile"/>
<attribute name="VALUE" value="621024245821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX245821_621304245821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header Low Profile&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Low Profile

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PS"/>
</gates>
<devices>
<device name="" package="621304245821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621304245821?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621304245821"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Low Profile"/>
<attribute name="VALUE" value="621304245821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21121_62004421121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2PT"/>
</gates>
<devices>
<device name="" package="62004421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62004421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62004421121"/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62004421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX245821_621004245821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header Low Profile&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Low Profile

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PS"/>
</gates>
<devices>
<device name="" package="621004245821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621004245821?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621004245821"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Low Profile"/>
<attribute name="VALUE" value="621004245821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX245821_621310245821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header Low Profile&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Low Profile

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PS"/>
</gates>
<devices>
<device name="" package="621310245821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621310245821?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621310245821"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Low Profile"/>
<attribute name="VALUE" value="621310245821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21921_62131621921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PS"/>
</gates>
<devices>
<device name="" package="62131621921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62131621921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62131621921"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62131621921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX284521_621304284521" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Angled Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 16 unitless; 20 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106798v209%20Family_WR-PHD_6213xx284521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106798v209%20Family_WR-PHD_6213xx284521.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_PIN_HEADER_6213XX284521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_PIN_HEADER_6213XX284521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-05&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PS_1"/>
</gates>
<devices>
<device name="" package="621304284521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621304284521?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="621304284521"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="621304284521"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX284521_621308284521" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Angled Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 16 unitless; 20 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106798v209%20Family_WR-PHD_6213xx284521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106798v209%20Family_WR-PHD_6213xx284521.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_PIN_HEADER_6213XX284521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_PIN_HEADER_6213XX284521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-05&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PS_1"/>
</gates>
<devices>
<device name="" package="621308284521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621308284521?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="621308284521"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="621308284521"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX245821_621014245821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header Low Profile&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Low Profile

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PS"/>
</gates>
<devices>
<device name="" package="621014245821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621014245821?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621014245821"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Low Profile"/>
<attribute name="VALUE" value="621014245821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21121_62000621121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PT"/>
</gates>
<devices>
<device name="" package="62000621121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000621121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62000621121"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62000621121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21821_62000821821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-27&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2ST"/>
</gates>
<devices>
<device name="" package="62000821821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000821821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62000821821"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62000821821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX284521_621306284521" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Angled Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 16 unitless; 20 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106798v209%20Family_WR-PHD_6213xx284521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106798v209%20Family_WR-PHD_6213xx284521.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_PIN_HEADER_6213XX284521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_PIN_HEADER_6213XX284521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-05&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PS_1"/>
</gates>
<devices>
<device name="" package="621306284521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621306284521?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="621306284521"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="621306284521"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21821_62002421821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-27&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2ST"/>
</gates>
<devices>
<device name="" package="62002421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62002421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62002421821"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62002421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX11821_62000411821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  2 unitless; 4 unitless; 6 unitless; 8 unitless; 10 unitless; 20 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33220v209%20Family_WR-PHD_6200xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33220v209%20Family_WR-PHD_6200xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SOCKET_HEADER_6200XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SOCKET_HEADER_6200XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4ST"/>
</gates>
<devices>
<device name="" package="62000411821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000411821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62000411821"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62000411821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21821_62000421821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-27&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2ST"/>
</gates>
<devices>
<device name="" package="62000421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62000421821"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62000421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX245821_621308245821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header Low Profile&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Low Profile

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PS"/>
</gates>
<devices>
<device name="" package="621308245821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621308245821?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621308245821"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Low Profile"/>
<attribute name="VALUE" value="621308245821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX245821_621306245821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header Low Profile&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Low Profile

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PS"/>
</gates>
<devices>
<device name="" package="621306245821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621306245821?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621306245821"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Low Profile"/>
<attribute name="VALUE" value="621306245821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX245821_621316245821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header Low Profile&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Low Profile

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PS"/>
</gates>
<devices>
<device name="" package="621316245821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621316245821?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621316245821"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Low Profile"/>
<attribute name="VALUE" value="621316245821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21921_62132021921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57941v209%20Family_WR-PHD_Dual_SMT_Pin_Header_621xxx21921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_6210XX21921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PS"/>
</gates>
<devices>
<device name="" package="62132021921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62132021921?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62132021921"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62132021921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21821_62001021821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-27&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2ST"/>
</gates>
<devices>
<device name="" package="62001021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62001021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62001021821"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62001021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21121_62002421121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57938v209%20Family_WR-PHD_Dual_Pin_Header_6200xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_THT_DUAL_PIN_HEADER_6200XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2PT"/>
</gates>
<devices>
<device name="" package="62002421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62002421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="62002421121"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62002421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX242921_621008242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2SS"/>
</gates>
<devices>
<device name="" package="621008242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621008242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621008242921"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621008242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21821_62002021821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-27&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2ST"/>
</gates>
<devices>
<device name="" package="62002021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62002021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62002021821"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62002021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21821_62003221821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-27&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16X2ST"/>
</gates>
<devices>
<device name="" package="62003221821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62003221821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62003221821"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62003221821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX284521_621310284521" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Angled Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 16 unitless; 20 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106798v209%20Family_WR-PHD_6213xx284521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106798v209%20Family_WR-PHD_6213xx284521.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_PIN_HEADER_6213XX284521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_PIN_HEADER_6213XX284521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-05&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PS_1"/>
</gates>
<devices>
<device name="" package="621310284521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621310284521?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="621310284521"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="621310284521"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21821_62001621821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-27&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2ST"/>
</gates>
<devices>
<device name="" package="62001621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62001621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62001621821"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62001621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX242921_621004242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2SS"/>
</gates>
<devices>
<device name="" package="621004242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621004242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621004242921"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621004242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX245821_621320245821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Dual Pin Header Low Profile&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Low Profile

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57944v209%20Family_SMD_Low%20Profile_621xxx245821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_PIN_HEADER_LOW_PROFILE_6210XX245821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PS"/>
</gates>
<devices>
<device name="" package="621320245821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621320245821?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621320245821"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight Low Profile"/>
<attribute name="VALUE" value="621320245821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX11821_62000611821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  2 unitless; 4 unitless; 6 unitless; 8 unitless; 10 unitless; 20 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33220v209%20Family_WR-PHD_6200xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33220v209%20Family_WR-PHD_6200xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SOCKET_HEADER_6200XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SOCKET_HEADER_6200XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6ST"/>
</gates>
<devices>
<device name="" package="62000611821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000611821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62000611821"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62000611821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX242921_621032242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="16X2SS"/>
</gates>
<devices>
<device name="" package="621032242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621032242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621032242921"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621032242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX11821_62002011821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  2 unitless; 4 unitless; 6 unitless; 8 unitless; 10 unitless; 20 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33220v209%20Family_WR-PHD_6200xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33220v209%20Family_WR-PHD_6200xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SOCKET_HEADER_6200XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SOCKET_HEADER_6200XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20ST"/>
</gates>
<devices>
<device name="" package="62002011821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62002011821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62002011821"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62002011821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX284521_621316284521" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Angled Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 16 unitless; 20 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106798v209%20Family_WR-PHD_6213xx284521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106798v209%20Family_WR-PHD_6213xx284521.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_PIN_HEADER_6213XX284521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_PIN_HEADER_6213XX284521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-05&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PS_1"/>
</gates>
<devices>
<device name="" package="621316284521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621316284521?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="621316284521"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="621316284521"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21821_62002821821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-27&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14X2ST"/>
</gates>
<devices>
<device name="" package="62002821821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62002821821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62002821821"/>
<attribute name="PINS" value=" 28 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62002821821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21821_62000621821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-27&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2ST"/>
</gates>
<devices>
<device name="" package="62000621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62000621821"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62000621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX11821_62000211821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  2 unitless; 4 unitless; 6 unitless; 8 unitless; 10 unitless; 20 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33220v209%20Family_WR-PHD_6200xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33220v209%20Family_WR-PHD_6200xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SOCKET_HEADER_6200XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SOCKET_HEADER_6200XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2ST"/>
</gates>
<devices>
<device name="" package="62000211821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000211821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62000211821"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62000211821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX11821_62001011821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  2 unitless; 4 unitless; 6 unitless; 8 unitless; 10 unitless; 20 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33220v209%20Family_WR-PHD_6200xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33220v209%20Family_WR-PHD_6200xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SOCKET_HEADER_6200XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SOCKET_HEADER_6200XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10ST"/>
</gates>
<devices>
<device name="" package="62001011821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62001011821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62001011821"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62001011821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21821_62001421821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-27&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2ST"/>
</gates>
<devices>
<device name="" package="62001421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62001421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62001421821"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62001421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21821_62004021821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-27&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2ST"/>
</gates>
<devices>
<device name="" package="62004021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62004021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62004021821"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62004021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX284521_621312284521" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Angled Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 16 unitless; 20 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106798v209%20Family_WR-PHD_6213xx284521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106798v209%20Family_WR-PHD_6213xx284521.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_PIN_HEADER_6213XX284521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_PIN_HEADER_6213XX284521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-05&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2PS_1"/>
</gates>
<devices>
<device name="" package="621312284521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621312284521?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="621312284521"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="621312284521"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX242921_621316242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2SS"/>
</gates>
<devices>
<device name="" package="621316242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621316242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621316242921"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621316242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX242921_621016242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2SS"/>
</gates>
<devices>
<device name="" package="621016242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621016242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621016242921"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621016242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX242921_621304242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2SS"/>
</gates>
<devices>
<device name="" package="621304242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621304242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621304242921"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621304242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX284521_621320284521" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Angled Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 16 unitless; 20 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106798v209%20Family_WR-PHD_6213xx284521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106798v209%20Family_WR-PHD_6213xx284521.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_PIN_HEADER_6213XX284521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_PIN_HEADER_6213XX284521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-05&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PS_1"/>
</gates>
<devices>
<device name="" package="621320284521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621320284521?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="621320284521"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="621320284521"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX242921_621006242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2SS"/>
</gates>
<devices>
<device name="" package="621006242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621006242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621006242921"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621006242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX11821_62003211821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  2 unitless; 4 unitless; 6 unitless; 8 unitless; 10 unitless; 20 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33220v209%20Family_WR-PHD_6200xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33220v209%20Family_WR-PHD_6200xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SOCKET_HEADER_6200XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SOCKET_HEADER_6200XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="32ST"/>
</gates>
<devices>
<device name="" package="62003211821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62003211821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62003211821"/>
<attribute name="PINS" value=" 32 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62003211821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX242921_621320242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2SS"/>
</gates>
<devices>
<device name="" package="621320242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621320242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621320242921"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621320242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX284521_621314284521" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm SMT Angled Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 16 unitless; 20 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106798v209%20Family_WR-PHD_6213xx284521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106798v209%20Family_WR-PHD_6213xx284521.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_PIN_HEADER_6213XX284521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_PIN_HEADER_6213XX284521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-05&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PS_1"/>
</gates>
<devices>
<device name="" package="621314284521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621314284521?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="2A"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="621314284521"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="621314284521"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX11821_62000811821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  2 unitless; 4 unitless; 6 unitless; 8 unitless; 10 unitless; 20 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33220v209%20Family_WR-PHD_6200xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33220v209%20Family_WR-PHD_6200xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_SOCKET_HEADER_6200XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SOCKET_HEADER_6200XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8ST"/>
</gates>
<devices>
<device name="" package="62000811821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62000811821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62000811821"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62000811821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX242921_621010242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2SS"/>
</gates>
<devices>
<device name="" package="621010242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621010242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621010242921"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621010242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX242921_621020242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2SS"/>
</gates>
<devices>
<device name="" package="621020242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621020242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621020242921"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621020242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6200XX21821_62004421821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 28 unitless; 32 unitless; 40 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33221v209%20Family_WR-PHD_6200xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_DUAL_SOCKET_HEADER_6200XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-27&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2ST"/>
</gates>
<devices>
<device name="" package="62004421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62004421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62004421821"/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62004421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX242921_621324242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2SS"/>
</gates>
<devices>
<device name="" package="621324242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621324242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621324242921"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621324242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX242921_621014242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2SS"/>
</gates>
<devices>
<device name="" package="621014242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621014242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621014242921"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621014242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX242921_621310242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2SS"/>
</gates>
<devices>
<device name="" package="621310242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621310242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621310242921"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621310242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX242921_621344242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2SS"/>
</gates>
<devices>
<device name="" package="621344242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621344242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621344242921"/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621344242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21821_62101421821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Low Profile Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2SS"/>
</gates>
<devices>
<device name="" package="62101421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62101421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62101421821"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62101421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21821_62100621821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Low Profile Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2SS"/>
</gates>
<devices>
<device name="" package="62100621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62100621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62100621821"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62100621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX242921_621024242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2SS"/>
</gates>
<devices>
<device name="" package="621024242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621024242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621024242921"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621024242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21821_62101621821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Low Profile Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2SS"/>
</gates>
<devices>
<device name="" package="62101621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62101621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62101621821"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62101621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX242921_621308242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2SS"/>
</gates>
<devices>
<device name="" package="621308242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621308242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621308242921"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621308242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX242921_621044242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2SS"/>
</gates>
<devices>
<device name="" package="621044242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621044242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="621044242921"/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621044242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21821_62100421821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Low Profile Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2SS"/>
</gates>
<devices>
<device name="" package="62100421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62100421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62100421821"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62100421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21821_62130421821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Low Profile Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2SS"/>
</gates>
<devices>
<device name="" package="62130421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62130421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62130421821"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62130421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX242921_621306242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2SS"/>
</gates>
<devices>
<device name="" package="621306242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621306242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621306242921"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621306242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21821_62131021821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Low Profile Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2SS"/>
</gates>
<devices>
<device name="" package="62131021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62131021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62131021821"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62131021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21821_62100821821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Low Profile Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2SS"/>
</gates>
<devices>
<device name="" package="62100821821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62100821821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62100821821"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62100821821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6211XX284621_621104284621" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 16 unitless; 20 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled; Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106797v209%20Family_WR-PHD_6211xx284621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106797v209%20Family_WR-PHD_6211xx284621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_SOCKET_HEADER_6211XX284621/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_SOCKET_HEADER_6211XX284621&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="621104284621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621104284621?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="621104284621"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="621104284621"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21821_62130621821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Low Profile Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2SS"/>
</gates>
<devices>
<device name="" package="62130621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62130621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62130621821"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62130621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21821_62102021821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Low Profile Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2SS"/>
</gates>
<devices>
<device name="" package="62102021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62102021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62102021821"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62102021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX242921_621314242921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless; 32 unitless; 44 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57956v209%20Family_Dual_Socket_Header_WR-PHD_6130xx242921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_DUAL_SOCKET_HEADER_6210XX242921&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2SS"/>
</gates>
<devices>
<device name="" package="621314242921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621314242921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="621314242921"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="621314242921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21821_62130821821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Low Profile Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2SS"/>
</gates>
<devices>
<device name="" package="62130821821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62130821821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62130821821"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62130821821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21821_62131621821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Low Profile Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2SS"/>
</gates>
<devices>
<device name="" package="62131621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62131621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62131621821"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62131621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21821_62101021821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Low Profile Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2SS"/>
</gates>
<devices>
<device name="" package="62101021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62101021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62101021821"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62101021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6211XX284621_621114284621" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 16 unitless; 20 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled; Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106797v209%20Family_WR-PHD_6211xx284621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106797v209%20Family_WR-PHD_6211xx284621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_SOCKET_HEADER_6211XX284621/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_SOCKET_HEADER_6211XX284621&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="621114284621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621114284621?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="621114284621"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="621114284621"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6220XX21121_62200421121" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	500 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33223v209%20Family_WR-PHD_6220xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33223v209%20Family_WR-PHD_6220xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_THT_DUAL_PIN_HEADER_6220XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_THT_DUAL_PIN_HEADER_6220XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-05&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PT"/>
</gates>
<devices>
<device name="" package="62200421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62200421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="62200421121"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62200421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6220XX21121_62201021121" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	500 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33223v209%20Family_WR-PHD_6220xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33223v209%20Family_WR-PHD_6220xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_THT_DUAL_PIN_HEADER_6220XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_THT_DUAL_PIN_HEADER_6220XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-05&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PT"/>
</gates>
<devices>
<device name="" package="62201021121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62201021121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="62201021121"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62201021121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21821_62102421821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Low Profile Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2SS"/>
</gates>
<devices>
<device name="" package="62102421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62102421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62102421821"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62102421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21821_62132021821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Low Profile Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2SS"/>
</gates>
<devices>
<device name="" package="62132021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62132021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62132021821"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62132021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21021_62101021021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PS"/>
</gates>
<devices>
<device name="" package="62101021021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62101021021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62101021021"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62101021021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6211XX284621_621108284621" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 16 unitless; 20 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled; Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106797v209%20Family_WR-PHD_6211xx284621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106797v209%20Family_WR-PHD_6211xx284621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_SOCKET_HEADER_6211XX284621/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_SOCKET_HEADER_6211XX284621&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="621108284621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621108284621?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="621108284621"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="621108284621"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6211XX284621_621116284621" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 16 unitless; 20 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled; Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106797v209%20Family_WR-PHD_6211xx284621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106797v209%20Family_WR-PHD_6211xx284621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_SOCKET_HEADER_6211XX284621/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_SOCKET_HEADER_6211XX284621&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="621116284621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621116284621?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="621116284621"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="621116284621"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6211XX284621_621120284621" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 16 unitless; 20 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled; Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106797v209%20Family_WR-PHD_6211xx284621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106797v209%20Family_WR-PHD_6211xx284621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_SOCKET_HEADER_6211XX284621/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_SOCKET_HEADER_6211XX284621&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="621120284621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621120284621?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="621120284621"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="621120284621"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6211XX284621_621110284621" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 16 unitless; 20 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled; Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106797v209%20Family_WR-PHD_6211xx284621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106797v209%20Family_WR-PHD_6211xx284621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_SOCKET_HEADER_6211XX284621/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_SOCKET_HEADER_6211XX284621&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="621110284621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621110284621?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="621110284621"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="621110284621"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21021_62102821021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14X2PS"/>
</gates>
<devices>
<device name="" package="62102821021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62102821021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62102821021"/>
<attribute name="PINS" value=" 28 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62102821021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6211XX284621_621112284621" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 16 unitless; 20 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled; Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106797v209%20Family_WR-PHD_6211xx284621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106797v209%20Family_WR-PHD_6211xx284621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_SOCKET_HEADER_6211XX284621/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_SOCKET_HEADER_6211XX284621&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="621112284621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621112284621?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="621112284621"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="621112284621"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21021_62130421021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PS"/>
</gates>
<devices>
<device name="" package="62130421021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62130421021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62130421021"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62130421021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6220XX21121_62202021121" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	500 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33223v209%20Family_WR-PHD_6220xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33223v209%20Family_WR-PHD_6220xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_THT_DUAL_PIN_HEADER_6220XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_THT_DUAL_PIN_HEADER_6220XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-05&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PT"/>
</gates>
<devices>
<device name="" package="62202021121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62202021121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="62202021121"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62202021121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6220XX21121_62200821121" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	500 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33223v209%20Family_WR-PHD_6220xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33223v209%20Family_WR-PHD_6220xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_THT_DUAL_PIN_HEADER_6220XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_THT_DUAL_PIN_HEADER_6220XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-05&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PT"/>
</gates>
<devices>
<device name="" package="62200821121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62200821121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="62200821121"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62200821121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21821_62131421821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Low Profile Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2SS"/>
</gates>
<devices>
<device name="" package="62131421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62131421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62131421821"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62131421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21021_62100821021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PS"/>
</gates>
<devices>
<device name="" package="62100821021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62100821021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62100821021"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62100821021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21021_62105021021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2PS"/>
</gates>
<devices>
<device name="" package="62105021021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62105021021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62105021021"/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62105021021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21821_62132421821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Low Profile Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33222v209%20Family_WR-PHD_621xxx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_0_SMT_DUAL_SOCKET_HEADER_LOW_PROFILE_6210XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12X2SS"/>
</gates>
<devices>
<device name="" package="62132421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62132421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62132421821"/>
<attribute name="PINS" value=" 24 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62132421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21021_62102021021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PS"/>
</gates>
<devices>
<device name="" package="62102021021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62102021021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62102021021"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62102021021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21021_62135021021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2PS"/>
</gates>
<devices>
<device name="" package="62135021021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62135021021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62135021021"/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62135021021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21021_62134421021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2PS"/>
</gates>
<devices>
<device name="" package="62134421021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62134421021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62134421021"/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62134421021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21021_62101421021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PS"/>
</gates>
<devices>
<device name="" package="62101421021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62101421021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62101421021"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62101421021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21021_62100421021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2PS"/>
</gates>
<devices>
<device name="" package="62100421021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62100421021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62100421021"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62100421021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6220XX21121_62201421121" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	500 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33223v209%20Family_WR-PHD_6220xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33223v209%20Family_WR-PHD_6220xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_THT_DUAL_PIN_HEADER_6220XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_THT_DUAL_PIN_HEADER_6220XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-05&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PT"/>
</gates>
<devices>
<device name="" package="62201421121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62201421121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="62201421121"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62201421121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21021_62104421021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="22X2PS"/>
</gates>
<devices>
<device name="" package="62104421021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62104421021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62104421021"/>
<attribute name="PINS" value=" 44 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62104421021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21021_62132021021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2PS"/>
</gates>
<devices>
<device name="" package="62132021021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62132021021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62132021021"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62132021021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21021_62101621021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PS"/>
</gates>
<devices>
<device name="" package="62101621021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62101621021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62101621021"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62101621021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21021_62131021021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PS"/>
</gates>
<devices>
<device name="" package="62131021021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62131021021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62131021021"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62131021021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6233XX235521_623350235521" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=1.80 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;10 unitless; 26 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight


&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	300 MΩ; 500 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57946v209%20Family_Pin%20Header_WR-PHD_6233xx235521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57946v209%20Family_Pin%20Header_WR-PHD_6233xx235521.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6233XX235521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6233XX235521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2PS"/>
</gates>
<devices>
<device name="" package="623350235521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/623350235521?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="623350235521"/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="623350235521"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21021_62132821021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14X2PS"/>
</gates>
<devices>
<device name="" package="62132821021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62132821021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62132821021"/>
<attribute name="PINS" value=" 28 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62132821021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21021_62131421021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2PS"/>
</gates>
<devices>
<device name="" package="62131421021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62131421021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62131421021"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62131421021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6233XX235321_623310235321" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header Bottom Entry, H=2.20 mm (Reel)
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;10 unitless; 26 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33197v209%20Family_Wr-PDH_6233xx235321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33197v209%20Family_Wr-PDH_6233xx235321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_REEL_6233XX235321/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_REEL_6233XX235321&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2SS"/>
</gates>
<devices>
<device name="" package="623310235321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/623310235321?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="623310235321"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="623310235321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6233XX235321_623326235321" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header Bottom Entry, H=2.20 mm (Reel)
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;10 unitless; 26 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33197v209%20Family_Wr-PDH_6233xx235321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33197v209%20Family_Wr-PDH_6233xx235321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_REEL_6233XX235321/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_REEL_6233XX235321&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2SS"/>
</gates>
<devices>
<device name="" package="623326235321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/623326235321?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="623326235321"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="623326235321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6220XX21121_62202821121" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	500 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33223v209%20Family_WR-PHD_6220xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33223v209%20Family_WR-PHD_6220xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_THT_DUAL_PIN_HEADER_6220XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_THT_DUAL_PIN_HEADER_6220XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-05&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14X2PT"/>
</gates>
<devices>
<device name="" package="62202821121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62202821121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="62202821121"/>
<attribute name="PINS" value=" 28 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62202821121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21021_62130821021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2PS"/>
</gates>
<devices>
<device name="" package="62130821021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62130821021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62130821021"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62130821021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6220XX21821_62201021821" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm Dual Socket Header
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33224v209%20Family_WR-PHD_6220xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33224v209%20Family_WR-PHD_6220xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_DUAL_SOCKET_HEADER_6220XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_DUAL_SOCKET_HEADER_6220XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2ST_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62201021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62201021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62201021821"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62201021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21021_62131621021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PS"/>
</gates>
<devices>
<device name="" package="62131621021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62131621021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62131621021"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62131621021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6233XX235521_623310235521" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=1.80 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;10 unitless; 26 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight


&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	300 MΩ; 500 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57946v209%20Family_Pin%20Header_WR-PHD_6233xx235521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57946v209%20Family_Pin%20Header_WR-PHD_6233xx235521.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6233XX235521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6233XX235521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2PS"/>
</gates>
<devices>
<device name="" package="623310235521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/623310235521?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="623310235521"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="623310235521"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21021_62134021021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2PS"/>
</gates>
<devices>
<device name="" package="62134021021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62134021021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62134021021"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62134021021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6220XX21821_62201621821" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm Dual Socket Header
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33224v209%20Family_WR-PHD_6220xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33224v209%20Family_WR-PHD_6220xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_DUAL_SOCKET_HEADER_6220XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_DUAL_SOCKET_HEADER_6220XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2ST_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62201621821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62201621821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62201621821"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62201621821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6210XX21021_62104021021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2PS"/>
</gates>
<devices>
<device name="" package="62104021021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62104021021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62104021021"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62104021021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6213XX21021_62130621021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=3.80 mm&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless; 40 unitless; 44 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33195v209%20Family_WR-PDH_621xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6210XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2PS"/>
</gates>
<devices>
<device name="" package="62130621021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62130621021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Cap"/>
<attribute name="PART-NUMBER" value="62130621021"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62130621021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6220XX21821_62200821821" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm Dual Socket Header
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33224v209%20Family_WR-PHD_6220xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33224v209%20Family_WR-PHD_6220xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_DUAL_SOCKET_HEADER_6220XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_DUAL_SOCKET_HEADER_6220XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2ST_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62200821821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62200821821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62200821821"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62200821821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6230XX21021_62300421021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header, H=4.50 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62300421021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62300421021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62300421021"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62300421021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6220XX21821_62201421821" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm Dual Socket Header
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33224v209%20Family_WR-PHD_6220xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33224v209%20Family_WR-PHD_6220xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_DUAL_SOCKET_HEADER_6220XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_DUAL_SOCKET_HEADER_6220XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2ST_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62201421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62201421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62201421821"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62201421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6233XX235321_623350235321" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header Bottom Entry, H=2.20 mm (Reel)
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;10 unitless; 26 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33197v209%20Family_Wr-PDH_6233xx235321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33197v209%20Family_Wr-PDH_6233xx235321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_REEL_6233XX235321/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_REEL_6233XX235321&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="25X2SS"/>
</gates>
<devices>
<device name="" package="623350235321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/623350235321?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="623350235321"/>
<attribute name="PINS" value=" 50 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry"/>
<attribute name="VALUE" value="623350235321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX13321_61001513321" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15SS_1"/>
</gates>
<devices>
<device name="" package="61001513321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001513321?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001513321"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 2"/>
<attribute name="VALUE" value="61001513321"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6220XX21821_62200421821" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm Dual Socket Header
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33224v209%20Family_WR-PHD_6220xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33224v209%20Family_WR-PHD_6220xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_DUAL_SOCKET_HEADER_6220XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_DUAL_SOCKET_HEADER_6220XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2ST_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62200421821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62200421821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62200421821"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62200421821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6233XX235521_623326235521" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Pin Header, H=1.80 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;10 unitless; 26 unitless; 50 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight


&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	300 MΩ; 500 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o57946v209%20Family_Pin%20Header_WR-PHD_6233xx235521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o57946v209%20Family_Pin%20Header_WR-PHD_6233xx235521.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6233XX235521/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_PIN_HEADER_6233XX235521&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="13X2PS"/>
</gates>
<devices>
<device name="" package="623326235521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/623326235521?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="623326235521"/>
<attribute name="PINS" value=" 26 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="623326235521"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6230XX21021_62301021021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header, H=4.50 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62301021021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62301021021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62301021021"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62301021021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11821_61301511821" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins (Value)	2 pcs; 3 pcs; 4 pcs; 5 pcs; 6 pcs; 7 pcs; 8 pcs; 9 pcs; 10 pcs; 12 pcs; 13 pcs; 14 pcs; 15 pcs; 16 pcs; 18 pcs; 20 pcs; 22 pcs; 24 pcs; 32 pcs; 36 pcs; 40 pcs
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	30 Mating cycles; 500 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33218v209%20Family-WR-PHD-6130xx11821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SOCKET_HEADER_6130XX11821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SOCKET_HEADER_6130XX11821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-04-23&lt;BR&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15ST"/>
</gates>
<devices>
<device name="" package="61301511821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301511821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="61301511821"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="61301511821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6233XX21021_62331421021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header, H=4.50 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62331421021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62331421021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="62331421021"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62331421021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6230XX21021_62301621021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header, H=4.50 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62301621021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62301621021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62301621021"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62301621021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6211XX284621_621106284621" prefix="J">
<description>&lt;b&gt;WR-PHD 2.00 mm Dual SMT Socket Header Angled&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 16 unitless; 20 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled; Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	LCP
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	2 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o106797v209%20Family_WR-PHD_6211xx284621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o106797v209%20Family_WR-PHD_6211xx284621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_SOCKET_HEADER_6211XX284621/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_00_SMT_ANGLED_DUAL_SOCKET_HEADER_6211XX284621&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="621106284621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/621106284621?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel"/>
<attribute name="PART-NUMBER" value="621106284621"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.00 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="621106284621"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX143121_613015143121" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Angled Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 	2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 13 unitless; 15 unitless; 16 unitless; 18 unitless; 20 unitless; 24 unitless; 32 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PBT
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tray

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33212v209%20Family_WR-PHD_6130xx143121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_ANGLED_SOCKET_HEADER_6130XX143121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-04-23&lt;BR&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15ST"/>
</gates>
<devices>
<device name="" package="613015143121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613015143121?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="613015143121"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="613015143121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6220XX21821_62202021821" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm Dual Socket Header
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33224v209%20Family_WR-PHD_6220xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33224v209%20Family_WR-PHD_6220xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_DUAL_SOCKET_HEADER_6220XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_DUAL_SOCKET_HEADER_6220XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2ST_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62202021821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62202021821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62202021821"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62202021821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX243021_610040243021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Dual Socket Header Bottom Entry&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy; Phosphor Bronze
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Cap; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC); 600 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33207v209%20Family_WR-PHD_610xxx243021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_6100XX243021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2SS"/>
</gates>
<devices>
<device name="" package="610040243021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/610040243021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="610040243021"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Low Profile"/>
<attribute name="VALUE" value="610040243021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6233XX21021_62330421021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header, H=4.50 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62330421021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62330421021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="62330421021"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62330421021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6233XX21021_62331021021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header, H=4.50 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62331021021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62331021021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="62331021021"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62331021021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX21021_61301621021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Dual Pin Header &lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;ARTICLE PROPERTIES:&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins:4;​ 6;​ 8;​ 10;​ 12;​ 14;​ 16;​ 18;​ 20;​ 22;​ 24;​ 26;​ 32;​ 34;​ 36;​ 40;​ 64;​ 72
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;KIND PROPERTIES&lt;/B&gt;:
&lt;BR&gt;
&lt;BR&gt;Pitch：2.54 mm
&lt;BR&gt;Quality Class:3 as per CECC 75 301-802
&lt;BR&gt;Rows：Dual
&lt;BR&gt;Gender：Pin Header
&lt;BR&gt;Type：Angled;​ Board Stacker
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;MATERIAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material :PA6T
&lt;BR&gt;Insulator Flammability Rating:UL94 V-0
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Contact Type:Stamped
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;GENERAL INFORMATION&lt;/B&gt;
&lt;BR&gt;Operating Temperature:-40 up to +105 °C
&lt;BR&gt;Compliance:RoHS
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;ELECTRICAL PROPERTIES:&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Rated Current:3 A
&lt;BR&gt;IR 1:3 A
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Contact Resistance:20 mΩ
&lt;BR&gt;RISO:1000 MΩ
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;CERTIFICATION&lt;/B&gt;
&lt;BR&gt;UL Approval:E323964
&lt;BR&gt;&lt;B&gt;PACKAGING PROPERTIES&lt;/B&gt;
&lt;BR&gt;Packaging:Bag
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33214v209%20Family_wr-phd_6130XX21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021"&gt;https://katalog.we-online.com/en/em/PHD_2_54_THT_ANGLED_DUAL_PIN_HEADER_6130XX21021&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;
Updated by Yingchun,Shan 2019-10-16
&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PT_1"/>
</gates>
<devices>
<device name="" package="61301621021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301621021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301621021"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61301621021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX11021_61301511021" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm THT Angled Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 2 unitless; 3 unitless; 4 unitless; 5 unitless; 6 unitless; 7 unitless; 8 unitless; 9 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 18 unitless; 22 unitless; 32 unitless; 34 unitless; 36 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Angled

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;ithstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33210v209%20Family_WR-PHD_6130xx11021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_THT_ANGLED_PIN_HEADER_6130XX11021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-04-23&lt;BR&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15PT_1"/>
</gates>
<devices>
<device name="" package="61301511021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61301511021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value="61301511021"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Angled"/>
<attribute name="VALUE" value="61301511021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6230XX21021_62302821021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header, H=4.50 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62302821021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62302821021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62302821021"/>
<attribute name="PINS" value=" 28 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62302821021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX18221_61001518221" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 6 unitless; 10 unitless; 14 unitless; 15 unitless; 16 unitless; 24 unitless; 32 unitless; 34 unitless; 36 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA6T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33202v209%20Family_WR-PHD_6100xx18221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_PIN_HEADER_6100XX18X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_PIN_HEADER_6100XX18X21&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15PS_1"/>
</gates>
<devices>
<device name="" package="61001518221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001518221?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001518221"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61001518221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6230XX21021_62301421021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header, H=4.50 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62301421021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62301421021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62301421021"/>
<attribute name="PINS" value=" 14 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62301421021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6233XX21021_62332021021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header, H=4.50 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62332021021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62332021021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="62332021021"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62332021021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6233XX21021_62330821021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header, H=4.50 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62330821021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62330821021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="62330821021"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62330821021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6230XX21021_62300821021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header, H=4.50 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62300821021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62300821021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62300821021"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62300821021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6233XX21021_62331621021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header, H=4.50 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62331621021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62331621021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="62331621021"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62331621021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6100XX11921_61001511921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm SMT Socket Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins 4 unitless; 5 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 14 unitless; 15 unitless; 16 unitless; 20 unitless; 24 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;General Information
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C; -40 °C up to +125 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Single
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight Type 1; Straight Type 2

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 46; PA 9T; PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Bag

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	3 A
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o64612v209%20Family_WR-PHD_6100xx13321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_SMT_SOCKET_HEADER_6100XXXXX21&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-01-31&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="15SS"/>
</gates>
<devices>
<device name="" package="61001511921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61001511921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="61001511921"/>
<attribute name="PINS" value=" 15 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight Type 1"/>
<attribute name="VALUE" value="61001511921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6220XX21121_62201621121" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm THT Dual Pin Header&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Pin Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Box

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	500 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33223v209%20Family_WR-PHD_6220xx21121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33223v209%20Family_WR-PHD_6220xx21121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_THT_DUAL_PIN_HEADER_6220XX21121/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_THT_DUAL_PIN_HEADER_6220XX21121&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-05&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8X2PT"/>
</gates>
<devices>
<device name="" package="62201621121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62201621121?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Box"/>
<attribute name="PART-NUMBER" value="62201621121"/>
<attribute name="PINS" value=" 16 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62201621121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6130XX216921_613040216921" prefix="J">
<description>&lt;b&gt;WR-PHD 2.54 mm Dual Socket Header Bottom Entry Large&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;Pins  4 unitless; 6 unitless; 8 unitless; 10 unitless; 12 unitless; 16 unitless; 18 unitless; 20 unitless; 22 unitless; 24 unitless; 26 unitless; 32 unitless; 34 unitless; 40 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	2.54 mm
&lt;BR&gt;Durability	25 Mating cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Bottom Entry Large

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	Nylon 9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	500 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ

&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33194v209%20Family_WR-PDH_6130xx216921.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/catalog/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_2_54_DUAL_SOCKET_HEADER_BOTTOM_ENTRY_LARGE_6130XX216921&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2019-10-23&lt;BR&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="20X2ST"/>
</gates>
<devices>
<device name="" package="613040216921">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/613040216921?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="613040216921"/>
<attribute name="PINS" value=" 40 "/>
<attribute name="PITCH" value="2.54 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Bottom Entry Large"/>
<attribute name="VALUE" value="613040216921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6230XX21021_62302021021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header, H=4.50 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62302021021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62302021021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62302021021"/>
<attribute name="PINS" value=" 20 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62302021021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6233XX21021_62332821021" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm SMT Dual Socket Header, H=4.50 mm
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Compliance	Lead free / RoHS
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tape and Reel with Pad; Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;IR	1 A
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33198v209%20Family_Wr-PDH_623xxx21021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_SMT_DUAL_SOCKET_HEADER_6230XX21021&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14X2SS_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62332821021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62332821021?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PACKAGING" value="Tape and Reel with Pad"/>
<attribute name="PART-NUMBER" value="62332821021"/>
<attribute name="PINS" value=" 28 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62332821021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6220XX21821_62202821821" prefix="J">
<description>&lt;b&gt;WR-PHD 1.27 mm Dual Socket Header
&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Article Properties&lt;/b&gt;
&lt;BR&gt;
&lt;BR&gt;4 unitless; 8 unitless; 10 unitless; 14 unitless; 16 unitless; 20 unitless; 28 unitless
&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;General Information&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Operating Temperature	-40 °C up to +105 °C
&lt;BR&gt;Pitch	1.27 mm
&lt;BR&gt;Durability	50 Cycles
&lt;BR&gt;Rows	Dual
&lt;BR&gt;Gender	Socket Header
&lt;BR&gt;Type	Straight

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Insulator Material	PA9T
&lt;BR&gt;Insulator Flammability Rating	UL94 V-0
&lt;BR&gt;Contact Material	Copper Alloy
&lt;BR&gt;Contact Plating	Gold
&lt;BR&gt;Contact Type	Stamped

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Certification&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;UL Approval	E323964

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Packaging	Tube

&lt;BR&gt;
&lt;BR&gt;&lt;B&gt;Electrical Properties&lt;/B&gt;
&lt;BR&gt;
&lt;BR&gt;Withstanding Voltage	300 V (AC)
&lt;BR&gt;Contact Resistance	20 mΩ
&lt;BR&gt;RISO	1000 MΩ


&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33224v209%20Family_WR-PHD_6220xx21821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33224v209%20Family_WR-PHD_6220xx21821.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="www.we-online.com/en/components/products/PHD_1_27_DUAL_SOCKET_HEADER_6220XX21821/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/PHD_1_27_DUAL_SOCKET_HEADER_6220XX21821&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-02-26&lt;BR&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="14X2ST_RIGHTBOTTOM"/>
</gates>
<devices>
<device name="" package="62202821821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62202821821?ae"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62202821821"/>
<attribute name="PINS" value=" 28 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE" value="62202821821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
