<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Wire-to-Board Connectors - WR-RAST &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2026a, 2026-05-13&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="637101120204">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101110202">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110109">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110102">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101120202">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120203">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120703">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="667101120104">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 5mm, 4pins</description>
</package>
<package name="637101110703">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110103">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110207">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="667101110109">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 9pins</description>
</package>
<package name="637101110204">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101120107">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120103">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120105">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101110203">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110503">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110108">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110104">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101120102">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120109">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101110205">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101120307">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120108">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120106">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120503">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120104">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101110106">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="667101110105">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 5pins</description>
</package>
<package name="667101110102">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 2pins</description>
</package>
<package name="637101120207">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="667101210107">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 7pins</description>
</package>
<package name="667101210108">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 8pins</description>
</package>
<package name="667101220105">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 5mm, 5pins</description>
</package>
<package name="637101110107">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="667101120102">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 5mm, 2pins</description>
</package>
<package name="637101110105">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="667101210103">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 3pins</description>
</package>
<package name="667101220102">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 5mm, 2pins</description>
</package>
<package name="637101120205">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="667101110103">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 3pins</description>
</package>
<package name="637101110307">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="667101110110">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 10pins</description>
</package>
<package name="667101110107">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 7pins</description>
</package>
<package name="667101210106">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 6pins</description>
</package>
<package name="667101210104">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 4pins</description>
</package>
<package name="667101210109">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 9pins</description>
</package>
<package name="667101210110">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 10pins</description>
</package>
<package name="667101220103">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 5mm, 3pins</description>
</package>
<package name="667101210105">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 5pins</description>
</package>
<package name="637101120110">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101110110">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="667101110106">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 6pins</description>
</package>
<package name="667101220104">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 5mm, 4pins</description>
</package>
<package name="667101110108">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 8pins</description>
</package>
<package name="667101120103">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 5mm, 3pins</description>
</package>
<package name="667101210102">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 2pins</description>
</package>
<package name="667101120105">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 5mm, 5pins</description>
</package>
<package name="667101110104">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Pitch 2.5mm, 4pins</description>
</package>
</packages>
<symbols>
<symbol name="11PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="12PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="9PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="2PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="4PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="4PT_LEFT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="3PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="7PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="9PT_LEFT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="5PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="8PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="6PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="5PT_LEFT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="7PS-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="2PT_LEFT-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="5PS-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="8PS">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="3PS-2">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="2PT_LEFT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="10PT_LEFT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="2PS">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="7PT_LEFT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="6PS-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="3PT_LEFT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="4PS-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="9PS-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="3PS-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="10PS">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="5PS">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="6PS">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="3PS">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="5PS-3">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="7PS">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="10PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="6PT_LEFT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="9PS">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="3PT_LEFT-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="2PS-2">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="2PS-3">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="4PS-3">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="10PS-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="8PT_LEFT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="5PT_LEFT-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="8PS-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="2PS-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="4PS">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="4PT_LEFT-1">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="4PS-2">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="5PS-2">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="3PS-3">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="637101120204" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="637101120204">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0B"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120204?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120204"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="4"/>
<attribute name="VALUE" value="637101120204"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110202" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="637101110202">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0B"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110202?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110202"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="2"/>
<attribute name="VALUE" value="637101110202"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110109" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT"/>
</gates>
<devices>
<device name="" package="637101110109">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110109?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110109"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="9"/>
<attribute name="VALUE" value="637101110109"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110102" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="637101110102">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110102?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110102"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="2"/>
<attribute name="VALUE" value="637101110102"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120202" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="637101120202">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0B"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120202?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120202"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="2"/>
<attribute name="VALUE" value="637101120202"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120203" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="637101120203">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0B"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120203?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120203"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="3"/>
<attribute name="VALUE" value="637101120203"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120703" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="637101120703">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0K"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120703?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120703"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="3"/>
<attribute name="VALUE" value="637101120703"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101120104" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm &lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT_LEFT"/>
</gates>
<devices>
<device name="" package="667101120104">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101120104?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101120104"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="04"/>
<attribute name="VALUE" value="667101120104"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110703" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="637101110703">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0K"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110703?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110703"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="3"/>
<attribute name="VALUE" value="637101110703"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110103" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="637101110103">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110103?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110103"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="3"/>
<attribute name="VALUE" value="637101110103"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110207" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="637101110207">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0B"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110207?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110207"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="7"/>
<attribute name="VALUE" value="637101110207"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101110109" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm &lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT_LEFT"/>
</gates>
<devices>
<device name="" package="667101110109">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101110109?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101110109"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="09"/>
<attribute name="VALUE" value="667101110109"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110204" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="637101110204">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0B"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110204?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110204"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="4"/>
<attribute name="VALUE" value="637101110204"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120107" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="637101120107">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120107?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120107"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="7"/>
<attribute name="VALUE" value="637101120107"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120103" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="637101120103">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120103?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120103"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="3"/>
<attribute name="VALUE" value="637101120103"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120105" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="637101120105">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120105?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120105"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="5"/>
<attribute name="VALUE" value="637101120105"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110203" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="637101110203">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0B"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110203?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110203"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="3"/>
<attribute name="VALUE" value="637101110203"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110108" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="637101110108">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110108?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110108"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="8"/>
<attribute name="VALUE" value="637101110108"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110104" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="637101110104">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110104?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110104"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="4"/>
<attribute name="VALUE" value="637101110104"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110503" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="637101110503">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0F"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110503?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110503"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="3"/>
<attribute name="VALUE" value="637101110503"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120102" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="637101120102">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120102?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120102"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="2"/>
<attribute name="VALUE" value="637101120102"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110205" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="637101110205">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0B"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110205?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110205"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="5"/>
<attribute name="VALUE" value="637101110205"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120109" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT"/>
</gates>
<devices>
<device name="" package="637101120109">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120109?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120109"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="9"/>
<attribute name="VALUE" value="637101120109"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120307" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="637101120307">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0C"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120307?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120307"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="7"/>
<attribute name="VALUE" value="637101120307"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120108" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="637101120108">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120108?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120108"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="8"/>
<attribute name="VALUE" value="637101120108"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120106" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="637101120106">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120106?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120106"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="6"/>
<attribute name="VALUE" value="637101120106"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120503" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="637101120503">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0F"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120503?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120503"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="3"/>
<attribute name="VALUE" value="637101120503"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120104" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="637101120104">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120104?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120104"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="4"/>
<attribute name="VALUE" value="637101120104"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110106" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="637101110106">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110106?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110106"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="6"/>
<attribute name="VALUE" value="637101110106"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101110105" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm &lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT_LEFT"/>
</gates>
<devices>
<device name="" package="667101110105">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101110105?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101110105"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="05"/>
<attribute name="VALUE" value="667101110105"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101110102" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm &lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT_LEFT-1"/>
</gates>
<devices>
<device name="" package="667101110102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101110102?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101110102"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="02"/>
<attribute name="VALUE" value="667101110102"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120207" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="637101120207">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0B"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120207?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120207"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="7"/>
<attribute name="VALUE" value="637101120207"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101210107" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PS"/>
</gates>
<devices>
<device name="" package="667101210107">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
<connect gate="G$1" pin="5" pad="A5 B5"/>
<connect gate="G$1" pin="6" pad="A6 B6"/>
<connect gate="G$1" pin="7" pad="A7 B7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101210107?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101210107"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="07"/>
<attribute name="VALUE" value="667101210107"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101210108" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PS-1"/>
</gates>
<devices>
<device name="" package="667101210108">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
<connect gate="G$1" pin="5" pad="A5 B5"/>
<connect gate="G$1" pin="6" pad="A6 B6"/>
<connect gate="G$1" pin="7" pad="A7 B7"/>
<connect gate="G$1" pin="8" pad="A8 B8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101210108?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101210108"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="08"/>
<attribute name="VALUE" value="667101210108"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101220105" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PS-2"/>
</gates>
<devices>
<device name="" package="667101220105">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
<connect gate="G$1" pin="5" pad="A5 B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101220105?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101220105"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="05"/>
<attribute name="VALUE" value="667101220105"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101240105" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PS-1"/>
</gates>
<devices>
<device name="" package="667101220105">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
<connect gate="G$1" pin="5" pad="A5 B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101240105?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101240105"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="05"/>
<attribute name="VALUE" value="667101240105"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101230107" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PS-1"/>
</gates>
<devices>
<device name="" package="667101210107">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
<connect gate="G$1" pin="5" pad="A5 B5"/>
<connect gate="G$1" pin="6" pad="A6 B6"/>
<connect gate="G$1" pin="7" pad="A7 B7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101230107?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101230107"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="07"/>
<attribute name="VALUE" value="667101230107"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110107" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="637101110107">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110107?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110107"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="7"/>
<attribute name="VALUE" value="637101110107"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101230108" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PS"/>
</gates>
<devices>
<device name="" package="667101210108">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
<connect gate="G$1" pin="5" pad="A5 B5"/>
<connect gate="G$1" pin="6" pad="A6 B6"/>
<connect gate="G$1" pin="7" pad="A7 B7"/>
<connect gate="G$1" pin="8" pad="A8 B8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101230108?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101230108"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="08"/>
<attribute name="VALUE" value="667101230108"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101120102" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm &lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT_LEFT"/>
</gates>
<devices>
<device name="" package="667101120102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101120102?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101120102"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="02"/>
<attribute name="VALUE" value="667101120102"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101230103" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PS-2"/>
</gates>
<devices>
<device name="" package="667101210103">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101230103?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101230103"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="03"/>
<attribute name="VALUE" value="667101230103"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110105" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="637101110105">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110105?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110105"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="5"/>
<attribute name="VALUE" value="637101110105"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101210103" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PS-3"/>
</gates>
<devices>
<device name="" package="667101210103">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101210103?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101210103"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="03"/>
<attribute name="VALUE" value="667101210103"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101240102" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PS"/>
</gates>
<devices>
<device name="" package="667101220102">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101240102?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101240102"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="02"/>
<attribute name="VALUE" value="667101240102"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120205" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="637101120205">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0B"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120205?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120205"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="5"/>
<attribute name="VALUE" value="637101120205"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101220102" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PS-1"/>
</gates>
<devices>
<device name="" package="667101220102">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101220102?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101220102"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="02"/>
<attribute name="VALUE" value="667101220102"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101110103" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm &lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT_LEFT"/>
</gates>
<devices>
<device name="" package="667101110103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101110103?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101110103"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="03"/>
<attribute name="VALUE" value="667101110103"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110307" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="637101110307">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0C"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110307?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110307"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="7"/>
<attribute name="VALUE" value="637101110307"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101110110" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm &lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT_LEFT"/>
</gates>
<devices>
<device name="" package="667101110110">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101110110?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101110110"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="10"/>
<attribute name="VALUE" value="667101110110"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101110107" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm &lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT_LEFT"/>
</gates>
<devices>
<device name="" package="667101110107">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101110107?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101110107"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="07"/>
<attribute name="VALUE" value="667101110107"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101210106" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PS"/>
</gates>
<devices>
<device name="" package="667101210106">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
<connect gate="G$1" pin="5" pad="A5 B5"/>
<connect gate="G$1" pin="6" pad="A6 B6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101210106?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101210106"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="06"/>
<attribute name="VALUE" value="667101210106"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101230106" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PS-1"/>
</gates>
<devices>
<device name="" package="667101210106">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
<connect gate="G$1" pin="5" pad="A5 B5"/>
<connect gate="G$1" pin="6" pad="A6 B6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101230106?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101230106"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="06"/>
<attribute name="VALUE" value="667101230106"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101210104" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PS-1"/>
</gates>
<devices>
<device name="" package="667101210104">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101210104?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101210104"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="04"/>
<attribute name="VALUE" value="667101210104"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101210109" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PS"/>
</gates>
<devices>
<device name="" package="667101210109">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
<connect gate="G$1" pin="5" pad="A5 B5"/>
<connect gate="G$1" pin="6" pad="A6 B6"/>
<connect gate="G$1" pin="7" pad="A7 B7"/>
<connect gate="G$1" pin="8" pad="A8 B8"/>
<connect gate="G$1" pin="9" pad="A9 B9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101210109?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101210109"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="09"/>
<attribute name="VALUE" value="667101210109"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101230110" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PS"/>
</gates>
<devices>
<device name="" package="667101210110">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="10" pad="A10 B10"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
<connect gate="G$1" pin="5" pad="A5 B5"/>
<connect gate="G$1" pin="6" pad="A6 B6"/>
<connect gate="G$1" pin="7" pad="A7 B7"/>
<connect gate="G$1" pin="8" pad="A8 B8"/>
<connect gate="G$1" pin="9" pad="A9 B9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101230110?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101230110"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="10"/>
<attribute name="VALUE" value="667101230110"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101230109" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PS-1"/>
</gates>
<devices>
<device name="" package="667101210109">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
<connect gate="G$1" pin="5" pad="A5 B5"/>
<connect gate="G$1" pin="6" pad="A6 B6"/>
<connect gate="G$1" pin="7" pad="A7 B7"/>
<connect gate="G$1" pin="8" pad="A8 B8"/>
<connect gate="G$1" pin="9" pad="A9 B9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101230109?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101230109"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="09"/>
<attribute name="VALUE" value="667101230109"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101220103" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PS"/>
</gates>
<devices>
<device name="" package="667101220103">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101220103?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101220103"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="03"/>
<attribute name="VALUE" value="667101220103"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101230105" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PS-3"/>
</gates>
<devices>
<device name="" package="667101210105">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
<connect gate="G$1" pin="5" pad="A5 B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101230105?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101230105"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="05"/>
<attribute name="VALUE" value="667101230105"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101210105" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PS"/>
</gates>
<devices>
<device name="" package="667101210105">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
<connect gate="G$1" pin="5" pad="A5 B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101210105?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101210105"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="05"/>
<attribute name="VALUE" value="667101210105"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101230104" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PS"/>
</gates>
<devices>
<device name="" package="667101210104">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101230104?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101230104"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="04"/>
<attribute name="VALUE" value="667101230104"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110110" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="637101110110">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110110?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101110110"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="10"/>
<attribute name="VALUE" value="637101110110"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120110" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header Crimp 5 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 16 A
&lt;br&gt;Working Voltage: 380 V
&lt;br&gt;Operating temperature: -40 °C up to +120 °C
&lt;br&gt;UL approval: E323964
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Glow-Wire Compliancy
&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o871475v209%20Family-Image-WR-Rasts-Male.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WTB_WR-RAST_MALE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WTB_WR-RAST_MALE&lt;/a&gt;&lt;p&gt;

Updated by Ella 2026-05-13 &lt;br&gt;
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="637101120110">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="0A"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120110?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16 A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="637101120110"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="10"/>
<attribute name="VALUE" value="637101120110"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101240103" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PS-1"/>
</gates>
<devices>
<device name="" package="667101220103">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101240103?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101240103"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="03"/>
<attribute name="VALUE" value="667101240103"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101210110" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PS-1"/>
</gates>
<devices>
<device name="" package="667101210110">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="10" pad="A10 B10"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
<connect gate="G$1" pin="5" pad="A5 B5"/>
<connect gate="G$1" pin="6" pad="A6 B6"/>
<connect gate="G$1" pin="7" pad="A7 B7"/>
<connect gate="G$1" pin="8" pad="A8 B8"/>
<connect gate="G$1" pin="9" pad="A9 B9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101210110?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101210110"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="10"/>
<attribute name="VALUE" value="667101210110"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101110106" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm &lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT_LEFT"/>
</gates>
<devices>
<device name="" package="667101110106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101110106?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101110106"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="06"/>
<attribute name="VALUE" value="667101110106"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101220104" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PS-3"/>
</gates>
<devices>
<device name="" package="667101220104">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101220104?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101220104"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="04"/>
<attribute name="VALUE" value="667101220104"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101240104" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PS-2"/>
</gates>
<devices>
<device name="" package="667101220104">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
<connect gate="G$1" pin="3" pad="A3 B3"/>
<connect gate="G$1" pin="4" pad="A4 B4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101240104?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101240104"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="04"/>
<attribute name="VALUE" value="667101240104"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101110108" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm &lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT_LEFT"/>
</gates>
<devices>
<device name="" package="667101110108">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101110108?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101110108"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="08"/>
<attribute name="VALUE" value="667101110108"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101120103" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm &lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT_LEFT-1"/>
</gates>
<devices>
<device name="" package="667101120103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101120103?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101120103"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="03"/>
<attribute name="VALUE" value="667101120103"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101210102" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PS-3"/>
</gates>
<devices>
<device name="" package="667101210102">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101210102?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101210102"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="02"/>
<attribute name="VALUE" value="667101210102"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101230102" prefix="J">
<description>&lt;b&gt;WR-RAST Female Housing IDC 2.50/5.00 mm&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870310v209%20Multi-WR-RAST2.5-667101210103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_FEMALE_HOUSING_IDC_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PS-2"/>
</gates>
<devices>
<device name="" package="667101210102">
<connects>
<connect gate="G$1" pin="1" pad="A1 B1"/>
<connect gate="G$1" pin="2" pad="A2 B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101230102?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101230102"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="02"/>
<attribute name="VALUE" value="667101230102"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101120105" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm &lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT_LEFT-1"/>
</gates>
<devices>
<device name="" package="667101120105">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101120105?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101120105"/>
<attribute name="PITCH" value="5 mm"/>
<attribute name="POLARITY" value="05"/>
<attribute name="VALUE" value="667101120105"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="667101110104" prefix="J">
<description>&lt;b&gt;WR-RAST Male Header IDC Vertical 2.50/5.00 mm &lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Rated Current: 4 A
&lt;br&gt;Working Voltage: 32 V / 250 V
&lt;br&gt;UL approval: E323964
&lt;br&gt;UL 94-V0
&lt;br&gt;Operating temperature: -40°C up to +110°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o870305v209%20Multi-WR-RAST2.5-667101110103.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_IDC_MALE_HEADER_IDC_VERTICAL_2_50_5_00_MM&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-12-12 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT_LEFT-1"/>
</gates>
<devices>
<device name="" package="667101110104">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CODING" value="OA"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/667101110104?ae"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="4A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value="667101110104"/>
<attribute name="PITCH" value="2.5 mm"/>
<attribute name="POLARITY" value="04"/>
<attribute name="VALUE" value="667101110104"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
