<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Coaxial Connectors - WR-RPSMA &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-11-05&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="63012052121509">
<description>&lt;b&gt;WR-RPSMA Straight SMA PCB THT Jack IP67</description>
</package>
<package name="63012002124503">
<description>&lt;B&gt;WR-RPSMA Straight</description>
</package>
<package name="63012242121508">
<description>&lt;b&gt;6.35SQ Flange Round Post Rear Mount Bulkhead for PCB 1.6mm</description>
</package>
<package name="63012042124504">
<description>&lt;B&gt;WR-RPSMA Straight Rear Mount Bulkhead</description>
</package>
<package name="63011042124502">
<description>&lt;b&gt;WR-RPSMA Right Angle Rear Mount Bulkhead</description>
</package>
<package name="63011052121510">
<description>&lt;b&gt;WR-RPSMA Right Angle PCB THT Jack IP67</description>
</package>
<package name="63012252111511">
<description>&lt;b&gt;WR-RPSMA PCB End Launch Jack IP67 for PCB 1.6 mm</description>
</package>
<package name="63011002124501">
<description>&lt;B&gt;WR-RPSMA Right Angle</description>
</package>
<package name="63012202124505">
<description>&lt;B&gt;WR-RPSMA Round Post for PCB 1.6mm</description>
</package>
<package name="63012242124506">
<description>&lt;B&gt;WR-RPSMA Round Post Rear Mount Bulkhead for PCB 1.6mm</description>
</package>
</packages>
<symbols>
<symbol name="JACK">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="63012052121509" prefix="J">
<description>&lt;b&gt;WR-RPSMA Straight SMA PCB THT Jack IP67 
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PTFE 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Nut Material Brass 
&lt;br&gt;Nut Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Lock Washer Material Brass 
&lt;br&gt;Lock Washer Plating Gold, min. 0.076µm over Nickel 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type RP SMA 
&lt;br&gt;Gender Jack 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C 
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~6 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o659740v209%20family-wr-rpsma-63012052121509.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o659740v209%20family-wr-rpsma-63012052121509.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/RPSMA_STRAIGHT_SMA_THT_JACK_IP67"&gt;https://www.we-online.com/catalog/en/RPSMA_STRAIGHT_SMA_THT_JACK_IP67&lt;/a&gt;&lt;p&gt;
Created by Ella Wu  2021-11-05&lt;br&gt;
2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="63012052121509">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/63012052121509.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="MIL-STD-350"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="63012052121509"/>
<attribute name="VALUE" value="63012052121509"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="63012002124503" prefix="J">
<description>&lt;b&gt;WR-RPSMA Straight
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PTFE 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.76µm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type RP SMA 
&lt;br&gt;Gender Jack 
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~18 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o122893v209%20WR-RPSMA_63012002124503.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o122893v209%20WR-RPSMA_63012002124503.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/WR-RPSMA_THT_63012002124503"&gt;https://katalog.we-online.com/en/em/WR-RPSMA_THT_63012002124503&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu  2019-11-04&lt;br&gt;
2019(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="63012002124503">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/63012002124503.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="63012002124503"/>
<attribute name="VALUE" value="63012002124503"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="63012242121508" prefix="J">
<description>&lt;b&gt;6.35SQ Flange Round Post Rear Mount Bulkhead for PCB 1.6mm
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PTFE 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Nut Material Brass 
&lt;br&gt;Nut Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Lock Washer Material Brass 
&lt;br&gt;Lock Washer Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type RP SMA 
&lt;br&gt;Gender Jack 
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~6GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o176659v209%20Family_WR-RPSMA_63012242121508.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o176659v209%20Family_WR-RPSMA_63012242121508.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/RPSMA_6.35_SQ_FLANGE_RP_RMBH/"&gt;https://www.we-online.com/catalog/en/RPSMA_6.35_SQ_FLANGE_RP_RMBH/&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu  2020-05-29&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="63012242121508">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/63012242121508.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="ORIENTATION-TYPE" value="End Launch "/>
<attribute name="PART-NUMBER" value="63012242121508"/>
<attribute name="VALUE" value="63012242121508"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="63012042124504" prefix="J">
<description>&lt;b&gt;WR-RPSMA Straight Rear Mount Bulkhead
&lt;br&gt;
&lt;br&gt;
RTICLE PROPERTIES 
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Panel Thickness 1.6-2.4 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PTFE 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.76µm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Nut Material Brass 
&lt;br&gt;Nut Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Lock Washer Material Brass 
&lt;br&gt;Lock Washer Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type RP SMA 
&lt;br&gt;Gender Jack 
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~18 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o122895v209%20WR-RPSMA_63012042124504.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o122895v209%20WR-RPSMA_63012042124504.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/WR-RPSMA_THT_63012042124504"&gt;https://katalog.we-online.com/en/em/WR-RPSMA_THT_63012042124504&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu  2019-11-04&lt;br&gt;
2019(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="63012042124504">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/63012042124504.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="63012042124504"/>
<attribute name="VALUE" value="63012042124504"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="63011042124502" prefix="J">
<description>&lt;b&gt;WR-RPSMA Right Angle Rear Mount Bulkhead
&lt;br&gt;
&lt;br&gt;
ARTICLE PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Panel Thickness 2.9 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PTFE 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.76µm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Nut Material Brass 
&lt;br&gt;Nut Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Lock Washer Material Brass 
&lt;br&gt;Lock Washer Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type RP SMA 
&lt;br&gt;Gender Jack 
&lt;br&gt;Orientation Type Right Angle 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~18 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o122891v209%20WR-RPSMA_63011042124502.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o122891v209%20WR-RPSMA_63011042124502.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/WR-RPSMA_THT_63011042124502"&gt;https://katalog.we-online.com/en/em/WR-RPSMA_THT_63011042124502&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu  2019-11-04&lt;br&gt;
2019(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="63011042124502">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/63011042124502.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="ORIENTATION-TYPE" value="Right Angle"/>
<attribute name="PART-NUMBER" value="63011042124502"/>
<attribute name="VALUE" value="63011042124502"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="63011052121510" prefix="J">
<description>&lt;b&gt;WR-RPSMA Right Angle PCB THT Jack IP67
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PTFE 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Nut Material Brass 
&lt;br&gt;Nut Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Lock Washer Material Brass 
&lt;br&gt;Lock Washer Plating Gold, min. 0.076µm over Nickel 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type RP SMA 
&lt;br&gt;Gender Jack 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C 
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~6 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o659748v209%20family-wr-rpsma-63011052121510.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o659748v209%20family-wr-rpsma-63011052121510.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_RPSMA_RIGHT_ANGLE_PCB_THT_IP67"&gt;https://www.we-online.com/catalog/en/WR_RPSMA_RIGHT_ANGLE_PCB_THT_IP67&lt;/a&gt;&lt;p&gt;
Created by Ella Wu  2021-11-05&lt;br&gt;
2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="63011052121510">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/63011052121510.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="MIL-STD-349"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="ORIENTATION-TYPE" value="Right Angle"/>
<attribute name="PART-NUMBER" value="63011052121510"/>
<attribute name="VALUE" value="63011052121510"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="63012252111511" prefix="J">
<description>&lt;b&gt;WR-RPSMA PCB End Launch Jack IP67 for PCB 1.6 mm 
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PTFE 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Nut Material Brass 
&lt;br&gt;Nut Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Lock Washer Material Brass 
&lt;br&gt;Lock Washer Plating Gold, min. 0.076µm over Nickel 

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type RP SMA 
&lt;br&gt;Gender Jack 

&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C 
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~6 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o659750v209%20family-wr-rpsma-63012252111511.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o659750v209%20family-wr-rpsma-63012252111511.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WR_RPSMA_PCB_END_LAUNCH_IP67_1_6MM"&gt;https://www.we-online.com/catalog/en/WR_RPSMA_PCB_END_LAUNCH_IP67_1_6MM&lt;/a&gt;&lt;p&gt;
Created by Ella Wu  2021-11-05&lt;br&gt;
2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="63012252111511">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/63012252111511.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="MIL-STD-351"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="ORIENTATION-TYPE" value="End Launch "/>
<attribute name="PART-NUMBER" value="63012252111511"/>
<attribute name="VALUE" value="63012252111511"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="63011002124501" prefix="J">
<description>&lt;b&gt;WR-RPSMA Right Angle
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PTFE 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.76µm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type RP SMA 
&lt;br&gt;Gender Jack 
&lt;br&gt;Orientation Type Right Angle 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C 
&lt;br&gt;&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~18 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o122889v209%20WR-RPSMA_63011002124501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o122889v209%20WR-RPSMA_63011002124501.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/WR-RPSMA_THT_63011002124501"&gt;https://katalog.we-online.com/en/em/WR-RPSMA_THT_63011002124501&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu  2019-11-04&lt;br&gt;
2019(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="63011002124501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/63011002124501.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="ORIENTATION-TYPE" value="Right Angle"/>
<attribute name="PART-NUMBER" value="63011002124501"/>
<attribute name="VALUE" value="63011002124501"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="63012242124506" prefix="J">
<description>&lt;b&gt;WR-RPSMA Round Post Rear Mount Bulkhead for PCB 1.6mm
&lt;br&gt;
&lt;br&gt;
RTICLE PROPERTIES 
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Panel Thickness 2-2.4 mm 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PTFE 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.76µm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Nut Material Brass 
&lt;br&gt;Nut Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;Lock Washer Material Brass 
&lt;br&gt;Lock Washer Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type RP SMA 
&lt;br&gt;Gender Jack 
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~18 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o122899v209%20WR-RPSMA_63012242124506.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o122899v209%20WR-RPSMA_63012242124506.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/WR-RPSMA_63012242124506"&gt;https://katalog.we-online.com/en/em/WR-RPSMA_63012242124506&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu  2019-11-04&lt;br&gt;
2019(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="63012242124506">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/63012242124506.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="63012242124506"/>
<attribute name="VALUE" value="63012242124506"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="63012202124505" prefix="J">
<description>&lt;b&gt;WR-RPSMA Round Post for PCB 1.6mm
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PTFE 
&lt;br&gt;Insulator Color White 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.76µm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.076µm over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type RP SMA 
&lt;br&gt;Gender Jack 
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~18 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o122897v209%20WR-RPSMA_63012202124505.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o122897v209%20WR-RPSMA_63012202124505.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/WR-RPSMA_63012202124505"&gt;https://katalog.we-online.com/en/em/WR-RPSMA_63012202124505&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu  2019-11-04&lt;br&gt;
2019(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="63012202124505">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/63012202124505.pdf"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="63012202124505"/>
<attribute name="VALUE" value="63012202124505"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
