<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Coaxial Connectors - SMA Connectors  - WR-SMA &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-02-10&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="60316002111357">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Right Angle Jack with THR Grounding Pins</description>
</package>
<package name="60312202114511">
<description>&lt;B&gt;WR-SMA PCB End Launch Jack Flat Tab with THT Grounding Pins 2.8 mm</description>
</package>
<package name="60312202114512">
<description>&lt;b&gt;WR-SMA PCB End Launch Jack Flat Tab for 1.1 mm</description>
</package>
<package name="60312102114506">
<description>&lt;B&gt;WR-SMA PCB SMT Jack Straight with THT Grounding Pins</description>
</package>
<package name="60311082111559">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Right Angle Jack, THT</description>
</package>
<package name="60312102114405">
<description>&lt;b&gt;WR-SMA PCB SMT Jack Straight</description>
</package>
<package name="60311052111534">
<description>&lt;b&gt;WR-SMA Right Angle PCB THT Jack IP67 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;THT, 4pins</description>
</package>
<package name="60312042111532">
<description>&lt;b&gt;WR-SMA Straight Rear Mount Bulkhead 11mm</description>
</package>
<package name="60312202114508">
<description>&lt;B&gt;WR-SMA PCB End Launch Jack Round Post 1.1 mm</description>
</package>
<package name="60312202111562">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Straight Jack, End Launch</description>
</package>
<package name="60312202111561">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Straight Jack, End Launch</description>
</package>
<package name="60314202124525">
<description>&lt;b&gt;WR-SMA PCB End Launch Plug Round Post 1.6 mm</description>
</package>
<package name="60312202114509">
<description>&lt;b&gt;WR-SMA PCB End Launch Jack Round Post 1.6 mm</description>
</package>
<package name="60311002111526">
<description>&lt;B&gt;WR-SMA SMA PCB THT Jack</description>
</package>
<package name="60312082111560">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Straight Jack, THT</description>
</package>
<package name="60312202111527">
<description>&lt;B&gt; WR-SMA SMA PCB End Launch Jack</description>
</package>
<package name="60312202114513">
<description>&lt;b&gt;WR-SMA PCB End Launch Jack Flat Tab 6.35 SQ Flange 1.6 mm</description>
</package>
<package name="60312252111535">
<description>&lt;b&gt;WR-SMA PCB End Launch Jack IP67 for PCB 1.6 mm
&lt;br&gt;&lt;br&gt;&lt;/b&gt;SMT</description>
</package>
<package name="60312872112545">
<description>&lt;b&gt;WR-SMA PCB Solderless</description>
</package>
<package name="60312202114514">
<description>&lt;B&gt;WR-SMA PCB End Launch Jack Flat Tab 1.6 mm</description>
</package>
<package name="60311002114501">
<description>&lt;B&gt;WR-SMA PCB THT Jack Right Angle</description>
</package>
<package name="60312862112552">
<description>&lt;b&gt;WR-SMA PCB Solderless</description>
</package>
<package name="60312242114510">
<description>&lt;b&gt;WR-SMA PCB End Launch Jack Round Post Rear Mount Bulkhead 1.6 mm</description>
</package>
<package name="60313002124523">
<description>&lt;B&gt;WR-SMA PCB THT Plug Right Angle</description>
</package>
<package name="60312042114504">
<description>&lt;b&gt;WR-SMA PCB THT Jack Straight Rear Mount Bulkhead</description>
</package>
<package name="60312002114503">
<description>&lt;B&gt;WR-SMA PCB THT Jack Straight</description>
</package>
<package name="60312052111533">
<description>&lt;B&gt;WR-SMA Straight PCB THT JACK IP67</description>
</package>
<package name="60312202111563">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Straight Jack, End Launch</description>
</package>
<package name="60311042114502">
<description>&lt;B&gt;WR-SMA PCB THT Jack Right Angle Rear Mount Bulkhead</description>
</package>
<package name="60314002124524">
<description>&lt;b&gt;WR-SMA PCB THT Plug Straight</description>
</package>
<package name="60312872112546">
<description>&lt;b&gt;WR-SMA PCB Solderless</description>
</package>
<package name="60312202114307">
<description>&lt;b&gt;WR-SMA PCB End Launch Jack SMT Edge Card 1.6 mm</description>
</package>
</packages>
<symbols>
<symbol name="JACK">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="PLUG">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="60316002111357" prefix="J">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt; Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt; Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humidity environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-10&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60316002111357">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 1.27"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60316002111357?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~12.4 GHz"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60316002111357"/>
<attribute name="SIZE" value="Right Angle Jack"/>
<attribute name="VALUE" value="60316002111357"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312202114511" prefix="J">
<description>&lt;b&gt;WR-SMA PCB End Launch &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humid environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_END_LAUNCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_END_LAUNCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312202114511">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 0.51 WIDE x 0.25 THK"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312202114511?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312202114511"/>
<attribute name="PCB-THICKNESS" value="2.8mm"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312202114511"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312202114512" prefix="J">
<description>&lt;b&gt;WR-SMA PCB End Launch &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humid environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_END_LAUNCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_END_LAUNCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312202114512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 0.51 WIDE x 0.25 THK"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312202114512?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312202114512"/>
<attribute name="PCB-THICKNESS" value="1.1mm"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312202114512"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312102114506" prefix="J">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humidity environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312102114506">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 1.27"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312102114506?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312102114506"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312102114506"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60311082111559" prefix="J">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt; Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt; Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humidity environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-10&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60311082111559">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 1.27"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60311082111559?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~6 GHz"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PANEL-THICKNESS" value="2.8mm"/>
<attribute name="PART-NUMBER" value="60311082111559"/>
<attribute name="SIZE" value="Right Angle Jack"/>
<attribute name="VALUE" value="60311082111559"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312102114405" prefix="J">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humidity environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312102114405">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 1.27"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312102114405?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312102114405"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312102114405"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60311052111534" prefix="J">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humidity environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60311052111534">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 1.27"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60311052111534?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~6 GHz"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PANEL-THICKNESS" value="2.8mm"/>
<attribute name="PART-NUMBER" value="60311052111534"/>
<attribute name="SIZE" value="Right Angle Jack"/>
<attribute name="VALUE" value="60311052111534"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312042111532" prefix="J">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humidity environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312042111532">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 1.27"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312042111532?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~6 GHz"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312042111532"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312042111532"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312202114508" prefix="J">
<description>&lt;b&gt;WR-SMA PCB End Launch &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humid environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_END_LAUNCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_END_LAUNCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312202114508">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 0.76"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312202114508?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312202114508"/>
<attribute name="PCB-THICKNESS" value="1.1mm"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312202114508"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312202111562" prefix="J">
<description>&lt;b&gt;WR-SMA PCB End Launch&lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humid environment
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_END_LAUNCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_END_LAUNCH&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-10&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312202111562">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 0.3"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312202111562?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312202111562"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312202111562"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312202111561" prefix="J">
<description>&lt;b&gt;WR-SMA PCB End Launch&lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humid environment
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_END_LAUNCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_END_LAUNCH&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-10&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312202111561">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 0.25"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312202111561?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312202111561"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312202111561"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60314202124525" prefix="J">
<description>&lt;b&gt;WR-SMA PCB End Launch &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humid environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_END_LAUNCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_END_LAUNCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60314202124525">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 0.76"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60314202124525?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60314202124525"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="SIZE" value="Straight Plug"/>
<attribute name="VALUE" value="60314202124525"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312202114509" prefix="J">
<description>&lt;b&gt;WR-SMA PCB End Launch &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humid environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_END_LAUNCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_END_LAUNCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312202114509">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 0.76"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312202114509?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312202114509"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312202114509"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60311002111526" prefix="J">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humidity environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60311002111526">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 1.27"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60311002111526?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~6 GHz"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60311002111526"/>
<attribute name="SIZE" value="Right Angle Jack"/>
<attribute name="VALUE" value="60311002111526"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312082111560" prefix="J">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt; Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt; Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humidity environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-10&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312082111560">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 1.27"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312082111560?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~6 GHz"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PANEL-THICKNESS" value="4.4mm"/>
<attribute name="PART-NUMBER" value="60312082111560"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312082111560"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312202111527" prefix="J">
<description>&lt;b&gt;WR-SMA PCB End Launch &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humid environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_END_LAUNCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_END_LAUNCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312202111527">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 0.76"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312202111527?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312202111527"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312202111527"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312202114513" prefix="J">
<description>&lt;b&gt;WR-SMA PCB End Launch &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humid environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_END_LAUNCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_END_LAUNCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312202114513">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 0.51 WIDE x 0.25 THK"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312202114513?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312202114513"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312202114513"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312252111535" prefix="J">
<description>&lt;b&gt;WR-SMA PCB End Launch &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humid environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_END_LAUNCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_END_LAUNCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312252111535">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312252111535?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~6 GHz"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PANEL-THICKNESS" value="4.7mm"/>
<attribute name="PART-NUMBER" value="60312252111535"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312252111535"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312872112545" prefix="J">
<description>&lt;b&gt;WR-SMA PCB Solderless &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt; Interface: MIL-STD-348
&lt;br&gt; Mating Cycle: 500 Cycles
&lt;br&gt; Impedance: 50Ω
&lt;br&gt; Insulation Resistance: 5000M Ω (min.)
&lt;br&gt; Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt; Network and communications
&lt;br&gt; RF Test and measurement equipment
&lt;br&gt; Industrial applications
&lt;br&gt; Electronic device

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o758568v209%20Family-WR-SMA%20PCB%20Solderless.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o758568v209%20Family-WR-SMA%20PCB%20Solderless.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/CM_SMA_CONNECTORS_PCB_SOLDERLESS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/CM_SMA_CONNECTORS_PCB_SOLDERLESS&lt;/a&gt;&lt;p&gt;
Created by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312872112545">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 0.51"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312872112545?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~27 GHz"/>
<attribute name="MOUNT" value="Solderless Compression"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312872112545"/>
<attribute name="PCB-THICKNESS" value="mm"/>
<attribute name="SIZE" value="CWP Microstrip Line"/>
<attribute name="VALUE" value="60312872112545"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60311002114501" prefix="J">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humidity environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60311002114501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 1.27"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60311002114501?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60311002114501"/>
<attribute name="SIZE" value="Right Angle Jack"/>
<attribute name="VALUE" value="60311002114501"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312202114514" prefix="J">
<description>&lt;b&gt;WR-SMA PCB End Launch &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humid environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_END_LAUNCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_END_LAUNCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312202114514">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 0.51 WIDE x 0.25 THK"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312202114514?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312202114514"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312202114514"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312862112552" prefix="J">
<description>&lt;b&gt;WR-SMA PCB Solderless &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt; Interface: MIL-STD-348
&lt;br&gt; Mating Cycle: 500 Cycles
&lt;br&gt; Impedance: 50Ω
&lt;br&gt; Insulation Resistance: 5000M Ω (min.)
&lt;br&gt; Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt; Network and communications
&lt;br&gt; RF Test and measurement equipment
&lt;br&gt; Industrial applications
&lt;br&gt; Electronic device

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o758568v209%20Family-WR-SMA%20PCB%20Solderless.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o758568v209%20Family-WR-SMA%20PCB%20Solderless.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/CM_SMA_CONNECTORS_PCB_SOLDERLESS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/CM_SMA_CONNECTORS_PCB_SOLDERLESS&lt;/a&gt;&lt;p&gt;
Created by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312862112552">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5 6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 0.25"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312862112552?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="Solderless End Lunch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312862112552"/>
<attribute name="PCB-THICKNESS" value="mm"/>
<attribute name="SIZE" value="CWP Microstrip Line"/>
<attribute name="VALUE" value="60312862112552"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312242114510" prefix="J">
<description>&lt;b&gt;WR-SMA PCB End Launch &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humid environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_END_LAUNCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_END_LAUNCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312242114510">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 0.76"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312242114510?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PANEL-THICKNESS" value="2.4mm"/>
<attribute name="PART-NUMBER" value="60312242114510"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312242114510"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60313002124523" prefix="J">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humidity environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60313002124523">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 1.27"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60313002124523?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60313002124523"/>
<attribute name="SIZE" value="Right Angle Plug"/>
<attribute name="VALUE" value="60313002124523"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312042114504" prefix="J">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humidity environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312042114504">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 1.27"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312042114504?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312042114504"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312042114504"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312002114503" prefix="J">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humidity environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312002114503">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 1.27"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312002114503?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312002114503"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312002114503"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312052111533" prefix="J">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humidity environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312052111533">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 1.27"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312052111533?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~6 GHz"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PANEL-THICKNESS" value="4.4mm"/>
<attribute name="PART-NUMBER" value="60312052111533"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312052111533"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312202111563" prefix="J">
<description>&lt;b&gt;WR-SMA PCB End Launch&lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humid environment
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_END_LAUNCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_END_LAUNCH&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-02-10&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312202111563">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 0.25"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312202111563?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312202111563"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312202111563"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60311042114502" prefix="J">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humidity environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60311042114502">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 1.27"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60311042114502?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~12.4 GHz"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60311042114502"/>
<attribute name="SIZE" value="Right Angle Jack"/>
<attribute name="VALUE" value="60311042114502"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60314002124524" prefix="J">
<description>&lt;b&gt;WR-SMA PCB THT/THR/SMT &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humidity environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o176646v209%20Family-WR-SMA%20PCB%20THT-THR-SMT.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_THT_THR_SMT&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60314002124524">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 1.27"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60314002124524?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60314002124524"/>
<attribute name="SIZE" value="Straight Plug"/>
<attribute name="VALUE" value="60314002124524"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312872112546" prefix="J">
<description>&lt;b&gt;WR-SMA PCB Solderless &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt; Interface: MIL-STD-348
&lt;br&gt; Mating Cycle: 500 Cycles
&lt;br&gt; Impedance: 50Ω
&lt;br&gt; Insulation Resistance: 5000M Ω (min.)
&lt;br&gt; Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt; Network and communications
&lt;br&gt; RF Test and measurement equipment
&lt;br&gt; Industrial applications
&lt;br&gt; Electronic device

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o758568v209%20Family-WR-SMA%20PCB%20Solderless.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o758568v209%20Family-WR-SMA%20PCB%20Solderless.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/CM_SMA_CONNECTORS_PCB_SOLDERLESS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/CM_SMA_CONNECTORS_PCB_SOLDERLESS&lt;/a&gt;&lt;p&gt;
Created by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312872112546">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 0.51"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312872112546?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~27 GHz"/>
<attribute name="MOUNT" value="Solderless Compression"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312872112546"/>
<attribute name="PCB-THICKNESS" value="mm"/>
<attribute name="SIZE" value="Strip Line"/>
<attribute name="VALUE" value="60312872112546"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60312202114307" prefix="J">
<description>&lt;b&gt;WR-SMA PCB End Launch &lt;/b&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50Ω
&lt;br&gt;Insulation Resistance: 5000MΩ(min.)
&lt;br&gt;Withstanding Voltage: 1000Vrms(min.)
&lt;br&gt;Ingress Protection: None l IP67
&lt;br&gt;Mating: Screw (Recommended by torque wrench tool)

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Network and communications
&lt;br&gt;RF Test and measurement equipment
&lt;br&gt;Industrial applications
&lt;br&gt;Electronic consumers and device
&lt;br&gt;Outdoor or humid environment

&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o122886v209%20Family-WR-SMA%20End%20Launch%20Connectors.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/COAX_SMA_CONNECTOR_PCB_END_LAUNCH/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/COAX_SMA_CONNECTOR_PCB_END_LAUNCH&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-10-10&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60312202114307">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø 0.76"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60312202114307?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~18 GHz"/>
<attribute name="MOUNT" value="End Launch"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 °C up to +165 °C"/>
<attribute name="PART-NUMBER" value="60312202114307"/>
<attribute name="PCB-THICKNESS" value="1.6mm"/>
<attribute name="SIZE" value="Straight Jack"/>
<attribute name="VALUE" value="60312202114307"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
